|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2025/118 |
| _unlogo | **Economic and Social Council** | Distr.: General27 August 2025Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**197th session**

Geneva, 11–14 November 2025

Item 4.8.9 of the provisional agenda

**1958 Agreement:**

**Consideration of draft amendments to existing**

**UN Regulations submitted by GRE**

Proposal for Supplement 10 to the 00 series of amendments to UN Regulation No. 149 (Road Illumination Devices)

 Submitted by the Working Party on Lighting and Light-Signalling[[1]](#footnote-2)\*

 The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its ninety-second session (ECE/TRANS/WP.29/GRE/92, para. 25). It is based on ECE/TRANS/WP.29/GRE/2025/8. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2025 sessions.

*Paragraph 4.11. and related subparagraphs,* renumber and amend to read:

“4.11. Testing of mechanical or electromechanical structures

 On headlamps or a system designed to provide alternately a driving-beam and a passing-beam, or a passing-beam and/or a driving-beam designed to become bend lighting, any mechanical, electromechanical or other device incorporated in the headlamp and lighting unit(s) for these purposes shall be so constructed that:

4.11.1. The device is robust enough to withstand 50,000 operations under normal conditions of use. In order to verify compliance with this requirement, the Technical Service responsible for approval tests may:

(a) Require the applicant to supply the equipment necessary to perform the test;

(b) Forego the test if the headlamp presented by the applicant is accompanied by a test report, issued by a Technical Service responsible for approval tests for headlamps of the same construction (assembly), confirming compliance with this requirement.

… ”

*Paragraph 5.3.1.4.4.2.,* amendto read:

“5.3.1.4.4.2. At least 3,100 cd shall be attained at point 50 V when the Class C passing-beam is activated, for systems producing passing-beam only or alternately producing passing-beam and driving-beam functions as described in paragraphs 4.11. and 4.11.4.”

1. \* In accordance with the programme of work of the Inland Transport Committee for 2025 as outlined in proposed programme budget for 2025 (A/79/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)