|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRBP/2025/11 |
| _unlogo | **Economic and Social Council** | Distr.: General4 December 2024Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Noise and Tyres**

**Eighty-first session**

Geneva, 18-21 February 2025

Item 6 (c) of the provisional agenda

**Tyres: UN Regulation No. 75 (Tyres for Motorcycles/Mopeds)**

 **Proposal for Supplement 21 to UN Regulation No. 75**

 **Submitted by the experts from the European Tyre and Rim Technical Organization[[1]](#footnote-2)\***

The text reproduced below was prepared by the experts from the European Tyre and Rim Technical Organization (ETRTO). The modifications to the existing text of the UN Regulation are marked in bold for new or strikethrough for deleted characters.

 **I. Proposal**

*Paragraph 2.1. (c)*, amend to read:

"(c) Category of use (normal tyre~~: for normal highway service~~; snow tyre, **special-use tyre,** moped tyre, all terrain ~~tyre~~ (AT) **tyre**~~, special tyre: for special application such as on- and off-road~~);"

*Second occurrence of footnote 2*, renumber as footnote 3:

"~~2~~ **3** See the explanatory figure in the appendix."

*Paragraphs 2.7., 2.8., 2.9., 2.10., 2.11., 2.12., 2.13., 2.15.,2.16., 2.17., 2.19. and 2.22.*, replace the reference to footnote 2 by a reference to footnote 3.

*Paragraph 2.14.*, amend to read:

"2.14. "*Principal ~~groove~~****grooves***" means the wide **tread** grooves ~~situated in the central zone of the tread~~**of the tyre**."

*Paragraph 2.20.5.*, amend to read:

"2.20.5.  **the nominal rim diameter;** ~~A conventional number "d" denoting the nominal diameter of the rim and corresponding to its diameter expressed either by code (numbers below 100) or in millimetres' (numbers above 100).~~"

*Paragraph 2.20.5.1.*, renumber as 2.21.1. and amend to read:

"2.~~20.5.~~**21.**1. **When the nominal rim diameter ("d" symbol) is expressed by code, the values of the "d" symbol expressed in millimetres** ~~The values in millimetres of the symbol "d" when indicated by a code~~ are as follows:

|  |  |
| --- | --- |
| *~~Symbol "d" indicated by one or two figures according to the nominal rim diameter~~****Nominal rim diameter code ("d" symbol)*** | *Value of* ***the*** *"d"* ***symbol expressed*** *in mm* |
| 4 | 102 |
| 5 | 127 |
| 6 | 152 |
| 7 | 178 |
| 8 | 203 |
| 9 | 229 |
| 10 | 254 |
| 11 | 279 |
| 12 | 305 |
| 13 | 330 |
| 14 | 356 |
| 15 | 381 |
| 16 | 406 |
| 17 | 432 |
| 18 | 457 |
| 19 | 483 |
| 20 | 508 |
| 21 | 533 |
| 22 | 559 |
| 23 | 584 |

"

*Paragraph 2.20.6.*, amend to read:

"2.20.6. The suffix "M/C" **after the nominal rim diameter** for tyres intended to be fitted on rims designed for ~~motorcycles~~**motor cycles as shown in the example in Annex 3**; this suffix is mandatory for tyres having a nominal rim diameter equivalent to code 13 (330 mm) or above**,** and optional for tyres with nominal rim diameter equivalent to code 12 (305 mm) or below. Tyres not intended to be fitted on rims designed for ~~motorcycles~~**motor cycles** shall not be marked with M/C."

*Paragraph 2.21.,* amend to read:

"2.21. "*Nominal rim diameter*~~(d)~~" means **a conventional number denoting** the diameter of the rim on which a tyre is designed to be ~~mounted.~~~~2~~ **mounted3; the diameter of the rim is expressed either by code (numbers below 100) or in millimetres (numbers above 100) but not both;**"

*Paragraph 2.24.,* amend to read:

"2.24. "*Measuring rim*" means the rim on which a tyre is required to be fitted for ~~size measurements~~ **the measurement of the tyre dimensions**."

*Paragraph 2.30.*, amend to read:

"2.30. "*Load****-****capacity index*" means a figure associated with the maximum load a tyre can carry at the speed corresponding to its speed-**category** symbol according to the operating conditions specified by the tyre manufacturer. A list of those indices and of the corresponding loads is given in ~~annex 4~~ **Annex 4** to this Regulation."

*Add new paragraphs 2.33. and 2.33.1.*, to read:

"**2.33. Category of use:**

**2.33.1. "*Normal tyre*" means a tyre intended for normal, on-road use;**"

*Paragraph 2.33. (former)*, renumber as 2.33.2.:

"2.33.**2.** "*Snow tyre*" means a tyre whose tread pattern, tread compound or construction is primarily designed to achieve in mud and/or snow conditions a performance better than that of a normal tyre with regard to its ability to initiate and control vehicle motion."

*Paragraph 2.34. (former)*, delete:

"~~2.34. "~~*~~MST~~*~~" means "multiservice tyre", suitable both on and off road.~~"

*Paragraph 2.35. (former)*, renumber as 2.33.4. and amend to read:

"2.~~35.~~**33.4.** "*Moped tyre*" means a tyre designed for the equipment of mopeds (**vehicles of** categories L1 and L2)."

*Paragraph 2.36. (former)*, renumber as 2.34. and amend to read

"2.~~36.~~**34.** "*~~Motor cycle~~* ***Motor-cycle*** *tyre*" means a tyre designed primarily for the equipment of motor cycles (**vehicles of** categories L3, L4 and L5). However, they may also equip mopeds (**vehicles of** categories L1 and L2) and light trailers (**vehicles of** category O1)."

*Paragraphs 2.37. to 2.37.6. (former)*, renumber as 2.35. to 2.35.6.

*Paragraph 2.38. (former)*, renumber as 2.33.5. and amend to read:

"2.~~38.~~**33.5.** ~~AT (all terrain) tyre:~~ **"*All terrain (AT) tyre*"** means a low-pressure tyre designed primarily for the equipment **of vehicles** of categories ~~L6~~ **L6** and ~~L7~~ **L7**."

*Paragraph 2.39. (former)*, renumber as 2.36. and amend to read:

"2.~~39.~~**36.** "*Service description*" means the association of the load-**capacity** index with a ~~speed category~~ **speed-category** symbol (for example, ~~72H);~~ **72H).**"

*Paragraph 2.40. (former)*, renumber as 2.33.3. and amend to read:

"2.~~40.~~**33.3.** "*Special****-use*** *tyre*" means a tyre intended for mixed use both on- and off-road or for other special duty. These tyres are primarily designed to initiate and control the vehicle motion in off-road conditions."

*Paragraph 3.1.5.1.,* amend to read:

"3.1.5.1. For tyres suitable for speeds above 240 km/h but below 270 km/h and identified with the letter code "V" within the **tyre-**size designation, the service description shall be marked within ~~parenthesis~~ **parentheses** and shall consist of the ~~load capacity~~ **load-capacity** index applicable at a speed of 210 km/h and the ~~speed category~~ **speed-category** symbol."

*Paragraph 3.1.5.2.,* amend to read:

"3.1.5.2. For tyres suitable for speeds above 270 km/h and identified with the letter code "Z" within the **tyre-**size designation, the service description shall be marked within ~~parenthesis~~ **parentheses** and shall consist of the ~~load capacity~~ **load-capacity** index applicable at a speed of 240 km/h and the ~~speed category~~ **speed-category** symbol."

*Paragraph 3.1.9.*, amend to read:

"3.1.9. The inscription of "M+S" or "M.S" or "M&S" if the tyre is classified in the category of use "snow tyre" or if the tyre is classified in the category of use ~~"special tyre"~~ **"special-use tyre"** when declared by the tyre manufacturer at paragraph 4.1.3. as complying also with the definition given in paragraph **2.33.2.;** **the** ~~2.33. The~~ inscription "DP" (i.e. Dual Purpose) is accepted as a permitted alternative;

"M+S" or "M.S" or "M&S" means "Mud and Snow";"

*Paragraph 3.1.10.*, amend to read:

"3.1.10. The inscription MST in the case of ~~multiservice~~ **special-use** tyres**; "MST" means "multiservice tyre"**."

*Paragraphs 4.1.3. and 4.1.3.1.*, amend to read:

"4.1.3. The category of use (normal, snow, **special-use,** moped, ~~all-terrain~~ **all terrain** (AT)~~, special~~);

4.1.3.1. For the tyres belonging to the category of use "special**-use** tyre", those which may bear the inscription **"**M+S**"** or **"**M.S**"** or **"**M&S**"**."

*Paragraph 4.1.9.*, amend to read:

"4.1.9. The ply-rating number of tyres for ~~motor cycle~~**motor-cycle** derivatives (see table 5 of ~~annex 5~~ **Annex 5** to this Regulation);~~2~~**4**"

*Footnote 2,* renumber as footnote 4:

"~~2~~**4** From the date of entry into force of Supplement 8 to this Regulation no new approvals for these tyres should be issued pursuant to UN Regulation No. 75. These tyre sizes are now included in UN Regulation No. 54."

*Paragraph 5.4.1.*, amend to read:

"5.4.1. A circle surrounding the letter "E" followed by the distinguishing number of the country which has granted approval;~~3~~**5**"

*Footnote 3,* renumber as footnote 5 and amend to read:

"~~3~~**5** **The distinguishing numbers of the Contracting Parties to the 1958 Agreement are reproduced in Annex 3 to the Consolidated Resolution on the Construction of Vehicles (R.E.3).** ~~1 for Germany, 2 for France, 3 for Italy, 4 for the Netherlands, 5 for Sweden, 6 for Belgium, 7 for Hungary, 8 for the Czech Republic, 9 for Spain, 10 for Serbia, 11 for the United Kingdom, 12 for Austria, 13 for Luxembourg, 14 for Switzerland, 15 (vacant), 16 for Norway, 17 for Finland, 18 for Denmark, 19 for Romania, 20 for Poland, 21 for Portugal, 22 for the Russian Federation, 23 for Greece, 24 for Ireland, 25 for Croatia, 26 for Slovenia, 27 for Slovakia, 28 for Belarus, 29 for Estonia, 30 (vacant), 31 for Bosnia and Herzegovina, 32 for Latvia, 33 (vacant), 34 for Bulgaria, 35 (vacant), 36 for Lithuania, 37 for Turkey, 38 (vacant), 39 for Azerbaijan, 40 for The former Yugoslav Republic of Macedonia, 41 (vacant), 42 for the European Union (Approvals are granted by its Member States using their respective ECE symbol), 43 for Japan, 44 (vacant), 45 for Australia, 46 for Ukraine, 47 for South Africa, 48 for New Zealand, 49 for Cyprus, 50 for Malta, 51 for the Republic of Korea, 52 for Malaysia, 53 for Thailand, 54 and 55 (vacant), 56 for Montenegro, 57 (vacant) and 58 for Tunisia. Subsequent numbers shall be assigned to other countries in the chronological order in which they ratify or accede to the Agreement Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, and the numbers thus assigned shall be communicated by the Secretary-General of the United Nations to the Contracting Parties to the Agreement.~~"

*Paragraph 6.1.1.2.*, amend to read:

"6.1.1.2. However, for types of tyres for which the **tyre-**size designation is shown in the first column of the tables in ~~annex 5~~ **Annex 5** to this Regulation, the section width shall be ~~allowed to be~~ that given opposite the tyre**-size** designation in the tables."

*Paragraph 6.1.2.2.*, amend to read:

"6.1.2.2. However, for types of tyres for which the **tyre-**size designation is shown in the first column of the tables in ~~annex 5~~ **Annex 5** to this Regulation, the outer diameter shall be ~~allowed to be~~ that given opposite the tyre**-size** designation in the tables."

*Paragraph 6.1.4.2.*, amend to read:

"6.1.4.2. It may exceed that value,

**(a) for sizes shown in Annex 5,** up to the value ~~shown in Annex 5 or~~ **specified for the respective tyre-size designation in the tables in Annex 5 and,**

**(b)** for sizes not included in Annex 5**,** by the following percentages, whereby the limits shall be rounded to the nearest millimetre (mm):

|  |  |
| --- | --- |
| **Category of use** |  |
| **Normal tyres, snow tyres and moped tyres** |  |
|  | **Rim diameter code 12 and below** | **8 %** |
|  | **Rim diameter code 13 and above** | **10 %** |
| **Special-use tyres** | **25 %** |

"

*Paragraphs 6.1.4.2.1. and 6.1.4.2.2.*, delete.

*Paragraph 6.1.5.1.*, amend to read:

"6.1.5.1. ~~The~~ **For sizes listed in** **Annex 5, the** outer diameter of a tyre must not be outside the values *D*min and *D*max specified **for the respective tyre-size designation in the tables** in Annex 5."

*Paragraph 6.1.5.2.1.*, amend to read:

"6.1.5.2.1. ~~For normal highway service tyres and snow tyres a~~

 ~~Rim diameter code 13 and above 0.97~~

 ~~Rim diameter codes up to 12 inclusive 0.93~~

 ~~For special service tyres 1.00~~

|  |  |
| --- | --- |
| **Category of use** | ***a*** |
| **Normal tyres, snow tyres and moped tyres** |  |
|  | **Rim diameter code 12 and below** | **0.93** |
|  | **Rim diameter code 13 and above** | **0.97** |
| **Special-use tyres** | **1.00** |

"

*Paragraph 6.1.5.2.2.*, amend to read:

"6.1.5.2.2 ~~For normal highway service tyres b~~

 ~~Rim diameter code 13 and above 1.07~~

 ~~Rim diameter codes up to 12 inclusive 1.10~~

 ~~For snow tyres and special service tyres 1.12~~

|  |  |
| --- | --- |
| **Category of use** | ***b*** |
| **Normal tyres and moped tyres** |  |
|  | **Rim diameter code 12 and below** | **1.10** |
|  | **Rim diameter code 13 and above** | **1.07** |
| **Snow tyres and special-use tyres** | **1.12** |

"

*Paragraph 6.2.1.1.*, amend to read:

"6.2.1.1. Where application is made for tyres identified by means of letter code "V" within the **tyre-**size designation and suitable for speeds over 240 km/h or for tyres identified by means of letter code "Z" within the **tyre-**size designation and suitable for speeds over 270 km/h (see paragraph 4.1.15.), the above load/speed test is carried out on one tyre at the load and speed conditions marked within parenthesis on the tyre (see paragraphs 3.1.5.1. and 3.1.5.2.). Another load/speed test must be carried out on a second tyre of the same type at the load and speed conditions, if any, specified as maximum by the tyre manufacturer (see paragraph 4.1.15.). For tyres identified by means of letter code "V'' within the **tyre-**size designation and suitable for speeds over 240 km/h, the maximum load specified by the manufacturer shall not exceed the maximum load rating indicated in paragraph ~~2.37.4.~~ **2.35.4.** with reference to the maximum speed specified by the manufacturer."

*Annex 1, item 4.2*, amend to read:

"4.2. Category of use: normal/snow**/special-use/**moped/all terrain (AT)~~/special~~ 2 "

*Annex 3, Example of the markings,* amend to read:

"

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | ↓ |  |  |  | ↓ |  |  |  | ↓ |  |  |  | ↓ |  |
| 100/80 B 18 **M/C** |  | *b* |  | 53 S |  | *b* |  | TUBELESS |  | *b* |  | M + S |  | *b* |
|  | ↑ |  |  |  | ↑ |  |  |  | ↑ |  |  |  | ↑ |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  | ↓ |  |  |  |  |  |  |  |  |  |
|  |  |  |  | 2503 |  | *b* |  |  |  |  |  |  |  |  |
|  |  |  |  |  | ↑ |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

*b* = 4 mm min."

*Annex 3,* amend to read:

"…

* Having a load capacity of 206 kg, corresponding to load-**capacity** index 53 in Annex 4 to this Regulation;
* ~~Of~~ **Having a** speed category ~~S (maximum speed~~ of 180 km/h (expressed by the ~~speed category~~ **speed-category** symbol S);

…

(a) The **tyre-**size designation~~, comprising the nominal section width, the nominal aspect ratio, the type-of-structure symbol (where applicable) and the nominal rim diameter~~ shall be grouped as shown in the above example: 100/80 B l8**M/C**;

(b) The load-**capacity** index and the ~~speed category~~ **speed-category** symbol shall be placed together near the **tyre-**size ~~designation. They~~ **designation; they** may either follow it or be placed above or below it;

(c) The markings "TUBELESS" and "REINFORCED" or "REINF" and "M + S" and "MST" and/or "MOPED" (or **"**CYCLOMOTEUR**"** or **"**CICLOMOTORE**"**) may be at a distance from the ~~size designation symbol.~~ **tyre-size designation;**

…"

*Annex 5,*

*Table 1(a), footnote 1*, amend to read:

"1 Normal ~~road (highway) service~~ **tyres**."

*Table 2, footnotes 1 and 2*, amend to read:

"1 Normal ~~highway service~~ **tyres**.

2 Special**-use** ~~service~~ **tyres** and snow tyres."

*Table 3, footnotes 1 to 5*, amend to read:

"1 ~~Tyres for normal highway service~~ **Normal tyres**.

2 ~~Tyres for special service~~ **Special-use tyres** and snow tyres.

3 ~~Tyres for normal highway service up to~~ **Normal tyres with a** speed category **less than or equal to** **150 km/h (speed-category symbol** **"**P**")** ~~inclusive~~.

4 ~~Tyres for normal highway service above~~ **Normal tyres with a** speed category **greater than or equal to** **160 km/h (speed-category symbol** ~~P~~ **"Q")** and snow tyres.

5 ~~Tyres for special service~~ **Special-use tyres**."

*Table 7,* amend to read:

"Table 7
**Motor-cycle tyres
Sizes and dimensions of American tyres**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Tyre****-****size designation\** | *Measuring rimwidth Code* | *Overall diameter (mm)* | *Section width* *(mm)* | *Maximum overall width(mm)* |
| *~~D.min~~* ***Dmin*** | *D* | *~~D.max~~* ***Dmax*** |
| MH90  | - | 21 | 1.85 | 682 | 686 | 700 | 80 | 89 |
| MJ90 | - | 18 | 2.15 | 620 | 625 | 640 | 89 | 99 |
| MJ90 | - | 19 | 2.15 | 645 | 650 | 665 |
| ML90 | - | 18 | 2.15 | 629 | 634 | 650 | 93 | 103 |
| ML90 | - | 19 | 2.15 | 654 | 659 | 675 |
| MM90 | - | 19 | 2.15 | 663 | 669 | 685 | 95 | 106 |
| MN90 | - | 18 | 2.15 | 656 | 662 | 681 | 104 | 116 |
| MP90 | - | 18 | 2.15 | 667 | 673 | 692 | 108 | 120 |
| MR90 | - | 18 | 2.15 | 680 | 687 | 708 | 114 | 127 |
| MS90 | - | 17 | 2.50 | 660 | 667 | 688 | 121 | 134 |
| MT90 | - | 16 | 3.00 | 642 | 650 | 672 | 130 | 144 |
| MT90 | - | 17 | 3.00 | 668 | 675 | 697 |
| MU90 | - | 15~~M/C~~ | 3.50 | 634 | 642 | 665 | 142 | 158 |
| MU90 | - | 16 | 3.50 | 659 | 667 | 690 |
| MV90 | - | 15~~M/C~~ | 3.50 | 643 | 651 | 675 | 150 | 172 |
| MP85 | - | 18 | 2.15 | 654 | 660 | 679 | 108 | 120 |
| MR85 | - | 16 | 2.15 | 617 | 623 | 643 | 114 | 127 |
| MS85 | - | 18 | 2.50 | 675 | 682 | 702 | 121 | 134 |
| MT85 | - | 18 | 3.00 | 681 | 688 | 709 | 130 | 144 |
| MU85 | - | 16~~M/C~~ | 3.50 | 650 | 658 | 681 | 142 | 158 |
| MV85 | - | 15~~M/C~~ | 3.50 | 627 | 635 | 658 | 150 | 172 |

\*~~If the~~ **The** suffix "M/C" ~~is not already part of the tyre size designation, it~~ may be added optionally as part of the ~~tyre size~~ **tyre-size** designation (e.g. ~~4.00-5 M/C~~ **MH90 - 21 M/C**); this is recommended for tyres having a nominal rim diameter equivalent to code 13 (330 mm) or above. **Tyres in bias-belted construction shall be identified by the letter "B" in place of "-" (e.g. MM90 B 19 M/C).**"

*Table 8, headings,* replace "Tyres for all terrain vehicles (AT)" and "Tyres for all terrain vehicles (AT tyres)" by "All terrain (AT) tyres"

*Annex 7, paragraphs 2.2.1. to 2.2.3.,* amend to read:

"2.2.1. The maximum load rating ~~equated~~**corresponding** to the ~~Load Capacity Index~~ **load-capacity index** for tyres with **a** speed **category less than or equal to 210 km/h (speed-category symbol "H")**~~symbols up to H inclusive~~;

2.2.2. The maximum load rating associated with a maximum **operating** speed of 240 km/h for tyres with speed**-category** symbol "V" (see paragraph ~~2.37.3.~~ **2.35.3.** of this Regulation);

2.2.3. The maximum load rating associated with a maximum **operating** speed of 270 km/h for tyres with speed-**category** symbol"W" (see paragraph ~~2.37.5.~~ **2.35.5.** of this Regulation);"

*Annex 8,*

*Table "Table load capacities at various speeds"*, replace "Speed Symbol" by "Speed-Category Symbol".

*"Table for all terrain tyres (AT) with speed symbol "F"",* rename to "Table for all terrain **(AT)** tyres ~~(AT)~~ with speed**-category** symbol "F"".

*Annex 9, paragraph 4.1, table*, amend to read:

"

|  |  |
| --- | --- |
| *Speed****-****Category* ***Symbol*** | *H dyn (mm)* |
|  | *Category of Use:Normal* | *Category of Use:Snow and special****-use*** |
| P/Q/R/S | *H* × 1.10 | *H* × 1.15 |
| T/U/H | *H* × 1.13 | *H* × 1.18 |
| ~~Over 210 km/h~~ **V/W** | *H* × 1.16 | ***H* × 1.21** |

"

 **II. Justification**

1. A generic reference to the Consolidated Resolution on the Construction of Vehicles (R.E.3) is given in footnote 5.
2. It is proposed to align the categories of use to "normal tyre", "snow tyre" and "special-use tyre" in line with UN Regulations Nos. 30 and 54, to introduce a definition of "normal tyre" and consequently make use of the terms "snow tyre" and "special-use tyre" that are already defined.
3. Annex 5, Table 7 does not present the tyre-size designations in a consistent way and does not consider that there may be tyres with bias-belted structure and an alphanumeric tyre-size designation (which is allowed in the applicable industry standard). It is proposed to reformat the table and present the tyre-size designations in a consistent way and to provide explicitly that tyre-size designations from this table may also be used for tyres in bias-belted structure.
4. It is proposed to include the suffix "M/C" that is defined as mandatory for motor-cycle tyres with rim diameter code 13 and above in the figure illustrating the sidewall markings in Annex 3 and to present the markings in a clearer way.
5. It is proposed to add provisions for the dimensional requirements of moped tyres.
6. It is proposed to add a factor for the centrifugal radius of snow tyres and special-use tyres with a speed category above 210 km/h.
7. It is proposed to give the footnotes in the main body of the regulation an unequivocal number to avoid confusion when referencing to a particular footnote.
8. It is proposed to include several editorial corrections to increase the consistency of the text (e.g. consistent use of the terms defined in section 2, such as "tyre-size designation", "load-capacity index", "speed-category symbol")

1. \* In accordance with the programme of work of the Inland Transport Committee for 2025 as outlined in proposed programme budget for 2025 (A/79/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)