|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2025/159 |
| _unlogo | **Economic and Social Council** | Distr.: General1 September 2025Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**197th session**

Geneva, 11–14 November 2025

Items 4.3.1. of the provisional agenda

**1958 Agreement:**

**Development of the International Whole
Vehicle Type Approval (IWVTA) system**

 Proposal for the 08 series of amendments to UN Regulation No. 0 (IWVTA)

 Submitted by the Informal Working Group on the International Whole Vehicle Type Approval[[1]](#footnote-2)\*

The text reproduced below was considered by the World Forum for Harmonization of Vehicle Regulations at its 196th session, held in June 2025 (ECE/TRANS/WP.29/1186, para. 59). It is based on WP.29-196-22. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and the Administrative Committee of the 1958 Agreement (AC.1) for consideration and vote at their November 2025 sessions.

.

 *Paragraphs 4.6., amend to read:*

“4.6. (Reserved)”

 *Insert new paragraphs 12.13. and 12.14.,* to read:

“12.13. As from the official date of entry into force of the 08 series of amendments, no Contracting Party applying this UN Regulation shall refuse to grant or refuse to accept an IWVTA issued pursuant to this UN Regulation as amended by the 08 series of amendments.

12.14. As from 1 September 2026, Contracting Parties applying this UN Regulation shall not be obliged to accept type approvals to any of the preceding series of amendments, first issued after 1 September 2026.”

*Annex 4, Part A, Section I (List of requirements for U-IWVTA),* amend to read:

“

| *Topic* | *UN Regulation1* | *Series of amendments2* |
| --- | --- | --- |
| Vehicles with regard to electromagnetic compatibility | 10 | 06 |
| Vehicles with regard to door latches and door retention components  | 11 | 04 |
| Vehicles with regard to the protection of the driver against the steering mechanism in the event of impact | 12 | 05 |
| Brakes of M1 and N1 vehicles | 13-H | 01 |
| Vehicles with regard to safety-belt anchorages | 14 | 09 |
| Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems  | 16 | 09 |
| Vehicles with regard to the seats, their anchorages and any head restraints | 17 | 11 |
| Vehicles with regard to their interior fittings | 21 | 01 |
| Vehicles with regard to their external projections | 26 | 04 |
| Audible warning devices and of motor vehicles with regard to their audible signals | 28 | 00 |
| Pneumatic tyres for motor vehicles and their trailers (Tyres should be type approved to UN Regulation No. 30 or UN Regulation No. 54.) | 30 | 02 |
| Vehicles with regard to the prevention of fire risks | 34 | 04 |
| The speedometer and odometer equipment including installation | 39 | 01 |
| Safety glazing materials and their installation on vehicles | 43 | 01 |
| Devices for indirect vision including installation | 46 | 06 |
| Installation of lighting and light-signaling devices | 48 | 08 |
| Motor vehicles having at least four wheels with regard to their sound emissions | 51 | 03 |
| Pneumatic tyres for commercial vehicles and their trailers (Tyres should be type approved to UN Regulation No. 30 or UN Regulation No. 54.) | 54 | 00 |
| Rear Underrun Protective Devices (RUPDs) and the installation of a RUPD of an approved type, Rear Underrun Protection (RUP) | 58 | 03 |
| A temporary-use spare unit, run-flat tyres | 64\* | 03 |
| Vehicles with regard to steering equipment | 79 | 04 |
| Internal combustion engines or electric drive trains intended for the propulsion of motor vehicles of categories M and N with regard to the measurement of the net power and the maximum 30 minutes power of electric drive trains (Engine power) | 85 | 00 |
| Protection of occupants in the event of a frontal collision | 94 | 04 |
| Protection of occupants in the event of a lateral collision | 95 | 05 |
| Vehicles with regard to specific requirements for the electric power train  | 100\* | 03 |
| Vehicles with regard to the installation of specific components for the use of CNG and/or LNG in their propulsion system | 110\* | 06 |
| Tyres with regard to rolling sound emissions and/or to adhesion on wet surfaces and/or to rolling resistance | 117 | 04 |
| Vehicles with regard to the location and identification of hand controls, tell-tales and indicators | 121 | 01 |
| Motor vehicles with regard to the forward field of vision of the motor vehicle driver | 125 | 03 |
| Motor vehicles with regard to their pedestrian safety performance | 127 | 04 |
| Enhanced Child Restraint Systems used on board of motor vehicles (only in as much as it relates to built-in "*specific vehicle booster seats*" but not covering standalone child seats) | 129\* | 04 |
| Motor vehicles with regard to the safety related performance of hydrogen-fuelled vehicles | 134\* | 00 |
| Vehicles with regard to their Pole Side Impact performance | 135 | 02 |
| Passenger cars in the event of a frontal collision with focus on the restraint system | 137 | 02 |
| Quiet Road Transport Vehicles with regard to their reduced audibility | 138\* | 02 |
| Brake assist systems | 139 | 00 |
| Electronic stability control systems | 140 | 00 |
| Tyre pressure monitoring systems | 141 | 01 |
| Tyre installation  | 142 | 01 |
| WLTP | 154 | 03 |
| The protection of motor vehicles against unauthorized use (Locking system) | 161 | 00 |
| Immobilizers | 162\* | 00 |
| Vehicle alarm system | 163\* | 00 |
| Notes:1 If a UN Regulation number is followed by an asterisk "\*" this indicates that the respective requirement applies only if the corresponding system is fitted to the vehicle. This then means that for the purpose of a U-IWVTA both vehicles with or without this system are acceptable. However, where the system is fitted to the vehicle, the requirement applies. The same also applies to systems not identified by "\*" where it can be demonstrated that the corresponding requirements are not applicable to the IWVTA type.2 The entry is understood as the required minimum, i.e. including all supplements in force at the time the approval is issued. Approvals to any later versions have to be equally accepted in accordance with paragraph 13.3. of this Regulation.3 All component lamp/signalling approvals are required under UN Regulation No. 48, therefore these approvals are not mentioned under UN Regulation No. 0.4 The series of amendments indicated in Annex 4 is without prejudice to the transitional provisions in the respective series of UN Regulations. (See UN Regulation No. 0, para. 12.2, and 13.1).” |

1. \* In accordance with the programme of work of the Inland Transport Committee for 2023 as outlined in proposed programme budget for 2024 (A/78/6 (Sect. 20), table 20.5), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)