Proposal for amendments to ECE/TRANS/WP.29/GRVA/2025/9

I. Proposal

*Paragraph 4.4.2.,* shall be deleted (Paras 4.4 and 4.4.1 reproduced for context information):

4.4. There shall be affixed, conspicuously and in a readily accessible place specified on the approval form, to every vehicle conforming to a vehicle type approved under this UN Regulation, an international approval mark conforming to the model described in Annex 2, consisting of either:

4.4.1. A circle surrounding the letter “E” followed by:

(a) The distinguishing number of the country which has granted approval; and

(b) The number of this Regulation, followed by the letter “R”, a dash and the approval number to the right of the circle prescribed in this paragraph;

~~Or,~~

~~4.4.2. An oval surrounding the letters “UI” followed by the Unique Identifier.~~

*Paragraphs 6.2.1.1.,* amend to read:

“6.2.1.1. The full ELKS function shall be automatically and fully reinstated upon a new initiation of the powertrain#.

**A new engine start (or run cycle) which is performed automatically, e.g. the operation of a stop/start system, shall not be considered an “initiation of the powertrain” wherever that term is used in this Regulation.”**

Insert new *footnote #*, to read:

**#As defined in Mutual Resolution No. 2 (M.R.2) of the 1958 and the 1998 Agreements containing vehicle propulsion system definitions, see document ECE/TRANS/WP.29/1121.**

II. Justification

. This proposal aims to insert provisions in paragraph 6.2.1.1 aligned with text under consideration by GRVA.