Proposal for corrigendum to Supplement 1 to the 01 Series of Amendments to UN Regulation No. 118 (Fire resistance of interior materials)(ECE/TRANS/WP.29/2024/112)

Submitted by the Working Party on General Safety Provisions

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 127th session (ECE/TRANS/WP.29/GRSG/106, para. 34). It is based on ECE/TRANS/WP.29/GRSG/2024/33, not amended. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2024 sessions and GRSG recommends that the World Forum for Harmonization of Vehicle Regulations (WP.29) and the Administrative Committee of the 1958 Agreement (AC.1) adopt ECE/TRANS/WP.29/2024/112 together with the proposals below:

*Annex 5,*

*Example 2*, amend to read:

…

V

The symbol ~~and or~~ indicates that the component fulfils the requirements in paragraph 6.2.2.

The symbol indicates an approval as a complete device such as seats, separation walls, etc.

**CD**

The additional symbols are only used if applicable.

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**