Corrigendum for ECE/TRANS/WP.29/GRSG/2025/10, revision 8 to the Consolidated Resolution on the Construction of Vehicles

Submitted by the experts of OICA

The text reproduced below was prepared by the experts from OICA to clarify the definition of bi-directional vehicle. The modifications to the document ECE/TRANS/WP.29/GRSG/2025/10 are marked in bold for new characters and strikethrough for deleted characters.

 I. Proposal

*Paragraphs 1.18 and 1.19*. amend to read:

"1.18. “Bidirectional vehicle" means a vehicle that can operate in two opposite forward directions **in successive journeys**.

1.19. “Forward direction (of a ~~vehicle~~ **journey**)" means the direction that is intended to be used as the **vehicle** main travelling direction ~~of~~ **for** the ~~vehicle~~ **journey**."

 II. Justification

1. A timing context is added to clarify both definitions.