|  |  |  |
| --- | --- | --- |
|  | ECE/TRANS/WP.29/GRPE/2025/3 | |
| _unlogo | **Economic and Social Council** | Distr.: General  13 January 2025  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Pollution and Energy**

**Ninety second session**

Geneva, 25–28 March 2025

Item 3(a) of the provisional agenda

**Light vehicles:  
UN Regulations Nos. 68 (Measurement of the maximum speed,  
including electric vehicles), 83 (Emissions of M1 and N1 vehicles),  
101 (CO2 emissions/fuel consumption),   
103 (Replacement pollution control devices) and   
154 (Worldwide harmonized Light vehicles Test Procedures (WLTP))**

Proposal for a new Supplement to the 01 series of amendments to UN Regulation No. 154 (WLTP)

Submitted by the experts from the International Organization of Motor Vehicle Manufacturers [[1]](#footnote-2)\*

This document aims to propose a new Supplement to the 01 series of amendments to UN Regulation No. 154, as a consolidated version. This is a clean version.

Uniform provisions concerning the approval of light duty passenger and commercial vehicles with regards to criteria emissions, emissions of carbon dioxide and fuel consumption and/or the measurement of electric energy consumption and electric range (WLTP)

Contents

*Page[[2]](#footnote-3)*

Regulation

1. Scope 5

2. Abbreviations 5

3. Definitions 7

4. Application for approval 18

5. Approval 19

6. Specifications and tests 22

7. Modification and extension of the type approval 39

8. Conformity of production (COP) 41

9. Penalties for non-conformity of production 48

10. Production definitively discontinued 49

11. Special provisions 49

12. Transitional provisions 49

13. Names and addresses of Technical Services responsible for conducting approval tests, and of Type Approval Authorities 49

Appendix

1. Type 1 test CoP verification for specific vehicle types 50

2. Verification of conformity of production for Type 1 test - statistical method 54

3. Run-in test procedure to determine run-in factors 63

4. Conformity of production for Type 4 test 67

5. Devices for monitoring on board the vehicle the consumption of fuel and/or electric energy 69

6. Requirements for vehicles that use a reagent for the exhaust after-treatment system 72

Annexes Part A

A1. Engine and vehicle characteristics and information concerning the conduct of tests 78

Appendix

1. WLTP Test Report 98

2. WLTP Road Load Test Report 122

3. WLTP Test Sheet 130

4. Evaporative Emissions Test Report 133

A2. Communication 136

A3. Arrangements of the approval mark 152

Annexes Part B

B1. Worldwide light-duty test cycles (WLTC) 155

B2. Gear selection and shift point determination for vehicles equipped with manual transmissions 214

B3. Specifications of reference fuels 229

B4. Road load and dynamometer setting 240

B5. Test equipment and calibrations 287

B6. Type 1 test procedures and test conditions 324

Appendix

1. Emissions test procedure for all vehicles equipped with periodically regenerating systems 348

2. Test procedure for rechargeable electric energy storage system monitoring 353

3. Calculation of gas energy ratio for gaseous fuels (LPG and NG/biomethane) 358

B6a. Ambient Temperature Correction Test for the determination of CO2 emissions under representative regional temperature conditions 359

B7. Calculations 365

B8. Pure electric, hybrid electric and compressed hydrogen fuel cell hybrid vehicles 394

Appendix

1. REESS state of charge profile 464

2. REESS energy change-based correction procedure 469

3. Determination of REESS current and REESS voltage for NOVC-HEVs, OVC-HEVs, PEVs and NOVC-FCHVs 478

4. Preconditioning, soaking and REESS charging conditions of PEVs and OVC-HEVs 480

5. Utility factors (UF) for OVC-HEVs 482

6. Selection of driver-selectable modes 483

7. Fuel consumption measurement of compressed hydrogen fuel cell hybrid vehicles 489

8. Calculation of additional values required for checking the Conformity of Production of electric energy consumption of PEVs and OVC-HEVs 492

Annexes Part C

C1. (Reserved) 496

C2. (Reserved) 496

C3. Type 4 test - Determination of evaporative emissions from vehicles fuelled with petrol 497

C4. Type 5 test – Durability 522

Appendix

1. Reserved 525

2. Reserved 526

3. Standard Road Cycle (SRC) 527

4. Special requirements for Hybrid Vehicles 530

C5. On-Board Diagnostics (OBD) for motor vehicles 531

Appendix

1. Functional aspects of On-Board Diagnostic (OBD) systems 539

Introduction

The intention of this Regulation is to establish uniform provisions concerning the approval of motor vehicles with regard to the emissions of light-duty vehicles based on the new World harmonized Light vehicle Test Procedure (WLTP) included in UN GTR No. 15 and the updated Evaporative Emissions test procedure (Type 4 test) which has been developed in UN GTR No. 19. It will enable Contracting Parties (CPs) to issue and accept approvals based on these new type approval tests.

The WLTP Type 1 test replaces both the current Type 1 test in UN Regulation No. 83 and UN Regulation No. 101, whilst the updated Evaporative Emissions test procedure (Type 4 test) replaces that currently in UN Regulation No 83.

In addition, this new Regulation includes an update to the Type 5 test for verifying the durability of pollution control devices and updated On-Board Diagnostic (OBD) requirements. These updates are in order to reflect the changes from the previous NEDC based Type 1 test to the new WLTP Type 1 test.

The 00 series of this Regulation covers two sets of requirements – termed Level 1A and Level 1B. Level 1A is based on a four phase test cycle (Low, Medium, High and Extra-High), whilst Level 1B is based on a three phase test cycle (Low, Medium and High), with different type 1 limits applying to these different levels. The majority of the regulatory text is applicable to both Level 1A and Level 1B. Where the requirements are specific to either Level 1A or Level 1B the relevant sections are labelled accordingly. This series of amendments covers regional requirements and does not require mutual recognition by other Contracting Parties.

The 01 series of this Regulation includes a harmonised procedure which contains the most stringent procedures/limits which shall be subject to full mutual recognition. A type approval to the 01 series shall therefore be accepted by all CPs having adopted this Regulation.

**1. Scope**

This Regulation applies to the type approval of vehicles of categories M1 with a reference mass not exceeding 2,610 kg and vehicles of categories M2 and N1 with a reference mass not exceeding 2,610 kg and a technical permissible maximum laden mass not exceeding 3,500 kg with regard to the WLTP Type 1 test for emissions of gaseous compounds, particulate matter, particle number and to emissions of carbon dioxide and fuel consumption and/or the measurement of electric energy consumption and electric range and to the Type 4 test on evaporative emissions.

In addition, this Regulation lays down rules for verifying the durability of pollution control devices and On-Board Diagnostic (OBD) systems.

At the manufacturer's request, type approval granted under this Regulation may be extended from vehicles mentioned above to vehicles of categories M1 with a reference mass not exceeding 2,840 kg and vehicles of categories M2 and N1 with a reference mass not exceeding 2,840 kg and a technical permissible maximum laden mass not exceeding 3,500 kg and which meet the conditions laid down in this Regulation.

OVC-FCHVs are out of the scope of this Regulation.

**2. Abbreviations**

2.1. General abbreviations

|  |  |  |
| --- | --- | --- |
| AC | Alternating current | |
| APF | Assigned permeability factor | |
| BWC  CD | Butane working capacity  Charge-Depleting | |
| CFD | Computational fluid dynamics | |
| CFV | Critical flow venturi | |
| CFO | Critical flow orifice | |
| CLA  CS | Chemiluminescent analyser  Charge-Sustaining | |
| CVS | Constant volume sampler | |
| DC | Direct current | |
| EAF | Sum of ethanol, acetaldehyde and formaldehyde | |
| ECD | Electron capture detector | |
| ET | Evaporation tube | |
| Extra High2 | Class 2 WLTC extra high speed phase | |
| Extra High3 | Class 3 WLTC extra high speed phase | |
| FCHV | Fuel cell hybrid vehicle | |
| FID | Flame ionization detector | |
| FSD | Full scale deflection | |
| GC | Gas chromatograph | |
| GFV | Gas Fuelled Vehicle | |
| HEPA | High efficiency particulate air (filter) | |
| HFID | Heated flame ionization detector | |
| High2 | Class 2 WLTC high speed phase | |
| High3a | Class 3a WLTC high speed phase | |
| High3b | Class 3b WLTC high speed phase | |
| ICE | Internal combustion engine | |
| LoD | Limit of detection | |
| LoQ | Limit of quantification | |
| Low1 | Class 1 WLTC low speed phase | |
| Low2 | Class 2 WLTC low speed phase | |
| Low3 | Class 3 WLTC low speed phase | |
| Medium1 | Class 1 WLTC medium speed phase | |
| Medium2 | Class 2 WLTC medium speed phase | |
| Medium3a | Class 3a WLTC medium speed phase | |
| Medium3b | Class 3b WLTC medium speed phase | |
| LC | Liquid chromatography | |
| LPG | Liquefied petroleum gas | |
| NDIR | Non-dispersive infrared (analyser) | |
| NDUV | Non-dispersive ultraviolet | |
| NG/biomethane | Natural gas/biomethane | |
| NMC | Non-methane cutter | |
| NOVC-FCHV | Not off-vehicle charging fuel cell hybrid vehicle | |
| NOVC  NOVC-HEV | Not off-vehicle charging  Not off-vehicle charging hybrid electric vehicle | |
| OBD | On-board Diagnostics | |
| OBFCM | On-board fuel and/or energy consumption monitoring | |
| OVC-FCHV | Off-vehicle charging fuel cell hybrid vehicle | |
| OVC-HEV | Off-vehicle charging hybrid electric vehicle | |
| Pa | Particulate mass collected on the background filter | |
| Pe | Particulate mass collected on the sample filter | |
| PAO | Poly-alpha-olefin | |
| PCF | Particle pre-classifier | |
| PCRF | Particle concentration reduction factor | |
| PDP | Positive displacement pump | |
| PER | Pure electric range | |
| PF | Permeability factor | |
| PM | Particulate matter emissions | |
| PN | Particle number emissions | |
| PNC | Particle number counter | |
| PND1 | First particle number dilution device | |
| PND2 | Second particle number dilution device | |
| PTS | Particle transfer system | |
| PTT | Particle transfer tube | |
| QCL-IR | Infrared quantum cascade laser | |
| RCDA | Charge-depleting actual range | |
| RCB | REESS charge balance | |
| REESS | Rechargeable electric energy storage system | |
| RRC | Rolling resistance coefficient | |
| SHED | Sealed housing evaporative determination | |
| SSV | Subsonic venturi | |
| UBE | | Usable Battery (REESS) Energy | |
| USFM | | Ultrasonic flow meter | |
| VH | | Vehicle High | |
| VL | | Vehicle Low | |
| VPR | | Volatile particle remover | |
| WLTC | Worldwide light-duty test cycle | |

2.2. Chemical symbols and abbreviations

|  |  |
| --- | --- |
| C1 | Carbon 1 equivalent hydrocarbon |
| CH4 | Methane |
| C2H6 | Ethane |
| C2H5OH | Ethanol |
| C3H8 | Propane |
| CH3CHO | Acetaldehyde |
| CO | Carbon monoxide |
| CO2 | Carbon dioxide |
| DOP | Di-octylphthalate |
| H2O | Water |
| HCHO | Formaldehyde |
| NH3 | Ammonia |
| NMHC | Non-methane hydrocarbons |
| NOx | Oxides of nitrogen |
| NO | Nitric oxide |
| NO2 | Nitrogen dioxide |
| N2O | Nitrous oxide |
| THC | Total hydrocarbons |

**3. Definitions**

For the purposes of this Regulation the following definitions shall apply:

3.0.1. "*Vehicle type with regard to emissions*" means a group of vehicles which:

(a) Do not differ with respect to the criteria constituting an "interpolation family" as defined in paragraph 6.3.2.;

(b) Fall in a single "CO2 interpolation range" within the meaning of paragraph 2.3.2. of Annex B6;

(c) Do not differ with respect to any characteristics that have a non-negligible influence on tailpipe emissions, such as, but not limited to, the following:

(i) Types and sequence of pollution control devices (e.g. three-way catalyst, oxidation catalyst, lean NOx trap, SCR, lean NOx catalyst, particulate trap or combinations thereof in a single unit);

(ii) Exhaust gas recirculation (with or without, internal/external, cooled/non-cooled, low/high/combined pressure).

3.0.2. "*Engine capacity*" means:

For reciprocating piston engines, the nominal engine swept volume.

For rotary piston engines (Wankel), twice the nominal swept volume of a combustion chamber per piston.

3.0.3. "*Engine displacement*" means:

For reciprocating piston engines, the nominal engine swept volume.

For rotary piston engines (Wankel), the nominal swept volume of a combustion chamber per piston.

3.0.4. "*Approval of a vehicle*" means the approval of a vehicle type with regard to the scope of this Regulation.

3.1. Test equipment

3.1.1. "*Accuracy*" means the difference between a measured value and a reference value, traceable to a national standard and describes the correctness of a result. See Figure 1.

3.1.2. "*Calibration*" means the process of setting a measurement system's response so that its output agrees with a range of reference signals.

3.1.3. "*Calibration gas*" means a gas mixture used to calibrate gas analysers.

3.1.4. "*Double dilution method*" means the process of separating a part of the diluted exhaust flow and mixing it with an appropriate amount of dilution air prior to the particulate sampling filter.

3.1.5. "*Full flow exhaust dilution system*" means the continuous dilution of the total vehicle exhaust with ambient air in a controlled manner using a Constant Volume Sampler (CVS).

3.1.6. "*Linearization*" means the application of a range of concentrations or materials to establish a mathematical relationship between concentration and system response.

3.1.7. "*Major maintenance*" means the adjustment, repair or replacement of a component or module that could affect the accuracy of a measurement.

3.1.8. "*Non-Methane Hydrocarbons*" (NMHC) are the Total Hydrocarbons (THC) minus the methane (CH4) contribution.

3.1.9. "*Precision*" means the degree to which repeated measurements under unchanged conditions show the same results (Figure 1) and, in this Regulation, always refers to one standard deviation.

3.1.10. "*Reference value*" means a value traceable to a national standard. See Figure 1.

3.1.11. "*Set point*" means the target value a control system aims to reach.

3.1.12. "*Span*" means to adjust an instrument so that it gives a proper response to a calibration standard that represents between 75 per cent and 100 per cent of the maximum value in the instrument range or expected range of use.

3.1.13. "*Total hydrocarbons*" (THC) means all volatile compounds measurable by a flame ionization detector (FID).

3.1.14. "*Verification*" means to evaluate whether or not a measurement system's outputs agrees with applied reference signals within one or more predetermined thresholds for acceptance.

3.1.15. "*Zero gas*" means a gas containing no analyte which is used to set a zero response on an analyser.


3.1.16. "*Response time*" means the difference in time between the change of the component to be measured at the reference point and a system response of 90 per cent of the final reading (t90) with the sampling probe being defined as the reference point, whereby the change of the measured component is at least 60 per cent full scale (FS) and takes place in less than 0.1 second. The system response time consists of the delay time to the system and of the rise time of the system.

3.1.17. "*Delay time*" means the difference in time between the change of the component to be measured at the reference point and a system response of 10 per cent of the final reading (t10) with the sampling probe being defined as the reference point. For gaseous components, this is the transport time of the measured component from the sampling probe to the detector.

3.1.18. "*Rise time*" means the difference in time between the 10 per cent and 90 per cent response of the final reading (t90 – t10).

Figure 1

**Definition of accuracy, precision and reference value**



3.2. Road load and dynamometer setting

3.2.1. "*Aerodynamic drag*" means the force opposing a vehicle’s forward motion through air.

3.2.2. "*Aerodynamic stagnation point*" means the point on the surface of a vehicle where wind velocity is equal to zero.

3.2.3. "*Anemometer blockage*" means the effect on the anemometer measurement due to the presence of the vehicle where the apparent air speed is different than the vehicle speed combined with wind speed relative to the ground.

3.2.4. "*Constrained analysis*" means the vehicle’s frontal area and aerodynamic drag coefficient have been independently determined and those values shall be used in the equation of motion.

3.2.5. "*Mass in running order*" means the mass of the vehicle, with its fuel tank(s) filled to at least 90 per cent of its or their capacity/capacities, including the mass of the driver, fuel and liquids, fitted with the standard equipment in accordance with the manufacturer’s specifications and, when they are fitted, the mass of the bodywork, the cabin, the coupling and the spare wheel(s) as well as the tools.

3.2.6. "*Mass of the driver*" means a mass rated at 75 kg located at the driver’s seating reference point.

3.2.7. "*Maximum vehicle load*" means the technically permissible maximum laden mass minus the mass in running order, 25 kg and the mass of the optional equipment as defined in paragraph 3.2.8.

3.2.8. "*Mass of the optional equipment*" means maximum mass of the combinations of optional equipment which may be fitted to the vehicle in addition to the standard equipment in accordance with the manufacturer's specifications.

3.2.9. "*Optional equipment*" means all the features not included in the standard equipment which are fitted to a vehicle under the responsibility of the manufacturer, and that can be ordered by the customer.

3.2.10. "*Reference atmospheric conditions (regarding road load measurements)*" means the atmospheric conditions to which these measurement results are corrected:

(a) Atmospheric pressure: p0 = 100 kPa;

(b) Atmospheric temperature: T0 = 20 °C;

(c) Dry air density: ρ0 = 1.189 kg/m3;

(d) Wind speed: 0 m/s.

3.2.11. "*Reference speed*" means the vehicle speed at which road load is determined or chassis dynamometer load is verified.

3.2.12. "*Road load*" means the force resisting the forward motion of a vehicle as measured with the coastdown method or methods that are equivalent regarding the inclusion of frictional losses of the drivetrain.

3.2.13. "*Rolling resistance*" means the forces of the tyres opposing the motion of a vehicle.

3.2.14. "*Running resistance*" means the torque resisting the forward motion of a vehicle measured by torque meters installed at the driven wheels of a vehicle.

3.2.15. "*Simulated road load*" means the road load experienced by the vehicle on the chassis dynamometer which is intended to reproduce the road load measured on the road, and consists of the force applied by the chassis dynamometer and the forces resisting the vehicle while driving on the chassis dynamometer and is approximated by the three coefficients of a second order polynomial.

3.2.16. "*Simulated running resistance*" means the running resistance experienced by the vehicle on the chassis dynamometer which is intended to reproduce the running resistance measured on the road, and consists of the torque applied by the chassis dynamometer and the torque resisting the vehicle while driving on the chassis dynamometer and is approximated by the three coefficients of a second order polynomial.

3.2.17. "*Stationary anemometry*" means measurement of wind speed and direction with an anemometer at a location and height above road level alongside the test road where the most representative wind conditions will be experienced.

3.2.18. "*Standard equipment*" means the basic configuration of a vehicle which is equipped with all the features that are required under the regulatory acts of the Contracting Party including all features that are fitted without giving rise to any further specifications on configuration or equipment level.

3.2.19. "*Target road load*" means the road load to be reproduced on the chassis dynamometer.

3.2.20. "*Target running resistance*" means the running resistance to be reproduced.

3.2.21. "*Vehicle coastdown mode*" means a system of operation enabling an accurate and repeatable determination of road load and an accurate dynamometer setting.

3.2.22. "*Wind correction*" means correction of the effect of wind on road load based on input of the stationary or on-board anemometry.

3.2.23. "*Technically permissible maximum laden mass*" means the maximum mass allocated to a vehicle on the basis of its construction features and its design performances.

3.2.24. "*Actual mass of the vehicle*" means the mass in running order plus the mass of the fitted optional equipment to an individual vehicle.

3.2.25. "*Test mass of the vehicle*" means the sum of the actual mass of the vehicle, 25 kg and the mass representative of the vehicle load.

3.2.26. "*Mass representative of the vehicle load*" means x per cent of the maximum vehicle load where x is 15 per cent for category M vehicles and 28 per cent for category N vehicles.

3.2.27. "*Technically permissible maximum laden mass of the combination*" (MC) means the maximum mass allocated to the combination of a motor vehicle and one or more trailers on the basis of its construction features and its design performances or the maximum mass allocated to the combination of a tractor unit and a semi-trailer.

3.2.28. "*n/v ratio*" means the engine rotational speed divided by vehicle speed.

3.2.29. "*Single roller dynamometer*" means a dynamometer where each wheel on a vehicle's axle is in contact with one roller.

3.2.30. "*Twin-roller dynamometer*" means a dynamometer where each wheel on a vehicle's axle is in contact with two rollers.

3.2.31. "*Powered axle*" means an axle of a vehicle which is able to deliver propulsion energy and/or recuperate energy, independent of whether that is only temporarily or permanently possible and/or selectable by the driver.

3.2.32. "*2WD dynamometer*" means a dynamometer where only the wheels on one vehicle axle are in contact with the roller(s).

3.2.33. "*4WD dynamometer*" means a dynamometer where all wheels on both vehicle axles are in contact with the rollers.

3.2.34. "*Dynamometer in 2WD operation*" means a 2WD dynamometer, or a 4WD dynamometer which only simulates inertia and road load on the powered axle of the test vehicle and where the rotating wheels on the non-powered axle shall have no influence on the measurement results compared to a situation where the wheels on the non-powered axle are not rotating.

3.2.35. "*Dynamometer in 4WD operation*" means a 4WD dynamometer which simulates inertia and road load on both axles of the test vehicle.

3.2.36. "*Coasting*" means a functionality of either an automatic transmission or a clutch which, when no propulsion or a slow reduction of speed is needed, decouples the engine from the drivetrain automatically and neither a propulsion energy is applied to the wheels nor recuperation energy is taken from the wheels nor friction braking is applied. During application of this function the engine may be idling or switched off.

3.2.37. "*Reference mass*" means the vehicle’s mass in running order less the uniform mass of the driver of 75 kg and increased by a uniform mass of 100 kg.

3.3. Pure electric, pure ICE, hybrid electric, fuel cell and alternatively-fuelled vehicles

3.3.1. "*All-Electric Range*" (AER) means the total distance travelled by an OVC-HEV from the beginning of the charge-depleting test to the point in time during the test when the combustion engine starts to consume fuel.

3.3.2. "*Pure Electric Range*" (PER) means the total distance travelled by a PEV from the beginning of the charge-depleting test until the break-off criterion is reached.

3.3.3. "*Charge-Depleting Actual Range*" (RCDA) means the distance travelled in a series of WLTCs in charge-depleting operating condition until the Rechargeable Electric Energy Storage System (REESS) is depleted.

3.3.4. "*Charge-Depleting Cycle Range*" (RCDC) means the distance from the beginning of the charge-depleting test to the end of the last cycle prior to the cycle or cycles satisfying the break-off criterion, including the transition cycle where the vehicle may have operated in both depleting and sustaining conditions.

3.3.5. "*Charge-depleting operating condition*" means an operating condition in which the energy stored in the REESS may fluctuate but decreases on average while the vehicle is driven until transition to charge-sustaining operation.

3.3.6. "*Charge-sustaining operating condition*" means an operating condition in which the energy stored in the REESS may fluctuate but, on average, is maintained at a neutral charging balance level while the vehicle is driven.

3.3.7. "*Utility Factors*" are ratios based on driving statistics depending on the range achieved in charge-depleting condition and are used to weigh the charge-depleting and charge-sustaining exhaust emission compounds, CO2 emissions and fuel consumption for OVC-HEVs.

3.3.8. "*Electric machine*" (EM) means an energy converter transforming between electrical and mechanical energy.

3.3.9. "*Energy converter*" means a system where the form of energy output is different from the form of energy input.

3.3.9.1. "*Propulsion energy converter*" means an energy converter of the powertrain which is not a peripheral device whose output energy is used directly or indirectly for the purpose of vehicle propulsion.

3.3.9.2. "*Category of propulsion energy converter*" means (i) an internal combustion engine, or (ii) an electric machine, or (iii) a fuel cell.

3.3.10. "*Energy storage system*" means a system which stores energy and releases it in the same form as was input.

3.3.10.1. "*Propulsion energy storage system*" means an energy storage system of the powertrain which is not a peripheral device and whose output energy is used directly or indirectly for the purpose of vehicle propulsion.

3.3.10.2. "*Category of propulsion energy storage system*" means (i) a fuel storage system, or (ii) a rechargeable electric energy storage system, or (iii) a rechargeable mechanical energy storage system.

3.3.10.3. "*Form of energy*" means (i) electrical energy, or (ii) mechanical energy, or (iii) chemical energy (including fuels).

3.3.10.4. "*Fuel storage system*" means a propulsion energy storage system that stores chemical energy as liquid or gaseous fuel.

3.3.11. "*Equivalent all-electric range*" (EAER) means that portion of the total charge-depleting actual range (RCDA) attributable to the use of electricity from the REESS over the charge-depleting range test.

3.3.12. "*Hybrid electric vehicle*" (HEV) means a hybrid vehicle where one of the propulsion energy converters is an electric machine.

3.3.13. "*Hybrid vehicle*" (HV) means a vehicle equipped with a powertrain containing at least two different categories of propulsion energy converters and at least two different categories of propulsion energy storage systems.

3.3.14. "*Net energy change*" means the ratio of the REESS energy change divided by the cycle energy demand of the test vehicle.

3.3.15. "*Not off-vehicle charging hybrid electric vehicle*" (NOVC-HEV) means a hybrid electric vehicle that cannot be charged from an external source.

3.3.16. "*Off-vehicle charging hybrid electric vehicle*" (OVC-HEV) means a hybrid electric vehicle that can be charged from an external source.

3.3.17. "*Pure electric vehicle*" (PEV) means a vehicle equipped with a powertrain containing exclusively electric machines as propulsion energy converters and exclusively rechargeable electric energy storage systems as propulsion energy storage systems.

3.3.18. "*Fuel cell*" means an energy converter transforming chemical energy (input) into electrical energy (output) or vice versa.

3.3.19. "*Fuel cell vehicle*" (FCV) means a vehicle equipped with a powertrain containing exclusively fuel cell(s) and electric machine(s) as propulsion energy converter(s).

3.3.20. "*Fuel cell hybrid vehicle*" (FCHV) means a fuel cell vehicle equipped with a powertrain containing at least one fuel storage system and at least one rechargeable electric energy storage system as propulsion energy storage systems.

3.3.20.1. "*Not off-vehicle charging fuel cell hybrid electric vehicle*" (NOVC-FCHV) means a fuel cell hybrid electric vehicle that cannot be charged from an external source.

3.3.20.2. "*Off-vehicle charging fuel cell hybrid electric vehicle*" (OVC-FCHV) means a fuel cell hybrid electric vehicle that can be charged from an external source.

3.3.21. "*Bi-fuel vehicle*" means a vehicle with two separate fuel storage systems that is designed to run primarily on only one fuel at a time; however, the simultaneous use of both fuels is permitted in limited amount and duration.

3.3.22. "*Bi-fuel gas vehicle*" means a bi-fuel vehicle where the two fuels are petrol (petrol mode) and either LPG, NG/biomethane, or hydrogen.

3.3.23. "*Pure ICE vehicle*" means a vehicle where all of the propulsion energy converters are internal combustion engines.

3.3.24. "*On-board charger*" means the electric power converter between the traction REESS and the vehicle's recharging socket.

3.3.25. "*Flex fuel vehicle*" means a vehicle with one fuel storage system that can run on different mixtures of two or more fuels.

3.3.26. "*Flex fuel ethanol vehicle*" means a flex fuel vehicle that can run on petrol or a mixture of petrol and ethanol up to an 85 per cent ethanol blend (E85).

3.3.27. *"Mono-fuel vehicle"* means a vehicle that is designed to run primarily on one type of fuel.

3.3.28. *"Mono-fuel gas vehicle"* means a mono-fuel vehicle that is designed primarily for permanent running on LPG or NG/biomethane or hydrogen, but may also have a petrol system for emergency purposes or starting only, where the nominal capacity of the petrol tank does not exceed 15 litres.

3.4. Powertrain

3.4.1. "*Powertrain*" means the total combination in a vehicle of propulsion energy storage system(s), propulsion energy converter(s) and the drivetrain(s) providing the mechanical energy at the wheels for the purpose of vehicle propulsion, plus peripheral devices.

3.4.2. "*Auxiliary devices*" means energy consuming, converting, storing or supplying non-peripheral devices or systems which are installed in the vehicle for purposes other than the propulsion of the vehicle and are therefore not considered to be part of the powertrain.

3.4.3. *"Peripheral devices"* means any energy consuming, converting, storing or supplying devices, where the energy is not directly or indirectly used for the purpose of vehicle propulsion but which are essential to the operation of the powertrain and are therefore considered to be part of the powertrain.

3.4.4. "*Drivetrain*" means the connected elements of the powertrain for transmission of the mechanical energy between the propulsion energy converter(s) and the wheels.

3.4.5. "*Manual transmission*" means a transmission where gears can only be shifted by action of the driver.

3.5. General

3.5.1. "*Criteria emissions*" means those emission compounds for which limits are set in this Regulation.

3.5.2. (Reserved)

3.5.3. (Reserved)

3.5.4. (Reserved)

3.5.5. (Reserved)

3.5.6. "*Cycle energy demand*" means the calculated positive energy required by the vehicle to drive the prescribed cycle.

3.5.7. "*Defeat device*" means any element of design which senses temperature, vehicle speed, engine speed (RPM), transmission gear, manifold vacuum or any other parameter for the purpose of activating, modulating, delaying or deactivating the operation of any part of the emission control system, that reduces the effectiveness of the emission control system under conditions which may reasonably be expected to be encountered in normal vehicle operation and use.

3.5.8. "*Driver-selectable mode*" means a distinct driver-selectable condition which could affect emissions, or fuel and/or energy consumption.

3.5.9. *"Predominant mode"* for the purpose of this Regulation means a single driver-selectable mode that is always selected when the vehicle is switched on, regardless of the driver-selectable mode in operation when the vehicle was previously shut down, and which cannot be redefined to another mode. After the vehicle is switched on, the predominant mode can only be switched to another driver-selectable mode by an intentional action of the driver.

3.5.10. "*Reference conditions (with regards to calculating mass emissions)*" means the conditions upon which gas densities are based, namely 101.325 kPa and 273.15 K (0 °C).

3.5.11. "*Exhaust emissions*" means the emission of gaseous, solid and liquid compounds from the tailpipe.

3.5.12. *”Configurable start mode”* for the purpose of this Regulation means a driver-selectable mode that can be set by the driver as a mode which is automatically selected when the vehicle is switched on. After the vehicle is switched on, the configurable start mode can only be switched to another mode by an intentional action of the driver.

3.6. PM/PN

The term "particle" is conventionally used for the matter being characterised (measured) in the airborne phase (suspended matter), and the term "particulate" for the deposited matter.

3.6.1. "*Particle number emissions*" (PN) means the total number of solid particles emitted from the vehicle exhaust quantified according to the dilution, sampling and measurement methods as specified in this Regulation.

3.6.2. "*Particulate matter emissions*" (PM) means the mass of any particulate material from the vehicle exhaust quantified according to the dilution, sampling and measurement methods as specified in this Regulation.

3.7. WLTC

3.7.1. "*Rated engine power*" (Prated) means maximum net power of the engine or motor in kW as per the requirements of UN Regulation No. 85.

3.7.2. "*Maximum speed*" (vmax) means the maximum speed of a vehicle as declared by the manufacturer. In the absence of a declaration, the maximum speed shall be determined according to UN Regulation No. 68.

3.8. Procedure

3.8.1. "*Periodically regenerating system*" means an exhaust emissions control device (e.g. catalytic converter, particulate trap) that requires a periodical regeneration.

3.9. Evaporative emissions

3.9.1. "*Fuel tank system*" means the devices which allow storing the fuel, comprising the fuel tank, the fuel filler, the filler cap and the fuel pump when it is fitted in or on the fuel tank.

3.9.2. "*Fuel system*" means the components which store or transport fuel on board the vehicle and comprise the fuel tank system, all fuel and vapour lines, any non-tank mounted fuel pumps and the activated carbon canister.

3.9.3. "*Butane working capacity*" (BWC) means the mass of butane which a carbon canister can adsorb.

3.9.4. "*BWC300*" means the butane working capacity after 300 cycles of fuel ageing cycles experienced.

3.9.5. "*Permeability Factor*" (PF) means the factor determined from hydrocarbon losses over a period of time and used to determine the final evaporative emissions.

3.9.6. "*Monolayer non-metal tank*" means a fuel tank constructed with a single layer of non-metal material including fluorinated/sulfonated materials.

3.9.7. "*Multilayer tank*" means a fuel tank constructed with at least two different layered materials, one of which is a hydrocarbon barrier material.

3.9.8. "*Sealed fuel tank system*" means a fuel tank system where the fuel vapours do not vent during parking over the 24-hour diurnal cycle defined in paragraph 6.5.9. of Annex C3 when performed with the applicable reference fuel defined in paragraph 7 of Annex B3.

3.9.9. "*Evaporative emissions*" means in the context of this Regulation the hydrocarbon vapours lost from the fuel system of a motor vehicle during parking and immediately before refuelling of a sealed fuel tank.

3.9.10. "*Depressurisation puff loss*" means hydrocarbons venting from a sealed fuel tank system pressure relief exclusively through the carbon canister allowed by the system.

3.9.11. "*Depressurisation puff loss overflow*" are the depressurisation puff loss hydrocarbons that pass through the carbon canister during depressurisation.

3.9.12. "*Fuel tank relief pressure*" is the minimum pressure value at which the sealed fuel tank system starts venting in response only to pressure inside the tank.

3.9.13. "*2 gram breakthrough*" shall be considered accomplished when the cumulative quantity of hydrocarbons emitted from the activated carbon canister equals 2 grams.

3.10. On-Board Diagnostics (OBD)

3.10.1. "*On-Board Diagnostic (OBD) system*" means in context of this Regulation, a system on-board the vehicle which has the capability of detecting malfunctions of the monitored emission control systems, identifying the likely area of a malfunction by means of fault codes stored in computer memory, and illumination of the Malfunction Indicator (MI) to notify the operator of the vehicle.

3.10.2. "*OBD family*" means a manufacturer's grouping of vehicles which, through their design, are expected to have similar exhaust emission and OBD system characteristics. Each vehicle of this family shall have complied with the requirements of this Regulation as defined in paragraph 6.8.1.

3.10.3. "*Emission control system*" means in the context of OBD the electronic engine management controller and any emission-related component in the exhaust or evaporative system which supplies an input to or receives an output from this controller.

3.10.4. "*Malfunction indicator (MI)*" means a visible or audible indicator that clearly informs the driver of the vehicle in the event of a malfunction of any emission-related component connected to the OBD system, or the OBD system itself.

3.10.5. "*Malfunction*" means the failure of an emission-related component or system that would result in emissions exceeding the OBD thresholds in paragraph 6.8.2. or if the OBD system is unable to fulfil the basic monitoring requirements of Annex C5.

3.10.6. "*Secondary air*" refers to air introduced into the exhaust system by means of a pump or aspirator valve or other means that is intended to aid in the oxidation of HC and CO contained in the exhaust gas stream.

3.10.7. "*Engine misfire*" means lack of combustion in the cylinder of a positive ignition engine due to absence of spark, poor fuel metering, poor compression or any other cause. In terms of OBD monitoring it is that percentage of misfires out of a total number of firing events (as declared by the manufacturer) that would result in emissions exceeding the OBD thresholds given in paragraph 6.8.2. or that percentage that could lead to an exhaust catalyst, or catalysts, overheating causing irreversible damage.

3.10.8. An "*OBD driving cycle*" consists of key-on, a driving mode where a malfunction would be detected if present, and key-off.

3.10.9. A "*warm-up cycle*" means sufficient vehicle operation such that the coolant temperature has risen by at least 22 K from engine starting and reaches a minimum temperature of 343 K (70 °C).

3.10.10. A "*Fuel trim*" refers to feedback adjustments to the base fuel schedule. Short-term fuel trim refers to dynamic or instantaneous adjustments. Long-term fuel trim refers to much more gradual adjustments to the fuel calibration schedule than short-term trim adjustments. These long-term adjustments compensate for vehicle differences and gradual changes that occur over time.

3.10.11. A "*Calculated load value*" refers to an indication of the current airflow divided by peak airflow, where peak airflow is corrected for altitude, if available. This definition provides a dimensionless number that is not engine specific and provides the service technician with an indication of the proportion of engine capacity that is being used (with wide open throttle as 100 per cent);

3.10.12. *"Permanent emission default mode"* refers to a case where the engine management controller permanently switches to a setting that does not require an input from a failed component or system where such a failed component or system would result in an increase in emissions from the vehicle to a level above the OBD thresholds given in paragraph 6.8.2.

3.10.12.1. Permanent in this context means that the default mode is not recoverable, i.e. the diagnostic or control strategy that caused the emission default mode cannot run in the next driving cycle and cannot confirm that the conditions that caused the emission default mode is not present anymore. All other emission default modes are considered not to be permanent.

3.10.13. *"Power take-off unit"* means an engine-driven output provision for the purposes of powering auxiliary, vehicle mounted, equipment.

3.10.14. *"Access"* means the availability of all emission-related OBD data including all fault codes required for the inspection, diagnosis, servicing or repair of emissions-related parts of the vehicle, via the serial interface for the standard diagnostic connection (pursuant to paragraph 6.5.3.5. of Appendix 1 to Annex C5).

3.10.15. *"Unrestricted"* means:

3.10.15.1. Access not dependent on an access code obtainable only from the manufacturer, or a similar device; or

3.10.15.2. Access allowing evaluation of the data produced without the need for any unique decoding information, unless that information itself is standardised.

3.10.16. *"Standardised"* means that all data stream information, including all fault codes used, shall be produced only in accordance with industry standards which, by virtue of the fact that their format and their permitted options are clearly defined, provide for a maximum level of harmonisation in the motor vehicle industry, and whose use is expressly permitted in this Regulation.

3.10.17. (Reserved).

3.10.18. "*Deficiency*" means, in respect of vehicle OBD systems, that components or systems that are monitored contain temporary or permanent operating characteristics that impair the otherwise efficient OBD monitoring of those components or systems or do not meet all of the other detailed requirements for OBD.

3.10.19. "*Limp-home routines*" means any default mode other than emission default mode.

3.10.20. "*Pending fault code*" is a diagnostic trouble code stored upon the initial detection of a malfunction prior to illumination of the malfunction indicator.

3.10.21. "*Readiness*" means a status indicating whether a monitor or a group of monitors have run since the last erasing by an external request or command (for example through an OBD scan-tool).

3.11. Ambient Temperature Correction Test (Annex B6a)

3.11.1. "Active heat storage device" means a technology that stores heat within any device of a vehicle and releases the heat to a powertrain component over a defined time period at engine start. It is characterised by the stored enthalpy in the system and the time for heat release to the powertrain components.

3.11.2. “Insulation materials” means any material in the engine compartment attached to the engine and/or the chassis with a thermal insulation effect and characterised by a maximum heat conductivity of 0.1 W/(mK).

4. Application for approval

4.1. The application for approval of a vehicle type with regard to the requirements of this Regulation shall be submitted by the vehicle manufacturer or by their authorized representative to the Type Approval Authority.

4.1.1. The application referred to in paragraph 4.1. shall be drawn up in accordance with the model of the information document set out in Annex A1 to this Regulation.

4.1.2. In addition, the manufacturer shall submit the following information:

(a) In the case of vehicles equipped with positive ignition engines, a declaration by the manufacturer of the minimum percentage of misfires out of a total number of firing events that would either result in emissions exceeding the OBD thresholds given in paragraph 6.8.2., if that percentage of misfire had been present from the start of a Type 1 test as described in Annexes Part B to this Regulation, or that could lead to an exhaust catalyst, or catalysts, overheating prior to causing irreversible damage;

(b) Detailed written information fully describing the functional operation characteristics of the OBD system, including a listing of all relevant parts of the emission control system of the vehicle that are monitored by the OBD system;

(c) A description of the malfunction indicator used by the OBD system to signal the presence of a fault to a driver of the vehicle;

(d) A declaration by the manufacturer that the OBD system complies with the provisions of paragraph 7. of Appendix 1 to Annex C5 to this Regulation relating to in-use performance under all reasonably foreseeable driving conditions;

(e) A plan describing the detailed technical criteria and justification for incrementing the numerator and denominator of each monitor that shall fulfil the requirements of paragraphs 7.2. and 7.3. of Appendix 1 to Annex C5 to this Regulation, as well as for disabling numerators, denominators and the general denominator under the conditions outlined in paragraph 7.7. of Appendix 1 to Annex C5 to this Regulation;

(f) A description of the provisions taken to prevent tampering with and modification of the emission control computer;

(g) If applicable, the particulars of the OBD family as referred to in paragraph 6.8.1.;

(h) Where appropriate, copies of other type approvals with the relevant data to enable extension of approvals and establishment of deterioration factors.

4.1.3. For the tests described in paragraph 3. of Annex C5 to this Regulation, a vehicle representative of the vehicle type or vehicle family fitted with the OBD system to be approved shall be submitted to the Technical Service responsible for the type approval test. If the Technical Service determines that the submitted vehicle does not fully represent the OBD family described in paragraph 6.8.1., an alternative and, if necessary, an additional vehicle shall be submitted for test in accordance with paragraph 3. of Annex C5 to this Regulation.

4.2. A model of the information document relating to exhaust emissions, emissions of carbon dioxide and fuel consumption and/or the measurement of electric energy consumption and electric range, evaporative emissions, durability and OBD, is given in Annex A1 to this Regulation.

4.2.1. Where appropriate, copies of other type approvals with the relevant data to enable extensions of approvals and establishment of deterioration factors shall be submitted.

4.3. For the tests specified in Table A in paragraph 6. a vehicle representative of the vehicle type to be approved shall be submitted to the Technical Service responsible for the approval tests.

4.3.1. For the purposes of paragraph 4.1.2.(e), the Type Approval Authority that grants the approval shall make the information referred to in that point available to other Type Approval Authorities upon request.

4.3.2. For the purposes of subparagraphs 4.1.2. (d) and (e), Type Approval Authorities shall not approve a vehicle if the information submitted by the manufacturer is inappropriate for fulfilling the requirements of paragraph 7. of Appendix 1 to Annex C5 to this Regulation. Paragraphs 7.2., 7.3. and 7.7. of Appendix 1 to Annex C5 to this Regulation shall apply under all reasonably foreseeable driving conditions. For the assessment of the implementation of the requirements set out in the paragraphs 7.2. and 7.3. of Appendix 1 to Annex C5, the Type Approval Authority shall take into account the state of technology.

4.3.3. For the purposes of paragraph 4.1.2. (f), the provisions taken to prevent tampering with and modification of the emission control computer shall include the facility for updating using a manufacturer-approved programme or calibration.

4.3.4. The application for type approval of flex-fuel, mono fuel, and bi-fuel vehicles shall comply with the additional requirements laid down in paragraphs 5.8. and 5.9.

4.3.5. Changes to the make of a system, component or separate technical unit that occur after a type approval shall not automatically invalidate a type approval, unless its original characteristics or technical parameters are changed in such a way that the functionality of the engine or pollution control system is affected.

4.4. The Type Approval Authority shall verify the existence of satisfactory provisions to ensure an effective check of conformity of production before approval of the vehicle type is granted.

5. Approval

5.1. If the vehicle type submitted for approval meets all the relevant requirements of paragraph 6., approval of that vehicle type shall be granted.

5.2. An approval number shall be assigned to each type approved.

5.2.1. The type approval number shall consist of four sections. Each section shall be separated by the '\*' character.

Section 1: The capital letter 'E' followed by the distinguishing number of the Contracting Party which has granted the type approval[[3]](#footnote-4).

Section 2: The number 154, followed by the letter 'R', successively followed by:

(a) Two digits (with leading zeros as applicable) indicating the series of amendments incorporating the technical provisions of the UN Regulation applied to the approval (00 for the UN Regulation in its original form);

(b) A slash (/) and two digits (with leading zeros as applicable) indicating the number of supplement to the series of amendments applied to the approval (00 for the series of amendments in its original form);

(c) A slash (/) and two character(s) indicating the implementing stage/level (e.g. 1A, 1B).

Section 3: A four-digit sequential number (with leading zeros as applicable). The sequence shall start from 0001.

Section 4: A two-digit sequential number (with leading zeros if applicable) to denote the extension. The sequence shall start from 00.

All digits shall be Arabic digits.

5.2.2. Example of an Approval Number to this Regulation:

E11\*154R01/01/02\*0123\*01

The first extension of the Approval numbered 0123, issued by the United Kingdom to Series of Amendments 01, Supplement 01, which is a Level 2 Approval.

5.2.3. The same Contracting Party shall not assign the same number to another vehicle type.

5.3. Notice of approval or of extension or refusal of approval of a vehicle type pursuant to this Regulation shall be communicated to the Contracting Parties to the 1958 Agreement which apply this Regulation by means of a form conforming to the model in Annex A2 to this Regulation.

5.3.1. In the event of amendment to the present text, for example, if new limit values are prescribed, the Contracting Parties to the 1958 Agreement shall be informed which vehicle types already approved comply with the new provisions.

5.4. There shall be affixed, conspicuously and in a readily accessible place specified on the approval form, to every vehicle conforming to a vehicle type approved under this Regulation, an international approval mark consisting of:

5.4.1. A circle surrounding the letter "E" followed by the distinguishing number of the Contracting Party that has granted approval.

5.4.2. The number of this Regulation, followed by the letter "R", a dash and the approval number to the right of the circle described in paragraph 5.4.1.

5.4.3. The approval mark shall contain an additional code after the type approval number, the purpose of which is to distinguish the level (Level 1A, 1B or 2) for which the approval has been granted. This code should be chosen according to the Table A3/1 of Annex A3 to this Regulation.

5.5. If the vehicle conforms to a vehicle type approved, under one or more other Regulations annexed to the 1958 Agreement, in the country which has granted approval under this Regulation, the symbol prescribed in paragraph 5.4.1. need not be repeated; in such a case, the Regulation, approval numbers and the additional symbols of all the Regulations under which approval has been granted in the country which has granted approval under this Regulation shall be placed in vertical columns to the right of the symbol prescribed in paragraph 5.4.1. (see Annex A3).

5.6. The approval mark shall be clearly legible and be indelible.

5.7. The approval mark shall be placed close to or on the vehicle data plate.

5.7.1. Annex A3 to this Regulation gives examples of arrangements of the approval mark.

5.8. Additional requirements for approval of flex fuel vehicles

5.8.1. For the type approval of a flex fuel ethanol vehicle, the vehicle manufacturer shall describe the capability of the vehicle to adapt to any mixture of petrol and ethanol fuel (up to an 85 per cent ethanol blend).

5.9. Additional requirements for mono fuel gas vehicles, and bi-fuel gas vehicles.

5.9.1. For LPG or NG, the fuel to be used shall be specified in the information document set out in Annex A1 to this Regulation.

5.10. Requirements for approval regarding the OBD system

5.10.1. The manufacturer shall ensure that all vehicles are equipped with an OBD system.

5.10.2. The OBD system shall be designed, constructed and installed on a vehicle so as to enable it to identify types of deterioration or malfunction over the entire life of the vehicle.

5.10.3. The OBD system shall comply with the requirements of this Regulation during conditions of normal use.

5.10.4. When tested with a defective component in accordance with Appendix 1 to Annex C5 to this Regulation, the OBD system malfunction indicator shall be activated. The OBD system malfunction indicator may also activate during this test at levels of emissions below the OBD thresholds specified in paragraph 6.8.

5.10.5. The manufacturer shall ensure that the OBD system complies with the requirements for in-use performance set out in paragraph 7. of Appendix 1 to Annex C5 to this Regulation under all reasonably foreseeable driving conditions.

5.10.6. In-use performance related data to be stored and reported by a vehicle's OBD system according to the provisions of paragraph 7.6. of Appendix 1 to Annex C5 to this Regulation shall be made readily available by the manufacturer to national authorities and independent operators without any encryption.

5.11. Requirements for type-approval regarding devices for monitoring the consumption of fuel and/or electric energy

5.11.1. The manufacturer shall ensure that the following vehicles of categories M1, N1 and N2 are equipped with a device for determining, storing and making available data on the quantity of fuel and/or electric energy used for the operation of the vehicle:

(a) Pure ICE and Not-Off-Vehicle Charging Hybrid Electric vehicles (NOVC-HEVs) powered exclusively by mineral diesel, biodiesel, petrol, ethanol or any combination of these fuels;

(b) Off-Vehicle Charging Hybrid Electric Vehicles (OVC-HEVs) powered by electricity and any of the fuels mentioned in point (a).

5.11.2. The device for monitoring the consumption of fuel and/or electric energy shall comply with the requirements laid down in Appendix 5.

6. Specifications and tests

6.1. General

6.1.1. The vehicle and its components liable to affect CO2 and fuel consumption or electric energy consumption and the emissions of gaseous compounds, including evaporative emissions, particulate matter, particle number shall be so designed, constructed and assembled as to enable the vehicle in normal use and under normal conditions of use such as humidity, rain, snow, heat, cold, sand, dirt, vibrations, wear, etc. to comply with the provisions of this Regulation during its useful life. This shall include the security of all hoses, joints and connections used within the emission control systems and the evaporative emission control systems.

For exhaust emissions, CO2 and fuel consumption or electric energy consumption these provisions are deemed to be met if the provisions of paragraph 6.3. and paragraph 8.2. are complied with.

For evaporative emissions, these conditions are deemed to be met if the provisions of paragraph 6.6. and paragraph 8.3. are complied with.

6.1.2. The test vehicle shall be representative in terms of its emissions-related components and functionality of the intended production series to be covered by the approval. The manufacturer and the responsible authority shall agree which vehicle test model is representative.

6.1.3. With respect to evaporative emissions, for vehicles with a sealed fuel tank system, this shall also include having a system which, just before refuelling, releases the tank pressure exclusively through a carbon canister which has the sole function of storing fuel vapour. This ventilation route shall also be the only one used when the tank pressure exceeds its safe working pressure.

6.1.4. Vehicle testing condition

6.1.4.1. The types and amounts of lubricants and coolant for emissions testing shall be as specified for normal vehicle operation by the manufacturer.

6.1.4.2. The type of fuel for emissions testing shall be as specified in Annex B3 to this Regulation.

6.1.4.3. All emissions controlling systems, including evaporative emissions controlling systems shall be in working order.

6.1.4.4. The engine shall be designed to avoid crankcase emissions.

6.1.4.5. The tyres used for emissions testing shall be as defined in paragraph 2.4.5. of Annex B6 to this Regulation.

6.1.5. Fuel tank inlet orifices

6.1.5.1. Subject to paragraph 6.1.5.2., the inlet orifice of the petrol or ethanol tank shall be so designed as to prevent the tank from being filled from a fuel pump delivery nozzle which has an external diameter of 23.6 mm or greater.

6.1.5.2. Paragraph 6.1.5.1. shall not apply to a vehicle in respect of which both of the following conditions are satisfied:

6.1.5.2.1. The vehicle is so designed and constructed that no device designed to control the emissions shall be adversely affected by leaded petrol; and

6.1.5.2.2. The vehicle is conspicuously, legibly and indelibly marked with the symbol for unleaded petrol, specified in ISO 2575:2010 "Road vehicles -- Symbols for controls, indicators and tell-tales", in a position immediately visible to a person filling the petrol tank. Additional markings are permitted.

6.1.6. Provision shall be made to prevent excess evaporative emissions and fuel spillage caused by a missing fuel filler cap. This may be achieved by using one of the following:

6.1.6.1. An automatically opening and closing, non-removable fuel filler cap;

6.1.6.2. Design features which avoid excess evaporative emissions in the case of a missing fuel filler cap; or

6.1.6.3. Any other provision which has the same effect. Examples may include, but are not limited to, a tethered filler cap, a chained filler cap or one utilising the same locking key for the filler cap as for the vehicle's ignition. In this case, the key shall be removable from the filler cap only in the locked condition.

6.1.7. Provisions for electronic system security

6.1.7.1. Any vehicle with an emission control computer, including an evaporative emission control computer, including when integrated in an exhaust emissions control computer, shall include features to deter modification, except as authorised by the manufacturer. The manufacturer shall authorise modifications if those modifications are necessary for the diagnosis, servicing, inspection, retrofitting or repair of the vehicle. Any reprogrammable computer codes or operating parameters shall be resistant to tampering and afford a level of protection at least as good as the provisions in ISO 15031-7: 2013. Any removable calibration memory chips shall be potted, encased in a sealed container or protected by electronic algorithms and shall not be changeable without the use of specialized tools and procedures.

6.1.7.1.1. Only features directly associated with emissions calibration or prevention of vehicle theft may be protected in accordance with paragraph 6.1.7.1.

6.1.7.2. Computer-coded engine operating parameters shall not be changeable without the use of specialized tools and procedures (e.g. soldered or potted computer components or sealed (or soldered) enclosures).

6.1.7.3. Manufacturers may seek approval from the responsible authority for an exemption to one of these requirements for those vehicles that are unlikely to require protection. The criteria that the responsible authority shall evaluate in considering an exemption shall include, but are not limited to, the current availability of performance chips, the high-performance capability of the vehicle and the projected sales volume of the vehicle.

6.1.7.4. Manufacturers using programmable computer code systems shall deter unauthorised reprogramming. Manufacturers shall include enhanced tamper protection strategies and write-protect features requiring electronic access to an off-site computer maintained by the manufacturer. Methods giving an adequate level of tamper protection shall be approved by the responsible authority.

6.1.8. Rounding

Unless specified elsewhere in this Regulation, paragraphs 6.1.8.1. and 6.1.8.2. provide rules for rounding to fulfil the requirements of this Regulation.

6.1.8.1. When the digit immediately to the right of the last place to be retained is less than 5, that last digit retained shall remain unchanged.

Example:

If a result is 1.234 grams but only two places of decimal are to be retained, the final result shall be 1.23 grams.

6.1.8.2. When the digit immediately to the right of the last place to be retained is greater than or equal to 5, that last digit retained shall be increased by 1.

Example:

If a result is 1.236 grams but only two places of decimal are to be retained, and because 6 is greater than 5, the final result shall be 1.24 grams.

6.1.9. The use of defeat devices that reduce the effectiveness of emission control systems shall be prohibited. The prohibition shall not apply where:

(a) The need for the device is justified in terms of protecting the engine against damage or accident and for safe operation of the vehicle;

(b) The device does not function beyond the requirements of engine starting;

or

(c) The conditions are substantially included in the test procedures for verifying evaporative emissions and average tailpipe emissions.

6.1.10. Division by zero

In the case that the data input to a formula in this Regulation justifiably leads to division by zero, e.g. when an OVC-HEV consumes zero fuel under charge-depleting conditions, good engineering judgement shall be applied.

6.2. Test procedure

Table A specifies the various test requirements for type approval of a vehicle.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Table A* | | | | | | | | | | | | |
| *Application of test requirements for type-approval and extensions* | | | | | | | | | | | | |
| *Vehicle category* | *Vehicles with positive ignition engines including hybrids1,2* | | | | | | | | *Vehicles with compression ignition engines including hybrids* | | *Pure electric vehicles* | *Hydrogen fuel cell vehicles* |
|  | *Mono fuel* | | | | *Bi-fuel3* | | | *Flex-fuel3* | *Mono fuel* | |  |  |
| Reference fuel | Petrol | LPG | NG/ Biomethane | Hydrogen (ICE) | Petrol | Petrol | Petrol | Petrol | Diesel | Petrol | — | Hydrogen (Fuel Cell) |
| LPG | NG/ Biomethane | Hydrogen (ICE) 4 | Ethanol (E85) |
| Type 1 test (for applicability of measured components to fuels and vehicle technology and therefore measurement procedures, see Table 1A and Table 1B) (limits) | Yes | Yes5 | Yes5 | Yes4 | Yes  (both fuels) | Yes  (both fuels) | Yes  (both fuels) | Yes  (both fuels) | Yes | Yes | — | — |
| ATCT  (14°C test) | Yes | Yes | Yes | Yes4 | Yes  (both fuels) | Yes  (both fuels) | Yes  (both fuels) | Yes  (both fuels) | Yes | Yes | — | — |
| Evaporative emissions  (Type 4 test) | Yes | Yes | Yes | — | Yes  (petrol only) | Yes  (petrol only) | Yes  (petrol only) | Yes  (petrol only) | — | Yes | — | — |
| Durability  (Type 5 test) | Yes | Yes | Yes | Yes | Yes  (petrol only) | Yes  (petrol only) | Yes  (petrol only) | Yes  (petrol only) | Yes | Yes | — | — |
| OBD | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | — | — |
| OBFCM | Yes | — | — | — | — | — | — | Yes  (both fuels) | Yes | Yes | — | — |

1 Specific test procedures for hydrogen vehicles will be defined at a later stage.

2 Particulate mass and particle number limits and respective measurement procedures shall apply only to vehicles with direct injection engines

3 When a bi-fuel vehicle is combined with a flex fuel vehicle, both test requirements are applicable.

4 Only NOx emissions shall be determined when the vehicle is running on hydrogen.

5 In the case that a mono-fuel gas vehicle has a petrol tank it shall also be tested using the applicable petrol reference fuel. Particle number limits and respective measurement procedures shall not apply

6.2.1. Each of the vehicle families specified below shall be attributed a unique identifier of the following format:

FT-nnnnnnnnnnnnnnn-WMI

Where:

FT is an identifier of the family type:

1. IP = Interpolation family as defined in paragraph 6.3.2. with or without using the interpolation method
2. RL = Road load family as defined in paragraph 6.3.3.
3. RM = Road load matrix family as defined in paragraph 6.3.4.
4. PR = Periodically regenerating systems (Ki) family as defined in paragraph 6.3.5.
5. AT = ATCT family as defined in paragraph 2. of Annex B6a.
6. EV = Evaporative emissions family, as defined in paragraph 6.6.3.
7. DF = Durability family, as defined in paragraph 6.7.5.
8. OB = OBD family identifier, as defined paragraph 6.8.1.
9. ER = Exhaust after-treatment system using reagent (ER)family identifier, as defined in paragraph 6.9.2.
10. GV = GFV family identifier, as defined in paragraph 6.3.6.3.
11. KC = KCO2 correction factor family identifier, as defined in paragraph 6.3.11.

nnnnnnnnnnnnnnn is a string with a maximum of fifteen characters, restricted to using the characters 0-9, A-Z and the underscore character '\_'.

WMI (world manufacturer identifier) is a code that identifies the manufacturer in a unique manner defined in ISO 3780:2009.

It is the responsibility of the owner of the WMI to ensure that the combination of the string nnnnnnnnnnnnnnn and the WMI is unique to the family and that the string nnnnnnnnnnnnnnn is unique within that WMI to the approval tests performed to obtain the approval.

6.3. Description of Type 1 test (WLTP)

The Type 1 test shall be carried out on all vehicles referred to in paragraph 1. The test procedures and requirements of this paragraph and Annexes Part B shall be followed (as applicable).

6.3.1. The Type 1 test shall be performed according to:

(a) The WLTCs as described in Annex B1;

(b) The gear selection and shift point determination as described in Annex B2;

(c) The appropriate fuel(s) as specified in Annex B3;

(d) The road load and dynamometer settings as described in Annex B4;

(e) The test equipment as described in Annex B5;

(f) The test procedures as described in Annexes B6 and B8;

(g) The methods of calculation as described in Annexes B7 and B8.

6.3.2. Interpolation family

6.3.2.1. Interpolation family for pure ICE vehicles

6.3.2.1.1. Vehicles may be part of the same interpolation family in any of the following cases including combinations of these cases:

(a) They belong to different vehicle classes as described in paragraph 2. of Annex B1;

(b) They have different levels of downscaling as described in paragraph 8. of Annex B1;

(c) They have different capped speeds as described in paragraph 9. of Annex B1.

6.3.2.1.2. Only vehicles that are identical with respect to the following vehicle/powertrain/transmission characteristics may be part of the same interpolation family:

(a) Type of internal combustion engine: fuel type (or types in the case of flex-fuel or bi-fuel vehicles), combustion process, engine capacity, full-load characteristics, engine technology, and charging system, and also other engine subsystems or characteristics that have a non-negligible influence on CO2 emission under WLTP conditions;

(b) Operation strategy of all CO2 emission influencing components within the powertrain;

(c) Transmission type (e.g. manual, automatic, CVT) and transmission model (e.g. torque rating, number of gears, number of clutches, etc.);

(d) n/v ratios (engine rotational speed divided by vehicle speed). This requirement shall be considered fulfilled if, for all transmission ratios concerned, the difference with respect to n/v ratios of the most commonly installed transmission type is within 8 per cent;

(e) Number of powered axles.

6.3.2.1.3. If an alternative parameter such as a higher nmin\_drive, as specified in paragraph 2.(k) of Annex B2, or ASM, as defined in paragraph 3.4. of Annex B2 is used, this parameter shall be the same within an interpolation family.

6.3.2.2. Interpolation family for NOVC-HEVs and OVC-HEVs

In addition to the requirements of paragraph 6.3.2.1., only OVC-HEVs and NOVC-HEVs that are identical with respect to the following characteristics may be part of the same interpolation family:

(a) Type and number of electric machines: construction type (asynchronous/ synchronous, etc.), type of coolant (air, liquid) and any other characteristics having a non-negligible influence on CO2 emission and electric energy consumption under WLTP conditions;

(b) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));

(c) Type of electric energy converter between the electric machine and traction REESS, between the traction REESS and low voltage power supply and between the recharge-plug-in and traction REESS, and any other characteristics having a non-negligible influence on CO2 emission and electric energy consumption under WLTP conditions. At the request of the manufacturer and with the approval of the approval authority, electric energy converters between recharge-plug-in and traction REESS with lower recharge losses may be included in the family;

(d) The difference between the number of charge-depleting cycles from the beginning of the test up to and including the transition cycle shall not be more than one.

6.3.2.3. Interpolation family for PEVs

Only PEVs that are identical with respect to the following electric powertrain/transmission characteristics may be part of the same interpolation family:

(a) Type and number of electric machines: construction type (asynchronous/ synchronous, etc.), type of coolant (air, liquid) and any other characteristics having a non-negligible influence on electric energy consumption and range under WLTP conditions;

(b) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));

(c) Transmission type (e.g. manual, automatic, CVT) and transmission model (e.g. torque rating, number of gears, numbers of clutches, etc.);

(d) Number of powered axles;

(e) Type of electric energy converter between the electric machine and traction REESS, between the traction REESS and low voltage power supply and between the recharge-plug-in and traction REESS, and any other characteristics having a non-negligible influence on electric energy consumption and range under WLTP conditions. At the request of the manufacturer and with the approval of the approval authority, electric energy converters between recharge-plug-in and traction REESS with lower recharge losses may be included in the family;

(f) Operation strategy of all components influencing the electric energy consumption within the powertrain;

(g) n/v ratios (engine rotational speed divided by vehicle speed). This requirement shall be considered fulfilled if, for all transmission ratios concerned, the difference with respect to the n/v ratios of the most commonly installed transmission type and model is within 8 per cent.

6.3.2.4. Interpolation family for OVC-FCHVs and NOVC-FCHVs

Only OVC-FCHVs and NOVC-FCHVs that are identical with respect to the following electric powertrain/fuel cell/transmission characteristics may be part of the same interpolation family:

(a) Type and number of electric machines: construction type (asynchronous/ synchronous, etc.), type of coolant (air, liquid) and any other characteristics having a non-negligible influence on fuel consumption (or fuel efficiency) and electric energy consumption under WLTP conditions;

(b) Type of fuel cell (model, nominal voltage, type of coolant (air, liquid)), and also other fuel cell subsystems or characteristics that have a non-negligible influence on fuel consumption (or fuel efficiency) under WLTP conditions;

(c) Type of traction REESS (type of cell, capacity, nominal voltage, nominal power, type of coolant (air, liquid));

(d) Transmission type (e.g. manual, automatic, CVT) and transmission model (e.g. torque rating, number of gears, numbers of clutches, etc.);

(e) Number of powered axles;

(f) Type of electric energy converter between the electric machine and traction REESS, between the traction REESS and low voltage power supply and between the recharge-plug-in and traction REESS, and any other characteristics having a non-negligible influence on fuel consumption (or fuel efficiency) and electric energy consumption under WLTP conditions. At the request of the manufacturer and with the approval of the approval authority, electric energy converters between recharge-plug-in and traction REESS with lower recharge losses may be included in the family;

(g) Operation strategy of all components influencing the fuel consumption (or fuel efficiency) and electric energy consumption within the powertrain;

(h) n/v ratios. This requirement shall be considered fulfilled if, for all transmission ratios concerned, the difference with respect to the n/v ratios of the most commonly installed transmission type and model is within 8 per cent.

6.3.3. Road load family

Only vehicles that are identical with respect to the following characteristics may be part of the same road load family:

(a) Transmission type (e.g. manual, automatic, CVT) and transmission model (e.g. torque rating, number of gears, number of clutches, etc.). At the request of the manufacturer and with approval of the responsible authority, a transmission with lower power losses may be included in the family;

(b) Number of powered axles.

If at least one electric machine is coupled in the gearbox position neutral and the vehicle is not equipped with a coastdown mode (paragraph 4.2.1.8.5. of Annex B4) such that the electric machine has no influence on the road load, the criteria in paragraph 6.3.2.2. (a) and paragraph 6.3.2.3. (a) shall apply.

If there is a difference, apart from vehicle mass, rolling resistance and aerodynamics, that has a non-negligible influence on road load, that vehicle shall not be considered to be part of the family unless approved by the responsible authority.

6.3.4. Road load matrix family

The road load matrix family may be applied for vehicles with a technically permissible maximum laden mass ≥ 3,000 kg.

Vehicles with a technically permissible maximum laden mass ≥ 2,500 kg may be part of the road load matrix family provided the driver seat R-point height is above 850 mm from the ground.

“R-point” means “R” point or “seating reference point” as defined in paragraph 2.4. of Annex 1 to the Consolidated Resolution on the Construction of Vehicles (R.E.3.).

Only vehicles which are identical with respect to the following characteristics may be part of the same road load matrix family:

(a) Transmission type (e.g. manual, automatic, CVT);

(b) Number of powered axles.

6.3.5. Periodically regenerating systems (Ki) family

Only vehicles that are identical with respect to the following characteristics may be part of the same periodically regenerating systems family:

(a) Type of internal combustion engine: fuel type, combustion process;

(b) Periodically regenerating system (i.e. catalyst, particulate trap);

(i) Construction (i.e. type of enclosure, type of precious metal, type of substrate, cell density);

(ii) Type and working principle;

(iii) Volume ±10 per cent;

(iv) Location (temperature ±100 °C at second highest reference speed).

(c) The test mass of each vehicle in the family shall be less than or equal to the test mass of the vehicle used for the Ki demonstration test plus 250 kg.

6.3.6. Gas Fuelled Vehicles (GFV) Family

6.3.6.1. GFVs may be grouped into a family of vehicle types fuelled by LPG or NG/biomethane which are then identified by a parent vehicle. For vehicles which can also be fuelled by liquid fuels, this grouping only applies when the vehicle is operated in a gas fuelled mode.

6.3.6.2. A GFV parent vehicle is a vehicle that is selected to act as the vehicle on which the self-adaptability of a fuelling system is going to be demonstrated, and to which the members of a GFV family refer. It is possible to have more than one parent vehicle in a GFV family.

6.3.6.3. Member of the GFV family

6.3.6.3.1. Only vehicles which share the following essential characteristics with its GFV parent(s) may be grouped in a GFV family:

(a) It is produced by the same manufacturer;

(b) It is subject to the same emission limits;

(c) If the gas fuelling system has a central metering for the whole engine:

It has a certified power output between 0.7 and 1.15 times that of the GFV parent vehicle;

(d) If the gas fuelling system has an individual metering per cylinder:

It has a certified power output per cylinder between 0.7 and 1.15 times that of the GFV parent vehicle;

(e) If fitted with a catalyst, it has the same type of catalyst i.e. three-way, oxidation, de-NOx;

(f) It has a gas fuelling system (including the pressure regulator) from the same system manufacturer and of the same type: induction, vapour injection (single point, multipoint), liquid injection (single point, multipoint);

(g) This gas fuelling system is controlled by an ECU of the same type and technical specification, containing the same software principles and control strategy. The vehicle may have a second ECU compared to the GFV parent vehicle, provided that the ECU is only used to control the injectors, additional shut-off valves and the data acquisition from additional sensors.

6.3.6.3.2. With regard to requirements of paragraph 6.3.6.3.1. (c) and (d):

In the case where a demonstration shows that two gas-fuelled vehicles could be members of the same family with the exception of their certified power output, respectively P1 and P2 (P1 < P2), and both are tested as if were parent vehicles the family relation will be considered valid for any vehicle with a certified power output between 0.7 P1 and 1.15 P2.

6.3.7. Additional requirements for vehicles fuelled by LPG or NG/biomethane

6.3.7.1. The additional requirements for vehicles fuelled by LPG or NG/biomethane are provided in Annex B6.

6.3.7.2. For the Type 1 test set out in Annexes Part B, mono-fuel gas vehicles shall be tested in the Type 1 test for variation in the composition of either LPG or NG/biomethane, as set out in Annex B6 for pollutant emissions, with the fuel used for the measurement of the net power in accordance with UN Regulation No. 85.

6.3.7.3. Bi-fuel gas vehicles shall be tested with petrol and either LPG or NG/biomethane. The tests on LPG or NG/biomethane shall be performed for variation in the composition of LPG or NG/biomethane, as set out in Annex B6 for pollutant emissions, and with the fuel used for the measurement of the net power in accordance with UN Regulation No. 85.

6.3.8. Additional requirements for flex fuel vehicles

6.3.8.1. For flex fuel vehicles, the transition from one reference fuel to another between the tests shall take place without manual adjustment of the engine settings.

6.3.9. OBFCM

The OBFCM device shall determine the parameters and store the lifetime values on board the vehicle in accordance to Appendix 5.

6.3.10. Limits for gaseous emissions and the mass of particulates and number of particles (if PN measurement is required)

The resulting masses of gaseous emissions and the mass of particulates and number of particles (if PN measurement is required) obtained shall be less than the limits shown in Table 1A and Table 1B (as applicable):

Table 1A

**Emissions limits for the Type 1 test which apply to the emissions from the 4 phases of a WLTP test**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | *Reference mass*  *(RM) (kg)* | *Limit values* | | | | | | | | | | | | | |
| *Mass of carbon monoxide (CO)* | | *Mass of total hydrocarbons*  *(THC)* | | *Mass of non-methane hydrocarbons*  *(NMHC)* | | *Mass of oxides  of nitrogen*  *(NOx)* | | *Combined mass of hydrocarbons and oxides of nitrogen*  *(THC + NOx)* | | *Mass of  particulate matter*  *(PM)* | | *Particle Number*  *(PN)* | |
| *L1*  *(mg/km)* | | *L2*  *(mg/km)* | | *L3*  *(mg/km)* | | *L4*  *(mg/km)* | | *L2 + L4*  *(mg/km)* | | *L5*  *(mg/km)* | | *L6*  *(#/km)* | |
| *Category* | *Class* |  | *PI* | *CI* | *PI* | *CI* | *PI* | *CI* | *PI* | *CI* | *PI* | *CI* | *PI1* | *CI* | *PI1,* | *CI* |
| M | — | All | 1,000 | 500 | 100 | — | 68 | — | 60 | 80 | — | 170 | 4.5 | 4.5 | 6.0 × 1011 | 6.0 × 1011 |
| N1 | I | RM ≤ 1,305 | 1,000 | 500 | 100 | — | 68 | — | 60 | 80 | — | 170 | 4.5 | 4.5 | 6.0 × 1011 | 6.0 × 1011 |
| II | 1,305 < RM ≤ 1,760 | 1,810 | 630 | 130 | — | 90 | — | 75 | 105 | — | 195 | 4.5 | 4.5 | 6.0 × 1011 | 6.0 × 1011 |
| III | 1,760 < RM | 2,270 | 740 | 160 | — | 108 | — | 82 | 125 | — | 215 | 4.5 | 4.5 | 6.0 × 1011 | 6.0 × 1011 |
| N2 | — | All | 2,270 | 740 | 160 | — | 108 | — | 82 | 125 | — | 215 | 4.5 | 4.5 | 6.0 × 1011 | 6.0 × 1011 |
| PI Positive Ignition  CI Compression Ignition  1 Positive ignition particulate mass and number limits shall apply only to vehicles with direct injection engines. | | | | | | | | | | | | | | | | |

Table 1B

**Emissions limits for the Type 1 test which apply to the emissions from the first 3 phases of a WLTP test**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | *Technically permissible maximum laden mass*  *(GVW) (kg)* |  | *Limit values* | | | | | | | | |
| *Mass of carbon monoxide (CO)* | | | *Mass of non-methane hydrocarbons*  *(NMHC)* | | *Mass of oxides  of nitrogen*  *(NOx)* | | | *Mass of  particulate matter*  *(PM)* | |
| *L1*  *(mg/km)* | | | *L3*  *(mg/km)* | | *L4*  *(mg/km)* | | | *L5*  *(mg/km)* | |
| *Category* | | *Class* |  | *G, O* | | *D* | *G,O* | *D* | *G* | *D* | *O* | *G\*1, O* | *D* |
| M | | — | All | 1,150 | | 630 | 100 | 24 | 50 | 150 | 150 | 5 | 5 |
| N1 | | —\*2 | GVW≤ 1,700 | 1,150 | | 630 | 100 | 24 | 50 | 150 | 150 | 5 | 5 |
| — | 1,700 < GVW ≤ 3,500 | 2,550 | | 630 | 150 | 24 | 70 | 240 | 240 | 7 | 7 |
| —\*3 | All | 4,020 | | — | 100 | — | 50 | — | 150 | 5 | — |
|  | |  |  |  | |  |  |  |  |  |  |  |  |
|  | G Petrol, LPG  D Diesel  O Other fuel  1 For petrol or LPG, particulate mass limits shall apply only to vehicles with direct injection engines.  2 Except vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg  3 Vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg | | | | | | | | | | | | |

6.3.11. KCO2 correction factor family for OVC-HEVs and NOVC-HEVs

It is allowed to merge two or more interpolation families into the same KCO2 correction factor family if newly merged interpolation families meet at least one of the following criteria defined in (a) to (e) of this paragraph. The representative KCO2 shall be determined with preferably highest energy demand vehicle H within a family. At the request of the responsible authority, the manufacturer shall provide evidence on the justification and technical criteria for merging these interpolation families in the following cases:

Two or more interpolation families are merged:

1. Which were split because the maximum interpolation range of 20 g/km CO2 is exceeded (in case vehicle M measured: 30 g/km);
2. Which were split due to different engine power ratings of the same physical combustion engine (different power only related to software);
3. Which were split because the n/v ratios are just outside the tolerance of 8 per cent;
4. Which were split, but still fulfil all the family criteria of a single IP family;
5. Which were split because there is a different number of powered axles.

Different electric energy converters between recharge-plug-in and traction REESS shall not be considered as a criterion in the context of the correction factor family.

6.4. (Reserved)

6.5. (Reserved)

6.6. Type 4 test (Determination of evaporative emissions)

6.6.1. The Type 4 test shall be carried out on all vehicles with a petrol tank in accordance with the requirements of paragraphs 6.6.2. to 6.6.4. and Annex C3.

6.6.2. When tested in accordance with Annex C3 to this Regulation, evaporative emissions shall be less than that specified in Table 2.

Table 2

**Emission limit for evaporative emissions test**

|  |
| --- |
| Mass of Evaporative Emission (g/test) |
| 2.0 |

6.6.3. Evaporative emission family

6.6.3.1. Only vehicles that are identical with respect to the characteristics listed in (a), (d) and (e), technically equivalent with respect to the characteristics listed in (b) and (c) and similar or, where applicable, within the stated tolerance regarding the characteristics listed in (f) and (g) may be part of the same evaporative emission family:

(a) Fuel tank system material and construction;

(b) Vapour hose material;

(c) Fuel line material and connection technique;

(d) Sealed tank or non-sealed tank system;

(e) Fuel tank relief valve setting (air ingestion and relief);

(f) Carbon canister butane working capacity (BWC300) within a 10 per cent range of the highest value (for carbon canisters with the same type of charcoal, the volume of charcoal shall be within 10 per cent of that for which the BWC300 was determined);

(g) Purge control system (for example, type of valve, purge control strategy).

The manufacturer shall demonstrate the technical equivalence of points (b) and (c) to the responsible authority.

6.6.3.2. The vehicle shall be considered to produce worst-case evaporative emissions and shall be used for testing if it has the largest ratio of fuel tank capacity to BWC300 within the family. The vehicle selection shall be agreed in advance with the responsible authority.

6.6.3.3. The use of any innovative system calibration, configuration, or hardware related to the evaporative control system shall place the vehicle model in a different family.

6.6.4. The responsible authority shall not grant type approval if the information provided is insufficient to demonstrate that the evaporative emissions are effectively limited during the normal use of the vehicle.

6.7. Type 5 test (Description of the endurance test for verifying the durability of pollution control devices)

6.7.1. This test shall be carried out on all vehicles referred to in paragraph 1. to which the test specified in paragraph 6.3. applies. The test represents an ageing test up to the target useful life driven in accordance with the programme described in Annex C4 to this Regulation on a test track, on the road or on a chassis dynamometer.

The target useful life is 160,000 km.

6.7.1.1. Vehicles that can be fuelled either with petrol or with LPG or NG should be tested in the Type 5 test on petrol only. In that case the deterioration factor found with unleaded petrol will also be taken for LPG or NG.

6.7.1.2. Special requirements for hybrid vehicles are provided in Appendix 4 to Annex C4.

6.7.2. Notwithstanding the requirement of paragraph 6.7.1., a manufacturer may choose to have the deterioration factors from Tables 3a and 3b used as an alternative to testing to paragraph 6.7.1.

Table 3a

**Multiplicative Deterioration factors (for emissions measurements to be compared against the limits in Table 1A)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Engine Category* | *Assigned multiplicative deterioration factors* | | | | | | |
| *CO* | *THC* | *NMHC* | *NOx* | *HC + NOx* | *Particulate*  *Matter (PM)* | *Particles (PN)* |
| Positive ignition | 1.5 | 1.3 | 1.3 | 1.6 | - | 1.0 | 1.0 |
| Compression-ignition | As there are no assigned deterioration factors for compression ignition vehicles, manufacturers shall use the whole vehicle or bench ageing durability test procedures to establish deterioration factors. | | | | | | |

Table 3b

**Additive Deterioration factors (for emissions measurements to be compared against the limits in Table 1B)**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | *Technically Permissible Maximum Laden Mass*  *(GVW) (kg)* | *Assigned additive deterioration factors* | | | | | | | | |
| *Mass of carbon monoxide (CO)* | | *Mass of non-methane hydrocarbons*  *(NMHC)* | | *Mass of oxides  of nitrogen*  *(NOx)* | | | *Mass of  particulate matter*  *(PM)* | |
| *L1*  *(mg/km)* | | *L3*  *(mg/km)* | | *L4*  *(mg/km)* | | | *L5*  *(mg/km)* | |
| *Category* | *Class* |  | *G* | *D, O* | *G* | *D,O* | *G* | *D* | *O* | *G\*1* | *D, O* |
| M | — | All | 127 | \*4 | 12 | \*4 | 11 | \*4 | \*4 | 0 | \*4 |
| N1 | —\*2 | GVW≤ 1,700 | 127 | 12 | 11 | 0 |
| — | 1,700 < GVW ≤ 3,500 | 281 | 18 | 15 | 0 |
| —\*3 | All | 327 | — | 9 | — | 8 | — | 0 | — |
| G Petrol, LPG  D Diesel  O Other fuel  \*1For petrol or LPG, particulate mass and particle number limits shall apply only to vehicles with direct injection engines.  \*2Except vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg.  \*3Vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40m, vehicle width less than or equal to 1.48m, and vehicle height less than or equal to 2.00m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350kg.  \*4As there are no assigned deterioration factors for compression ignition vehicles, manufacturers shall use the whole vehicle ageing durability test procedures to establish deterioration factors. | | | | | | | | | | | |

6.7.2.1. This paragraph is only applicable for emissions measurements to be compared

against the limits in Table 1B

In the case that the limit value is different from the value defined in Table 1B, the assigned additive deterioration factor shall be calculated using the following equation and shall be rounded according to approval authority instruction:

the assigned additive deterioration factor = Limit value \* A \* (Useful life –3,000)/(80,000 – 3,000)

where :

A 0.11 for CO, 0.12 for NMHC, 0.21 for NOx and 0.00 for PM.

6.7.3. (Reserved)

6.7.4. Deterioration factors are determined using one of the procedures specified in paragraph 1.1. of Annex C4 (as applicable). The factors are used to establish compliance with the requirements of paragraphs 6.3. and 8.2.

6.7.5. Durability family

Only vehicles whose engine or pollution control system parameters are identical or remain within the prescribed tolerances with reference to the vehicle used for the determination of the Deterioration Factor may be part of the same Durability family:

(a) Engine

(i) Ratio between engine cylinder capacity and the volume of each catalytic component and/or filter (-10 to +5 per cent);

(ii) Difference in engine capacity within either ±15 per cent of the capacity of the tested vehicle or ±820 cm3 whichever value presents the least difference;

(iii) Cylinder configuration (number of cylinders, shape, distance between bores and other configurations);

(iv) Number of valves, control of valves, and camshaft driven method;

(v) Fuel type and fuel system;

(vi) Combustion process.

(b) Pollution control system parameters:

(i) Catalytic converters and particulate filters:

number and layout of catalytic converters, filters and elements,

type of catalytic activity (oxidizing, three-way, lean NOx trap, SCR, lean NOx catalyst or other), and filtering characteristics;

precious metal load (identical or higher),

precious metal type and ratio (± 15 per cent),

substrate (structure and material),

cell density.

(ii) Air injection:

with or without

type (pulsair, air pumps, other(s))

(iii) EGR:

with or without

type (cooled or non-cooled, active or passive control, high pressure/low pressure/combined pressure).

(iv) other devices having an influence on durability.

6.8. On-board diagnostics OBD – Test

This test shall be carried out on vehicle types as indicated in Table A. The test procedure described in paragraph 3. of Annex C5 to this Regulation shall be followed.

6.8.1. OBD family

6.8.1.1. Parameters defining the OBD family

The OBD family means a manufacturer's grouping of vehicles which, through their design, are expected to have similar exhaust emission and OBD system characteristics. Each engine of this family shall comply with the requirements of this Regulation.

The OBD family may be defined by basic design parameters which shall be common to vehicles within the family. In some cases there may be interaction of parameters. These effects shall also be taken into consideration to ensure that only vehicles with similar exhaust emission characteristics are included within an OBD family.

6.8.1.2. To this end, those vehicles whose parameters described below are identical may be considered to belong to the same OBD family.

Engine:

(a) Combustion process (i.e. positive ignition, compression-ignition, two-stroke, four-stroke/rotary);

(b) Method of engine fuelling (i.e. single or multi-point fuel injection); and

(c) Fuel type (i.e. petrol, diesel, flex fuel petrol/ethanol, flex fuel diesel/ biodiesel, NG/biomethane, LPG, bi fuel petrol/NG/biomethane, bi- fuel petrol/LPG).

Emission control system:

(a) Type of catalytic converter (i.e. oxidation, three-way, heated catalyst, SCR, other);

(b) Type of particulate trap;

(c) Secondary air injection (i.e. with or without); and

(d) Exhaust gas recirculation (i.e. with or without);

OBD parts and functioning:

The methods of OBD functional monitoring malfunction detection and malfunction indication to the vehicle driver.

6.8.2. OBD thresholds

The OBD thresholds referred to in Annex C5 are specified in Table 4A and Table 4B.

Table 4A

**OBD thresholds**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | *Reference mass*  *(RM)*  *(kg)* | *Mass of carbon monoxide* | | *Mass of non-methane hydrocarbons* | | *Mass of oxides of nitrogen* | | *Mass of particulate matter1* | | |
| *(CO)*  *(mg/km)* | | *(NMHC)*  *(mg/km)* | | *(NOx)*  *(mg/km)* | | *(PM)*  *(mg/km)* | | |
| Category | Class |  | PI | CI | PI | CI | PI | CI | CI | PI |  |
| M | — | All | 1,900 | 1,750 | 170 | 290 | 90 | 140 | 12 | 12 |  |
| N1 | I | RM ≤ 1305 | 1,900 | 1,750 | 170 | 290 | 90 | 140 | 12 | 12 |  |
| II | 1305 < RM ≤ 1760 | 3,400 | 2,200 | 225 | 320 | 110 | 180 | 12 | 12 |  |
| III | 1760 < RM | 4,300 | 2,500 | 270 | 350 | 120 | 220 | 12 | 12 |  |
| N2 | — | All | 4,300 | 2,500 | 270 | 350 | 120 | 220 | 12 | 12 |  |

PI Positive Ignition

CI Compression Ignition.

1 Positive ignition particulate mass OBD thresholds apply only to vehicles with direct injection engines

Table 4B

**OBD thresholds**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | *Reference mass*  *(RM)*  *(kg)* | *Mass of carbon monoxide* | | *Mass of non-methane hydrocarbons* | | *Mass of oxides of nitrogen* | | *Mass of particulate matter1* | | |
| *(CO)*  *(mg/km)* | | *(NMHC)*  *(mg/km)* | | *(NOx)*  *(mg/km)* | | *(PM)*  *(mg/km)* | | |
| Category | Class |  | G | D | G | D | G | D | G | D |  |
| M | — | All | 4,060 | — | 320 | — | 300 | — | — | — |  |
| N1 | —\*1 | GVW≤ 1,700 | 4,060 | — | 320 | — | 300 | — | — | — |  |
| — | 1,700 < GVW ≤ 3,500 | 8,960 | — | 460 | — | 410 | — | — | — |  |
|  |  |  |  |  |  |  |  |  |  |  |
| —\*2 | All | 14,120 | — | 320 | — | 300 | — | — | — |  |

G Petrol, LPG

D Diesel

\*1 Except vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40 m, vehicle width less than or equal to 1.48 m, and vehicle height less than or equal to 2.00 m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350 kg

\*2 Vehicles having engine displacement less than or equal to 0.660 litre, vehicle length less than or equal to 3.40 m, vehicle width less than or equal to 1.48 m, and vehicle height less than or equal to 2.00 m, seats less than or equal to 3 in addition to a driver, and payload less than or equal to 350 kg

6.9. Vehicles that use a reagent for the exhaust after-treatment system

6.9.1. Vehicles that use a reagent for the exhaust after-treatment system shall meet the requirements specified in Appendix 6 to this Regulation.

6.9.2. Exhaust after-treatment system using reagent (ER) family definition

Only vehicles that are identical with respect to the following characteristics may be part of the same ER family:

1. Reagent injector (principle, construction)
2. Reagent injector location
3. Detection strategies (for reagent level, dosing and quality or for reagent level and monitoring NOx emissions)
4. Warning display: messages, tell-tales lighting sequences and audible component sequences, if any
5. Inducement option
6. NOx sensor (application of option described in paragraph 6 of Appendix 6) or reagent quality sensor (application of option described in paragraphs 4 and 5 of Appendix 6)

The manufacturer and the approval authority shall agree which vehicle model is representative for the ER family.

7. Modification and extension of the type approval

7.1. Every modification of the vehicle type shall be notified to the Type Approval Authority that approved the vehicle type. The Type Approval Authority may then either:

7.1.1. Consider that the modifications made are contained within the families covered by the approval or are unlikely to have an appreciable adverse effect on the values of CO2 and fuel consumption or electric energy consumption and that, in this case, the original approval will be valid for the modified vehicle type; or

7.1.2. Require a further test report from the Technical Service responsible for conducting the tests.

7.2. Confirmation or refusal of approval, specifying the alterations, shall be communicated by the procedure specified in paragraph 5.3. to the Contracting Parties to the Agreement which apply this Regulation.

7.3. The Type Approval Authority issuing the extension of approval shall assign a series number to the extension and inform thereof the other Contracting Parties to the 1958 Agreement applying this Regulation by means of a communication form conforming to the model in Annex A2 to this Regulation.

7.4. Extensions for tailpipe emissions (Type 1 test) and OBFCM

7.4.1. The type-approval shall be extended without the need for further testing to vehicles if they conform to the criteria of paragraph 3.0.1. (a) and (c).

Additionally to the criteria above, in the cases when the Interpolation Family Vehicle High and/ or Vehicle Low are changed, the new Vehicle High and/or Vehicle Low shall be tested and the CO2 emission values of the tested vehicle resulting from the table below shall be less than or equal to the CO2 emission which lies on a straight line through the CO2 values of the original Vehicles Low and High when plotted against cycle energy and corresponding to the cycle energy demand of the tested vehicle.

|  |  |  |
| --- | --- | --- |
|  | For 4-phase WLTP test | For 3-phase WLTP test |
| Vehicles tested according to the Annex B6 | step 9 of Table A7/1 of Annex B7 | step 6 of Table A7/1 of Annex B7 |
| Vehicles tested according to the Annex B8 | step 8 of Table A8/5 in Annex B8 | step 6 of Table A8/5 in Annex B8 |

The measured criteria emissions shall respect the limits set out in paragraph 6.3.10.

The accuracy of the OBFCM shall be calculated for any Type 1 tests performed in order to gain an extension and shall respect the criteria set out in paragraph 4.2 of Appendix 5.

7.4.1.1. If The type-approval has been granted only in relation to Vehicle High, it shall only be extended under the circumstances (a), (b) or (c) below:

(a) To include additional vehicles which conform to the criteria of paragraph 3.0.1. (a) and (c) and have a cycle energy lower than that of Vehicle High.

(b) To create an interpolation family by testing Vehicle Low (preferably using the vehicle which was tested as Vehicle High for the original approval). In this case all vehicles covered by the extended approval shall conform to the criteria of paragraph 3.0.1. (a), (b) and (c).

(c) To create an interpolation family by renaming Vehicle High as Vehicle Low and testing Vehicle High (preferably using the vehicle which was tested as Vehicle High for the original approval). In this case all vehicles covered by the extended approval shall conform to the criteria of paragraph 3.0.1. (a), (b) and (c).

7.4.2. Vehicles with periodically regenerating systems

For Ki tests undertaken under Appendix 1 to Annex B6, the type-approval shall be extended to vehicles if they conform to the criteria of paragraph 6.3.5.

7.5. Extensions for evaporative emissions (Type 4 test)

7.5.1. For tests performed in accordance with Annex C3 the type-approval shall be extended to vehicles belonging to an approved evaporative emission family as defined in paragraph 6.6.3.

7.6. Extensions for durability of pollution control devices (Type 5 test)

7.6.1. For tests performed in accordance with Annex C4 the deterioration factors shall be extended to different vehicles and vehicle types, provided that both of the following conditions apply:

(a) The vehicles belong to the same Durability family, as defined in the paragraph 6.7.5.;

(b) The worst case Deterioration Factor (DF) derived within the Durability Family is applied. If vehicles with a cycle energy demand higher than that of the vehicle for which the DFs were established are to be included by extension, the worst case DF is determined on the vehicle with the highest temperature at the inlet of the pollution control system, measured as prescribed in paragraph 7.6.2.

7.6.2. The temperature at the inlet of the pollution control device shall be lower than the temperature of the vehicle tested for DF determination plus 50°C. It shall be checked under following stabilized conditions. A vehicle meeting the requirements of paragraph 1.2. of Annex C4 for the extended durability family shall be brought to a speed of 120 km/h or the maximum vehicle speed minus 10km/h, whichever is lower, and kept at that constant speed for at least 15 minutes at the load setting of the Type 1 test. At any time after this period, the temperature at catalyst inlet shall be measured for at least 2 continued minutes while the vehicle is kept at that constant speed and the average temperature value shall be taken as representative value.

7.7. Extension for OBD

For OBD the type approval can be extended to vehicles belonging to an approved OBD family as defined in paragraph 6.8.1.

8. Conformity of production (COP)

8.1. Every vehicle produced under a type approval according to this Regulation shall conform with regard to the vehicle type approved. The conformity of production procedures shall comply with those set out in the 1958 Agreement, Schedule 1 (E/ECE/324-E/ECE/TRANS/505/Rev.3), with the following requirements:

8.1.1. The manufacturer shall implement adequate arrangements and documented control plans and carry-out, at intervals specified in this Regulation, the necessary tests to verify continued conformity with the approved type. The manufacturer shall obtain agreement for these arrangements and control plans from the responsible authority. The responsible authority shall perform audits at specific intervals. This audit shall include production and test facilities as part of the product conformity and continued verification arrangements. Where necessary the responsible authority may require additional tests to be conducted.

8.1.2. The manufacturer shall check the conformity of production by conducting the appropriate tests in accordance with Table 8/1 and Table 8/2 and with the OBD requirements, where applicable according to Table A in paragraph 6. Where applicable and if required according to Table A, the manufacturer shall determine and report the OBFCM device accuracy in accordance with Appendix 5.

The specific procedures for conformity of production are set out in paragraphs 8.2. to 8.4. and Appendices 1 to 4.

Table 8/1

**Type 1 Applicable Type-1 CoP requirements for the different types of vehicle**

| *Type of vehicle* | *Criteria emissions* | *CO2 emissions* | *Fuel Efficiency* | *Electric energy consumption* |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
| Pure ICE | Yes | As applicable | As applicable | Not Applicable |
| NOVC-HEV | Yes | As applicable | As applicable | Not Applicable |
| OVC-HEV | Yes:  CD(1) and CS | As applicable: CS only | As applicable:  CS only | Yes:  CD only |
| PEV | Not Applicable | Not Applicable | Not Applicable | Yes |
| NOVC-FCHV | Not Applicable | Not Applicable | Exempted | Not Applicable |
| OVC-FCHV | Not Applicable | Not Applicable | Exempted | Exempted |

(1) Only if there is combustion engine operation during a valid CD Type 1 test for CoP verification

Table 8/2

**Type 4 Applicable Type 4 CoP requirements for the different vehicle types**

| *Vehicle type* | *Evaporative emissions* |
| --- | --- |
|  |  |
| ICE | Yes (1) |
| NOVC-HEV | Yes (1) |
| OVC-HEV | Yes (1) |
| PEV | Not Applicable |
| NOVC-FCHV | Not Applicable |
| OVC-FCHV | Not Applicable |

(1) Only for vehicles fuelled by petrol

8.1.3. CoP family

The manufacturer is allowed to split the CoP family into smaller CoP families.

If the vehicle production takes place in different production facilities, different CoP families shall be created for each facility. An interpolation family can be represented in one or more CoP families.

The manufacturer may request to merge these CoP families.

At the request of the manufacturer, CoP families from different production facilities may be merged. For Type 1 testing this is only permitted if the planned annual production volume of each production plant is less than 1,000. The responsible authority shall evaluate on the basis of the supplied evidence by the manufacturer whether such a merge is justified.

8.1.3.1. CoP family for Type 1 test

For the purposes of the manufacturer's conformity of production check on the Type 1 test, including, where applicable and if required, the check of the OBFCM device accuracy, the family means the conformity of production (CoP) family as specified in paragraphs 8.1.3.1.1. and 8.1.3.1.2.

8.1.3.1.1. For interpolation families as described in paragraph 6.3.2. with a planned vehicle production volume of more than 1,000 vehicles per 12 months, the CoP family for the Type 1 test shall be identical to the interpolation family.

8.1.3.1.2. For interpolation families as described in paragraph 6.3.2. with a planned production volume of 1,000 vehicles or less per 12 months, it is allowed to include other interpolation families into the same CoP family, up to a combined maximum production volume of 5,000 vehicles per 12 months. At the request of the responsible authority the manufacturer shall provide evidence on the justification and technical criteria for merging these interpolation families, ensuring that there is a large similarity between those families, for example in the following cases:

1. Two or more interpolation families are merged which were split because the maximum interpolation range of 30 g/km CO2 is exceeded;
2. Interpolation families that were split because there are different engine power ratings of the same combustion engine;
3. Interpolation families that were split because the n/v ratios are just outside the tolerance of 8%;
4. Interpolation families that were split, but still fulfil all the family criteria of a single IP family.

8.1.3.2. CoP family for Type 4 test

For the purposes of the manufacturer's conformity of production check on the Type 4 test, the family means the conformity of production (CoP) family, which shall be identical to the evaporative emissions family, as described in paragraph 6.6.3.

8.1.3.3. CoP family for OBD

For the purposes of the manufacturer's conformity of production check on OBD, the family means the conformity of production (CoP) family, which shall be identical to the OBD family, as described in paragraph 6.8.1.

8.1.4. Test frequency for the Type 1 test

8.1.4.1. The frequency for product verification on the Type 1 test performed by the manufacturer shall be based on a risk assessment methodology consistent with the international standard ISO 31000:2018 — Risk Management — Principles and guidelines, and shall have a minimum frequency per CoP family of one verification per 12 months.

8.1.4.2. If the number of vehicles produced within the CoP family exceeds 7,500 vehicles per 12 months, the minimum verification frequency per CoP family shall be determined by dividing the planned production volume per 12 months by 5,000 and mathematically rounding this number to the nearest integer.

8.1.4.3. If the number of vehicles produced within the CoP family exceeds 5,000 vehicles per month, the frequency per CoP family shall be at least one verification per month.

8.1.4.4. The product verifications shall be evenly distributed over the period of 12 months or over the production period in the case that this is less than 12 months. The last product verification shall reach a decision within 12 months unless the manufacturer can justify that an extension of a maximum of one month is necessary.

8.1.4.5. The planned production volume of the CoP family per 12-month period shall be monitored by the manufacturer on a monthly basis, and the responsible authority shall be informed if any change in the planned production volume causes changes to either the size of the CoP family or the Type 1 test frequency.

8.1.5. Test frequency for the Type 4 test

Once per 12-month period a vehicle shall be randomly taken from the CoP family described in paragraph 8.1.3.2. and subjected to the test described in Annex C3 or as an alternative at least the three tests described in Appendix 4.

8.1.6. Audits by the responsible authority

The responsible authority shall perform audits for verifying the manufacturer’s arrangements and documented control plans at the facility of the manufacturer, in all cases, with a minimum frequency of one audit per 12 months.

Where the interpolation method is used, verification of the interpolation calculation may be carried out by, or at the request of, the responsible authority as part of the audit process.

If the responsible authority is not satisfied with the audit results, physical tests shall directly be carried out on production vehicles as described in paragraphs 8.2. to 8.4. to verify the conformity of the vehicle production.

The manufacturers arrangements and documented control plans shall be based on a risk assessment methodology consistent with the international standard ISO 31000:2018 — Risk Management — Principles and guidelines.

8.1.7. Physical test verifications by the responsible authority

The normal frequency of physical test verifications by the responsible authority shall be based on the results of the auditing procedure of the manufacturer on a risk assessment methodology and in all cases with a minimum frequency of one verification test per three years. The responsible authority shall conduct these physical emission tests on production vehicles as described in paragraphs 8.2. to 8.4.

In the case that the manufacturer is conducting the physical tests, the responsible authority shall witness these tests at the manufacturer's facility.

8.1.8. Reporting

The responsible authority shall report the results of all audit checks and physical tests performed on verifying conformity of the manufacturers and file it for a period of a minimum of 10 years. These reports should be available for other responsible authorities

8.1.9. Non-conformity

In the case that a non-conformity is observed, Article 4 of the 1958 Agreement shall apply.

8.2. Checking the conformity for a Type 1 test

8.2.1. The Type 1 test shall be carried out on a minimum of three production vehicles, which shall be valid members of the CoP family as described in paragraph 8.1.3.1.

8.2.2. Vehicles shall be selected at random in the CoP family. The manufacturer shall not undertake any adjustment to the vehicles selected.

In the case that vehicles in the CoP family are assembled in different production facilities, at the request of the responsible authority the manufacturer shall adapt the selection of vehicles from across the different production facilities, without prejudice to the principle of random selection within a production facility.

In the case that multiple IP families are included in the CoP family, at the request of the responsible authority the manufacturer shall adapt the selection of vehicles from across the different interpolation families, without prejudice to the principle of random selection within an interpolation family.

8.2.3. Type 1 test procedure

8.2.3.1. Where applicable, in accordance with Table 8/1, the verification of the criteria emissions, CO2 emissions, fuel efficiency, electric energy consumption and OBFCM device accuracy, shall be carried out in accordance with the specific requirements and procedures in Appendix 1.

8.2.3.2. The statistical procedure for calculating the test criteria and to arrive at a pass or fail decision is described in Appendix 2 and in the flowchart of Figure 8/1.

Where applicable, in accordance with Table 8/1, the production of a CoP family shall be deemed to not conform when a fail decision is reached in accordance with the test criteria in Appendix 2. for one or more of the criteria emissions, CO2 emissions, fuel efficiency or electric energy consumption.

Where applicable, in accordance with Table 8/1, the production of a CoP family shall be deemed to conform once a pass decision is reached in accordance with the test criteria in Appendix 2 for all the criteria emissions, CO2 emissions, fuel efficiency or electric energy consumption.

Where applicable, in accordance with Table 8/1, when a pass decision has been reached for one criteria emission, that decision shall not be changed by any additional tests carried out to reach a decision for the other criteria emissions, CO2 emissions, fuel efficiency or electric energy consumption.

Where applicable, in accordance with Table 8/1, if a pass decision is not reached for all the criteria emissions, CO2 emissions, fuel efficiency or electric energy consumption, another vehicle is added to the sample by selecting this according to paragraph 8.2.2. and performing the Type 1 test. The statistical procedure described in Appendix 2 shall be repeated until a pass decision is reached for all the criteria emissions, CO2 emissions, fuel efficiency or electric energy consumption.

The maximum sample size shall be:

16 vehicles for CO2 emissions, fuel efficiency and electric energy consumption.

32 vehicles for criteria emissions

Figure 8/1

**Flowchart of the CoP test procedure for the Type 1 test**

Test of three vehicles

Computation of test statistic in accordance with Appendix 2

Test another vehicle, up to a maximum sample as specified

CoP family is rejected

CoP family is accepted

YES

YES

NO

NO

Is a pass decision reached for all criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption where applicable and in accordance with Table A8/1?

YES

Evaluation of the test statistic shall be omitted for those criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table A8/1, for which a pass decision is reached

NO

Does the test statistic of Appendix 2 agree with the criteria for passing the family for any criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table A8/1?

Does the test statistic of Appendix 2 agree with the criteria for failing the family for any criteria emission, CO2 emission, fuel efficiency and/or electric energy consumption, where applicable and in accordance with Table A8/1?

8.2.4. Run-in factors

8.2.4.1. At the request of the manufacturer and with the acceptance of the responsible authority, a run-in test procedure may be carried out on a vehicle of the CoP family to establish derived run-in factors for criteria emissions, CO2 emissions, fuel efficiency and/or electric energy consumption according to the test procedure in Appendix 3.

8.2.4.2. For the application of derived run-in factors, the system odometer of the CoP test vehicle Dj shall preferably be within -10 km of the mileage at the start of the 1st test and +10 km of the mileage at the start of the 2nd test on the run-in test vehicle Di, prior to when it was run in.

8.2.4.3. At the option of the manufacturer, for CO2 emissions, in g/km an assigned run-in factor of 0.98 may be applied if the system odometer setting at the start of the CoP test is less than or equal to 80 km.

At the option of the manufacturer, for fuel efficiency, in km/l, an assigned run-in factor of 1.02 may be applied if the system odometer setting at the start of the CoP test is less than or equal to 80 km.

If the assigned run-in factors for CO2 emissions and fuel efficiency are applied, no run-in factors shall be applied for criteria emissions and electric energy consumption.

8.2.4.4. (Reserved)

8.2.5. Test fuel

8.2.5.1. For the Type 4 test, the reference fuel shall be used in accordance with the specifications in paragraph 7. of Annex B3.

All remaining tests shall be conducted with reference fuels in accordance with the specifications in Annex B3 for the Type 1 test. However, at the request of the manufacturer the mileage accumulation for the run-in in paragraph 1.7. of Appendix 3 may be conducted with commercial fuel.

8.2.5.2. Tests for conformity of production of vehicles fuelled by LPG or NG/biomethane may be performed with a commercial fuel of which the C3/C4 ratio lies between those of the reference fuels in the case of LPG, or of one of the high or low caloric fuels in the case of NG/biomethane. In all cases a fuel analysis shall be presented to the responsible authority.

8.2.6. Criteria for validity of speed trace tolerances and drive trace indices of the Type 1 CoP test

The speed trace tolerances and drive trace indices shall fulfil the criteria specified in paragraph 2.6.8.3. of Annex B6.

8.3. Checking the conformity for a Type 4 test

8.3.1. The production shall be deemed to conform if the vehicle selected and tested according to paragraph 8.1.5. meets the requirements of paragraph 6.6.2., or the requirements of Appendix 4 as applicable.

8.3.2. If the vehicle tested does not satisfy the requirements of paragraph 8.3.1., a further random sample of four vehicles shall be taken from the same family without unjustified delay and subjected to the the Type 4 test described in Annex C3 or as an alternative at least the tests described in Appendix 4.

The production shall be deemed to conform if the requirements are met for at least three of these vehicles within 6 months after the initial failed test has been detected.

8.3.3. If the vehicles tested do not satisfy the requirements of paragraph 8.3.2., a further random sample shall be taken from the same family without unjustified delay and subjected to the Type 4 test described in Annex C3.

If the vehicle tested does not satisfy the requirements of Annex C3, a further random sample of four vehicles shall be taken from the same family and also subjected without unjustified delay to the Type 4 test described in Annex C3.

On request of the manufacturer, for CoP tests described in Annex C3 the Permeability Factor (PF) derived at Type Approval or the Assigned Permeability Factor (APF) may be applied.

The production shall be deemed to conform if the requirements are met for at least three of these vehicles within 24 months after the initial failed test has been detected.

8.3.4. For CoP tests described in Annex C3 which are performed on a vehicle which has completed a mileage of less than 20,000 km a canister which has been aged according to paragraph 5.1. of Annex C3 shall be used. This can be the original canister from the test vehicle or another canister of identical specification. On request of the manufacturer, for these tests either the Permeability Factor (PF) as defined in the paragraph 5.2. of Annex C3 which was established at Type Approval for the evaporative family or the Assigned Permeability Factor (APF) also defined in the paragraph 5.2. of Annex C3 shall be applied.

8.3.5. On request of the manufacturer, CoP tests described in Annex C3 may be carried out on a vehicle which has completed a minimum mileage of 20,000 km up to a maximum of 30,000 km with no modifications to the vehicle other than those described in the test procedure. When the test is carried out on a vehicle which has completed a mileage of between 20,000 km and 30,000 km, the canister aging shall be omitted and the Permeability Factor or Assigned Permeability Factor shall not be applied.

Independent of the accumulated mileage of the vehicle, non-fuel background emission sources (e.g. paint, adhesives, plastics, fuel/vapour lines, tyres, and other rubber or polymer components) can be eliminated according to paragraph 6.1. of Annex C3.

8.4. Checking the conformity of the vehicle for On-board Diagnostics (OBD)

8.4.1. When the approval authority determines that the quality of production seems unsatisfactory, a vehicle shall be randomly taken from the family and subjected to the tests described in Appendix 1 to Annex C5.

8.4.2. The production shall be deemed to conform if this vehicle meets the requirements of the tests described in Appendix 1 to Annex C5.

8.4.3. If the vehicle tested does not satisfy the requirements of paragraph 8.4.1., a further random sample of four vehicles shall be taken from the same family and subjected to the tests described in Appendix 1 to Annex C5. The tests may be carried out on vehicles which have completed a maximum of 15,000 km with no modifications.

8.4.4. The production shall be deemed to conform if at least three vehicles meet the requirements of the tests described in Appendix 1 to Annex C5.

9. Penalties for non-conformity of production

9.1. The approval granted in respect of a vehicle type pursuant to this Regulation, may be withdrawn if the requirements laid down in paragraph 8.1. are not complied with or if the vehicle or vehicles taken fail to pass the tests prescribed in paragraph 8.1.2.

9.2. If a Contracting Party to the 1958 Agreement which applies this Regulation withdraws an approval it has previously granted, it shall forthwith so notify the other Contracting Parties applying this Regulation, by means of a communication form conforming to the model in Annex A2 to this Regulation.

10. Production definitively discontinued

If the holder of the approval completely ceases to manufacture a type of vehicle approved in accordance with this Regulation, they shall so inform the Type Approval Authority which granted the approval. Upon receiving the relevant communication, that authority shall inform thereof the other Contracting Parties to the 1958 Agreement applying this Regulation by means of copies of the communication form conforming to the model in Annex A2 to this Regulation.

11.  Special provisions

11.1. By way of derogation to the obligations of Contracting Parties, the Contracting Parties applying this Regulation may refuse to accept type approvals granted on the basis of Level 1A or Level 1B to this Regulation.

12. Transitional provisions

12.1. As from the official date of entry into force of the 01 series of amendments to this Regulation, and by way of derogation to the obligations of Contracting Parties, the Contracting Parties applying this Regulation and also applying UN Regulation No. 83 may refuse to accept type approvals granted on the basis of this Regulation which are not accompanied by an approval to the 08 or a later series of amendments to UN Regulation No. 83.

12.2. Transitional provisions for Supplement 02

As from the official date of entry into force of Supplement 02 to the 01 series of amendments to this Regulation, no Contracting Party applying this Regulation shall refuse to accept type approvals according to previous Supplement versions to the 01 series of amendments to this Regulation.

Contracting Parties applying this Regulation may continue to grant extensions to existing type approvals granted prior to the entry into force of Supplement 02 to the 01 series of amendments according to Supplement 01 to the 01 series of amendments to this Regulation, where/when the extension does not require new type approval testing.

13. Names and addresses of Technical Services responsible for conducting approval tests, and of Type Approval Authorities

The Contracting Parties to the 1958 Agreement which apply this Regulation shall communicate to the United Nations Secretariat the names and addresses of the Technical Services responsible for conducting approval tests and of the Type Approval Authorities which grant approval and to which forms certifying approval or extension or refusal or withdrawal of approval, issued in other countries, are to be sent.

Appendix 1

Type 1 test CoP verification for specific vehicle types

1. General requirement

* 1. Each vehicle shall be tested on the chassis dynamometer set with the specific mass inertia setting and road load parameters of the individual vehicle. The chassis dynamometer shall be set to the target road load for the test vehicle according to the procedure specified in paragraph 7. of Annex B4.
  2. The applicable test cycle for the tested vehicle shall, in terms of cycle class, downscaling and capped speed, correspond to the test cycle used to derive cycle energy demand of that individual vehicle according to paragraph 5 of Annex B7. In the case that the alternative provision according to paragraph 10 of Annex B1 is applied (i.e. to test a vehicle on a numerically higher cycle class during type approval tests), the applicable test cycle for the tested vehicle shall also correspond to that used during type approval.

2. Verification of CoP on the criteria emissions for pure ICE vehicles, NOVC-HEVs and OVC-HEVs

2.1. The vehicle shall be tested according to the Type 1 test procedure described in Annex B6 or Annex B8.

2.2. Test value of criteria emissions (xi)

The criteria emissions test results (xi) shall be determined according to:

(a) Step 5 of Table A7/1 of Annex B7 for pure ICE vehicles;

(b) Step 5 of Table A8/5 of Annex B8 for NOVC-HEVs and charge-sustaining condition of OVC-HEVs;

(c) Step 5 of Table A8/8 of Annex B8 for the charge-depleting condition of OVC-HEVs

and, if available, applying a run-in factor as defined in paragraph 8.2.4. of this Regulation. Conformity against the applicable criteria emission limits shall be checked using the pass/fail criteria as defined in Appendix 2 of this Regulation.

3. Verification of CoP on CO2 emissions/ fuel efficiency of pure ICE vehicles

3.1. The vehicle shall be tested according to the Type 1 test procedure described in Annex B6.

3.2. Test values of CO2 emission (CO2 test-i) / Fuel efficiency (FE test-i)

The CO2 emission after 4 phases MCO2,c,5 shall be determined according to step 5 of Table A7/1 of Annex B7 and, if available, applying a run-in factor in paragraph 8.2.4. of this Regulation.

The fuel efficiency after 3 phases FEc,5 shall be determined according to step 5 of Table A7/1 of Annex B7 and, if available, applying a run-in factor in paragraph 8.2.4. of this Regulation.

3.3. Reference values of CO2 emission (CO2 declared-i) / Fuel efficiency values (FE declared-i)In the case the interpolation method is not applied, the CO2 emission value after 4 phases according to step 7 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the CO2 emission value after 4 phases MCO2,c,ind for the individual vehicle according to step 10 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

In the case the interpolation method is not applied, the fuel efficiency value after 3 phases FEc,8 according to step 8 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the fuel efficiency value after 3 phases FEc,ind for the individual vehicle according to step 10 of Table A7/1 of Annex B7 shall be used for verifying the conformity of production.

4. Verification of CoP on CO2 emissions/ fuel efficiency of NOVC-HEVs and OVC-HEVs charge-sustaining condition

4.1. The vehicle shall be tested as described in paragraph 3.3. of Annex B8 for NOVC-HEV and in paragraph 3.2.5. of Annex B8 for OVC-HEVs.

4.2. Test values of CO2 emission (CO2 test-i) / Fuel efficiency (FE test-i)

The CO2 emission after 4 phases MCO2,CS,c,5 of the NOVC-HEV and the charge-sustaining OVC-HEV shall be determined according to step 5 of Table A8/5 of Annex B8 and, if available, applying a run in factor as defined in paragraph 8.2.4. of this Regulation.

The fuel efficiency after 3 phases FECS,c,5 of the NOVC-HEV and the charge-sustaining OVC-HEV shall be determined according to step 5 of Table A8/5 of Annex B8 and, if available, applying a run-in factor as defined in paragraph 8.2.4. of this Regulation.

4.3. Reference values of CO2 emission (CO2 declared-i) / Fuel efficiency (FEdeclared-i)

In the case the interpolation method is not applied, the charge-sustaining CO2 emission value after 4 phases MCO2,CS,c,7 according to step 7 of Table A8/5 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the charge-sustaining CO2 emission value after 4 phases MCO2,CS,c,ind for the individual vehicle according to step 9 of Table A8/5 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is not applied, the charge-sustaining fuel efficiency value after 3 phases FECS,c,1 according to step 2 of Table A8/6 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the charge-sustaining fuel efficiency value after 3 phases FECS,c,ind for the individual vehicle according to step 3 of Table A8/6 of Annex B8 shall be used for verifying the conformity of production.

5. Verification of CoP on electric energy consumption of PEVs

5.1. The vehicle shall be prepared according to the procedures in paragraph 3.1.2. of Appendix 4 to Annex B8, then shall be tested as described in either paragraph 3.4.4.1. or paragraph 3.4.4.2. of Annex B8, whilst the break-off criterion for the Type 1 test procedure shall be considered to have been reached when having finished the first applicable WLTP test cycle.

5.2. Test values of electric energy consumption (ECtest-i)

The DC electric energy consumption from the REESS(s) shall be determined according to step 4 of Table A8/10 and according to step 3 of Table A8/11 of Annex B8 and, if available, applying a run-in factor as defined in paragraph 8.2.4. of this Regulation.

5.3. Reference value (ECCOP-i) of electric energy consumption

5.3.1. Consecutive cycle Type 1 test procedure values

In the case the interpolation method is not applied, the electric energy consumption value according to step 9 of Table A8/10 of Annex B8 shall be used for verifying the conformity of production.

In the case that the interpolation method is applied, the electric energy consumption value for the individual vehicle according to step 10 of Table A8/10 of Annex B8 shall be used for verifying the conformity of production.

5.3.2. Shortened Type 1 Test Procedure values

In the case the interpolation method is not applied, the electric energy consumption value according to step 8 of Table A8/11 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the electric energy consumption value for the individual vehicle according to step 9 of Table A8/11 of Annex B8 shall be used for verifying the conformity of production.

6. Verification of CoP on charge-depleting electric energy consumption of OVC-HEVs

6.1. At the request of the manufacturer it is allowed to use different test vehicles for the charge-sustaining test and charge-depleting test.

6.2. For 4-phase WLTP test

The vehicle shall be tested during conformity of production according to paragraph 6.2.1. If there is no engine start during the first cycle of the type approval procedure of this vehicle, at the option of the manufacturer the vehicle may be tested according to paragraph 6.2.2.

For 3-phase WLTP test

If there is no engine start during the first cycle of the type approval procedure of this vehicle, the vehicle shall be tested according to paragraph 6.2.2.

If there is an engine start during the first cycle of the type approval procedure of this vehicle, verification of electric energy consumption is exempted.

6.2.1. For 4-phaseWLTP test only

Charge-Depleting Type 1 test procedure

The vehicle shall be tested according to the charge-depleting Type 1 test procedure as described in paragraph 3.2.4. of Annex B8.

If deemed necessary, the manufacturer shall demonstrate that preconditioning of the traction REESS in advance of the CoP procedure is required. In such a case, at the request of the manufacturer and with approval of the approval authority, preconditioning of the traction REESS shall be done in advance of the CoP procedure according to manufacturer’s recommendation.

6.2.1.1. Test values of electric energy consumption (ECtest-i)

The electric energy consumption ECAC,CD after 4 phase WLTP test shall be determined according to step 9 of Table A8/8 of Annex B8 and, if available, applying a run-in factor as defined in paragraph 8.2.4. of this Regulation.

6.2.2. First cycle of the Charge-Depleting Type 1 Test

6.2.2.1. The vehicle shall be tested according to the charge-depleting Type 1 test as described in paragraph 3.2.4. of Annex B8, whilst the break-off criterion of the charge-depleting Type 1 test procedure shall be considered to have been reached when having finished the first applicable WLTP test cycle.

6.2.2.2. Test values of electric energy consumption (ECtest-i)

The DC electric energy consumption from the REESS(s) shall be determined according to step 12 of Table A8/8 of Annex B8 and if available, applying a run-in factor as defined in paragraph 8.2.4. of this Regulation.

6.2.2.3. In this cycle, there is no engine operation allowed. If there is engine operation, the test during conformity of production shall be considered as void.

6.3. Reference values (ECCOP-i) of electric energy consumption

6.3.1. For 4-phase WLTP test only

Conformity of production for a test according to paragraph 6.2.1.

In the case that the interpolation method is not applied, the charge-depleting electric energy consumption value ECAC,CD,final according to step 16 of Table A8/8 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the charge-depleting electric energy consumption value ECAC,CD,ind for the individual vehicle according to step 17 of Table A8/8 of Annex B8 shall be used for verifying the conformity of production.

6.3.2. Conformity of production for a test according to paragraph 6.2.2.

In the case the interpolation method is not applied, the charge-depleting electric energy consumption value according to step 16 of Table A8/8 of Annex B8 shall be used for verifying the conformity of production.

In the case the interpolation method is applied, the charge-depleting electric energy consumption value for the individual vehicle according to step 17 of Table A8/8 of Annex B8 shall be used for verifying the conformity of production.

7. The procedure for the final COP test results is shown in Table App1/1.

Table App1/1

**Procedure for calculating final COP test results**

**(CO2 applicable for 4 phase WLTP test only and FE applicable for 3 phase WLTP test only)**

| *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- |
| For criteria emissions, CO2 emission and fuel efficiency | | | |
| Annex B7 Table A7/1 Step 5  for pure ICE vehicles; | Mi,c,5, g/km;  MCO2,c,5, g/km;  FEc,5, km/l; | The criteria emissions, CO2 emission and the fuel efficiency shall be multiplied with the run-in factor determined according to paragraph 8.2.4. of this Regulation:  XN = RIC (j) × Mi,c,5 or Mi,CS, c,5 or Mi,CD,c,5  CO2 test-i = RICO2 (j) x MCO2,c,5 or MCO2,CS,c,5  FEtest-i = RIFE (j) x FEc,5  In the case that the run-in factor is not used:  XN = Mi,c,5 or Mi,CS, c,5 or Mi,CD,c,5  CO2 test-i = MCO2,c,5 or MCO2,CS,c,5  FEtest-i = FEc,5  . | XN, g/km;  CO2test-i, g/km;  FEtest-i, km/l; |
| Annex B8 Table A8/5 Step 5  for NOVC-HEVs and charge-sustaining condition of OVC-HEVs; | Mi,CS,c,5, g/km;  MCO2,CS,c,5, g/km;  FEc,5, km/l; |
| Annex B8 Table A8/8 Step 5  for the charge-depleting condition of OVC-HEVs | Mi,CD,c,5, g/km; |
| For electric energy consumption | | | |
| Annex B8 Table A8/10 Step 4 and Table A8/11 Step 3 for PEVs | ECDC,first, Wh/km; | The electric energy consumption shall be multiplied with the run-in factor determined according to paragraph 8.2.4. of this Regulation:  ECtest-i = RIEC (j) x ECDC,first or ECAC,CD or ECDC,CD,first  In the case that the run-in factor is not used:  ECtest-i = ECDC,first or ECAC,CD or ECDC,CD,first | ECtest-i, Wh/km; |
| For 4-phase WLTP test only  Annex B8 Table A8/8 Step 9  for the charge-depleting condition of OVC-HEVs tested according to paragraph 6.2.1. | ECAC,CD, Wh/km; |
| For 3-phase and 4-phase WLTP test  Annex B8 Table A8/8 Step 12  for the charge-depleting condition of OVC-HEVs tested according to paragraph 6.2.2. | ECDC,CD,first, Wh/km; |

**Appendix 2**

**Verification of conformity of production for Type 1 test - statistical method**

1. This Appendix describes the procedure to be used to verify the production conformity requirements for the Type 1 test for criteria emissions, CO2 emissions, fuel efficiency and electric energy consumption, as applicable and in accordance with Table 8/1 of this Regulation, for pure ICE, NOVC-HEV, PEV and OVC-HEV and, where applicable, to determine the OBFCM device accuracy.

Measurements of the criteria emissions, CO2 emissions, fuel efficiency and electric energy consumption, as applicable and in accordance with Table 8/1 of this Regulation, shall be carried out on a minimum number of 3 vehicles, and consecutively increase until a pass or fail decision is reached. Where applicable, the OBFCM device accuracy shall be determined for each of the N tests.

2. Criteria emissions

2.1. Statistical procedure and pass/fail criteria

2.1.1. For the criteria emissions from the 4 phases of a WLTP test:

For the total number of tests (N) and the measurement results of the tested vehicles, x1, x2, … xN, the average Xtests and the variance VAR shall be determined:

and

For OVC-HEV, in case of complete charge-depleting Type 1 test, the average emissions over the complete test of an individual vehicle shall be considered as a single value xi.

For each total number of tests, one of the three following decisions can be reached for criteria emissions, based on the criteria emission limit value L according to Table 1A in paragraph 6.3.10. of this Regulation:

(i) Pass the family if

(ii) Fail the family if

(iii) Take another measurement if:

For the measurement of criteria emissions the factor A is set at 1.05.

2.1.2. For criteria emissions from the first 3 phases of a WLTP test:

**Case A**: the manufacturer's production standard deviation is satisfactory.

With a minimum sample size of 3, the sampling procedure is set so that the probability of a lot passing a test with 40 per cent of the production defective is 0.95 (producer's risk = 5 per cent) while the probability of a lot being accepted with 65 per cent of the production defective is 0.1 (consumer's risk   
= 10 per cent).

For each of the criteria emissions given in Table 1B of paragraph 6.3.10. of this Regulation, the following procedure is used (see Figure 8/1 in paragraph 8.2.3.2. of this Regulation) where:

L = the natural logarithm of the limit value for the criteria emission,

xi = the natural logarithm of the measurement for the i-th vehicle of the sample,

s = an estimate of the production standard deviation (after taking the natural logarithm of the measurements),

n = the current sample number.

Compute for the sample the test statistic quantifying the sum of the standard deviations from the limit and defined as:



If the test statistic is greater than the pass decision number for the sample size given in Table A2/1, the criteria emission is passed;

If the test statistic is less than the fail decision number for the sample size given in Table A2/1, the pollutant is failed; otherwise, an additional vehicle is tested and the calculation reapplied to the sample with a sample size one unit greater.

Table A2/1

**Pass/fail decision criteria for the sample size**

|  |  |  |
| --- | --- | --- |
| *Cumulative number of tested vehicles (current sample size)* | *Pass decision threshold* | *Fail decision threshold* |
| 3 | 3.327 | -4.724 |
| 4 | 3.261 | -4.79 |
| 5 | 3.195 | -4.856 |
| 6 | 3.129 | -4.922 |
| 7 | 3.063 | -4.988 |
| 8 | 2.997 | -5.054 |
| 9 | 2.931 | -5.12 |
| 10 | 2.865 | -5.185 |
| 11 | 2.799 | -5.251 |
| 12 | 2.733 | -5.317 |
| 13 | 2.667 | -5.383 |
| 14 | 2.601 | -5.449 |
| 15 | 2.535 | -5.515 |
| 16 | 2.469 | -5.581 |
| 17 | 2.403 | -5.647 |
| 18 | 2.337 | -5.713 |
| 19 | 2.271 | -5.779 |
| 20 | 2.205 | -5.845 |
| 21 | 2.139 | -5.911 |
| 22 | 2.073 | -5.977 |
| 23 | 2.007 | -6.043 |
| 24 | 1.941 | -6.109 |
| 25 | 1.875 | -6.175 |
| 26 | 1.809 | -6.241 |
| 27 | 1.743 | -6.307 |
| 28 | 1.677 | -6.373 |
| 29 | 1.611 | -6.439 |
| 30 | 1.545 | -6.505 |
| 31 | 1.479 | -6.571 |
| 32 | -2.112 | -2.112 |

**Case B**: the manufacturer's evidence of production standard deviation is either not satisfactory or not available.

With a minimum sample size of 3, the sampling procedure is set so that the probability of a lot passing a test with 40 per cent of the production defective is 0.95 (producer's risk = 5 per cent) while the probability of a lot being accepted with 65 per cent of the production defective is 0.1 (consumer's risk = 10 per cent).

The measurements of the criteria emissions given in Table 1B of paragraph 6.3.10. of this Regulation are considered to be log normally distributed and shall first be transformed by taking their natural logarithms. Let m0 and m denote the minimum and maximum sample sizes respectively (m0= 3 and m = 32) and let n denote the current sample number.

If the natural logarithms of the measurements in the series are x1, x2 ..., xi and L is the natural logarithm of the limit value for the pollutant, then define:

d1 = x1 – L



and



Table A2/2

**Minimum sample size = 3**

|  |  |  |
| --- | --- | --- |
| *Sample size (n)* | *Pass decision threshold (An)* | *Fail decision threshold (Bn)* |
| 3 | -0.80381 | 16.64743 |
| 4 | -0.76339 | 7.68627 |
| 5 | -0.72982 | 4.67136 |
| 6 | -0.69962 | 3.25573 |
| 7 | -0.67129 | 2.45431 |
| 8 | -0.64406 | 1.94369 |
| 9 | -0.61750 | 1.59105 |
| 10 | -0.59135 | 1.33295 |
| 11 | -0.56542 | 1.13566 |
| 12 | -0.53960 | 0.97970 |
| 13 | -0.51379 | 0.85307 |
| 14 | -0.48791 | 0.74801 |
| 15 | -0.46191 | 0.65928 |
| 16 | -0.43573 | 0.58321 |
| 17 | -0.40933 | 0.51718 |
| 18 | -0.38266 | 0.45922 |
| 19 | -0.35570 | 0.40788 |
| 20 | -0.32840 | 0.36203 |
| 21 | -0.30072 | 0.32078 |
| 22 | -0.27263 | 0.28343 |
| 23 | -0.24410 | 0.24943 |
| 24 | -0.21509 | 0.21831 |
| 25 | -0.18557 | 0.18970 |
| 26 | -0.15550 | 0.16328 |
| 27 | -0.12483 | 0.13880 |
| 28 | -0.09354 | 0.11603 |
| 29 | -0.06159 | 0.09480 |
| 30 | -0.02892 | 0.07493 |
| 31 | 0.00449 | 0.05629 |
| 32 | 0.03876 | 0.03876 |

Table A2/2 shows values of the pass (An) and fail (Bn) decision numbers against current sample number. The test statistic is the ratio /Vn and shall be used to determine whether the series has passed or failed as follows:

For mo ≤ n ≤ m:

(i) Pass the series if 

(ii) Fail the series if 

(iii) Take another measurement if 

Remarks:

The following recursive formulae are useful for computing successive values of the test statistic:

2.1.3. A pass is reached only if a pass decision has been reached both for the requirements of paragraph 2.1.1. and 2.1.2.

If a pass decision has been reached only for the requirements in paragraph 2.1.1., the testing and statistical evaluation shall only continue for the requirements in paragraph 2.1.2. until a pass decision has been reached.

If a pass decision has been reached only for the requirements in paragraph 2.1.2., the testing and statistical evaluation shall only continue for the requirements in paragraph 2.1.1. until a pass decision has been reached.

3.CO2 emissions, fuel efficiency and electric energy consumption

3.1. Statistical procedure

3.1.1. For the CO2 emissions and electric energy consumption from the 4 phases of a WLTP test:

For the total number of tests (N) and the measurement results of the tested vehicles, x1, x2, … xN, the average Xtests and the standard deviation s shall be determined:

and

3.1.2. For fuel efficiency and electric energy consumption from the first 3 phases of a WLTP test:

For the total number of tests (N) and the measurement results of the tested vehicles, x1, x2, … xN, the average Xtests and the standard deviation σ shall be determined:

and

3.2. Statistical evaluation

3.2.1. For the CO2 emissions from the 4 phases of a WLTP test:

For the evaluation of CO2 emissions the normalised values shall be calculated as follows:

where:

CO2 test-i is the CO2 emission test value for the individual vehicle i determined according to Appendix 1 of this Regulation

CO2 declared-i is the reference CO2 value as declared for the individual vehicle i

The normalised xi values shall be used to determine the parameters Xtests and s according to paragraph 3.1.

3.2.2. For fuel efficiency from the first 3 phases of a WLTP test:

For the evaluation of fuel efficiency the normalised values shall be calculated as follows:

where:

FE test-i is the fuel efficiency test value for individual vehicle I determined according to Appendix 1 of this Regulation

FE declared-i is the reference fuel efficiency value as declared for the individual vehicle

3.2.3. For electric energy consumption from the 4 phases of WLTP test and from the first 3 phases of a WLTP test:

For the evaluation of electric energy consumption EC the normalised values shall be calculated as follows:

where:

ECtest-i is the electric energy consumption test value for individual vehicle i. determined according to Appendix 1 of this Regulation.

ECCOP-i is the reference electric energy consumption as declared for the individual vehicle i determined according to Appendix 1 of this Regulation.

The normalised xi values shall be used to determine the parameters Xtests and s according to paragraph 3.1.

3.3. Pass/fail criteria

3.3.1. Evaluation of CO2 emissions and electric energy consumption from the 4 phases of a WLTP test

For each total number of tests, one of the three following decisions can be reached, where the factor A shall be set at 1.01:

(i) Pass the family if

(ii) Fail the family if

(iii) Take another measurement if:

where:

parameters tP1,i, tP2,i, tF1,i, andtF2 are taken from the Table A2/3.

Table A2/3

**Pass/fail decision criteria for the sample size**

|  | *PASS* | | *FAIL* | |
| --- | --- | --- | --- | --- |
| *Tests (i)* | *tP1,i* | *tP2,i* | *tF1,i* | *tF2* |
| 3 | 1.686 | 0.438 | 1.686 | 0.438 |
| 4 | 1.125 | 0.425 | 1.177 | 0.438 |
| 5 | 0.850 | 0.401 | 0.953 | 0.438 |
| 6 | 0.673 | 0.370 | 0.823 | 0.438 |
| 7 | 0.544 | 0.335 | 0.734 | 0.438 |
| 8 | 0.443 | 0.299 | 0.670 | 0.438 |
| 9 | 0.361 | 0.263 | 0.620 | 0.438 |
| 10 | 0.292 | 0.226 | 0.580 | 0.438 |
| 11 | 0.232 | 0.190 | 0.546 | 0.438 |
| 12 | 0.178 | 0.153 | 0.518 | 0.438 |
| 13 | 0.129 | 0.116 | 0.494 | 0.438 |
| 14 | 0.083 | 0.078 | 0.473 | 0.438 |
| 15 | 0.040 | 0.038 | 0.455 | 0.438 |
| 16 | 0.000 | 0.000 | 0.438 | 0.438 |

3.3.2. Evaluation of fuel efficiency and electric energy consumption from the first 3 phases of a WLTP test

3.3.2.1. For the evaluation of FE (Fuel Efficiency in km/L) the following provisions apply:

(a) If 3 ≤ N\_Evaluation ≤ 10

(i) Pass the family if

(ii) Take another measurement if

(b) If N = 11

(i) Pass the family if all the following decisions can be reached

a.

b.

c.

(ii) Fail the family if one of the following decisions can be reached

a.

b.

c.

where:

N\_Evaluation is the total number of vehicle tested during the applicable evaluation

N\_CoP family is the total number of vehicle tested in the CoP family during the year

(e.g. If the total number of vehicles tested for the first evaluation is 11 and the total number of vehicles tested for the second evaluation is 4, N\_ Evaluation=4 and N\_CoP family=15)

In any case, if N\_CoP family > 10, shall be satisfied.

3.3.2.2. For the evaluation of EC (Electric consumption in Wh/km) the following provisions apply:

(a) If 3 ≤ N\_Evaluation ≤ 10

(i) Pass the family if

(ii) Take another measurement if

(b) If N = 11

(i) Pass the family if all the following decisions can be reached

a.

b.

c.

(ii) Fail the family if one of the following decisions can be reached

a.

b.

c.

where:

N\_Evaluation is the total number of vehicle tested during the applicable evaluation

N\_CoP family is the total number of vehicle tested in the CoP family during the year

(e.g. If the vehicle tested for the first evaluation is 11 and the vehicle tested for the second evaluation is 4, N\_ Evaluation=4 and N\_CoP family=15)

In any case, if N\_CoP family > 10, shall be satisfied.

3.3.2.3. If the number of vehicles produced within the CoP family exceeds 7,500 vehicles per 12 months, for the second or later evaluation, “a. If 3 ≤ N\_Evaluation ≤ 10” may be replaced by “a. If N\_Evaluation = 3” and “b. If N\_Evaluation = 11” may be replaced by “b. If N\_Evaluation = 4”. For the second or later year, this provision shall not be used for the first evaluation for the CoP family in the year.

shall be determined from the test result of first 10 tested vehicles after start of production for each CoP family. shall not be changed once σ is determined for the CoP family even for the second or later years. At the request of the manufacturer and with the approval of the responsible authority, and with reasonable evidence and appropriate data, may be changed.

3.3.3. A pass is reached only if a pass decision has been reached both for the requirements of paragraph 3.3.1. and paragraph 3.3.2.

If a pass decision has been reached only for the requirements in paragraph 3.3.1., the testing and statistical evaluation shall only continue for the requirements in paragraph 3.3.2. until a pass decision has been reached.

If a pass decision has been reached only for the requirements in paragraph 3.3.2., the testing and statistical evaluation shall only continue for the requirements in paragraph 3.3.1. until a pass decision has been reached.

3.4. For vehicles referred to in paragraph 5.11. of this Regulation the conformity of production of OBFCM devices as defined in paragraph 4.2. of Appendix 5 shall be evaluated as follows:

(1) For each single test i performed for the purposes of paragraph 3. of this appendix the value xi shall be set equal to:

1 / (1 - Accuracy)

where the Accuracy of the OBFCM device shall be determined in accordance with paragraph 4.2. of Appendix 5.

(2) The conformity of production of the OBFCM devices shall be evaluated according to the requirements of paragraph 3.3.1., but applying a factor A value of 1.0526.

(3) If for the last test N performed for the purposes of paragraph 3. the decision (iii) of paragraph 3.3.1. with regard to the conformity of production of the OBFCM devices is reached, the sequence of tests shall be continued until a final decision (i) or (ii) of paragraph 3.3.1. is reached.

The Type Approval authority shall keep a record of the determined accuracies of OBFCM device at each test as well as the decision according to paragraph 3.3.1. after each test.

Appendix 3

Run-in test procedure to determine run-in factors

1. Description of test procedure for the determination of the run-in factors

1.1. The run-in test procedure shall be conducted by the manufacturer, who shall not make any adjustments to the test vehicles that have an impact on the criteria emissions, CO2 emissions, fuel efficiency and electric energy consumption. The hardware and relevant ECU calibration of the test vehicle shall conform to the type approval vehicle. All the relevant hardware that has an impact on the criteria emissions, CO2 emissions, fuel efficiency and electric energy consumption shall have had no operation prior to the run-in test procedure.

1.2. The test vehicle shall be configured as vehicle H within the CoP family.

If the CoP family has multiple interpolation families, the test vehicle shall be configured as vehicle H of the interpolation family with the highest expected production volume within the CoP family. At the request of the manufacturer, and with approval of the responsible authority a different test vehicle may be selected.

1.2.1. Extension of run-in factor

At the request of the vehicle manufacturer and with approval by the responsible authority, the derived run-in factor for CO2, pollutant emissions, fuel efficiency and electric energy consumption can be extended to other CoP families. The vehicle manufacturer shall provide evidence on the justification and technical criteria for merging these COP families, ensuring that there is a large similarity between those families.

1.3. The test vehicle shall be a new vehicle, or a used test vehicle for which at least all of the following components are newly installed simultaneously:

1. Internal combustion engine;
2. Driveline components (at least, but not limited to, transmission, tyre, axles, etc.);
3. Brake components;
4. REESSs for EVs;
5. Exhaust system;

and any other component that has a non-negligible influence on criteria emissions, CO2 emissions, fuel efficiency and electric energy consumption.

For the new vehicle, or the used vehicle for which the above mentioned components have been replaced, the system odometer of the test vehicle Ds in km shall be recorded.

1.4. At the request of the manufacturer and with approval by the responsible authority, it is allowed to perform the run-in procedure on multiple test vehicles. In this case, the valid test results of all tested vehicles shall be considered for the determination of the run-in factors.

1.5. Chassis dynamometer setting

1.5.1. The chassis dynamometer shall be set to the target road load for the test vehicle, according to the procedure specified in paragraph 7. of Annex B4.

The chassis dynamometer shall be set independently prior to each test before the run-in mileage accumulation and shall be set once for the post-run-in tests after the run-in mileage accumulation.

1.6. Before the run-in, the test vehicle shall be tested according to the Type 1 test procedure specified in Annex B6 or Annex B8. The test shall be repeated until three valid test results have been obtained. Drive trace indexes shall be calculated according to paragraph 7. of Annex B7 and these shall fulfil the criteria specified in paragraph 2.6.8.3.1.4. of Annex B6. The system odometer setting Di shall be recorded prior to each test.

The signal of the acceleration control position shall be recorded during all tests at a sampling frequency of 10 Hz. It is allowed to use the OBD acceleration control position signal for this purpose. The responsible authority may request the manufacturer to evaluate this signal to ensure that the test result is performed correctly.

1.7. After the initial tests, the test vehicle shall be run-in under normal driving conditions. OVC-HEVs shall be driven predominantly in charge-sustaining operating conditions. The driving pattern, test conditions and fuel during the run-in shall be in accordance with the manufacturer’s engineering judgement. The run-in distance shall be less than or equivalent to the distance driven during the run-in of the vehicle which was tested for the type approval of the interpolation family, in accordance with paragraph 2.3.3. of Annex B6 or paragraph 2. of Annex B8.

1.8. After the run-in, the test vehicle shall be tested according to the Type 1 test procedure specified in Annex B6 or Annex B8. The test shall be repeated until three valid test results have been obtained.

Drive trace indexes shall be calculated according to paragraph 7. of Annex B7 and these shall fulfil the criteria specified in paragraph 2.6.8.3.1.4. of Annex B6.

These tests shall be performed in the same test cell as used for the tests prior to the run-in and by applying the same chassis dynamometer setting method. If this is not possible, the manufacturer shall justify the reason for using a different test cell. The system odometer setting Di in km shall be recorded prior to each test.

1.9. For the determination of the run-in factor for CO2 emissions of the 4 phase WLTP test, the coefficients CRI and Cconst in the following equation shall be calculated by a least squares regression analysis to four significant digits on all valid tests before and after the run-in:

where:

MCO2,i is the measured CO2 emission for test i, g/km

CRI is the slope of the logarithmic regression line

Cconst is the constant value of the logarithmic regression line

In the case that multiple vehicles have been tested, the CRI shall be calculated for each vehicle, and the resulting values shall be averaged. The manufacturer will provide statistical evidence to the responsible authority that the fit is sufficiently statistically justified.

1.9.1. Based on the deviation of the measurements from the fit, the slope CRI should be corrected downward with the standard errors of the slope:

and

MCO2,i-fit is the result of the applying the equation for each of the distances Di.

The slope CRI shall be corrected for the uncertainty in the fit by:

1.10. The run-in factor RICO2(j) for CO2 emissions after 4 phases of CoP test vehicle j shall be determined by the following equation:

where:

Dk is the average distance of the valid tests after the run-in, km

Dj is the system odometer setting of the CoP test vehicle, km

MCO2,j is the mass CO2 emission measured on the CoP test vehicle, g/km

In the case that Dj is lower than the minimum Di, Dj shall be replaced by the minimum Di.

1.11. For the determination of the run-in factor for all applicable criteria emissions after 4 phases, the coefficients CRI,c and Cconst, c shall be calculated with a least squares regression analysis to four significant digits on all valid tests before and after the run-in:

where:

MC,i is the measured mass criteria emission component C

CRI,c is the slope of the linear regression line, g/km2

Cconst,c is the constant value of the linear regression line, g/km

The manufacturer will provide statistical evidence to the responsible authority that the fit is sufficiently statistically justified and the uncertainty margin based on the variation in the data should be taken into account to avoid an overestimation of the run-in effect.

1.12. The run-in factor RIC(j) for criteria emission component C after 4 phases of CoP test vehicle j shall be determined by the following equation:

where:

Dk is the average distance of the valid tests after the run-in, km

Dj is the system odometer setting of the CoP test vehicle, km

MC,j is the mass emission of component C on the CoP test vehicle, g/km

In the case that Dj is lower than the minimum Di, Dj shall be replaced by the minimum Di.

1.13. The run-in factor RIEC(j) for electric energy consumption after 4 phases shall be determined according to the procedure specified in paragraphs 1.9., 1.9.1. and 1.10. of this appendix, where CO2 in the formulae is replaced by EC.

For fuel efficiency and electric energy consumption from the first 3 phases of a WLTP test

The run-in factor RIFE(j) for fuel efficiency and the run-in factor RIEC(j) for electric energy consumption shall be determined according to the procedure specified in paragraphs 1.9. (excluding paragraph 1.9.1.) and 1.10. of this appendix, where CO2 in the formulae is replaced by FE and EC respectively.

2. Prior to the application of the derived run-in factor for fuel efficiency, the manufacturer shall provide the following information to the responsible authority.

(a) Evidence of the derived run-in factor including the existence of statistical significance regarding the fit of the slope

(b) An explanation of the validation method to be used after the start of production, e.g. by measuring the run-in factor from selected vehicle(s) from the plant and then evaluating whether the run-in factor is appropriate or not.

Appendix 4

Conformity of production for Type 4 test

1. For routine end-of-production-line testing, as an alternative to conducting the Type 4 test as described in Annex C3 the holder of the approval may demonstrate compliance by sampling vehicles which shall meet the requirements in paragraphs 2. to 4. of this appendix.

1.1. In case of vehicles with a sealed fuel tank system, at the request of the manufacturer and in agreement with the responsible authority, alternative procedures to paragraphs 2. to 4. of this appendix can be applied.

1.2. When the manufacturer chooses to use any alternative procedure, all the details of the conformity test procedure shall be recorded in the type approval documentation.

2. Test for leakage

2.1. Vents to the atmosphere from the emission control system shall be isolated.

2.2. A pressure of 3.70 kPa ± 0.10 kPa shall be applied to the fuel system. At the request of manufacturer and with approval of the responsible authority, an alternative pressure can also be applied, taking into account the design pressures of the fuel system.

2.3. The pressure shall be allowed to stabilise prior to isolating the fuel system from the pressure source.

2.4. Following isolation of the fuel system, the pressure shall not drop by more than 0.50 kPa in five minutes.

2.5. At the request of the manufacturer and in agreement with the responsible authority the function for leakage can be demonstrated by an equivalent alternative procedure.

3. Test for venting

3.1. Vents to the atmosphere from the emission control shall be isolated.

3.2. A pressure of 3.70 kPa ± 0.10 kPa shall be applied to the fuel system. At the request of manufacturer and with approval of the responsible authority, an alternative pressure can also be applied, taking into account the pressure range in use of the fuel system.

3.3. The pressure shall be allowed to stabilise prior to isolating the fuel system from the pressure source.

3.4. The venting outlets from the emission control systems to the atmosphere shall be reinstated to the production condition.

3.5. The pressure of the fuel system shall drop to below a pressure less than 2.5 kPa above ambient pressure within one minute.

3.6. At the request of the manufacturer and in agreement with the responsible authority the functional capacity for venting can be demonstrated, when applicable, by an equivalent alternative procedure. In this case the pressures and times stated in paragraphs 3.2. and 3.5. may be adapted to take into account the design parameters of the fuel system.

4. Purge test

4.1. Equipment capable of detecting an airflow rate of 1.0 litres in one minute shall be attached to the purge inlet and a pressure vessel of sufficient size to have negligible effect on the purge system shall be connected via a switching valve to the purge inlet, or alternatively.

4.2. The manufacturer may use a flow meter of his own choosing, if acceptable to the responsible authority.

4.3. The vehicle shall be operated in such a manner that any design feature of the purge system that could restrict purge operation is detected and the circumstances noted.

4.4. Whilst the engine is operating within the bounds noted in paragraph 4.3. of this appendix, the air flow shall be determined by either:

4.4.1. The device indicated in paragraph 4.1. of this appendix being switched in. A pressure drop from atmospheric to a level indicating that a volume of 1.0 litre of air has flowed into the evaporative emission control system within one minute shall be observed; or

4.4.2. If an alternative flow measuring device is used, a reading of no less than 1.0 litre per minute shall be detectable.

4.4.3. At the request of the manufacturer and in agreement with the responsible authority an equivalent alternative purge test procedure can be used.

Appendix 5

Devices for monitoring on board the vehicle the consumption of fuel and/or electric energy

1. Introduction

This appendix sets out the definitions and requirements applicable to the devices for monitoring on board the vehicle the consumption of fuel and/or electric energy.

2. Definitions

2.1. "*On-board Fuel and/or Energy Consumption Monitoring Device*" ("OBFCM device") means any element of design, either software and/or hardware, which senses and uses vehicle, engine, fuel and/or electric energy parameters to determine and make available at least the information laid down in paragraph 3 of this appendix, and store the lifetime values on board the vehicle.

2.2. "*Lifetime*" value of a certain quantity determined and stored at a time *t* shall be the values of this quantity accumulated since the completion of production of the vehicle until time *t*.

2.3. "*Engine fuel rate*" means the amount of fuel injected into the engine per unit of time. It does not include fuel injected directly into the pollution control device.

2.4. "*Vehicle fuel rate*" means the amount of fuel injected into the engine and directly into the pollution control device per unit of time. It does not include the fuel used by a fuel operated heater.

2.5. "*Total Fuel Consumed (lifetime)*" means the accumulation of the calculated amount of fuel injected into the engine and the calculated amount of fuel injected directly into the pollution control device. It does not include the fuel used by a fuel operated heater.

2.6. "*Total Distance Travelled (lifetime)*" means the accumulation of the distance travelled using the same data source that the vehicle odometer uses.

2.7. "*Grid energy*" means, for OVC-HEVs, the electric energy flowing into the battery when the vehicle is connected to an external power supply and the engine is turned off. It shall not include electrical losses between the external power source and the battery.

2.8. "*Charge-sustaining operation*" means, for OVC-HEVs, the state of vehicle operation when the REESS state of charge (SOC) may fluctuate but the intent of the vehicle control system is to maintain, on average, the current state of charge.

2.9. "*Charge-depleting operation*" means, for OVC-HEVs, the state of vehicle operation when the current REESS SOC is higher than the charge-sustaining target SOC value and, while it may fluctuate, the intent of the vehicle control system is to deplete the SOC from a higher level down to the charge sustaining target SOC value.

2.10. "*Driver-selectable charge-increasing operation*" means, for OVC-HEVs, the operating condition in which the driver has selected a mode of operation, with the intention to increase the REESS SOC.

3. Information to be determined, stored and made available

The OBFCM device shall determine at least the following parameters and store the lifetime values on board the vehicle. The parameters shall be calculated and scaled according the standards referred to in paragraph 6.5.3.2 (a) of Appendix 1 to Annex C5.

The information listed in paragraph 3.1. and 3.2. shall be made available as signals through the serial port connector referred to in paragraph [6.5.3.2](https://protect-eu.mimecast.com/s/xajYCY5XYIL4zNC0wtmM?domain=6.5.3.2) (c). of Appendix 1 to Annex C5.

3.1. For all vehicles referred to in paragraph 5.11. of this Regulation, with the exception of OVC-HEVs:

(a) Total fuel consumed (lifetime) (litres);

(b) Total distance travelled (lifetime) (kilometres);

(c) Engine fuel rate (grams/second);

(d) Engine fuel rate (litres/hour);

(e) Vehicle fuel rate (grams/second);

(f) Vehicle speed (kilometres/hour).

3.2. For OVC-HEVs:

(a) Total fuel consumed (lifetime) (litres);

(b) Total fuel consumed in charge-depleting operation (lifetime) (litres);

(c) Total fuel consumed in driver-selectable charge-increasing operation (lifetime) (litres);

(d) Total distance travelled (lifetime) (kilometres);

(e) Total distance travelled in charge-depleting operation with engine off (lifetime) (kilometres);

(f) Total distance travelled in charge-depleting operation with engine running (lifetime) (kilometres);

(g) Total distance travelled in driver-selectable charge-increasing operation (lifetime) (kilometres);

(h) Engine fuel rate (grams/second);

(i) Engine fuel rate (litres/hour);

(j) Vehicle fuel rate (grams/second);

(k) Vehicle speed (kilometres/hour);

(l) Total grid energy into the battery (lifetime) (kWh).

4. Accuracy

4.1. With regard to the information specified in paragraph 3, the manufacturer shall ensure that the OBFCM device provides the most accurate values that can be achieved by the measurement and calculation system of the engine control unit.

4.2. Notwithstanding paragraph 4.1, the manufacturer shall ensure that the accuracy is higher than – 0.05 and lower than 0.05 calculated with three decimals using the following formula:



Where:

Fuel\_ConsumedWLTP (litres) is the fuel consumption determined at the first test carried out in accordance with paragraph 1.2. of Annex B6, calculated in accordance with paragraph 6. of Annex B7, using emission results over the total cycle before applying corrections (output of step 2 in Table A7/1 of Annex B7), multiplied by the actual distance driven and divided by 100.

Fuel\_ConsumedOBFCM (litres) is the fuel consumption determined for the same test using the differentials of the parameter ‘Total fuel consumed (lifetime)’ as provided by the OBFCM device.

For OVC-HEVs the charge-sustaining Type 1 test shall be used.

4.2.1. If the accuracy requirements set out in paragraph 4.2. are not met, the accuracy shall be recalculated for subsequent Type 1 tests performed in accordance with paragraph 1.2 of Annex B6, in accordance with the formulae in paragraph 4.2., using the fuel consumed determined and accumulated over all performed tests. The accuracy requirement shall be deemed to be fulfilled once the accuracy is higher than – 0.05 and lower than 0.05.

4.2.2. If the accuracy requirements set out in paragraph 4.2.1. are not met following the subsequent tests pursuant to this point, additional tests may be performed for the purpose of determining the accuracy, however, the total number of tests shall not exceed three tests for a vehicle tested without using the interpolation method (vehicle H), and six tests for a vehicle tested using the interpolation method (three tests for vehicle H and three tests for vehicle L). The accuracy shall be recalculated for the additional subsequent Type 1 tests in accordance with the formulae in paragraph 4.2., using the fuel consumed determined and accumulated over all performed tests. The requirement shall be deemed to be fulfilled once the accuracy is higher than – 0.05 and lower than 0.05. Where the tests have been performed only for the purpose of determining the accuracy of the OBFCM device, the results of the additional tests shall not be taken into account for any other purposes.

5. Access to the information provided by the OBFCM device

5.1. The OBFCM device shall provide for standardised and unrestricted access of the information specified in paragraph 3. and shall conform to the standards referred to in paragraphs 6.5.3.1. (a) and 6.5.3.2. (a) of Appendix 1 to Annex C5.

5.2. By way of exemption from the reset conditions specified in the standards referred to in paragraph 5.1. and notwithstanding paragraphs 5.3. and 5.4., once the vehicle has entered into service the values of the lifetime counters shall be preserved.

5.3. The values of the lifetime counters may be reset only for those vehicles for which the memory type of the engine control unit is unable to preserve data when not powered by electricity. For those vehicles the values may be reset simultaneously only in the case the battery is disconnected from the vehicle. The obligation to preserve the values of the lifetime counters shall in this case apply for new type approvals at the latest from 1 January 2022 and for new vehicles from 1 January 2023.

5.4. In the case of malfunctioning affecting the values of the lifetime counters, or replacement of the engine control unit, the counters may be reset simultaneously to ensure that the values remain fully synchronised.

Appendix 6

Requirements for vehicles that use a reagent for the exhaust after-treatment system

1. This appendix sets out the requirements for vehicles that rely on the use of a reagent for the after-treatment system in order to reduce emissions. Every reference in this appendix to 'reagent tank' shall be understood as also applying to other containers in which a reagent is stored.

1.1. The capacity of the reagent tank shall be such that a full reagent tank does not need to be replenished over an average driving range of 5 full fuel tanks providing the reagent tank can be easily replenished (e.g. without the use of tools and without removing vehicle interior trim. The opening of an interior flap, in order to gain access for the purpose of reagent replenishment, shall not be understood as the removal of interior trim). If the reagent tank is not considered to be easy to replenish as described above, the minimum reagent tank capacity shall be at least equivalent to an average driving distance of 15 full fuel tanks. However, in the case of the option in paragraph 3.5., where the manufacturer chooses to start the warning system at a distance which may not be less than 2,400 km before the reagent tank becomes empty, the above restrictions on a minimum reagent tank capacity shall not apply.

1.2. In the context of this appendix, the term "average driving distance" shall be taken to be derived from the fuel or reagent consumption during a Type 1 test for the driving distance of a fuel tank and the driving distance of a reagent tank respectively.

2. Reagent indication

2.1. The vehicle shall include a specific indicator on the dashboard that informs the driver when reagent levels are below the threshold values specified in paragraph 3.5.

3. Driver warning system

3.1. The vehicle shall include a warning system consisting of visual alarms that informs the driver when an abnormality is detected in the reagent dosing, e.g. when emissions are too high, the reagent level is low, reagent dosing is interrupted, or the reagent is not of a quality specified by the manufacturer. The warning system may also include an audible component to alert the driver.

3.2. The warning system shall escalate in intensity as the reagent approaches empty. It shall culminate in a driver notification that cannot be easily defeated or ignored. It shall not be possible to turn off the system until the reagent has been replenished.

3.3. The visual warning shall display a message indicating a low level of reagent. The warning shall not be the same as the warning used for the purposes of OBD or other engine maintenance. The warning shall be sufficiently clear for the driver to understand that the reagent level is low (e.g. "urea level low", "AdBlue level low", or "reagent low").

3.4. The warning system does not initially need to be continuously activated, however the warning shall escalate so that it becomes continuous as the level of the reagent approaches the point where the driver inducement system in paragraph 8. comes into effect. An explicit warning shall be displayed (e.g. "fill up urea"', "fill up AdBlue", or "fill up reagent"). The continuous warning system may be temporarily interrupted by other warning signals providing that they are important safety related messages.

3.5. The warning system shall activate at a distance equivalent to a driving range of at least 2,400 km in advance of the reagent tank becoming empty, or at the choice of the manufacturer at the latest when the level of reagent in the tank reaches one of the following levels:

(a) A level expected to be sufficient for driving 150 per cent of an average driving range with a complete tank of fuel; or

(b) 10 per cent of the capacity of the reagent tank,

whichever occurs earlier.

4. Identification of incorrect reagent

4.1. The vehicle shall include a means of determining that a reagent corresponding to the characteristics declared by the manufacturer and recorded in Annex A1 is present on the vehicle.

4.2. If the reagent in the storage tank does not correspond to the minimum requirements declared by the manufacturer the driver warning system in paragraph 3. shall be activated and shall display a message indicating an appropriate warning (e.g. "incorrect urea detected", "incorrect AdBlue detected", or "incorrect reagent detected"). If the reagent quality is not rectified within 50 km of the activation of the warning system then the driver inducement requirements of paragraph 8. shall apply.

5. Reagent consumption monitoring

5.1. The vehicle shall include a means of determining reagent consumption and providing off-board access to consumption information.

5.2. Average reagent consumption and average demanded reagent consumption by the engine system shall be available via the serial port of the standard diagnostic connector. Data shall be available over the previous complete 2,400 km period of vehicle operation.

5.3. In order to monitor reagent consumption, at least the following parameters within the vehicle shall be monitored:

(a) The level of reagent in the on-vehicle storage tank; and

(b) The flow of reagent or injection of reagent as close as technically possible to the point of injection into an exhaust after-treatment system.

5.4. A deviation of more than 50 per cent between the average reagent consumption and the average demanded reagent consumption by the engine system over a period of 30 minutes of vehicle operation, shall result in the activation of the driver warning system in paragraph 3., which shall display a message indicating an appropriate warning (e.g. "urea dosing malfunction", "AdBlue dosing malfunction", or "reagent dosing malfunction"). If the reagent consumption is not rectified within 50 km of the activation of the warning system then the driver inducement requirements of paragraph 8. shall apply.

5.5. In the case of interruption in reagent dosing activity the driver warning system as referred to in paragraph 3. shall be activated, which shall display a message indicating an appropriate warning. Where the reagent dosing interruption is initiated by the engine system because the vehicle operating conditions are such that the vehicle's emission performance does not require reagent dosing, the activation of the driver warning system as referred to in paragraph 3. may be omitted, provided that the manufacturer has clearly informed the approval authority when such operating conditions apply. If the reagent dosing is not rectified within 50 km of the activation of the warning system then the driver inducement requirements of paragraph 8. shall apply.

6. Monitoring NOx emissions

6.1. As an alternative to the monitoring requirements referred to in paragraphs 4. and 5., manufacturers may use exhaust gas sensors directly to sense excess NOx levels in the exhaust.

6.2. The manufacturer shall demonstrate that use of the sensors referred to in paragraph 6.1. and any other sensors on the vehicle, results in the activation of the driver warning system as referred to in paragraph 3., the display of a message indicating an appropriate warning (e.g. “emissions too high — check urea”, “emissions too high — check AdBlue”, “emissions too high — check reagent”), and the activation of the driver inducement system as referred to in paragraph 8.3., when the situations referred to in paragraphs 4.2., 5.4., or 5.5. occur.

For the purposes of this paragraph these situations are presumed to occur if the applicable NOx OBD threshold set out in Table 4 of paragraph 6.8.2. is exceeded.

NOx emissions during the test to demonstrate compliance with these requirements shall be no more than 20 per cent higher than the OBD threshold.

7. Storage of failure information

7.1. Where reference is made to this paragraph, non-erasable Parameter Identifiers (PID) shall be stored identifying the reason for and the distance travelled by the vehicle during the inducement system activation. The vehicle shall retain a record of the PID for at least 800 days or 30,000 km of vehicle operation. The PID shall be made available via the serial port of a standard diagnostic connector upon request of a generic scan tool in accordance with the provisions of paragraph 6.5.3.1. of Appendix 1 to Annex C5. The information stored in the PID shall be linked to the period of cumulated vehicle operation, during which it has occurred, with an accuracy of not less than 300 days or 10,000 km.

7.2. Malfunctions in the reagent dosing system attributed to technical failures (e.g. mechanical or electrical faults) shall also be subject to the OBD requirements in paragraph 6.8. of this Regulation and Annex C5.

8. Driver inducement system

8.1. The vehicle shall include a driver inducement system to ensure that the vehicle operates with a functioning emission control system at all times. The inducement system shall be designed so as to ensure that the vehicle cannot operate with an empty reagent tank.

8.1.1. The requirement for a driver inducement system shall not apply to vehicles designed and constructed for use by the rescue services, armed services, civil defence, fire services and forces responsible for maintaining public order. Permanent deactivation of the driver inducement system for these vehicles shall only be done by the vehicle manufacturer.

8.2. The inducement system shall activate at the latest when the level of reagent in the tank reaches:

(a) In the case that the warning system was activated at least 2,400 km before the reagent tank was expected to become empty, a level expected to be sufficient for driving the average driving range of the vehicle with a complete tank of fuel.

(b) In the case that the warning system was activated at the level described in paragraph 3.5.(a), a level expected to be sufficient for driving 75 per cent of the average driving range of the vehicle with a complete tank of fuel;

(c) In the case that the warning system was activated at the level described in paragraph 3.5.(b), 5 per cent of the capacity of the reagent tank.

(d) In the case that the warning system was activated ahead of the levels described in both paragraph 3.5.(a) and 3.5.(b) but less than 2,400 km in advance of the reagent tank becoming empty, whichever level described in (b) or (c) of this paragraph occurs earlier.

Where the alternative described in paragraph 6.1. is utilised, the system shall activate when the irregularities described in paragraphs 4. or 5. or the NOx levels described in paragraph 6.2. have occurred.

The detection of an empty reagent tank and the irregularities mentioned in paragraphs 4., 5., or 6. shall result in the failure information storage requirements of paragraph 7. taking effect.

8.3. The manufacturer shall select which type of inducement system to install. The options for a system are described in paragraphs 8.3.1., 8.3.2. and 8.3.3.

8.3.1. A "no engine restart after countdown" approach allows a countdown of restarts or distance remaining once the inducement system activates. Engine starts initiated by the vehicle control system, such as start-stop systems, are not included in this countdown.

8.3.1.1. In the case that the warning system was activated at least 2,400 km before the reagent tank was expected to become empty, or the irregularities described in paragraphs 4. or 5. or the NOx levels described in paragraph 6.2. have occurred, engine restarts shall be prevented immediately after the vehicle has travelled a distance expected to be sufficient for driving the average driving range of the vehicle with a complete tank of fuel since the activation of the inducement system.

8.3.1.2. In the case that the inducement system was activated at the level described in paragraph 8.2.(b), engine restarts shall be prevented immediately after the vehicle has travelled a distance expected to be sufficient for driving 75 per cent of the average driving range of the vehicle with a complete tank of fuel since the activation of the inducement system.

8.3.1.3. In the case that the inducement system was activated at the level described in paragraph 8.2.(c), engine restarts shall be prevented immediately after the vehicle has travelled a distance expected to be sufficient for driving the average driving range of the vehicle with 5 per cent of the capacity of the reagent tank, since the activation of the inducement system.

8.3.1.4. In addition, engine restarts shall be prevented immediately after the reagent tank becomes empty, should this situation occur earlier than the situations specified in paragraphs 8.3.1.1., 8.3.1.2., or 8.3.1.3.

8.3.2. A "no start after refuelling" system results in a vehicle being unable to start after re-fuelling if the inducement system has activated.

8.3.3. A "fuel-lockout" approach prevents the vehicle from being refuelled by locking the fuel filler system after the inducement system activates. The lockout system shall be robust to prevent it being tampered with.

8.4. Once the inducement system has prevented engine restarts, the inducement system shall only be deactivated if the irregularities specified in paragraphs 4., 5., or 6. have been rectified or if the quantity of reagent added to the vehicle meets at least one of the following criteria:

(a) Expected to be sufficient for driving 150 per cent of an average driving range with a complete tank of fuel; or

(b) At least 10 per cent of the capacity of the reagent tank.

After a repair has been carried out to correct a fault where the OBD system has been triggered under paragraph 7.2., the inducement system may be reinitialised via the OBD serial port (e.g. by a generic scan tool) to enable the vehicle to be restarted for self-diagnosis purposes. The vehicle shall operate for a maximum of 50 km to enable the success of the repair to be validated. The inducement system shall be fully reactivated if the fault persists after this validation.

8.5. The driver warning system referred to in paragraph 3. shall display a message indicating clearly:

(a) The number of remaining restarts and/or the remaining distance; and

(b) The conditions under which the vehicle can be restarted.

8.6. Detailed written information fully describing the functional operation characteristics of the driver inducement system shall be provided to the Type Approval Authority at the time of approval.

8.7. As part of the application for type approval under this Regulation, the manufacturer shall demonstrate the operation of the driver warning and inducement systems.

9. Information requirements

9.1. The manufacturer shall provide all owners of new vehicles with clear written information about any exhaust aftertreatment system which uses a reagent. This information shall state that if such an exhaust aftertreatment system is not functioning correctly, the driver shall be informed of a problem by the driver warning system and that the driver inducement system shall consequentially result in the vehicle being unable to start.

9.2. The instructions shall indicate requirements for the proper use and maintenance of vehicles, including the proper use of consumable reagents.

9.3. The instructions shall specify if consumable reagents have to be replenished by the vehicle driver between normal maintenance intervals. They shall indicate how the vehicle driver should replenish the reagent tank. The information shall also indicate a likely rate of reagent consumption for that type of vehicle and how often it should be replenished.

9.4. The instructions shall specify that use of, and replenishing of, a required reagent of the correct specifications is mandatory for the vehicle to comply with its certificate of conformity.

9.5. The instructions shall state that it may be a criminal offence to use a vehicle that does not consume any reagent if it is required for the reduction of emissions.

9.6. The instructions shall explain how the warning system and driver inducement systems work. In addition, the consequences of ignoring the warning system and not replenishing the reagent shall be explained.

10. Operating conditions of the after-treatment system

Manufacturers shall ensure that any exhaust aftertreatment system which uses a reagent retains its emission control function during all ambient conditions, especially at low ambient temperatures. This includes taking measures to prevent the complete freezing of the reagent during parking times of up to 7 days at 258 K (-15 °C) with the reagent tank 50 per cent full. If the reagent is frozen, the manufacturer shall ensure that the reagent shall be liquefied and ready for use within 20 minutes of the vehicle being started at 258 K (-15 °C) measured inside the reagent tank.

Annexes Part A

Where relevant the Type Approval requirements and documentation included in Annexes Part A provide separate reporting tables/fields for the results after 3-phases and the results after 4-phases.

Annex A1

Engine and vehicle characteristics and information concerning the conduct of tests (‘information document’)

The following information, when applicable, shall be supplied in triplicate and include a list of contents.

If there are drawings, they shall be to an appropriate scale and show sufficient detail; they shall be presented in A4 format or folded to that format. Photographs, if any, shall show sufficient detail.

If the systems, components or separate technical units have electronic controls, information concerning their performance shall be supplied.

|  |  |  |
| --- | --- | --- |
| 0 | GENERAL | |
| 0.1. | Make (trade name of manufacturer): … | |
| 0.2. | Type: … | |
| 0.2.1. | Commercial name(s) (if available): … | |
| 0.2.3. | Family identifiers: | |
| 0.2.3.1. | Interpolation family: … | |
| 0.2.3.2. | ATCT family(s): … | |
| 0.2.3.4. | Roadload family | |
| 0.2.3.4.1. | Roadload family of VH: … | |
| 0.2.3.4.2. | Roadload family of VL: … | |
| 0.2.3.4.3. | Roadload families applicable in the interpolation family: … | |
| 0.2.3.5. | Roadload Matrix family(s): … | |
| 0.2.3.6. | Periodic regeneration family(s): … | |
| 0.2.3.7. | Evaporative test family(s): … | |
| 0.2.3.8. | OBD family(s): … | |
| 0.2.3.9. | Durability family(s): … | |
| 0.2.3.10. | ER family(s): … | |
| 0.2.3.11. | Gas Fuelled Vehicle family(s): … | |
| 0.2.3.12. | (Reserved) | |
| 0.2.3.13. | KCO2 correction factor family : … | |
| 0.2.4. | other family(s): … | |
| 0.4. | Category of vehicle (c): … | |
| 0.8. | Name(s) and address(es) of assembly plant(s): … | |
| 0.9. | Name and address of the manufacturer's representative (if any): … | |
| 1. | GENERAL CONSTRUCTION CHARACTERISTICS | |
| 1.1. | Photographs and/or drawings of a representative vehicle/component/separate technical unit (1): | |
| 1.3.3. | Powered axles (number, position, interconnection): … | |
| 2. | MASSES AND DIMENSIONS (f) (g) (7)  (in kg and mm) (Refer to drawing where applicable) | |
| 2.6. | Mass in running order (h)  (a) maximum and minimum for each variant: … | |
| 2.6.3. | Rotational mass: 3 % of the sum of mass in running order and 25 kg or value, per axle (kg): … | |
| 2.8. | Technically permissible maximum laden mass stated by the manufacturer (i) (3): … | |
| 3. | PROPULSION ENERGY CONVERTER (k) | |
| 3.1. | Manufacturer of the propulsion energy converter(s): … | |
| 3.1.1. | Manufacturer's code (as marked on the propulsion energy converter or other means of identification): … | |
| 3.2. | Internal combustion engine | |
| 3.2.1.1. | Working principle: positive ignition/compression ignition/dual fuel (1)  Cycle: four stroke/two stroke/rotary (1) | |
| 3.2.1.2. | Number and arrangement of cylinders: … | |
| 3.2.1.2.1. | Bore (1): … mm | |
| 3.2.1.2.2. | Stroke (1): … mm | |
| 3.2.1.2.3. | Firing order: … | |
| 3.2.1.3. | Engine capacity (m): … cm3 | |
| 3.2.1.4. | Volumetric compression ratio (2): … | |
| 3.2.1.5. | Drawings of combustion chamber, piston crown and, in the case of positive ignition engines, piston rings: … | |
| 3.2.1.6. | Normal engine idling speed (2): … min–1 | |
| 3.2.1.6.1. | High engine idling speed (2): … min–1 | |
| 3.2.1.8. | Rated engine power (n): … kW at … min–1 (manufacturer's declared value) | |
| 3.2.1.9. | Maximum permitted engine speed as prescribed by the manufacturer: … min–1 | |
| 3.2.1.10. | Maximum net torque (n): … Nm at … min–1 (manufacturer's declared value) | |
| 3.2.2. | Fuel | |
| 3.2.2.1. | Diesel/Petrol/LPG/NG or Biomethane/Ethanol (E 85)/Biodiesel/Hydrogen (1), | |
| 3.2.2.1.1. | RON, unleaded: … | |
| 3.2.2.4. | Vehicle fuel type: Mono fuel, Bi fuel, Flex fuel (1) | |
| 3.2.2.5. | Maximum amount of biofuel acceptable in fuel (manufacturer's declared value): … % by volume | |
| 3.2.4. | Fuel feed | |
| 3.2.4.1. | By carburettor(s): yes/no (1) | |
| 3.2.4.2. | By fuel injection (compression ignition or dual fuel only): yes/no (1) | |
| 3.2.4.2.1. | System description (common rail/unit injectors/distribution pump etc.): … | |
| 3.2.4.2.2. | Working principle: direct injection/pre-chamber/swirl chamber (1) | |
| 3.2.4.2.3. | Injection/Delivery pump | |
| 3.2.4.2.3.1. | Make(s): … | |
| 3.2.4.2.3.2. | Type(s): … | |
| 3.2.4.2.3.3. | Maximum fuel delivery (1) (2): … mm3 /stroke or cycle at an engine speed of: … min–1 or, alternatively, a characteristic diagram: … (When boost control is supplied, state the characteristic fuel delivery and boost pressure versus engine speed) | |
| 3.2.4.2.4. | Engine speed limitation control | |
| 3.2.4.2.4.2.1. | Speed at which cut-off starts under load: … min–1 | |
| 3.2.4.2.4.2.2. | Maximum no-load speed: … min–1 | |
| 3.2.4.2.6. | Injector(s) | |
| 3.2.4.2.6.1. | Make(s): … | |
| 3.2.4.2.6.2. | Type(s): … | |
| 3.2.4.2.8. | Auxiliary starting aid | |
| 3.2.4.2.8.1. | Make(s): … | |
| 3.2.4.2.8.2. | Type(s): … | |
| 3.2.4.2.8.3. | System description: … | |
| 3.2.4.2.9. | Electronic controlled injection: yes/no (1) | |
| 3.2.4.2.9.1. | Make(s): … | |
| 3.2.4.2.9.2. | Type(s): | |
| 3.2.4.2.9.3 | Description of the system: … | |
| 3.2.4.2.9.3.1. | Make and type of the control unit (ECU): … | |
| 3.2.4.2.9.3.1.1. | Software version of the ECU: … | |
| 3.2.4.2.9.3.2. | Make and type of the fuel regulator: … | |
| 3.2.4.2.9.3.3. | Make and type of the air-flow sensor: … | |
| 3.2.4.2.9.3.4. | Make and type of fuel distributor: … | |
| 3.2.4.2.9.3.5. | Make and type of the throttle housing: … | |
| 3.2.4.2.9.3.6. | Make and type or working principle of water temperature sensor: … | |
| 3.2.4.2.9.3.7. | Make and type or working principle of air temperature sensor: … | |
| 3.2.4.2.9.3.8. | Make and type or working principle of air pressure sensor: … | |
| 3.2.4.3. | By fuel injection (positive ignition only): yes/no (1) | |
| 3.2.4.3.1. | Working principle: single-/multi-point/direct injection /other (specify)(1): … | |
| 3.2.4.3.2. | Make(s): … | |
| 3.2.4.3.3. | Type(s): … | |
| 3.2.4.3.4. | System description (In the case of systems other than continuous injection give equivalent details): … | |
| 3.2.4.3.4.1. | Make and type of the control unit (ECU): … | |
| 3.2.4.3.4.1.1. | Software version of the ECU: … | |
| 3.2.4.3.4.3. | Make and type or working principle of air-flow sensor: … | |
| 3.2.4.3.4.8. | Make and type of throttle housing: … | |
| 3.2.4.3.4.9. | Make and type or working principle of water temperature sensor: … | |
| 3.2.4.3.4.10. | Make and type or working principle of air temperature sensor: … | |
| 3.2.4.3.4.11. | Make and type or working principle of air pressure sensor: … | |
| 3.2.4.3.5. | Injectors | |
| 3.2.4.3.5.1. | Make: … | |
| 3.2.4.3.5.2. | Type: … | |
| 3.2.4.3.7. | Cold start system | |
| 3.2.4.3.7.1. | Operating principle(s): … | |
| 3.2.4.3.7.2. | Operating limits/settings (1) (2): … | |
| 3.2.4.4. | Feed pump | |
| 3.2.4.4.1. | Pressure (2): … kPa or characteristic diagram (2): … | |
| 3.2.4.4.2. | Make(s): … | |
| 3.2.4.4.3. | Type(s): … | |
| 3.2.5. | Electrical system | |
| 3.2.5.1. | Rated voltage: … V, positive/negative ground (1) | |
| 3.2.5.2. | Generator | |
| 3.2.5.2.1. | Type: … | |
| 3.2.5.2.2. | Nominal output: … VA | |
| 3.2.6. | Ignition system (spark ignition engines only) | |
| 3.2.6.1. | Make(s): … | |
| 3.2.6.2. | Type(s): … | |
| 3.2.6.3. | Working principle: … | |
| 3.2.6.6. | Spark plugs | |
| 3.2.6.6.1. | Make: … | |
| 3.2.6.6.2. | Type: … | |
| 3.2.6.6.3. | Gap setting: … mm | |
| 3.2.6.7. | Ignition coil(s) | |
| 3.2.6.7.1. | Make: … | |
| 3.2.6.7.2. | Type: … | |
| 3.2.7. | Cooling system: liquid/air (1) | |
| 3.2.7.1. | Nominal setting of the engine temperature control mechanism: … | |
| 3.2.7.2. | Liquid | |
| 3.2.7.2.1. | Nature of liquid: … | |
| 3.2.7.2.2. | Circulating pump(s): yes/no (1) | |
| 3.2.7.2.3. | Characteristics: … or | |
| 3.2.7.2.3.1. | Make(s): … | |
| 3.2.7.2.3.2. | Type(s): … | |
| 3.2.7.2.4. | Drive ratio(s): … | |
| 3.2.7.2.5. | Description of the fan and its drive mechanism: … | |
| 3.2.7.3. | Air | |
| 3.2.7.3.1. | Fan: yes/no (1) | |
| 3.2.7.3.2. | Characteristics: … or | |
| 3.2.7.3.2.1. | Make(s): … | |
| 3.2.7.3.2.2. | Type(s): … | |
| 3.2.7.3.3. | Drive ratio(s): … | |
| 3.2.8. | Intake system | |
| 3.2.8.1. | Pressure charger: yes/no (1) | |
| 3.2.8.1.1. | Make(s): … | |
| 3.2.8.1.2. | Type(s): … | |
| 3.2.8.1.3. | Description of the system (e.g. maximum charge pressure: … kPa; wastegate if applicable): … | |
| 3.2.8.2. | Intercooler: yes/no (1) | |
| 3.2.8.2.1. | Type: air-air/air-water (1) | |
| 3.2.8.3. | Intake depression at rated engine speed and at 100 % load (compression ignition engines only) | |
| 3.2.8.4. | Description and drawings of inlet pipes and their accessories (plenum chamber, heating device, additional air intakes, etc.): … | |
| 3.2.8.4.1. | Intake manifold description (include drawings and/or photos): … | |
| 3.2.8.4.2. | Air filter, drawings: … or | |
| 3.2.8.4.2.1. | Make(s): … | |
| 3.2.8.4.2.2. | Type(s): … | |
| 3.2.8.4.3. | Intake silencer, drawings: … or | |
| 3.2.8.4.3.1. | Make(s): … | |
| 3.2.8.4.3.2. | Type(s): … | |
| 3.2.9. | Exhaust system | |
| 3.2.9.1. | Description and/or drawing of the exhaust manifold: … | |
| 3.2.9.2. | Description and/or drawing of the exhaust system: … | |
| 3.2.9.3. | Maximum allowable exhaust back pressure at rated engine speed and at 100 % load (compression ignition engines only): … kPa | |
| 3.2.10. | Minimum cross-sectional areas of inlet and outlet ports: … | |
| 3.2.11. | Valve timing or equivalent data | |
| 3.2.11.1. | Maximum lift of valves, angles of opening and closing, or timing details of alternative distribution systems, in relation to dead centres. For variable timing system, minimum and maximum timing: … | |
| 3.2.11.2. | Reference and/or setting ranges (1): … | |
| 3.2.12. | Measures taken against air pollution | |
| 3.2.12.1. | Device for recycling crankcase gases (description and drawings): … | |
| 3.2.12.2. | Pollution control devices (if not covered by another heading) | |
| 3.2.12.2.1. | Catalytic converter | |
| 3.2.12.2.1.1. | Number of catalytic converters and elements (provide the information below for each separate unit): … | |
| 3.2.12.2.1.2. | Dimensions, shape and volume of the catalytic converter(s): … | |
| 3.2.12.2.1.3. | Type of catalytic action: … | |
| 3.2.12.2.1.4. | Total charge of precious metals: … | |
| 3.2.12.2.1.5. | Relative concentration: … | |
| 3.2.12.2.1.6. | Substrate (structure and material): … | |
| 3.2.12.2.1.7. | Cell density: … | |
| 3.2.12.2.1.8. | Type of casing for the catalytic converter(s): … | |
| 3.2.12.2.1.9. | Location of the catalytic converter(s) (place and reference distance in the exhaust line): … | |
| 3.2.12.2.1.10. | Heat shield: yes/no (1) | |
| 3.2.12.2.1.11. | Normal operating temperature range: … °C | |
| 3.2.12.2.1.12. | Make of catalytic converter: … | |
| 3.2.12.2.1.13. | Identifying part number: … | |
| 3.2.12.2.2. | Sensors | |
| 3.2.12.2.2.1. | Oxygen and/or lambda sensor(s): yes/no (1) | |
| 3.2.12.2.2.1.1. | Make: … | |
| 3.2.12.2.2.1.2. | Location: … | |
| 3.2.12.2.2.1.3. | Control range: … | |
| 3.2.12.2.2.1.4. | Type or working principle: … | |
| 3.2.12.2.2.1.5. | Identifying part number: … | |
| 3.2.12.2.2.2. | NOx sensor: yes/no (1) | |
| 3.2.12.2.2.2.1. | Make: … | |
| 3.2.12.2.2.2.2. | Type: … | |
| 3.2.12.2.2.2.3. | Location | |
| 3.2.12.2.2.3. | Particulate sensor: yes/no (1) | |
| 3.2.12.2.2.3.1. | Make: … | |
| 3.2.12.2.2.3.2. | Type: … | |
| 3.2.12.2.2.3.3. | Location: … | |
| 3.2.12.2.3. | Air injection: yes/no (1) | |
| 3.2.12.2.3.1. | Type (pulse air, air pump, etc.): … | |
| 3.2.12.2.4. | Exhaust gas recirculation (EGR): yes/no (1) | |
| 3.2.12.2.4.1. | Characteristics (make, type, flow, high pressure/low pressure/combined pressure, etc.): … | |
| 3.2.12.2.4.2. | Water-cooled system (to be specified for each EGR system e.g. low pressure/high pressure/combined pressure: yes/no (1) | |
| 3.2.12.2.5. | Evaporative emissions control system (petrol and ethanol engines only): yes/no (1) | |
| 3.2.12.2.5.1. | Detailed description of the devices: … | |
| 3.2.12.2.5.2. | Drawing of the evaporative control system: … | |
| 3.2.12.2.5.3. | Drawing of the carbon canister: … | |
| 3.2.12.2.5.4. | Mass of dry charcoal: … g | |
| 3.2.12.2.5.5. | Schematic drawing of the fuel tank (petrol and ethanol engines only): … | |
| 3.2.12.2.5.5.1. | Fuel tank system capacity, material and construction: … | |
| 3.2.12.2.5.5.2. | Description of vapour hose material, fuel line material and connection technique of the fuel system: … | |
| 3.2.12.2.5.5.3. | Sealed tank system: yes/no | |
| 3.2.12.2.5.5.4. | Description of fuel tank relief valve setting (air ingestion and relief): … | |
| 3.2.12.2.5.5.5. | Description of the purge control system: … | |
| 3.2.12.2.5.6. | Description and schematic of the heat shield between tank and exhaust system: … | |
| 3.2.12.2.5.7. | Permeability factor: … | |
| 3.2.12.2.6. | Particulate trap (PT): yes/no (1) | |
| 3.2.12.2.6.1. | Dimensions, shape and capacity of the particulate trap: … | |
| 3.2.12.2.6.2. | Design of the particulate trap: … | |
| 3.2.12.2.6.3. | Location (reference distance in the exhaust line): … | |
| 3.2.12.2.6.4. | Make of particulate trap: … | |
| 3.2.12.2.6.5. | Identifying part number: … | |
| 3.2.12.2.7. | On-board-diagnostic (OBD) system: yes/no (1) | |
| 3.2.12.2.7.1. | Written description and/or drawing of the MI: … | |
| 3.2.12.2.7.2. | List and purpose of all components monitored by the OBD system: … | |
| 3.2.12.2.7.3. | Written description (general working principles) for | |
| 3.2.12.2.7.3.1. | Positive-ignition engines | |
| 3.2.12.2.7.3.1.1. | Catalyst monitoring: … | |
| 3.2.12.2.7.3.1.2. | Misfire detection: … | |
| 3.2.12.2.7.3.1.3. | Oxygen sensor monitoring: … | |
| 3.2.12.2.7.3.1.4. | Other components monitored by the OBD system: … | |
| 3.2.12.2.7.3.2. | Compression-ignition engines: … | |
| 3.2.12.2.7.3.2.1. | Catalyst monitoring: … | |
| 3.2.12.2.7.3.2.2. | Particulate trap monitoring: … | |
| 3.2.12.2.7.3.2.3. | Electronic fuelling system monitoring: … | |
| 3.2.12.2.7.3.2.5. | Other components monitored by the OBD system: … | |
| 3.2.12.2.7.4. | Criteria for MI activation (fixed number of driving cycles or statistical method): … | |
| 3.2.12.2.7.5. | List of all OBD output codes and formats used (with explanation of each): … | |
| 3.2.12.2.7.6. | The following additional information shall be provided by the vehicle manufacturer for the purposes of enabling the manufacture of OBD-compatible replacement or service parts and diagnostic tools and test equipment. | |
| 3.2.12.2.7.6.1. | A description of the type and number of the preconditioning cycles or alternative preconditioning methods used for the original type approval of the vehicle and the reason for their usage. | |
| 3.2.12.2.7.6.2. | A description of the type of the OBD demonstration cycle used for the original type-approval of the vehicle for the component monitored by the OBD system. | |
| 3.2.12.2.7.6.3. | A comprehensive document describing all sensed components with the strategy for fault detection and MI activation (fixed number of driving cycles or statistical method), including a list of relevant secondary sensed parameters for each component monitored by the OBD system. A list of all OBD output codes and format used (with an explanation of each) associated with individual emission related powertrain components and individual non-emission related components, where monitoring of the component is used to determine MI activation, including in particular a comprehensive explanation for the data given in service $05 Test ID $21 to FF and the data given in service $06.  In the case of vehicle types that use a communication link in accordance with ISO 15765-4 ‘Road vehicles, diagnostics on controller area network (CAN) — Part 4: requirements for emissions-related systems’, a comprehensive explanation for the data given in service $06 Test ID $00 to FF, for each OBD monitor ID supported, shall be provided. | |
| 3.2.12.2.7.6.4. | The information required above may be defined by completing a table as described below. | |
| 3.2.12.2.7.6.4.1. | Light-duty vehicles | |
| |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | | Component | Fault code | Monitoring strategy | Fault detection criteria | MI activation criteria | Secondary parameters | Preconditioning | Demonstration test | | Catalyst | P0420 | Oxygen sensor 1 and sensor 2 signals | Difference between sensor 1 and sensor 2 signals- | 3rd cycle | Engine speed, engine load, A/F mode, catalyst temperature | Two Type 1 cycles | Type 1 | | | |
| 3.2.12.2.8. | | Other system: … |
| 3.2.12.2.8.2. | | Driver inducement system |
| 3.2.12.2.8.2.3. | | Type of inducement system: no engine restart after countdown/no start after refuelling/fuel-lockout/performance restriction |
| 3.2.12.2.8.2.4. | | Description of the inducement system |
| 3.2.12.2.8.2.5. | | Equivalent to the average driving range of the vehicle with a complete tank of fuel: … km |
| 3.2.12.2.10. | | Periodically regenerating system: (provide the information below for each separate unit) |
| 3.2.12.2.10.1. | | Method or system of regeneration, description and/or drawing: … |
| 3.2.12.2.10.2. | | The number of Type 1 operating cycles, or equivalent engine test bench cycles, between two cycles where regenerative phases occur under the conditions equivalent to Type 1 test (Distance ‘D’): … |
| 3.2.12.2.10.2.1. | | Applicable Type 1 cycle: … |
| 3.2.12.2.10.2.2. | | The number of complete applicable test cycles required for regeneration (distance ‘d’) |
| 3.2.12.2.10.3. | | Description of method employed to determine the number of cycles between two cycles where regenerative phases occur: … |
| 3.2.12.2.10.4. | | Parameters to determine the level of loading required before regeneration occurs (i.e. temperature, pressure etc.): … |
| 3.2.12.2.10.5. | | Description of method used to load system: … |
| 3.2.12.2.11. | | Catalytic converter systems using consumable reagents (provide the information below for each separate unit) yes/no (1) |
| 3.2.12.2.11.1. | | Type and concentration of reagent needed: … |
| 3.2.12.2.11.2. | | Normal operational temperature range of reagent: … |
| 3.2.12.2.11.3. | | International standard: … |
| 3.2.12.2.11.4. | | Frequency of reagent refill: continuous/maintenance (where appropriate): |
| 3.2.12.2.11.5. | | Reagent indicator: (description and location) |
| 3.2.12.2.11.6. | | Reagent tank |
| 3.2.12.2.11.6.1. | | Capacity: … |
| 3.2.12.2.11.6.2. | | Heating system: yes/no |
| 3.2.12.2.11.6.2.1. | | Description or drawing |
| 3.2.12.2.11.7. | | Reagent control unit: yes/no (1) |
| 3.2.12.2.11.7.1. | | Make: … |
| 3.2.12.2.11.7.2. | | Type: … |
| 3.2.12.2.11.8. | | Reagent injector (make type and location): … |
| 3.2.12.2.11.9. | | Reagent quality sensor (make, type and location): … |
| 3.2.12.2.12. | | Water injection: yes/no (1) |
| 3.2.14. | | Details of any devices designed to influence fuel economy (if not covered by other items):.… |
| 3.2.15. | | LPG fuelling system: yes/no (1) |
| 3.2.15.1. | | Approval number (approval number of UN Regulation No. 67): … |
| 3.2.15.2. | | Electronic engine management control unit for LPG fuelling |
| 3.2.15.2.1. | | Make(s): … |
| 3.2.15.2.2. | | Type(s): … |
| 3.2.15.2.3. | | Emission-related adjustment possibilities: … |
| 3.2.15.3. | | Further documentation |
| 3.2.15.3.1. | | Description of the safeguarding of the catalyst at switch-over from petrol to LPG or back: … |
| 3.2.15.3.2. | | System lay-out (electrical connections, vacuum connections compensation hoses, etc.): … |
| 3.2.15.3.3. | | Drawing of the symbol: … |
| 3.2.16. | | NG fuelling system: yes/no (1) |
| 3.2.16.1. | | Approval number (approval number of UN Regulation No. 110): |
| 3.2.16.2. | | Electronic engine management control unit for NG fuelling |
| 3.2.16.2.1. | | Make(s): … |
| 3.2.16.2.2. | | Type(s): … |
| 3.2.16.2.3. | | Emission-related adjustment possibilities: … |
| 3.2.16.3. | | Further documentation |
| 3.2.16.3.1. | | Description of the safeguarding of the catalyst at switch-over from petrol to NG or back: … |
| 3.2.16.3.2. | | System lay-out (electrical connections, vacuum connections compensation hoses, etc.): … |
| 3.2.16.3.3. | | Drawing of the symbol: … |
| 3.2.18. | | Hydrogen fuelling system: yes/no (1) |
| 3.2.18.1. | | Type approval number according to UN Regulation No. 134 (if applicable): ………... |
| 3.2.18.2. | | Electronic engine management control unit for hydrogen fuelling |
| 3.2.18.2.1. | | Make(s): … |
| 3.2.18.2.2. | | Type(s): … |
| 3.2.18.2.3. | | Emission-related adjustment possibilities: … |
| 3.2.18.3. | | Further documentation |
| 3.2.18.3.1. | | Description of the safeguarding of the catalyst at switch-over from petrol to hydrogen or back: … |
| 3.2.18.3.2. | | System lay-out (electrical connections, vacuum connections compensation hoses, etc.): … |
| 3.2.18.3.3. | | Drawing of the symbol: … |
| 3.2.19.4. | | Further documentation |
| 3.2.19.4.2. | | System lay-out (electrical connections, vacuum connections compensation hoses, etc.): … |
| 3.2.19.4.3. | | Drawing of the symbol: … |
| 3.2.20. | | Heat storage information |
| 3.2.20.1. | | Active heat storage device: yes/no (1) |
| 3.2.20.1.1. | | Enthalpy: … (J) |
| 3.2.20.2. | | Insulation materials: yes/no (1) |
| 3.2.20.2.1. | | Insulation material: … (x) |
| 3.2.20.2.2. | | Insulation nominal volume: … (l) (x) |
| 3.2.20.2.3. | | Insulation nominal weight: … (kg) (x) |
| 3.2.20.2.4. | | Insulation location: … (x) |
| 3.2.20.2.5. | | Worst case approach vehicle cool down: yes/no (1) |
| 3.2.20.2.5.1. | | (not worst case approach) Minimum soaking time, tsoak\_ATCT (hours):… (x) |
| 3.2.20.2.5.2. | | (not worst case approach) Location of the engine temperature measurement: … (x) |
| 3.2.20.2.6. | | Single interpolation family within the ATCT family approach: yes/no (1) |
| 3.2.20.2.7. | | Worst case approach with regards to insulation: yes/no (1) |
| 3.2.20.2.7.1. | | Description of the ATCT measured reference vehicle regarding insulation: … |
| 3.3. | | Electric powertrain (for PEV only) |
| 3.3.1. | | General description of electric powertrain |
| 3.3.1.1. | | Make: .......................... |
| 3.3.1.2. | | Type: .......................... |
| 3.3.1.3. | | Use (1): Monomotor/multimotors (number): .......................... |
| 3.3.1.4. | | Transmission arrangement: parallel/transaxial/others, to precise: .......................... |
| 3.3.1.5. | | Test voltage: .......................... V |
| 3.3.1.6. | | Motor nominal speed: .......................... min-1 |
| 3.3.1.7. | | Motor maximum speed: ..........................min-1 or by default: reducer outlet shaft/gear box speed (specify gear engaged): .......................... min-1 |
| 3.3.1.9. | | Maximum power: .......................... kW |
| 3.3.1.10. | | Maximum thirty minutes power: .......................... kW |
| 3.3.1.11. | | Flexible range (where P > 90 per cent of max. power):  speed at the beginning of range: .......................... min-1 speed at the end of range: .......................... min-1 |
| 3.3.2. | | Traction REESS |
| 3.3.2.1. | | Trade name and mark of the REESS: .......................... |
| 3.3.2.2. | | Kind of electro-chemical couple: .......................... |
| 3.3.2.3. | | Nominal voltage: .......................... V |
| 3.3.2.4. | | REESS maximum thirty minutes power (constant power discharge): .......................... kW |
| 3.3.2.5. | | REESS performance in 2 h discharge (constant power or constant current): (1) |
| 3.3.2.5.1. | | REESS energy: .......................... kWh |
| 3.3.2.5.2. | | REESS capacity: .......................... Ah in 2 h |
| 3.3.2.5.3. | | End of discharge voltage value: .......................... V |
| 3.3.2.6. | | Indication of the end of the discharge that leads to a compulsory stop of the vehicle: (1) .......................... |
| 3.3.2.7. | | REESS mass: .......................... kg |
| 3.3.2.8. | | Number of cells:…… |
| 3.3.2.9. | | REESS position:………… |
| 3.3.2.10. | | Type of coolant : air/liquid (1) |
| 3.3.2.11. | | Battery management system control unit |
| 3.3.2.11.1. | | Make: …….. |
| 3.3.2.11.2. | | Type: ……. |
| 3.3.2.11.3. | | Identification number: ….. |
| 3.3.3. | | Electric Motor |
| 3.3.3.1. | | Working principle: |
| 3.3.3.1.1. | | direct current/alternating current (1) /number of phases: .......................... |
| 3.3.3.1.2. | | separate excitation/series/compound (1) |
| 3.3.3.1.3. | | synchronous/asynchronous (1) |
| 3.3.3.1.4. | | coiled rotor/with permanent magnets/with housing (1) |
| 3.3.3.1.5. | | number of poles of the motor: .......................... |
| 3.3.3.2. | | Inertia mass: .......................... |
| 3.3.4. | | Power controller |
| 3.3.4.1. | | Make : .......................... |
| 3.3.4.2. | | Type : .......................... |
| 3.3.4.2.1. | | Identification number: …... |
| 3.3.4.3. | | Control principle: vectorial/open loop/closed/other (to be specified): (1) .......................... |
| 3.3.4.4. | | Maximum effective current supplied to the motor: (2) .......................... A during .......................... seconds |
| 3.3.4.5. | | Voltage range use: .......................... V to .......................... V |
| 3.3.5. | | Cooling system:  Motor: liquid/air (1)  Controller: liquid/air (1) |
| 3.3.5.1. | | Liquid-cooling equipment characteristics: |
| 3.3.5.1.1. | | Nature of the liquid .......................... circulating pumps: yes/no (1) |
| 3.3.5.1.2. | | Characteristics or make(s) and type(s) of the pump: .......................... |
| 3.3.5.1.3. | | Thermostat: setting: .......................... |
| 3.3.5.1.4. | | Radiator: drawing(s) or make(s) and type(s): .......................... |
| 3.3.5.1.5. | | Relief valve: pressure setting: .......................... |
| 3.3.5.1.6. | | Fan: characteristics or make(s) and type(s): .......................... |
| 3.3.5.1.7. | | Fan duct: .......................... |
| 3.3.5.2. | | Air-cooling equipment characteristics |
| 3.3.5.2.1. | | Blower: characteristics or make(s) and type(s): .......................... |
| 3.3.5.2.2. | | Standard air ducting: .......................... |
| 3.3.5.2.3. | | Temperature regulating system: yes/no (1) |
| 3.3.5.2.4. | | Brief description: .......................... |
| 3.3.5.2.5. | | Air filter: .......................... make(s): .......................... type(s): |
| 3.3.5.3. | | Temperatures admitted by the manufacturer (maximum) |
| 3.3.5.3.1. | | Motor outlet: ..........................° C |
| 3.3.5.3.2. | | controller inlet: ..........................° C |
| 3.3.5.3.3. | | at motor reference point(s): ..........................° C |
| 3.3.5.3.4. | | at controller reference point(s): ..........................° C |
| 3.3.6. | | Insulating category: .......................... |
| 3.3.7. | | International protection (IP)-code: .......................... |
| 3.3.8. | | Lubrication system principle: (1)  Bearings: friction/ball  Lubricant: grease/oil  Seal: yes/no  Circulation: with/without |
| 3.3.9. | | Charger |
| 3.3.9.1. | | Charger: on board/external (1)  in case of an external unit, define the charger (trademark, model): .......................... |
| 3.3.9.2. | | Description of the normal profile of charge: |
| 3.3.9.3. | | Specification of mains: |
| 3.3.9.3.1. | | Type of mains: single phase/three phase (1) |
| 3.3.9.3.2. | | Voltage: .......................... |
| 3.3.9.4. | | Rest period recommended between the end of the discharge and the start of the charge: .......................... |
| 3.3.9.5. | | Theoretical duration of a complete charge: .......................... |
| 3.3.10. | | Electric energy converters |
| 3.3.10.1. | | Electric energy converter between the electric machine and traction REESS |
| 3.3.10.1.1. | | Make : .......................... |
| 3.3.10.1.2. | | Type : .......................... |
| 3.3.10.1.3. | | Declared nominal power : .......................... W |
| 3.3.10.2. | | Electric energy converter between the traction REESS and low voltage  power supply |
| 3.3.10.2.1. | | Make : .......................... |
| 3.3.10.2.2. | | Type : .......................... |
| 3.3.10.2.3. | | Declared nominal power : .......................... W |
| 3.3.10.3. | | Electric energy converter between the recharge-plug-in and traction REESS |
| 3.3.10.3.1. | | Make : .......................... |
| 3.3.10.3.2. | | Type : .......................... |
| 3.3.10.3.3. | | Declared nominal power : .......................... W |
| 3.4. | | Combinations of propulsion energy converters |
| 3.4.1. | | Hybrid electric vehicle: yes/no (1) |
| 3.4.2. | | Category of hybrid electric vehicle: off-vehicle charging/not off-vehicle charging: (1) |
| 3.4.3. | | Operating mode switch: with/without (1) |
| 3.4.3.1. | | Selectable modes |
| 3.4.3.1.1. | | Pure electric: yes/no (1) |
| 3.4.3.1.2. | | Pure fuel consuming: yes/no (1) |
| 3.4.3.1.3. | | Hybrid modes: yes/no (1)  (if yes, short description): … |
| 3.4.4. | | Description of the energy storage device: (REESS, capacitor, flywheel/generator) |
| 3.4.4.1. | | Make(s): … |
| 3.4.4.2. | | Type(s): … |
| 3.4.4.3. | | Identification number: … |
| 3.4.4.4. | | Kind of electrochemical couple: … |
| 3.4.4.5. | | Energy: … (for REESS: voltage and capacity Ah in 2 h, for capacitor: J, …) |
| 3.4.4.6. | | Charger: on board/external/without (1) |
| 3.4.4.7. | | Type of coolant : air/liquid (1) |
| 3.4.4.8. | | Battery management system control unit |
| 3.4.4.8.1. | | Make: …….. |
| 3.4.4.8.2. | | Type: …. |
| 3.4.4.8.3. | | Identification number: .... |
| 3.4.5. | | Electric machine (describe each type of electric machine separately) |
| 3.4.5.1. | | Make: … |
| 3.4.5.2. | | Type: … |
| 3.4.5.3. | | Primary use: traction motor/generator (1) |
| 3.4.5.3.1. | | When used as traction motor: single-/multimotors (number) (1): … |
| 3.4.5.4. | | Maximum power: … kW |
| 3.4.5.5. | | Working principle |
| 3.4.5.5.5.1. | | Direct current/alternating current/number of phases: … |
| 3.4.5.5.2. | | Separate excitation/series/compound (1) |
| 3.4.5.5.3. | | Synchronous/asynchronous (1) |
| 3.4.5.6. | | Cooling system:  Motor: liquid/air (1)  Controller: liquid/air (1) |
| 3.4.5.6.1. | | Liquid-cooling equipment characteristics: |
| 3.4.5.6.1.1. | | Nature of the liquid .......................... circulating pumps: yes/no (1) |
| 3.4.5.6.1.2. | | Characteristics or make(s) and type(s) of the pump: .......................... |
| 3.4.5.6.1.3. | | Thermostat: setting: .......................... |
| 3.4.5.6.1.4. | | Radiator: drawing(s) or make(s) and type(s): .......................... |
| 3.4.5.6.1.5. | | Relief valve: pressure setting: .......................... |
| 3.4.5.6.1.6. | | Fan: characteristics or make(s) and type(s): .......................... |
| 3.4.5.6.1.7. | | Fan duct: .......................... |
| 3.4.5.6.2. | | Air-cooling equipment characteristics |
| 3.4.5.6.2.1. | | Blower: characteristics or make(s) and type(s): .......................... |
| 3.4.5.6.2.2. | | Standard air ducting: .......................... |
| 3.4.5.6.2.3. | | Temperature regulating system: yes/no (1) |
| 3.4.5.6.2.4. | | Brief description: .......................... |
| 3.4.5.6.2.5. | | Air filter: .......................... make(s): .......................... type(s): |
| 3.4.5.6.3. | | Temperatures admitted by the manufacturer (maximum) |
| 3.4.5.6.3.1. | | Motor outlet: ..........................° C |
| 3.4.5.6.3.2. | | controller inlet: ..........................° C |
| 3.4.5.6.3.3. | | at motor reference point(s): ..........................° C |
| 3.4.5.6.3.4. | | at controller reference point(s): ..........................° C |
| 3.4.6. | | Control unit |
| 3.4.6.1. | | Make(s): … |
| 3.4.6.2. | | Type(s): … |
| 3.4.6.3. | | Identification number: … |
| 3.4.7. | | Power controller |
| 3.4.7.1. | | Make: … |
| 3.4.7.2. | | Type: … |
| 3.4.7.3. | | Identification number: … |
| 3.4.9. | | Manufacturer's recommendation for preconditioning: … |
| 3.4.10. | | FCHV: yes/no (1) |
| 3.4.10.1. | | Type of Fuel Cell |
| 3.4.10.1.2. | | Make: … |
| 3.4.10.1.3. | | Type: … |
| 3.4.10.1.4. | | Nominal Voltage (V): … |
| 3.4.10.1.5. | | Type of coolant: air/liquid (1) |
| 3.4.10.2. | | System description (working principle of the fuel cell, drawing, etc.): … |
| 3.4.11. | | Electric energy converters |
| 3.4.11.1. | | Electric energy converter between the electric machine and traction REESS |
| 3.4.11.1.1. | | Make : .......................... |
| 3.4.11.1.2. | | Type : .......................... |
| 3.4.11.1.3. | | Declared nominal power : .......................... W |
| 3.4.11.2. | | Electric energy converter between the traction REESS and low voltage  power supply |
| 3.4.11.2.1. | | Make : .......................... |
| 3.4.11.2.2. | | Type : .......................... |
| 3.4.11.2.3. | | Declared nominal power : .......................... W |
| 3.4.11.3. | | Electric energy converter between the recharge-plug-in and traction REESS |
| 3.4.11.3.1. | | Make : .......................... |
| 3.4.11.3.2. | | Type : .......................... |
| 3.4.11.3.3. | | Declared nominal power : .......................... W |
| 3.5. | | Manufacturer’s declared values for determination of CO2 emissions/fuel consumption/electric energy consumption/electric range |
| 3.5.7. | | Manufacturer’s declared values |
| 3.5.7.1. | | Test vehicle parameters   | Vehicle | Vehicle Low (VL)  if existing | Vehicle High  (VH) | VM  if existing | V representative (only for road load matrix family\*) | Default values | | --- | --- | --- | --- | --- | --- | | Vehicle bodywork type |  |  | - |  |  | | Road load method used (measurement or calculation by road load family) |  |  | - | - |  | | Road load information: | | | | |  | | Tyres make and type,  if measurement |  |  | - |  |  | | Tyre dimensions (front/rear),  if measurement |  |  | - |  |  | | Tyre rolling resistance (front/rear) (kg/t) |  |  |  |  |  | | Tyre pressure (front/rear) (kPa),  if measurement |  |  |  |  |  | | Delta CD × A of vehicle L compared to vehicle H (IP\_H minus IP\_L) | - |  | - | - |  | | Delta CD × A compared to road load family vehicle L (IP\_H/L minus RL\_L), if calculation by road load family |  |  | - | - |  | | Vehicle test mass (kg) |  |  |  |  |  | | Road load coefficients | | | | |  | | f0 (N) |  |  |  |  |  | | f1 (N/(km/h)) |  |  |  |  |  | | f2 (N/(km/h)²) |  |  |  |  |  | | Frontal area m² (0.000 m²) | - | - | - |  |  | | Cycle Energy Demand (J) |  |  |  |  |  | | \* representative vehicle is tested for the road load matrix family | | | | |  | |
| 3.5.7.1.1. | | Fuel used for the Type 1 test and selected for the measurement of the net power in accordance with UN Regulation No. 85 (for LPG or NG vehicles only): … |
| 3.5.7.2. | | Combined CO2 emissions |
| 3.5.7.2.1. | | CO2 emission for pure ICE vehicles and NOVC-HEVs |
| 3.5.7.2.1.0. | | Minimum and maximum CO2 values within the interpolation family: … g/km |
| 3.5.7.2.1.1. | | Vehicle high: … g/km |
| 3.5.7.2.1.2. | | Vehicle low (if applicable): … g/km |
| 3.5.7.2.1.3. | | Vehicle M (if applicable): … g/km |
| 3.5.7.2.2. | | Charge-Sustaining CO2 emission for OVC-HEVs |
| 3.5.7.2.2.1. | | Charge Sustaining CO2 emission vehicle high: g/km |
| 3.5.7.2.2.2. | | Charge Sustaining CO2 emission vehicle low (if applicable): g/km |
| 3.5.7.2.2.3. | | Charge Sustaining CO2 emission vehicle M (if applicable): g/km |
| 3.5.7.2.3. | | Charge Depleting CO2 emission and weighted CO2 emission for OVC-HEVs |
| 3.5.7.2.3.1. | | Charge Depleting CO2 emission of Vehicle high: … g/km |
| 3.5.7.2.3.2. | | Charge Depleting CO2 emission of Vehicle low (if applicable): … g/km |
| 3.5.7.2.3.3. | | Charge Depleting CO2 emission of Vehicle M (if applicable): … g/km |
| 3.5.7.2.3.4. | | Minimum and maximum weighted CO2 values within the OVC interpolation family: … g/km |
| 3.5.7.3. | | Electric range for electrified vehicles |
| 3.5.7.3.1. | | Pure Electric Range (PER) for PEVs |
| 3.5.7.3.1.1. | | Vehicle high: … km |
| 3.5.7.3.1.2. | | Vehicle low (if applicable): … km |
| 3.5.7.3.2. | | All Electric Range AER and Equivalent All Electric Range EAER for OVC-HEVs and OVC-FCHVs (as applicable) |
| 3.5.7.3.2.1. | | Vehicle high: AER: … km, EAER: … km |
| 3.5.7.3.2.2. | | Vehicle low (if applicable): AER: … km, EAER: … km |
| 3.5.7.3.2.3. | | Vehicle M (if applicable): AER: … km, EAER: … km |
| 3.5.7.4. | | Fuel consumption (FCCS) for FCHVs |
| 3.5.7.4.1. | | Charge Sustaining fuel consumption for NOVC-FCHVs and OVC-FCHVs (as applicable) |
| 3.5.7.4.1.1. | | Vehicle high: … kg/100 km |
| 3.5.7.4.1.2. | | Vehicle low (if applicable): … kg/100 km |
| 3.5.7.4.1.3. | | Vehicle M (if applicable): … kg/100 km |
| 3.5.7.4.2. | | Charge-Depleting fuel consumption for OVC-FCHVs (as applicable) |
| 3.5.7.4.2.1. | | Vehicle high: … kg/100 km |
| 3.5.7.4.2.2. | | Vehicle low (if applicable): … kg/100 km |
| 3.5.7.5. | | Electric energy consumption for electrified vehicles |
| 3.5.7.5.1. | | Combined electric energy consumption (ECWLTC) for Pure electric vehicles |
| 3.5.7.5.1.1. | | Vehicle high: … Wh/km |
| 3.5.7.5.1.2. | | Vehicle low (if applicable): … Wh/km |
| 3.5.7.5.2. | | UF-weighted charge-depleting electric energy consumption ECAC,CD (combined) |
| 3.5.7.5.2.1. | | Vehicle high: … Wh/km |
| 3.5.7.5.2.2. | | Vehicle low (if applicable): … Wh/km |
| 3.5.7.5.2.3. | | Vehicle M (if applicable): … Wh/km |
| 3.5.7.6. | | Fuel efficiency |
| 3.5.7.6.1. | | Fuel efficiency for pure ICE vehicles and NOVC-HEVs |
| 3.5.7.6.1.1. | | Vehicle high: … km/l |
| 3.5.7.6.1.2. | | Vehicle low (if applicable): … km/l |
| 3.5.7.6.1.3. | | Vehicle M (if applicable): … km/l |
| 3.5.7.6.2. | | Charge-Sustaining fuel efficiency for OVC-HEVs |
| 3.5.7.6.2.1. | | Charge-Sustaining fuel efficiency vehicle high: km/l |
| 3.5.7.6.2.2. | | Charge-Sustaining fuel efficiency vehicle low (if applicable): km/l |
| 3.5.7.6.2.3. | | Charge-Sustaining fuel efficiency vehicle M (if applicable): km/l |
| 3.5.7.6.3. | | Charge-Depleting fuel efficiency for OVC-HEVs |
| 3.5.7.6.3.1. | | Charge-Depleting fuel efficiency of Vehicle high: … km/l |
| 3.5.7.6.3.2. | | Charge-Depleting fuel efficiency of Vehicle low (if applicable): … km/l |
| 3.5.7.6.3.3. | | Charge-Depleting fuel efficiency of Vehicle M (if applicable): … km/l |
| 3.5.7.6.4. | | Fuel efficiency for NOVC-FCHV |
| 3.5.7.6.4.1. | | Vehicle high: … km/kg |
| 3.5.7.6.4.2. | | Vehicle low (if applicable): … km/kg |
| 3.5.7.6.4.3. | | Vehicle M (if applicable): … km/kg |
| 3.6. | | Temperatures permitted by the manufacturer |
| 3.6.1. | | Cooling system |
| 3.6.1.1. | | Liquid cooling  Maximum temperature at outlet: … K |
| 3.6.1.2. | | Air cooling |
| 3.6.1.2.1. | | Reference point: … |
| 3.6.1.2.2. | | Maximum temperature at reference point: … K |
| 3.6.2. | | Maximum outlet temperature of the inlet intercooler: … K |
| 3.6.3. | | Maximum exhaust temperature at the point in the exhaust pipe(s) adjacent to the outer flange(s) of the exhaust manifold or turbocharger: … K |
| 3.6.4. | | Fuel temperature  Minimum: … K — maximum: … K  For diesel engines at injection pump inlet, for gas fuelled engines at pressure regulator final stage |
| 3.6.5. | | Lubricant temperature  Minimum: … K — maximum: … K |
| 3.8. | | Lubrication system |
| 3.8.1. | | Description of the system |
| 3.8.1.1. | | Position of lubricant reservoir: … |
| 3.8.1.2. | | Feed system (by pump/injection into intake/mixing with fuel, etc.) (1) |
| 3.8.2. | | Lubricating pump |
| 3.8.2.1. | | Make(s): … |
| 3.8.2.2. | | Type(s): … |
| 3.8.3. | | Mixture with fuel |
| 3.8.3.1. | | Percentage: … |
| 3.8.4. | | Oil cooler: yes/no (1) |
| 3.8.4.1. | | Drawing(s): … or |
| 3.8.4.1.1. | | Make(s): … |
| 3.8.4.1.2. | | Type(s): … |
| 3.8.5. | | Lubricant specification: …W… |
| 4. | | TRANSMISSION (p) |
| 4.3. | | Moment of inertia of engine flywheel: … |
| 4.3.1. | | Additional moment of inertia with no gear engaged: … |
| 4.4. | | Clutch(es) |
| 4.4.1. | | Type: … |
| 4.4.2. | | Maximum torque conversion: … |
| 4.5. | | Gearbox |
| 4.5.1. | | Type (manual/automatic/CVT (continuously variable transmission)) (1) |
| 4.5.1.4. | | Torque rating: … |
| 4.5.1.5. | | Number of clutches: … |
| 4.6. | | Gear ratios |
|  | | |  |  |  |  | | --- | --- | --- | --- | | Gear | Internal gearbox ratios (ratios of engine to gearbox output shaft revolutions) | Final drive ratio(s) (ratio of gearbox output shaft to driven wheel revolutions) | Total gear ratios | | Maximum for CVT |  |  |  | | 1 |  |  |  | | 2 |  |  |  | | 3 |  |  |  | | … |  |  |  | | Minimum for CVT |  |  |  | |
| 4.6.1. | | Gearshift |
| 4.6.1.1. | | Gear 1 excluded: yes/no (1) |
| 4.6.1.2. | | n95\_high for each gear: … min–1 |
| 4.6.1.3. | | nmin\_drive |
| 4.6.1.3.1. | | 1st gear: … min–1 |
| 4.6.1.3.2. | | 1st gear to 2nd: … min–1 |
| 4.6.1.3.3. | | 2nd gear to standstill: … min–1 |
| 4.6.1.3.4. | | 2nd gear: … min–1 |
| 4.6.1.3.5. | | 3rd gear and beyond: … min–1 |
| 4.6.1.4. | | nmin\_drive\_set for acceleration/constant speed phases (n\_min\_drive\_up): … min–1 |
| 4.6.1.5. | | nmin\_drive\_set for deceleration phases (nmin\_drive\_down): |
| 4.6.1.6. | | initial period of time |
| 4.6.1.6.1. | | tstart\_phase: … s |
| 4.6.1.6.2. | | nmin\_drive\_start: … min–1 |
| 4.6.1.6.3. | | nmin\_drive\_up\_start: … min–1 |
| 4.6.1.7. | | use of ASM: yes/no (1) |
| 4.6.1.7.1. | | ASM values: … at … min-1 |
| 4.7. | | Maximum vehicle design speed (in km/h) (q): … |
| 4.12. | | Gearbox lubricant: …W… |
| 6. | | SUSPENSION |
| 6.6. | | Tyres and wheels |
| 6.6.1. | | Tyre/wheel combination(s) |
| 6.6.1.1. | | Axles |
| 6.6.1.1.1. | | Axle 1: … |
| 6.6.1.1.1.1. | | Tyre size designation |
| 6.6.1.1.2. | | Axle 2: … |
| 6.6.1.1.2.1. | | Tyre size designation |
|  | | etc. |
| 6.6.2. | | Upper and lower limits of rolling radii |
| 6.6.2.1. | | Axle 1: … |
| 6.6.2.2. | | Axle 2: … |
| 6.6.3. | | Tyre pressure(s) as recommended by the vehicle manufacturer: … kPa |
| 9. | | BODYWORK |
| 9.1. | | Type of bodywork (c): … |
| 12. | | MISCELLANEOUS |
| 12.10. | | Devices or systems with driver selectable modes which influence CO2 emissions, electric energy consumption and/or criteria emissions and do not have a predominant mode: yes/no (1) |
| 12.10.1. | | Charge sustaining test (if applicable) (state for each device or system) |
| 12.10.1.0. | | Predominant mode under CS condition: yes/no (1) |
| 12.10.1.0.1. | | Predominant mode under CS condition: … (if applicable) |
| 12.10.1.1. | | Best case mode: … (if applicable) |
| 12.10.1.2. | | Worst case mode: … (if applicable) |
| 12.10.1.3. | | Mode which enables the vehicle to follow the reference test cycle: … (in case no predominant mode under CS condition and only one mode is able to follow the reference test cycle) |
| 12.10.2. | | Charge depleting test (if applicable) (state for each device or system) |
| 12.10.2.0. | | Predominant mode under CD condition: yes/no (1) |
| 12.10.2.0.1. | | Predominant mode under CD condition: … (if applicable) |
| 12.10.2.1. | | Most energy consuming mode: … (if applicable) |
| 12.10.2.2. | | Mode which enables the vehicle to follow the reference test cycle: … (in case no predominant mode under CD condition and only one mode is able to follow the reference test cycle) |
| 12.10.3. | | Type 1 test (if applicable) (state for each device or system) |
| 12.10.3.1. | | Best case mode: … |
| 12.10.3.2. | | Worst case mode: … |

***Explanatory notes***

(1) Delete where not applicable (there are cases where nothing needs to be deleted when more than one entry is applicable).

(2) Specify the tolerance.

(3) Please fill in here the upper and lower values for each variant.

(6) (Reserved)

(7) Optional equipment that affects the dimensions of the vehicle shall be specified.

(x) For insulation nominal volume and insulation nominal weight, state to 2 decimal places. A tolerance of +/- 10 per cent shall be applied for insulation volume and insulation weight, Not to be documented if “no” in paragraph 3.2.20.2.5. or 3.2.20.2.7.

(c) As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.6, paragraph 2. - www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html.

(f) Where there is one version with a normal cab and another with a sleeper cab, both sets of masses and dimensions are to be stated.

(g) Standard ISO 612: 1978 — Road vehicles — Dimensions of motor vehicles and towed vehicles — terms and definitions.

(h) The mass of the driver is assessed at 75 kg.

The liquid containing systems (except those for used water that must remain empty) are filled to 100 % of the capacity specified by the manufacturer.

(i) For trailers or semi-trailers, and for vehicles coupled with a trailer or a semi-trailer, which exert a significant vertical load on the coupling device or the fifth wheel, this load, divided by standard acceleration of gravity, is included in the maximum technically permissible mass.

(k) In the case of a vehicle that can run either on petrol, diesel, etc., or also in combination with another fuel, items shall be repeated.

In the case of non-conventional engines and systems, particulars equivalent to those referred to here shall be supplied by the manufacturer.

(l) This figure shall be rounded off to the nearest tenth of a millimetre.

(m) This value shall be calculated (π = 3.1416) and rounded off to the nearest cm3.

(n) Determined in accordance with the requirements of UN Regulation No. 85.

(p) The specified particulars are to be given for any proposed variants.

(q) With respect to trailers, maximum speed permitted by the manufacturer.

Annex 1A - Appendix 1

WLTP Test Report

**Test Reports**

A Test Report is the report issued by the technical service responsible for conducting the tests according this Regulation.

Part I

The following information, if applicable, is the minimum data required for the Type 1 test.

**Report number**

|  |  |  |  |
| --- | --- | --- | --- |
| **APPLICANT** |  | | |
| **Manufacturer** |  | | |
| **SUBJECT** | … | | |
| **Roadload family identifier(s)** | | **:** |  |
| Interpolation family identifier(s) | | **:** |  |
| **Object submitted to tests** | | | |
|  | Make | **:** |  |
|  | IP identifier | **:** |  |
| **CONCLUSION** | The object submitted to tests complies with the requirements mentioned in the subject. | | |

|  |  |
| --- | --- |
| place, | DD/MM/YYYY |

General notes:

If there are several options (references), the one tested should be described in the test report

If there are not, a single reference to the information document at the start of the test report may be sufficient.

Every Technical Service is free to include some additional information.

Characters are included in the sections of the test report relating to specific vehicle types, as follows:

"(a)" Specific to positive ignition engine vehicles or vehicles ‘G’ (as specified in Table 1B of UN Regulation No. 154) (as applicable).

"(b)" Specific to compression ignition engine vehicles or vehicles ‘D’ (as specified in Table 1B of UN Regulation No. 154) (as applicable).

**1.** **Description of tested vehicle(s): high, low and m (if applicable)**

**1.1. General**

|  |  |  |
| --- | --- | --- |
| Vehicle numbers | **:** | Prototype number and VIN |
| Category | **:** |  |
| Bodywork | **:** |  |
| Drive wheels | **:** |  |

**1.1.1. Powertrain Architecture**

|  |  |  |
| --- | --- | --- |
| Powertrain architecture | **:** | pure ICE, hybrid, electric or fuel cell |

**1.1.2. Internal combustion engine (if applicable)**

For more than one ICE, please repeat the point

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Make | **:** |  | | | | | |
| Type | **:** |  | | | | | |
| Working principle | **:** | two/four stroke | | | | | |
| Cylinders number and arrangement | **:** |  | | | | | |
| Engine capacity (cm3) | **:** |  | | | | | |
| Engine idling speed (min-1) | **:** |  | | +  - | | | |
| High engine idling speed (min-1) (a) | **:** |  | | +  - | | | |
| Rated engine power | **:** |  | kW | | at |  | rpm |
| Maximum net torque | **:** |  | Nm | | at |  | rpm |
| Engine lubricant | **:** | make and type | | | | | |
| Cooling system | **:** | Type: air/water/oil | | | | | |
| Insulation | **:** | material, amount, location, nominal volume and nominal weight(4) | | | | | |

(4) a tolerance of +/- 10 per cent is permitted for volume and weight

**1.1.3. Test fuel for Type 1 test (if applicable)**

For more than one test fuel, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : | Petrol - Diesel – LPG – NG - … |
| Density at 15°C | : |  |
| Sulphur content | : | Only for Diesel and Petrol |
|  | : |  |
| Batch number | : |  |
| Willans factors (for ICE) for CO2 emission (gCO2/MJ) | : |  |

**1.1.4. Fuel feed system (if applicable)**

For more than one fuel feed system, please repeat the point

|  |  |  |
| --- | --- | --- |
| Direct injection | **:** | yes/no or description |
| Vehicle fuel type | **:** | Monofuel / bifuel / flex fuel |
| Control unit | | |
| Part reference | **:** | same as information document |
| Software tested | **:** | read via scantool, for example |
| Air flowmeter | **:** |  |
| Throttle body | **:** |  |
| Pressure sensor | **:** |  |
| Injection pump | **:** |  |
| Injector(s) | **:** |  |

**1.1.5. Intake system (if applicable)**

For more than one intake system, please repeat the point

|  |  |  |
| --- | --- | --- |
| Pressure charger | **:** | Yes/no  make & type (1) |
| Intercooler | **:** | yes/no  type (air/air – air/water) (1) |
| Air filter (element) (1) | **:** | make & type |
| Intake silencer (1) | **:** | make & type |

**1.1.6. Exhaust system and anti-evaporative system (if applicable)**

For more than one, please repeat the point

|  |  |  |
| --- | --- | --- |
| First catalytic converter | **:** | make & reference (1)  principle: three way / oxidising / NOx trap / NOx storage system / Selective Catalyst Reduction… |
| Second catalytic converter | **:** | make & reference (1)  principle: three way / oxidising / NOx trap / NOx storage system / Selective Catalyst Reduction… |
| Particulate trap | **:** | with/without/not applicable  catalysed: yes/no  make & reference (1) |
| Reference and position of oxygen and/or lambda sensor(s) | **:** | before catalyst / after catalyst |
| Air injection | **:** | with/without/not applicable |
| Water injection | **:** | with/without/not applicable |
| EGR | **:** | with/without/not applicable  cooled/non-cooled  HP/LP |
| Evaporative emission control system | **:** | with/without/not applicable |
| Reference and position of NOx sensor(s) | **:** | Before/ after |
| Openings in the exhaust system designed to remove condensate (if applicable) | **:** | Position |
| General description (1) | **:** |  |

**1.1.7. Heat storage device (if applicable)**

For more than one Heat Storage System, please repeat the point

|  |  |  |
| --- | --- | --- |
| Heat storage device | **:** | yes/no |
| Heat capacity (enthalpy stored J) | **:** |  |
| Time for heat release (s) | **:** |  |

**1.1.8. Transmission (if applicable)**

For more than one Transmission, please repeat the point

|  |  |  |
| --- | --- | --- |
| Gearbox | **:** | manual / automatic / continuous variation |
| Gear shifting procedure | | |
| Predominant mode\* | **:** | yes/no  normal / drive / eco/… |
| Best case mode for CO2 emissions and fuel consumption (if applicable) | **:** |  |
| Worst case mode for CO2 emissions and fuel consumption (if applicable) | **:** |  |
| Highest electric energy consumption mode (if applicable) | **:** |  |
| Control unit | **:** |  |
| Gearbox lubricant | **:** | make and type |
| Tyres | | |
| Make | **:** |  |
| Type | **:** |  |
| Dimensions front/rear | **:** |  |
| Dynamic circumference (m) | **:** |  |
| Tyre pressure (kPa) | **:** |  |

\* for OVC-HEV, specify for charge sustaining and for charge depleting operating conditions.

Transmission ratios (R.T.), primary ratios (R.P.) and (vehicle speed (km/h)) / (engine speed (1000 (min-1)) (V1000) for each of the gearbox ratios (R.B.).

|  |  |  |  |
| --- | --- | --- | --- |
| R.B. | R.P. | R.T. | V1000 |
| 1st | 1/1 |  |  |
| 2nd | 1/1 |  |  |
| 3rd | 1/1 |  |  |
| 4th | 1/1 |  |  |
| 5th | 1/1 |  |  |
| … |  |  |  |
|  |  |  |  |

**1.1.9. Electric machine (if applicable)**

For more than one Electric Machine, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Peak Power (kW) | : |  |

**1.1.10. Traction REESS (if applicable)**

For more than one Traction REESS, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Capacity (Ah) | : |  |
| Nominal Voltage (V) | : |  |

**1.1.11. Fuel cell (if applicable)**

For more than one Fuel Cell stack, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |

**1.1.12. Power electronics (if applicable)**

Can be more than one PE (propulsion converter, low voltage system or charger)

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Power (kW) | : |  |

**1.2. Vehicle high description**

**1.2.1. Mass**

|  |  |  |
| --- | --- | --- |
| Test mass of VH (kg) | **:** |  |

**1.2.2. Road load parameters**

|  |  |  |
| --- | --- | --- |
| f0 (N) | **:** |  |
| f1 (N/(km/h)) | **:** |  |
| f2 (N/(km/h)²) | **:** |  |
| Cycle energy demand 4 phase cycle (J) | **:** |  |
| Cycle energy demand 3 phase cycle (J) | **:** |  |
| Road load test report reference | **:** |  |
| Road load family’s identifier | **:** |  |

**1.2.3. Cycle Selection parameters**

|  |  |  |
| --- | --- | --- |
| Cycle (without downscaling) | **:** | Class 1 / 2 / 3a / 3b |
| Ratio of rated power to mass in running order – 75kg (PMR)(W/kg) | **:** | (if applicable) |
| Capped speed process used during measurement | **:** | yes/no |
| Maximum speed of the vehicle (km/h) | **:** |  |
| Downscaling (if applicable) | **:** | yes/no |
| Downscaling factor fdsc | **:** |  |
| Cycle distance (m) | **:** |  |
| Constant speed (in the case of the shortened test procedure) | **:** | if applicable |

**1.2.4. Gear shift point (if applicable)**

|  |  |  |
| --- | --- | --- |
| Version of Gear Shift calculation |  | indicate the applicable amendment to UN GTR No 15 |
| Gear shifting | **:** | Average gear for v ≥ 1 km/h, x.xxxx |
| nmin\_drive | | |
| 1st gear | **:** | …min-1 |
| 1st gear to 2nd | **:** | …min-1 |
| 2nd gear to standstill | **:** | …min-1 |
| 2nd gear | **:** | …min-1 |
| 3rd gear and beyond | **:** | …min-1 |
| Gear 1 excluded | **:** | yes/no |
| n95\_high for each gear | **:** | …min-1 |
| nmin\_drive\_set  for acceleration/constant speed phases (nmin\_drive\_up) | **:** | …min-1 |
| nmin\_drive\_set for deceleration phases (nmin\_drive\_down) | **:** | …min-1 |
| tstart\_phase | **:** | …s |
| nmin\_drive\_start | **:** | …min-1 |
| nmin\_drive\_up\_start | **:** | …min-1 |
| use of ASM | **:** | yes/no |
| ASM values | **:** |  |

**1.3. Vehicle low description (if applicable)**

**1.3.1. Mass**

|  |  |  |
| --- | --- | --- |
| Test mass of VL(kg) | **:** |  |

**1.3.2. Road load parameters**

|  |  |  |
| --- | --- | --- |
| f0 (N) | **:** |  |
| f1 (N/(km/h)) | **:** |  |
| f2 (N/(km/h)²) | **:** |  |
| Cycle energy demand 4 phase cycle (J) | **:** |  |
| Cycle energy demand 3 phase cycle (J) | **:** |  |
| Δ(CD×Af)LH (m2) | **:** |  |
| Road load test report reference | **:** |  |
| Road load family’s identifier | **:** |  |

**1.3.3. Cycle Selection parameters**

|  |  |  |
| --- | --- | --- |
| Cycle (without downscaling) | **:** | Class 1 / 2 / 3a / 3b |
| Ratio of rated power to mass in running order – 75kg (PMR)(W/kg) | **:** | (if applicable) |
| Capped speed process used during measurement | **:** | yes/no |
| Maximum speed of the vehicle | **:** |  |
| Downscaling (if applicable) | **:** | yes/no |
| Downscaling factor fdsc | **:** |  |
| Cycle distance (m) | **:** |  |
| Constant speed (in the case of the shortened test procedure) | **:** | if applicable |

**1.3.4. Gear shift point (if applicable)**

|  |  |  |
| --- | --- | --- |
| Gear shifting | **:** | Average gear for v ≥ 1 km/h, x.xxxx |

**1.4. Vehicle M description (if applicable)**

**1.4.1. Mass**

|  |  |  |
| --- | --- | --- |
| Test mass of VM(kg) | **:** |  |

**1.4.2. Road load parameters**

|  |  |  |
| --- | --- | --- |
| f0 (N) | **:** |  |
| f1 (N/(km/h)) | **:** |  |
| f2 (N/(km/h)²) | **:** |  |
| Cycle energy demand 4 phase cycle (J) | **:** |  |
| Cycle energy demand 3 phase cycle (J) | **:** |  |
| Δ(CD×Af)LH (m2) | **:** |  |
| Road load test report reference | **:** |  |
| Road load family’s identifier | **:** |  |

**1.4.3. Cycle Selection parameters**

|  |  |  |
| --- | --- | --- |
| Cycle (without downscaling) | **:** | Class 1 / 2 / 3a / 3b |
| Ratio of rated power to mass in running order – 75kg (PMR)(W/kg) | **:** | (if applicable) |
| Capped speed process used during measurement | **:** | yes/no |
| Maximum speed of the vehicle | **:** |  |
| Downscaling (if applicable) | **:** | yes/no |
| Downscaling factor fdsc | **:** |  |
| Cycle distance (m) | **:** |  |
| Constant speed (in the case of the shortened test procedure) | **:** | if applicable |

**1.4.4. Gear shift point (if applicable)**

|  |  |  |
| --- | --- | --- |
| Gear shifting | **:** | Average gear for v ≥ 1 km/h, x.xxxx |

**2. Test results**

**2.1. Type 1 test**

|  |  |  |
| --- | --- | --- |
| Method of chassis dyno setting | **:** | Fixed run / iterative / alternative with its own warmup cycle |
| Dynamometer in 2WD/4WD operation | **:** | 2WD/4WD |
| For 2WD operation, was the non-powered axle rotating | **:** | yes/no/not applicable |
| Dynamometer operation mode  . |  | yes/no |
| Coastdown mode | **:** | yes/no |
| Additional preconditioning | **:** | yes/no  description |
| Deterioration factors | **:** | assigned / tested |

**2.1.1. Vehicle high**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date(s) of test(s) | | | **:** | (day/month/year) |
| Place of the test(s) | **:** | Chassis dyno, location, country | | |
| Height of the lower edge above ground of cooling fan (cm) | **:** |  | | |
| Lateral position of fan centre (if modified as request by the manufacturer) | **:** | in the vehicle centre-line/… | | |
| Distance from the front of the vehicle (cm) | **:** |  | | |
| IWR: Inertial Work Rating 4 phase cycle (%) | **:** | x.x | | |
| IWR: Inertial Work Rating 3 phase cycle (%) | **:** | x.x | | |
| RMSSE: Root Mean Squared Speed Error 4 phase cycle (km/h) | **:** | x.xx | | |
| RMSSE: Root Mean Squared Speed Error 3 phase cycle (km/h) | **:** | x.xx | | |
| Description of the accepted deviation of the driving cycle | **:** | PEV before break off criteria  or  Fully operated acceleration pedal | | |

**2.1.1.1. Pollutant emissions (if applicable)**

**2.1.1.1.1. Pollutant emissions of vehicles with at least one combustion engine, of NOVC-HEVs and of OVC-HEVs in case of a charge-sustaining type 1 test**

For each driver selectable mode tested the points below shall be repeated (predominant mode or best case mode and worst case, mode if applicable)

Test 1a Results after 4 Phase cycle

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *THC+NOx (b)* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Measured values |  |  |  |  |  |  |  |
| Regeneration factors (Ki)(2)  Additive |  |  |  |  |  |  |  |
| Regeneration factors (Ki)(2)  Multiplicative |  |  |  |  |  |  |  |
| Deterioration factors (DF) additive |  |  |  |  |  |  |  |
| Deterioration factors (DF) multiplicative |  |  |  |  |  |  |  |
| Final values |  |  |  |  |  |  |  |
| Limit values |  |  |  |  |  |  |  |

Test 1b – Results after 3 Phase cycle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Measured values |  |  |  |  |  |  |
| Regeneration factors (Ki)(2)  Additive |  |  |  |  |  |  |
| Regeneration factors (Ki)(2)  Multiplicative |  |  |  |  |  |  |
| Deterioration factors (DF) additive |  |  |  |  |  |  |
| Deterioration factors (DF) multiplicative |  |  |  |  |  |  |
| Final values |  |  |  |  |  |  |
| Limit values |  | - |  |  |  |  |

|  |  |  |
| --- | --- | --- |
| (2) See Ki family report(s) | **:** |  |
| Type 1 performed for Ki determination | **:** |  |
| Regeneration family’s identifier | **:** |  |

Test 2a and 2b if applicable: for CO2 reason (dCO21) / for pollutants reason (90% of the limits) / for both

Record test results in accordance with the table of Test 1

Test 3a and 3b if applicable: for CO2 reason (dCO22)

Record test results in accordance with the table of Test 1

**2.1.1.1.2. Pollutant emissions of OVC-HEVs in case of a charge-depleting type 1 test**

Test 1a - Results after 4 Phase cycle

Pollutant emission limits have to be fulfilled and the following point has to be repeated for each driven test cycle.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *THC+NOx (b)* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Measured single cycle values |  |  |  |  |  |  |  |
| Limit single cycle values |  |  |  |  |  |  |  |

Test 1b – Results after 3 Phase cycle

Pollutant emission limits have to be fulfilled and the following point has to be repeated for each driven test cycle.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Measured single cycle values |  |  |  |  |  |  |
| Limit single cycle values |  |  |  |  |  |  |

Test 2a and 2b (if applicable): for CO2 reason (dCO21) / for pollutants reason (90% of the limits) / for both

Record test results in accordance with the table of Test 1

Test 3a and 3b (if applicable): for CO2 reason (dCO22)

Record test results in accordance with the table of Test 1

**2.1.1.1.3. UF-weighted pollutant emissions of OVC-HEVs**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *THC+NOx (b)* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Calculated values 4 phase cycle |  |  |  |  |  |  |  |

**2.1.1.2. CO2 emission (if applicable)**

**2.1.1.2.1. CO2 emission of vehicles with at least one combustion engine, of NOVC-HEV and of OVC-HEV in the case of a charge-sustaining Type 1 test**

For each driver selectable mode tested the points below have to be repeated (predominant mode or best case mode and worst case, mode if applicable)

Test 1a – Results after 4 Phase cycle

| *CO2 emission* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| --- | --- | --- | --- | --- | --- |
| Measured value MCO2,p,1 / MCO2,c,2 |  |  |  |  | - |
| Speed and distance corrected value MCO2,p,2b / MCO2,c,2b |  |  |  |  |  |
| RCB correction coefficient: (5) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |
| Regeneration factors (Ki)  Additive |  | | | | |
| Regeneration factors (Ki)  Multiplicative |  | | | | |
| MCO2,c,4 | - | | | |  |
| AFKi= MCO2,c,3 / MCO2,c,4 | - | | | |  |
| MCO2,p,4 / MCO2,c,4 |  |  |  |  | - |
| ATCT correction (FCF) (4) |  | | | | |
| **Temporary values** MCO2,p,5 / MCO2,c,5 |  |  |  |  |  |
| **Declared value** | - | - | - | - |  |
| **dCO21 \* declared value** | - | - | - | - |  |

|  |  |  |
| --- | --- | --- |
| (4) FCF: family correction factor for correcting for representative regional temperature conditions (ATCT) | | |
| See ATCT family report(s) | **:** |  |
| ATCT family’s identifier | **:** |  |
| (5) correction as referred to in Appendix 2 to Annex B6 of UN Regulation 154 for pure ICE vehicles, and Appendix 2 to Annex B8 of UN Regulation 154 for HEVs (KCO2) | | |

Test 2a and 2b (if applicable)

Record test results in accordance with the table of Test 1

Test 3a and 3b (if applicable)

Record test results in accordance with the table of Test 1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Conclusion after 4 phase cycle  *CO2 emission (g/km)* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| Averaging MCO2,p,6/ MCO2,c,6 |  |  |  |  |  |
| Alignment MCO2,p,7 / MCO2,c,7 |  |  |  |  |  |
| **Final values** MCO2,p,H / MCO2,c,H |  |  |  |  |  |

**2.1.1.2.2. CO2 mass emission of OVC-HEVs in case of a charge-depleting Type 1 test**

Test 1:

|  |  |
| --- | --- |
| *CO2 mass emission (g/km)* | *Combined*  *4 phase cycle* |
| Calculated value MCO2,CD |  |
| **Declared value** |  |
| **dCO21** |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion

|  |  |
| --- | --- |
| *CO2 mass emission (g/km)* | *Combined*  *4 phase cycle* |
| Averaging MCO2,CD |  |
| **Final value** MCO2,CD |  |

**2.1.1.2.3. UF-weighted CO2 mass emission of OVC-HEVs**

|  |  |
| --- | --- |
| *CO2 mass emission (g/km)* | *Combined*  *4 phase cycle* |
| Calculated value MCO2,weighted |  |

**2.1.1.3. Fuel consumption (if applicable)**

**2.1.1.3.1. Fuel consumption of vehicles with only a combustion engine, of NOVC-HEVs and of OVC-HEVs in case of a charge-sustaining Type 1 test**

For each driver selectable mode tested the points below has to be repeated (predominant mode or best case mode and worst case, mode if applicable)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Fuel consumption (l/100 km) or fuel efficiency (km/l) (as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC* | *Combined FE* |
| Final values FCp,H / FCc,H (6) |  |  |  |  |  | - |
| Final values FEp, FEc |  |  |  |  | - |  |

(6) Calculated from aligned CO2 values

On-board Fuel and/or Energy Consumption Monitoring for vehicles referred to in paragraph 5.11. of this Regulation

Data accessibility

The parameters listed in paragraph 3 of Appendix 5 to this Regulation are accessible: yes/not applicable

Accuracy (if applicable**)**

|  |  |  |
| --- | --- | --- |
| Fuel\_ConsumedWLTP (litres) (8) | Vehicle HIGH - Test 1 | x.xxx |
| Vehicle HIGH - Test 2 (if applicable) | x.xxx |
| Vehicle HIGH - Test 3 (if applicable) | x.xxx |
| Vehicle LOW - Test 1 (if applicable) | x.xxx |
| Vehicle LOW Test 2 (if applicable) | x.xxx |
| Vehicle LOW - Test 3 (if applicable) | x.xxx |
| Total | x.xxx |
| Fuel\_ConsumedOBFCM (litres) (8) | Vehicle HIGH - Test 1 | x.xxx(9) |
| Vehicle HIGH - Test 2 (if applicable) | x.xxx(9) |
| Vehicle HIGH - Test 3 (if applicable) | x.xxx(9) |
| Vehicle LOW - Test 1 (if applicable) | x.xxx(9) |
| Vehicle LOW Test 2 (if applicable) | x.xxx(9) |
| Vehicle LOW - Test 3 (if applicable) | x.xxx(9) |
| Total | x.xxx(9) |
| Accuracy (8) | | x.xxx |

(8) in accordance with Appendix 5 to this Regulation

(9) In the case that the OBFCM signal can only be read-out to 2 decimal places, the third decimal place shall be introduced as a zero

**2.1.1.3.2. Fuel consumption of OVC-HEVs and OVC-FCHVs (as applicable) in case of a charge-depleting Type 1 test**

Test 1:

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (l/100 km or kg/100 km)*  *Combined*  *4-phase cycle* | *Fuel efficiency (km/l) Combined*  *3 phase cycle* |
| Calculated value FCCD, FECD |  |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (l/100km or kg/100 km)*  *Combined*  *4 phase cycle* | *Fuel efficiency (km/l)*  *Combined*  *3 phase cycle* |
| Averaging FCCD, FECD |  |  |
| **Final value** FCCD, FECD |  |  |

**2.1.1.3.3. UF-Weighted Fuel consumption of OVC-HEVs and OVC-FCHVs (as applicable)**

|  |  |
| --- | --- |
|  | *Fuel consumption (l/100km) or kg/100 km*  *Combined*  *4 phase cycle* |
| Calculated value FCweighted |  |

**2.1.1.3.4. Fuel consumption of vehicles of NOVC-FCHVs and OVC-FCHVs (as applicable) in case of a charge-sustaining Type 1 test**

For each driver selectable mode tested the points below has to be repeated (predominant mode or best case mode and worst case, mode if applicable)

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (kg/100 km)*  *Combined*  *4-phase cycle* | *Fuel efficiency (km/kg)*  *Combined*  *3 phase cycle* |
| Measured values |  |  |
| RCB correction coefficient |  |  |
| Final values FCc, FEc |  |  |

**2.1.1**.**4. Ranges (if applicable)**

**2.1.1.4.1. Ranges for OVC-HEVs and OVC-FCHVs (as applicable)**

2.1.1.4.1.1. All electric range

Test 1

|  |  |  |  |
| --- | --- | --- | --- |
| *AER (km)* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Measured/Calculated values AER |  |  |  |
| **Declared value** | - |  |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion

|  |  |  |  |
| --- | --- | --- | --- |
| *AER (km)* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Averaging AER (if applicable) |  |  |  |
| **Final values** AER |  |  |  |

2.1.1.4.1.2. Equivalent All electric Range

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *EAER (km)* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated value EAER |  |  |  |  |  |  |  |
| Declared value | - | - | - | - | - |  |  |
| **Final values** EAER |  |  |  |  |  |  |  |

2.1.1.4.1.3. Actual Charge-Depleting Range

|  |  |  |
| --- | --- | --- |
| *RCDA (km)* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| **Final value** RCDA |  |  |

2.1.1.4.1.4. Charge-Depleting Cycle Range

Test 1

|  |  |  |
| --- | --- | --- |
| *RCDC (km)* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| **Final value** RCDC |  |  |
| Index Number of the transition cycle |  |  |
| REEC of confirmation-cycle (%) |  |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

**2.1.1.4.2. Ranges for PEVs - Pure electric range (if applicable)**

Test 1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *PER (km)* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated values PER |  |  |  |  |  |  |  |
| **Declared value** | - | - | - | - | - |  |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion

|  |  |  |  |
| --- | --- | --- | --- |
| *PER (km)* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Averaging PER |  |  |  |
| Final values PER |  |  |  |

**2.1.1.5**. **Electric energy consumption (if applicable)**

**2.1.1.5.1. Electric energy consumption of OVC-HEVs and OVC-FCHVs (as applicable)**

2.1.1.5.1.1. Recharged electric energy (EAC)

|  |  |
| --- | --- |
| EAC(Wh) |  |

2.1.1.5.1.2. Electric energy consumption (EC)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Final values EC |  |  |  |  |  |  |  |

2.1.1.5.1.3. UF-weighted charge-depleting electric energy consumption

Test 1

|  |  |
| --- | --- |
| *EC*AC,CD *(Wh/km)* | *Combined*  *4 phase cycle* |
| Calculated value ECAC,CD |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion (if applicable)

|  |  |
| --- | --- |
| *ECAC,CD (Wh/km)* | *Combined*  *4 phase cycle* |
| Averaging ECAC,CD |  |
| **Final value** |  |

2.1.1.5.1.4. UF-weighted electric energy consumption

Test 1

|  |  |
| --- | --- |
| *ECAC,weighted (Wh)* | *Combined*  *4 phase cycle* |
| Calculated value ECAC,weighted |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3 (if applicable)

Record test results in accordance with the table of Test 1

Conclusion (if applicable)

|  |  |
| --- | --- |
| *ECAC,weighted (Wh/km)* | *Combined*  *4 phase cycle* |
| Averaging ECAC,weighted |  |
| **Final value** |  |

2.1.1.5.1.5. Information for COP

|  |  |  |
| --- | --- | --- |
|  | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Electric energy consumption (Wh/km) ECDC,CD,COP or EAAC,CD,COP (as applicable) |  |  |
| AFEC,AC,CD (as applicable) |  |  |

**2.1.1.5.2. Electric energy consumption of PEVs (if applicable)**

Test 1

|  |  |
| --- | --- |
| EAC(Wh) |  |

|  |  |  |  |
| --- | --- | --- | --- |
| *EC (Wh/km)* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated values EC |  |  |  |
| **Declared value** | - |  |  |

Test 2 (if applicable)

Record test results in accordance with the table of Test 1

Test 3a – Results after 4 Phase cycle (if applicable)

Record test results in accordance with the table of Test 1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Low* 4 Phase cycle | *Medium* 4 Phase cycle | *High* 4 Phase cycle | *Extra High* 4 Phase cycle | *City* 4 Phase cycle | *Combined*  *4 phase cycle* |  |
| Averaging EC |  |  |  |  |  |  |  |
| **Final values EC** |  |  |  |  |  |  |  |

Test 3b – Results after 3 Phase cycle (if applicable)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Low* 3 Phase cycle | *Medium* 3 Phase cycle | *High* 3 Phase cycle | *Combined*  *4 phase cycle* |
| Averaging EC |  |  |  |  |
| **Final values EC** |  |  |  |  |

Information for COP – Results after 4 phase cycle (if applicable)

|  |  |  |
| --- | --- | --- |
|  | *Combined*  *4 phase cycle* |  |
| Electric Energy Consumption (Wh/km) ECDC,COP |  |  |
| AFEC |  |  |

Information for COP – Results after 3 phase cycle (if applicable)

|  |  |
| --- | --- |
|  | *Combined*  *3 phase cycle* |
| Electric Energy Consumption (Wh/km) ECDC,COP |  |
| AFEC |  |

**2.1.2. Vehicle low (if applicable)**

Repeat paragraph 2.1.1.

**2.1.3. Vehicle M (if applicable)**

Repeat paragraph 2.1.1.

**2.1.4. Final criteria emissions values (if applicable)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* |  | *PM* | *PN* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* |  | *(mg/km)* | *(#.1011/km)* |
| **Highest values(3) 4 phase test** |  |  |  |  |  |  |  |

(3) for each pollutant within all test results of VH, VL (if applicable) and VM (if applicable)

**2.4. Type 4 (a) test**

|  |  |  |
| --- | --- | --- |
| Family’s identifier | **:** |  |
| See report(s) | **:** |  |

**2.5. Type 5 test**

|  |  |  |
| --- | --- | --- |
| Family’s identifier | **:** |  |
| See durability family report(s) | **:** |  |
| Type 1 cycle for criteria emissions testing | **:** |  |
| Durability family identifier |  |  |

**2.8. On board diagnostic system**

|  |  |  |
| --- | --- | --- |
| Family’s identifier | : |  |
| See family report(s) | : |  |

**2.11. Temperature information related to vehicle high (VH)**

|  |  |  |
| --- | --- | --- |
| Worst case approach with regards to vehicle insulation | : | yes/no (7) |
| Worst case approach vehicle cool down | : | yes/no (7) |
| ATCT family composed of a single Interpolation family | : | yes/no (7) |
| Engine coolant temperature at the end of soaking time (°C) | : |  |
| Average soak area temperature over the 3 last hours (°C) | : |  |
| Difference between engine coolant end temperature and average soak area temperature of the last 3 hours ∆T\_ATCT (°C) | : |  |
| The minimum soaking time tsoak\_ATCT (s) | : |  |
| Location of temperature sensor | : |  |
| Measured engine temperature | : | oil/coolant |

(7) if “yes” then the six last lines are not applicable

**2.12. Exhaust after-treatment system using reagent**

|  |  |  |
| --- | --- | --- |
| Family’s identifier | : |  |
| See family report(s) | : |  |

Part II

The following information, if applicable, is the minimum data required for the ATCT test.

**Report number**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **APPLICANT** |  | | | |
| **Manufacturer** |  | | | |
| **SUBJECT** | … | | | |
| **Roadload family identifier(s)** | | **:** | |  |
| **Interpolation family identifier(s)** | | **:** | |  |
| **ATCT identifier(s)** | | **:** | |  |
| **Object submitted to tests** | | | | |
|  | Make | | **:** |  |
|  | IP identifier | | **:** |  |
| **CONCLUSION** | The object submitted to tests complies with the requirements mentioned in the subject. | | | |

|  |  |
| --- | --- |
| place, | DD/MM/YYYY |

General notes:

If there are several options (references), the one tested should be described in the test report

If there are not, a single reference to the information document at the start of the test report may be sufficient.

Every Technical Service is free to include some additional information.

Characters are included in the sections of the test report relating to specific vehicle types, as follows:

“(a)” Specific to positive ignition engine vehicles or vehicles ‘G’ (as specified in Table 1B of UN Regulation No. 154) (as applicable).

“(b)” Specific to compression ignition engine vehicles or vehicles ‘D’ (as specified in Table 1B of UN Regulation No. 154) (as applicable).

**1.** **Description of tested vehicle**

**1.1. General**

|  |  |  |
| --- | --- | --- |
| Vehicle numbers | **:** | Prototype number and VIN |
| Category | **:** |  |
| Bodywork | **:** |  |
| Drive wheels | **:** |  |

**1.1.1. Powertrain Architecture**

|  |  |  |
| --- | --- | --- |
| Powertrain architecture | **:** | pure ICE, hybrid, electric or fuel cell |

**1.1.2. Internal combustion engine (if applicable)**

For more than one ICE, please repeat the point

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Make | **:** |  | | | | | |
| Type | **:** |  | | | | | |
| Working principle | **:** | two/four stroke | | | | | |
| Cylinders number and arrangement | **:** |  | | | | | |
| Engine capacity (cm3) | **:** |  | | | | | |
| Engine idling speed (min-1) | **:** |  | | ± | | | |
| High engine idling speed (min-1) (a) | **:** |  | | ± | | | |
| Rated engine power | **:** |  | kW | | At |  | rpm |
| Maximum net torque | **:** |  | Nm | | At |  | rpm |
| Engine lubricant | **:** | make and type | | | | | |
| Cooling system | **:** | Type: air/water/oil | | | | | |
| Insulation | **:** | material, amount, location, nominal volume and nominal weight(4) | | | | | |

(4) a tolerance of +/- 10 per cent is permitted for volume and weight

**1.1.3. Test fuel for type 1 test (if applicable)**

For more than one test fuel, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : | Petrol - Diesel – LPG – NG - … |
| Density at 15°C | : |  |
| Sulphur content | : | Only for Diesel and Petrol |
| Annex IX | : |  |
| Batch number | : |  |
| Willans factors (for ICE) for CO2 emission (gCO2/MJ) | : |  |
| Direct injection | **:** | yes/no or description |
| Vehicle fuel type | **:** | Monofuel / bifuel / flex fuel |
| Control unit | | |
| Part reference | **:** | same as information document |
| Software tested | **:** | read via scantool, for example |
| Air flowmeter | **:** |  |
| Throttle body | **:** |  |
| Pressure sensor | **:** |  |
| Injection pump | **:** |  |
| Injector(s) | **:** |  |

**1.1.4. Fuel feed system (if applicable)**

For more than one fuel feed system, please repeat the point

**1.1.5. Intake system (if applicable)**

For more than one intake system, please repeat the point

|  |  |  |
| --- | --- | --- |
| Pressure charger | **:** | Yes/no  make & type (1) |
| Intercooler | **:** | yes/no  type (air/air – air/water) (1) |
| Air filter (element) (1) | **:** | make & type |
| Intake silencer (1) | **:** | make & type |

**1.1.6. Exhaust system and anti-evaporative system (if applicable)**

For more than one, please repeat the point

|  |  |  |
| --- | --- | --- |
| First catalytic converter | **:** | make & reference (1)  principle: three way / oxidising / NOx trap / NOx storage system / Selective Catalyst Reduction… |
| Second catalytic converter | **:** | make & reference (1)  principle: three way / oxidising / NOx trap / NOx storage system / Selective Catalyst Reduction… |
| Particulate trap | **:** | with/without/not applicable  catalysed: yes/no  make & reference (1) |
| Reference and position of oxygen and/or lambda sensor(s) | **:** | before catalyst / after catalyst |
| Air injection | **:** | with/without/not applicable |
| Water injection | **:** | with/without/not applicable |
| EGR | **:** | with/without/not applicable  cooled/non-cooled  HP/LP |
| Evaporative emission control system | **:** | with/without/not applicable |
| Reference and position of NOx sensor(s) | **:** | Before/ after |
| Openings in the exhaust system designed to remove condensate (if applicable) | : | Position |
| General description (1) | **:** |  |

**1.1.7. Heat storage device (if applicable)**

For more than one Heat Storage System, please repeat the point

|  |  |  |
| --- | --- | --- |
| Heat storage device | **:** | yes/no |
| Heat capacity (enthalpy stored J) | **:** |  |
| Time for heat release (s) | **:** |  |

**1.1.8. Transmission (if applicable)**

For more than one Transmission, please repeat the point

|  |  |  |
| --- | --- | --- |
| Gearbox | **:** | manual / automatic / continuous variation |
| Gear shifting procedure | | |
| Predominant mode | **:** | yes/no  normal / drive / eco/… |
| Best case mode for CO2 emissions and fuel consumption (if applicable) | **:** |  |
| Worst case mode for CO2 emissions and fuel consumption (if applicable) | **:** |  |
| Control unit | **:** |  |
| Gearbox lubricant | **:** | make and type |
| Tyres | | |
| Make | **:** |  |
| Type | **:** |  |
| Dimensions front/rear | **:** |  |
| Dynamic circumference (m) | **:** |  |
| Tyre pressure (kPa) | **:** |  |

Transmission ratios (R.T.), primary ratios (R.P.) and (vehicle speed (km/h)) / (engine speed (1000 (min-1)) (V1000) for each of the gearbox ratios (R.B.).

|  |  |  |  |
| --- | --- | --- | --- |
| *R.B.* | *R.P.* | *R.T.* | *V1000* |
| 1st | 1/1 |  |  |
| 2nd | 1/1 |  |  |
| 3rd | 1/1 |  |  |
| 4th | 1/1 |  |  |
| 5th | 1/1 |  |  |
| … |  |  |  |
|  |  |  |  |

**1.1.9. Electric machine (if applicable)**

For more than one electric machine, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Peak Power (kW) | : |  |

**1.1.10. Traction REESS (if applicable)**

For more than one traction REESS, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Capacity (Ah) | : |  |
| Nominal Voltage (V) | : |  |

**1.1.11. (Reserved)**

**1.1.12. Power electronics (if applicable)**

Can be more than one PE (propulsion converter, low voltage system or charger)

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Power (kW) | : |  |

**1.2. Vehicle description**

**1.2.1. Mass**

|  |  |  |
| --- | --- | --- |
| Test mass of VH (kg) | **:** |  |

**1.2.2. Road load parameters**

|  |  |  |
| --- | --- | --- |
| f0 (N) | **:** |  |
| f1 (N/(km/h)) | **:** |  |
| f2 (N/(km/h)²) | **:** |  |
| f2\_TReg (N/(km/h)²) | **:** |  |
| Cycle energy demand 4 phase cycle (J) | **:** |  |
| Road load test report reference | **:** |  |
| Road load family’s identifier | **:** |  |

**1.2.3. Cycle selection parameters**

|  |  |  |
| --- | --- | --- |
| Cycle (without downscaling) | **:** | Class 1 / 2 / 3a / 3b |
| Ratio of rated power to mass in running order -75kg (PMR)(W/kg) | **:** | (if applicable) |
| Capped speed process used during measurement | **:** | yes/no |
| Maximum speed of the vehicle (km/h) | **:** |  |
| Downscaling (if applicable) | **:** | yes/no |
| Downscaling factor fdsc | **:** |  |
| Cycle distance (m) | **:** |  |
| Constant speed (in the case of the shortened test procedure) | **:** | if applicable |

**1.2.4. Gear shift point (if applicable)**

|  |  |  |
| --- | --- | --- |
| Version of Gear Shift calculation |  | (indicate the applicable amendment to UN GTR No. 15) |
| Gear shifting | **:** | Average gear for v ≥ 1 km/h, rounded to four places of decimal |
| nmin drive | | |
| 1st gear | **:** | …min-1 |
| 1st gear to 2nd | **:** | …min-1 |
| 2nd gear to standstill | **:** | …min-1 |
| 2nd gear | **:** | …min-1 |
| 3rd gear and beyond | **:** | …min-1 |
| Gear 1 excluded | **:** | yes/no |
| n95\_high for each gear | **:** | …min-1 |
| nmin\_drive\_set for acceleration/constant speed phases (nmin\_drive\_up) | **:** | …min-1 |
| nmin\_drive\_set for deceleration phases (nmin\_drive\_down) | **:** | …min-1 |
| tstart\_phase | **:** | …s |
| nmin\_drive\_start | **:** | …min-1 |
| nmin\_drive\_up\_start | **:** | …min-1 |
| use of ASM | **:** | yes/no |
| ASM values | **:** |  |

**2. Test results**

|  |  |  |
| --- | --- | --- |
| Method of chassis dyno setting | **:** | Fixed run / iterative / alternative with its own warmup cycle |
| Dynamometer in 2WD/4WD operation | **:** | 2WD/4WD |
| For 2WD operation, was the non-powered axle rotating | **:** | yes/no/not applicable |
| Dynamometer operation mode |  | yes/no |
| Coastdown mode | **:** | yes/no |

**2.1 . Test at 14°C**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date(s) of test(s) | | | **:** | (day/month/year) |
| Place of the test(s) | **:** |  | | |
| Height of the lower edge above ground of cooling fan (cm) | **:** |  | | |
| Lateral position of fan centre (if modified as request by the manufacturer) | **:** | in the vehicle centre-line/… | | |
| Distance from the front of the vehicle (cm) | **:** |  | | |
| IWR: Inertial Work Rating (%) | **:** | x.x | | |
| RMSSE: Root Mean Squared Speed Error (km/h) | **:** | x.xx | | |
| Description of the accepted deviation of the driving cycle | **:** | Fully operated acceleration pedal | | |

**2.1.1. Pollutant emissions of vehicle with at least one combustion engine, of NOVC-HEVs and of OVC-HEVs in case of a charge-sustaining *test***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *THC+NOx (b)* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Measured values |  |  |  |  |  |  |  |
| Limit values |  |  |  |  |  |  |  |

**2.1.2. CO2 emission of vehicle with at least one combustion engine, of NOVC-HEV and of OVC-HEV in case of a charge-sustaining test**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *CO2 emission (g/km)* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| Measured value MCO2,p,1 / MCO2,c,2 |  |  |  |  | - |
| Measured Speed and distance corrected value MCO2,p,2b / MCO2,c,2b |  |  |  |  |  |
| RCB correction coefficient (2) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |

(2) correction as referred to in Appendix 2 to Annex B6 of UN Regulation No. 154 for ICE vehicles, KCO2 for HEVs

**2.2. Test at 23°C**

Provide information or refer to type 1 test report

|  |  |  |
| --- | --- | --- |
| Date of tests | **:** | (day/month/year) |
| Place of the test | **:** |  |
| Height of the lower edge above ground of cooling fan (cm) | **:** |  |
| Lateral position of fan centre (if modified as request by the manufacturer) | **:** | in the vehicle centre-line/… |
| Distance from the front of the vehicle (cm) | **:** |  |
| IWR: Inertial Work Rating 4 phase cycle(%) | **:** | x.x |
| RMSSE: Root Mean Squared Speed Error 4 phase cycle (km/h) | **:** | x.xx |
| Description of the accepted deviation of the driving cycle | **:** | Fully operated acceleration pedal |

**2.2.1. Pollutant emissions of vehicle with at least one combustion engine, of NOVC-HEVs and of OVC-HEVs in case of a charge-sustainingtest**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Pollutants* | *CO* | *THC (a)* | *NMHC (a)* | *NOx* | *THC+NOx (b)* | *Particulate Matter* | *Particle Number* |
| *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(mg/km)* | *(#.1011/km)* |
| Final values |  |  |  |  |  |  |  |
| Limit values |  |  |  |  |  |  |  |

**2.2.2. CO2 emission of vehicle with at least one combustion engine, of NOVC-HEV and of OVC-HEV in case of a charge-sustaining test**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *CO2 emission (g/km)* | *Low* | *Medium* | *High* | *Extra High* | *Combined* |
| Measured value MCO2,p,1 / MCO2,c,2 |  |  |  |  | - |
| Measured Speed and distance corrected value MCO2,p,2b / MCO2,c,2b |  |  |  |  |  |
| RCB correction coefficient (2) |  |  |  |  |  |
| MCO2,p,3 / MCO2,c,3 |  |  |  |  |  |

(2) correction as referred to in Appendix 2 to Annex B6 of this Regulation for ICE vehicles, and Appendix 2 to Annex B8 of this Regulation for HEVs (KCO2)

**2.3. Conclusion**

|  |  |
| --- | --- |
| *CO2 emission (g/km)* | *Combined* |
| ATCT (14°C) MCO2,Treg |  |
| Type 1 (23°C) MCO2,23° |  |
| **Family correction factor (FCF)** |  |

**2.4. Temperature information of the reference vehicle after 23°C test**

|  |  |  |
| --- | --- | --- |
| Worst case approach with regards to vehicle insulation | : | yes/no (3) |
| Worst case approach vehicle cool down | : | yes/no (3) |
| ATCT family composed of a single Interpolation family | : | yes/no (3) |
| Engine coolant temperature at the end of soaking time (°C) | : |  |
| Average soak area temperature over the 3 last hours (°C) | : |  |
| Difference between engine coolant end temperature and average soak area temperature of the last 3 hours ∆T\_ATCT (°C) | : |  |
| The minimum soaking time tsoak\_ATCT (s) | : |  |
| Location of temperature sensor | : |  |
| Measured engine temperature | : | oil/coolant |

(3) if “yes” then the six last lines are not applicable

Appendix 2

WLTP Road Load Test Report

**Road Load Test Report**

The following information, if applicable, is the minimum data required for the road load determination test.

**Report number**

|  |  |  |  |
| --- | --- | --- | --- |
| **APPLICANT** |  | | |
| **Manufacturer** |  | | |
| **SUBJECT** | Determination of a vehicle road load /… | | |
| **Roadload family identifier(s)** | | **:** |  |
| **Object submitted to tests** | | | |
|  | Make | **:** |  |
|  | Type | **:** |  |
| **CONCLUSION** | The object submitted to tests complies with the requirements mentioned in the subject. | | |

|  |  |
| --- | --- |
| place, | DD/MM/YYYY |

**1. Concerned vehicle(s)**

|  |  |  |
| --- | --- | --- |
| Make(s) concerned | : |  |
| Type(s) concerned | : |  |
| Commercial description | : |  |
| Maximal speed (km/h) | : |  |
| Powered axle(s) | : |  |

**2. Description of tested vehicles**

If no interpolation: the worst-case vehicle (regarding energy demand) shall be described

**2.1. Wind tunnel method**

|  |  |  |
| --- | --- | --- |
| Combination with | : | Flat belt dynamometer / chassis dynamometer |

**2.1.1. General**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Wind tunnel** | | **Dynamometer** | |
|  | **HR** | **LR** | **HR** | **LR** |
| Make |  |  |  |  |
| Type |  |  |  |  |
| Version |  |  |  |  |
| Cycle energy demand over a complete WLTC Class 3 cycle (kJ) |  |  |  |  |
| Deviation from production series | - | - |  |  |
| Mileage (km) | - | - |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Version | : |  |
| Cycle energy demand over a complete WLTC (kJ) | : |  |
| Deviation from production series | : |  |
| Mileage (km) | : |  |

**2.1.2. Masses**

|  |  |  |
| --- | --- | --- |
|  | **Dynamometer** | |
|  | **HR** | **LR** |
| Test mass (kg) |  |  |
| Average mass mav (kg) |  |  |
| Value of mr (kg per axle) |  |  |
| Category M vehicle:  proportion of the vehicle mass in running order on the front axle (%) |  |  |
| Category N vehicle:  weight distribution (kg or %) |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Test mass (kg) | : |  |
| Average mass mav(kg) | : | (average before and after the test) |
| Technically permissible maximum laden mass | : |  |
| Estimated arithmetic average of the mass of optional equipment | : |  |
| Category M vehicle:  proportion of the vehicle mass in running order on the front axle (%) | : |  |
| Category N vehicle:  weight distribution (kg or %) | : |  |

**2.1.3. Tyres**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Wind tunnel** | | **Dynamometer** | |
|  | **HR** | **LR** | **HR** | **LR** |
| Size designation |  |  |  |  |
| Make |  |  |  |  |
| Type |  |  |  |  |
| Rolling resistance | | | | |
| Front (kg/t) | **-** | **-** |  |  |
| Rear (kg/t) | **-** | **-** |  |  |
| Tyre pressure | | | | |
| Front (kPa) | **-** | **-** |  |  |
| Rear (kPa) | **-** | **-** |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Size designation | | |
| Make | **:** |  |
| Type | **:** |  |
| Rolling resistance | | |
| Front (kg/t) | **:** |  |
| Rear (kg/t) | **:** |  |
| Tyre pressure | | |
| Front (kPa) | **:** |  |
| Rear (kPa) | **:** |  |

**2.1.4. Bodywork**

|  |  |  |
| --- | --- | --- |
|  | **Wind tunnel** | |
|  | **HR** | **LR** |
| Type | AA/AB/AC/AD/AE/AF BA/BB/BC/BD |  |
| Version |  |  |
| Aerodynamic devices | | |
| Movable aerodynamic body parts | y/n and list if applicable |  |
| Installed aerodynamic options list |  |  |
| Delta (CD × Af)LH compared to HR (m2) | - |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Body shape description | : | Square box (if no representative body shape for a complete vehicle can be determined) |
| Frontal area Afr (m²) | : |  |

**2.2. On road**

**2.2.1. General**

|  |  |  |
| --- | --- | --- |
|  | **HR** | **LR** |
| Make |  |  |
| Type |  |  |
| Version |  |  |
| Cycle energy demand over a complete WLTC Class 3 cycle (kJ) |  |  |
| Deviation from production series |  |  |
| Mileage |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Make | : |  |
| Type | : |  |
| Version | : |  |
| Cycle energy demand over a complete WLTC (kJ) | : |  |
| Deviation from production series | : |  |
| Mileage (km) | : |  |

**2.2.2. Masses**

|  |  |  |
| --- | --- | --- |
|  | **HR** | **LR** |
| Test mass (kg) |  |  |
| Average mass mav(kg) |  |  |
| Value of mr (kg per axle) |  |  |
| Category M vehicle:  proportion of the vehicle mass in running order on the front axle (%) |  |  |
| Category N vehicle:  weight distribution (kg or %) |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Test mass (kg) | : |  |
| Average mass mav(kg) | : | (average before and after the test) |
| Technically permissible maximum laden mass | : |  |
| Estimated arithmetic average of the mass of optional equipment | : |  |
| Category M vehicle:  proportion of the vehicle mass in running order on the front axle (%) |  |  |
| Category N vehicle:  weight distribution (kg or %) |  |  |

**2.2.3. Tyres**

|  |  |  |
| --- | --- | --- |
|  | **HR** | **LR** |
| Size designation |  |  |
| Make |  |  |
| Type |  |  |
| Rolling resistance | | |
| Front (kg/t) |  |  |
| Rear (kg/t) |  |  |
| Tyre pressure | | |
| Front (kPa) |  |  |
| Rear (kPa) |  |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Size designation | **:** |  |
| Make | **:** |  |
| Type | **:** |  |
| Rolling resistance | | |
| Front (kg/t) | **:** |  |
| Rear (kg/t) | **:** |  |
| Tyre pressure | | |
| Front (kPa) | **:** |  |
| Rear (kPa) | **:** |  |

**2.2.4. Bodywork**

|  |  |  |
| --- | --- | --- |
|  | **HR** | **LR** |
| Type | AA/AB/AC/AD/AE/AF BA/BB/BC/BD |  |
| Version |  |  |
| Aerodynamic devices | | |
| Movable aerodynamic body parts | y/n and list if applicable |  |
| Installed aerodynamic options list |  |  |
| Delta (CD ×Af)LH compared to HR (m2) | - |  |

**Or (in case of roadload matrix family):**

|  |  |  |
| --- | --- | --- |
| Body shape description | : | Square box (if no representative body shape for a complete vehicle can be determined) |
| Frontal area Afr (m²) | : |  |

**2.3. Powertrain**

**2.3.1. Vehicle High**

|  |  |  |
| --- | --- | --- |
| Engine code | : |  |
| Transmission type | : | manual, automatic, CVT |
| Transmission model  (manufacturer's codes) | : | (torque rating and no of clutches 🡪 to be included in info doc) |
| Covered transmission models  (manufacturer's codes) | : |  |
| Engine rotational speed divided by vehicle speed | : | |  |  |  | | --- | --- | --- | | Gear | Gear ratio | N/V ratio | | 1st | 1/.. |  | | 2nd | 1.. |  | | 3rd | 1/.. |  | | 4th | 1/.. |  | | 5th | 1/.. |  | | 6th | 1/.. |  | | .. |  |  | | .. |  |  | |
| Electric machine(s) coupled in position N | : | n.a. (no electric machine or no coastdown mode) |
| Type and number of electric machines | : | construction type: asynchronous/ synchronous… |
| Type of coolant | : | air, liquid, … |

**2.3.2. Vehicle Low**

Repeat paragraph 2.3.1. with VL data

**2.4. Test results**

**2.4.1. Vehicle High**

|  |  |  |
| --- | --- | --- |
| Dates of tests | : | dd/mm/yyyy (wind tunnel)  dd/mm/yyyy (dynamometer)  or  dd/mm/yyyy (on road) |

**On road**

|  |  |  |
| --- | --- | --- |
| Method of the test | : | coastdown  or torque meter method |
| Facility (name / location / track's reference) | : |  |
| Coastdown mode | : | y/n |
| Wheel alignment | : | Toe and camber values |
| Ground clearance | : |  |
| Vehicle height | : |  |
| Drivetrain lubricants | : |  |
| Wheel bearing lubricants | : |  |
| Brake adjustment to avoid unrepresentative parasitic drag | : |  |
| Maximum reference speed (km/h) | : |  |
| Anemometry | : | stationary  or on board: influence of anemometry (CD × A) and if it was corrected. |
| Number of split(s) | : |  |
| Wind | : | average, peaks and direction in conjunction with direction of the test track |
| Air pressure | : |  |
| Temperature (mean value) | : |  |
| Wind correction | : | y/n |
| Tyre pressure adjustment | : | y/n |
| Raw results | : | Torque method:  c0 =  c1 =  c2 =  Coastdown method:  f0  f1  f2 |
| Final results |  | Torque method:  c0 =  c1 =  c2 =  and  f0 =  f1 =  f2 =  Coastdown method:  f0 =  f1 =  f2 = |

**Or**

**Wind tunnel method**

|  |  |  |
| --- | --- | --- |
| Facility (name/location/dynamometer's reference) | : |  |
| Qualification of the facilities | : | Report reference and date |
| Dynamometer | | |
| Type of dynamometer | : | flat belt or chassis dynamometer |
| Method | : | stabilised speeds or deceleration method |
| Warm up | : | warm-up by dyno or by driving the vehicle |
| Correction of the roller curve | : | (for chassis dynamometer, if applicable) |
| Method of chassis dynamometer setting | : | Fixed run / iterative / alternative with its own warmup cycle |
| Measured aerodynamic drag coefficient multiplied by the frontal area | : | |  |  | | --- | --- | | Velocity (km/h) | CD × A (m²) | | … | … | | … | … | |
| Result | : | f0 =  f1 =  f2 = |

**Or**

**Road load matrix on road**

|  |  |  |
| --- | --- | --- |
| Method of the test | : | coastdown  or torque meter method |
| Facility (name/location/track's reference) | : |  |
| Coastdown mode | : | y/n |
| Wheel alignment | : | Toe and camber values |
| Ground clearance | : |  |
| Vehicle height | : |  |
| Drivetrain lubricants | : |  |
| Wheel bearing lubricants | : |  |
| Brake adjustment to avoid unrepresentative parasitic drag | : |  |
| Maximum reference speed (km/h) | : |  |
| Anemometry | : | stationary  or on board: influence of anemometry (CD × A) and if it was corrected. |
| Number of split(s) | : |  |
| Wind | : | average, peaks and direction in conjunction with direction of the test track |
| Air pressure | : |  |
| Temperature (mean value) | : |  |
| Wind correction | : | y/n |
| Tyre pressure adjustment | : | y/n |
| Raw results | : | Torque method:  c0r =  c1r =  c2r =  Coastdown method:  f0r =  f1r =  f2r = |
| Final results |  | Torque method:  c0r =  c1r =  c2r =  and  f0r (calculated for vehicle HM) =  f2r (calculated for vehicle HM) =  f0r (calculated for vehicle LM) =  f2r (calculated for vehicle LM) =  Coastdown method:  f0r (calculated for vehicle HM) =  f2r (calculated for vehicle HM) =  f0r (calculated for vehicle LM) =  f2r (calculated for vehicle LM) = |

**Or**

**Road load matrix wind tunnel method**

|  |  |  |
| --- | --- | --- |
| Facility (name/location/dynamometer's reference) | : |  |
| Qualification of the facilities | : | Report reference and date |
| Dynamometer | | |
| Type of dynamometer | : | flat belt or chassis dynamometer |
| Method | : | stabilised speeds or deceleration method |
| Warm up | : | warm-up by dyno or by driving the vehicle |
| Correction of the roller curve | : | (for chassis dynamometer, if applicable) |
| Method of chassis dynamometer setting | : | Fixed run / iterative / alternative with its own warmup cycle |
| Measured aerodynamic drag coefficient multiplied by the frontal area | : | |  |  | | --- | --- | | Velocity (km/h) | CD × A (m²) | | … | … | | … | … | |
| Result | : | f0r =  f1r =  f2r =  f0r (calculated for vehicle HM) =  f2r (calculated for vehicle HM) =  f0r (calculated for vehicle LM) =  f2r (calculated for vehicle LM) = |

**2.4.2. Vehicle Low**

Repeat paragraph 2.4.1. with VL data

Appendix 3

WLTP Test Sheet

**Template for Test Sheet**

The test sheet shall include the test data that are recorded, but not included in any test report.

The test sheet(s) shall be retained by the technical service or the manufacturer for at least 10 years.

The following information, if applicable, is the minimum data required for test sheets.

|  |  |  |
| --- | --- | --- |
| **Information from Annex B4 to this Regulation** | | |
| Adjustable wheel alignment parameters | : |  |
| Ground clearance | : |  |
| Vehicle height | : |  |
| Drivetrain lubricants | : |  |
| Wheel bearing lubricants | : |  |
| Brake adjustment to avoid unrepresentative parasitic drag | : |  |
| The coefficients, c0, c1 and c2,  The coastdown times measured on the chassis dynamometer | :  : | c0 =  c1 =  c2 =   |  |  | | --- | --- | | Reference speed (km/h) | Coastdown time (s) | | 130 |  | | 120 |  | | 110 |  | | 100 |  | | 90 |  | | 80 |  | | 70 |  | | 60 |  | | 50 |  | | 40 |  | | 30 |  | | 20 |  | |
| Additional weight may be placed on or in the vehicle to eliminate tyre slippage | : | weight (kg)  on/in the vehicle |
| The coastdown times after performing the vehicle coast down procedure | : | |  |  | | --- | --- | | Reference speed (km/h) | Coastdown time (s) | | 130 |  | | 120 |  | | 110 |  | | 100 |  | | 90 |  | | 80 |  | | 70 |  | | 60 |  | | 50 |  | | 40 |  | | 30 |  | | 20 |  | |
| **Information from Annex B5 to this Regulation** | | |
| **NOx converter efficiency**  Indicated concentrations (a); (b), (c), (d), and the concentration when the NOx analyser is in the NO mode so that the calibration gas does not pass through the converter | : | (a) =  (b) =  (c) =  (d) =  Concentration in NO mode = |
| **Information from Annex B6 to this Regulation** | | |
| The distance actually driven by the vehicle | : |  |
| For manual shift transmission vehicle, MT vehicle that cannot follow the cycle trace:  The deviations from the driving cycle | : |  |
| **Drive trace indices**:  The following indices shall be calculated in accordance with the standard SAE J2951(Revised Jan-2014):  IWR : Inertial Work Rating 4 phase cycle  IWR: Inertial Work Rating 3 phase cycle  RMSSE : Root Mean Squared Speed Error 4 phase cycle  RMSSE : Root Mean Squared Speed Error 3 phase cycle | :  :  :  :  :  : |  |
| **Particulate sample filter weighing**  Filter for phases 1-4 before the test where applicable  Filter for phases 1-3 before the test where applicable Filter for phase 4 before the test where applicable  Filter for phases 1-4 after the test where applicable  Filter for phases 1-3 after the test where applicable  Filter for phase 4 after the test where applicable Reference filter | :  :  : |  |
| Content of each of the compounds measured after stabilization of the measuring device | : |  |
| **Regeneration factor determination**  The number of cycles D between two WLTCs where regeneration events occur  The number of cycles over which emission measurements are made n  The mass emissions measurement for each compound i over each cycle j | :  :  : |  |
| **Regeneration factor determination**  The number of applicable test cycles measured for complete regeneration | : |  |
| **Regeneration factor determination**  Msi  Mpi  Ki | :  :  : |  |
| **Information from Annex B6a to this Regulation** | | |
| **ATCT**  The air temperature and humidity of the test cell measured at the vehicle cooling fan outlet at a minimum frequency of 0.1 Hz. |  | Temperature set point = Treg  Actual temperature value  ± 3 °C at the start of the test  ± 5 °C during the test |
| The temperature of the soak area measured continuously at a minimum frequency of 0.033 Hz. | : | Temperature set point = Treg  Actual temperature value  ± 3 °C at the start of the test  ± 5 °C during the test |
| The time of transfer from the preconditioning to the soak area | : | ≤ 10 minutes |
| The time between the end of the Type 1 test and the cool down procedure  The measured soaking time, and shall be recorded in all relevant test sheets. | :  : | ≤ 20 minutes  time between the measurement of the end temperature and the end of the Type 1 test at 23 °C |
| **Information from Annex C3 to this Regulation** | | |
| **Diurnal testing**  Ambient temperature during the two diurnal cycles (recorded at least every minute) | : |  |
| **Carbon canister puff loss loading**  Ambient temperature during the first 11-hour profile (recorded at least every 10 minutes) | : |  |

Appendix 4

Evaporative Emissions Test Report

The following information, if applicable, is the minimum data required for the evaporative emission test.

**Report number**

|  |  |  |  |
| --- | --- | --- | --- |
| **APPLICANT** |  | | |
| **Manufacturer** |  | | |
| **SUBJECT** | … | | |
| **Evaporative family identifier** | | **:** |  |
| **Object submitted to tests** | | | |
|  | Make | **:** |  |
| **CONCLUSION** | The object submitted to tests complies with the requirements mentioned in the subject. | | |

|  |  |
| --- | --- |
| place, | DD/MM/YYYY |

Every Technical Service is free to include additional information

**1. Description of tested vehicle high**

|  |  |  |
| --- | --- | --- |
| Vehicle numbers | **:** | Prototype number and VIN |
| Category | **:** |  |

**1.1. Powertrain architecture**

|  |  |  |
| --- | --- | --- |
| Powertrain architecture | **:** | internal combustion, hybrid, electric or fuel cell |

**1.2. Internal combustion engine**

For more than one ICE, please repeat the point

|  |  |  |
| --- | --- | --- |
| Make | **:** |  |
| Type | **:** |  |
| Working principle | **:** | two/four stroke |
| Cylinders number and arrangement | **:** |  |
| Engine capacity (cm3) | **:** |  |
| Supercharging | **:** | yes/no |
| Direct injection | **:** | yes/no or description |
| Vehicle fuel type | **:** | Monofuel / bifuel / flex fuel |
| Engine lubricant | **:** | Make and type |
| Cooling system | **:** | Type: air/water/oil |

**1.4. Fuel system**

|  |  |  |
| --- | --- | --- |
| Injection pump | **:** |  |
| Injector(s) | **:** |  |
| Fuel tank | | |
| Layer(s) | **:** | monolayer/ multilayer |
| Material for the fuel tank | **:** | metal / … |
| Material for other parts of the fuel system | **:** | … |
| Sealed | **:** | yes/no |
| Nominal tank capacity (l) | **:** |  |
| Carbon canister | | |
| Make and type | **:** |  |
| Type of activated carbon | **:** |  |
| Volume of charcoal (l) | **:** |  |
| Mass of charcoal (g) | **:** |  |
| Declared BWC (g) | **:** | xx.x |

**2. Test results**

**2.1. Carbon canister bench ageing**

|  |  |  |
| --- | --- | --- |
| Date of tests | **:** | (day/month/year) |
| Place of the test | **:** |  |
| Carbon canister ageing test report | **:** |  |
| Loading rate | **:** |  |
| Fuel specification | | |
| Make | **:** |  |
| Type | **:** | name of reference fuel… |
| Density at 15°C (kg/m3) | **:** |  |
| Ethanol content (%) | **:** |  |
| Batch number | **:** |  |

**2.2. Determination of the permeability factor (PF)**

|  |  |  |
| --- | --- | --- |
| Date of tests | **:** | (day/month/year) |
| Place of the test | **:** |  |
| Permeability factor test report | **:** |  |
| HC measured at week 3, HC3W (mg/24h) | **:** | xxx |
| HC measured at week 20, HC20W (mg/24h) | **:** | xxx |
| Permeability Factor, PF (mg/24h) | **:** | xxx |

In case of multilayer tanks or metal tanks

|  |  |  |
| --- | --- | --- |
| Alternative Permeability Factor, PF (mg/24h) | **:** | yes/no |

**2.3. Evaporative test**

|  |  |  |
| --- | --- | --- |
| Date of tests | **:** | (day/month/year) |
| Place of the test | **:** |  |
| Method of chassis dyno setting | **:** | Fixed run / iterative / alternative with its own warmup cycle |
| Dynamometer operation mode |  | yes/no |
| Coastdown mode | **:** | yes/no |

**2.3.1. Mass**

|  |  |  |
| --- | --- | --- |
| Test mass of VH (kg) | **:** |  |

**2.3.2. Roadload parameters**

|  |  |  |
| --- | --- | --- |
| f0 (N) | **:** |  |
| f1 (N/(km/h)) | **:** |  |
| f2 (N/(km/h)²) | **:** |  |

**2.3.3. Cycle and Gear shift point (if applicable)**

|  |  |  |
| --- | --- | --- |
| Cycle (without downscaling) | **:** | Class 1 / 2 / 3 |
| Gear shifting | **:** | Average gear for v ≥ 1 km/h, rounded to four places of decimal |

**2.3.4. Vehicle**

|  |  |  |
| --- | --- | --- |
| Tested vehicle | **:** | VH or description |
| Mileage (km) | **:** |  |
| Age (weeks) | **:** |  |

**2.3.5. Procedure of test and results**

|  |  |  |
| --- | --- | --- |
| Test procedure | **:** | Continuous (sealed fuel tank systems) / Continuous (non-sealed fuel tank systems) /  Stand –alone (sealed fuel tank systems) |
| Description of soak periods (time and temperature) | **:** |  |
| Puff loss loading value (g) | **:** | xx.x (if applicable) |

|  |  |  |  |
| --- | --- | --- | --- |
| **Evaporative test** | hot soak,  MHS | 1st 24h diurnal, MD1 | 2nd 24h diurnal, MD2 |
| Mean temperature (°C) |  | - | - |
| Evaporative emission (g/test) | x.xxx | x.xxx | x.xxx |
| Final result, MHS+MD1+MD2+(2xPF) (g/test) | x.xx | | |


**2.3.6. Demonstrated procedures for alternative conformity of production testing where applicable:**

|  |  |  |
| --- | --- | --- |
| Test for leakage | : | Alternative pressures and/or time or alternative test procedure |
| Test for venting | : | Alternative pressure and/or time or alternative test procedure |
| Purge test | : | Alternative flow rate or test procedure |
| Sealed tank | : | Alternative test procedure |

Annex A2

**Communication**

(maximum format: A4 (210 x 297 mm))



[[4]](#footnote-5)

Concerning:[[5]](#footnote-6) Approval granted

Approval extended

Approval refused

Approval withdrawn

Production definitively discontinued

of a vehicle type with regard to the emission of gaseous pollutants by the engine pursuant to UN Regulation No. WLTP

Approval No. ……….................................. Reason for extension :……………………

Section I

0.1. Make (trade name of manufacturer):

0.2. Type:

0.2.1. Commercial name(s) (if available):

0.3. Means of identification of type if marked on the vehicle[[6]](#footnote-7)

0.3.1. Location of that marking:

0.4. Category of vehicle:[[7]](#footnote-8)

0.5. Name and address of manufacturer:

0.8. Name(s) and address(es) of assembly plant(s):

0.9. If applicable, name and address of manufacturer's representative:

1.0. Remarks: …

Section II

1. Additional information (where applicable): (see addendum)

2. Technical Service responsible for carrying out the tests:

3. Date of Type 1 test report:

4. Number of Type 1 test report:

5. Remarks (if any): (see Section 3 of addendum)

6. Place:

7. Date:

8. Signature:

Attachments: 1. Information package.

2. Test reports.

Addendum to type approval communication No … concerning the type approval of a vehicle with regard to exhaust emissions pursuant to the 01 series of amendments to UN Regulation No. 154

**0. INTERPOLATION FAMILY IDENTIFIER AS DEFINED IN PARAGRAPH 5. OF UN REGULATION NO. 154**

0.1. Identifier: …

0.2. Base vehicle identifier (5a) (1): …

**1. ADDITIONAL INFORMATION**

1.1. Mass of the vehicle in running order:

VL (1): …

VH: …

1.2. Maximum mass:

VL (1): …

VH: …

1.3. Reference mass:

VL (1): …

VH: …

1.4. Number of seats: …

1.6. Type of bodywork:

1.6.1. for M1, M2: saloon, hatchback, station wagon, coupé, convertible, multipurpose vehicle(a)

1.6.2. for N1, N2: lorry, van(a)

1.7. Drive wheels: front, rear, 4 × 4(a)

1.8. Pure electric vehicle: yes/no(a)

1.9. Hybrid electric vehicle: yes/no(a)

1.9.1. Category of Hybrid Electric vehicle: Off Vehicle Charging/Not Off Vehicle charging / Off Vehicle Charging Fuel Cell / Not Off Vehicle Charging Fuel Cell (as applicable) (a)

1.9.2. Operating mode switch: with/without(a)

1.10. Engine identification:

1.10.1. Engine capacity/displacement (as applicable)

1.10.1.1. Reciprocating engine:

1.10.1.2. Wankel engine

1.10.1.2.1. Capacity:

1.10.1.2.2. Displacement:

1.10.2. Fuel supply system: direct injection/indirect injection(a)

1.10.3. Fuel recommended by the manufacturer:

1.10.4.1. Maximum power: kW at min–1

1.10.4.2. Maximum torque: Nm at min–1

1.10.5. Pressure charging device: yes/no(a)

1.10.6. Ignition system: compression ignition/positive ignition(a)

1.11. Powertrain (for pure electric vehicle or hybrid electric vehicle) (a)

1.11.1. Maximum net power: … kW, at: … to … min–1

1.11.2. Maximum thirty minutes power: … kW

1.11.3. Maximum net torque: … Nm, at … min–1

1.12. Traction battery (for pure electric vehicle or hybrid electric vehicle)

1.12.1. Nominal voltage: V

1.12.2. Capacity (2 h rate): Ah

1.13. Transmission: …, …

1.13.1. Type of gearbox: manual/automatic/variable transmission(a)

1.13.2. Number of gear ratios:

1.13.3. Total gear ratios (including the rolling circumferences of the tyres under load): (vehicle speed (km/h)) / (engine speed (1000 (min–1))

|  |  |
| --- | --- |
| First gear: … | Sixth gear: … |
| Second gear: … | Seventh gear: … |
| Third gear: … | Eighth gear: … |
| Fourth gear: … | Overdrive: … |
| Fifth gear: … |  |

1.13.4. Final drive ratio:

1.14. Tyres: …, …, …

Type: radial/bias/…[[8]](#footnote-9)

Dimensions: …

Rolling circumference under load:

Rolling circumference of tyres used for the Type 1 test

**2. TEST RESULTS**

**2.1. Tailpipe emissions test results**

Emissions classification: …

Type 1 test results, where applicable

Type approval number if not parent vehicle (1): …

**Test 1a 4 phase test**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Type 1 Result* | *CO*  *(mg/km)* | *THC*  *(mg/km)* | *NMHC*  *(mg/km)* | *NOx*  *(mg/km)* | *THC + NOx*  *(mg/km)* | *PM*  *(mg/km)* | *PN*  *(#.1011/km)* |
| Measured (8) (9) |  |  |  |  |  |  |  |
| Ki × (8) (10) |  |  |  |  | (11) |  |  |
| Ki + (8) (10) |  |  |  |  | (11) |  |  |
| Mean value calculated with Ki (M × Ki or M + Ki) (9) |  |  |  |  | (12) |  |  |
| DF (+) (8) (10a) |  |  |  |  |  |  |  |
| DF (×) (8) (10a) |  |  |  |  |  |  |  |
| Final mean value calculated with Ki and DF (13) |  |  |  |  |  |  |  |
| Limit value |  |  |  |  |  |  |  |

**Test 1b 3 phase test**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Type 1 Result* | *CO*  *(mg/km)* | *THC*  *(mg/km)* | *NMHC*  *(mg/km)* | *NOx*  *(mg/km)* | *PM*  *(mg/km)* | *PN*  *(#.1011/km)* |
| Measured (8) (9) |  |  |  |  |  |  |
| Ki × (8) (10) |  |  |  |  |  |  |
| Ki + (8) (10) |  |  |  |  |  |  |
| Mean value calculated with Ki (M × Ki or M + Ki) (9) |  |  |  |  |  |  |
| DF (+) (8) (10a) |  |  |  |  |  |  |
| DF (×) (8) (10a) |  |  |  |  |  |  |
| Final mean value calculated with Ki and DF (13) |  |  |  |  |  |  |
| Limit value |  |  |  |  |  |  |

**Test 2a and 2b (if applicable)**

Repeat Test 1a and 1b tables with the second test results.

**Test 3a and 3b (if applicable)**

Repeat Test 1a and 1b tables with the third test results.

Repeat Test 1a, 1b, test 2a, 2b (if applicable) and test 3a, 3b (if applicable) for Vehicle Low (if applicable), and VM (if applicable)

**ATCT test**

|  |  |
| --- | --- |
| *CO2 Emission (g/km)* | *Combined* |
| ATCT (14 °C) MCO2,Treg |  |
| Type 1 (23 °C) MCO2,23° |  |
| Family correction factor (FCF) |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *ATCT test Result* | *CO*  *(mg/km)* | *THC*  *(mg/km)* | *NMHC*  *(mg/km)* | *NOx*  *(mg/km)* | *THC + NOx*  *(mg/km)* | *PM*  *(mg/km)* | *PN*  *(#.1011/km)* |
| Measured[[9]](#footnote-10), [[10]](#footnote-11) |  |  |  |  |  |  |  |
| Limit values |  |  |  |  |  |  |  |

Difference between engine coolant end temperature and average soak area temperature of the last 3 hours ΔT\_ATCT (°C) for the reference vehicle: …

The minimum soaking time tsoak\_ATCT (s): …

Location of temperature sensor: …

ATCT family identifier: …

Type 4: … g/test;

Test procedure in accordance with: Annex C3 to UN Regulation No. 154 (1).

Type 5:

1. Durability test: whole vehicle test/bench ageing test/none (1)
2. Deterioration factor DF: calculated/assigned (1)
3. Specify the values: …
4. Applicable Type 1 cycle (Annex B4 to UN Regulation No. 154 (14): …

2.1.1. For bi fuel vehicles, the type 1 table shall be repeated for both fuels. For flex fuel vehicles, when the type 1 test is to be performed on both fuels according to Table A in paragraph 6. of UN Regulation No. 154, and for vehicles running on LPG or NG/Biomethane, either mono fuel or bi fuel, the table shall be repeated for the different reference gases used in the test, and an additional table shall display the worst results obtained.

2.1.2. Written description and/or drawing of the MI: …

2.1.3. List and function of all components monitored by the OBD system: …

2.1.4. Written description (general working principles) for: …

2.1.4.1. Misfire detection[[11]](#footnote-12): …

2.1.4.2. Catalyst monitoring8: …

2.1.4.3. Oxygen sensor monitoring8: …

2.1.4.4. Other components monitored by the OBD system8: …

2.1.4.5. Catalyst monitoring[[12]](#footnote-13): …

2.1.4.6. Particulate trap monitoring9: …

2.1.4.7. Electronic fuelling system actuator monitoring9: …

2.1.4.8. Other components monitored by the OBD system: …

2.1.5. Criteria for MI activation (fixed number of driving cycles or statistical method): …

2.1.6. List of all OBD output codes and formats used (with explanation of each): …

**2.2. Reserved**

**2.3. Catalytic converters yes/no(a)**

2.3.1. Original equipment catalytic converter tested to all relevant requirements of this Regulation yes/no(a)

**2.5. CO2 emissions and fuel consumption test results**

2.5.1. Pure ICE vehicle and Not Externally Chargeable (NOVC) Hybrid Electric Vehicle

2.5.1.0. Minimum and maximum CO2 values within the interpolation family: …

2.5.1.1. Vehicle High

2.5.1.1.1. Cycle Energy Demand

2.5.1.1.1.1. 4 phase cycle:… J

2.5.1.1.1.2. 3 phase cycle:… J2.5.1.1.2. Road load coefficients

2.5.1.1.2.1. f0, N: …

2.5.1.1.2.2. f1, N/(km/h): …

2.5.1.1.2.3. f2, N/(km/h)2: …

2.5.1.1.3. CO2 mass emissions (provide values for each reference fuel tested, for the phases: the measured values, for the combined see points 1.2.3.8. and 1.2.3.9. of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5 / MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| average |  |  |  |  |  |
| Final MCO2,p,H / MCO2,c,H | |  |  |  |  |  |

2.5.1.1.4. Fuel consumption (provide values for each reference fuel tested, for the phases: the measured values for the combined see paragraphs 1.2.3.8 and 1.2.3.9 of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1) (as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,H/FCc,H |  |  |  |  |  | - |
| Final values FEp,H, FEc,H |  |  |  | - | - |  |

2.5.1.2. Vehicle Low (if applicable)

2.5.1.2.1. Cycle Energy Demand

2.5.1.2.1.1. 4 phase cycle: … J

2.5.1.2.1.2. 3 phase cycle: … J

2.5.1.2.2. Road load coefficients

2.5.1.2.2.1. f0, N: …

2.5.1.2.2.2. f1, N/(km/h): …

2.5.1.2.2.3. f2, N/(km/h) (2): …

2.5.1.2.3. CO2 mass emissions (provide values for each reference fuel tested, for the phases: the measured values for the combined see points 1.2.3.8. and.1.2.3.9. of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5/MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| average |  |  |  |  |  |
| Final MCO2,p,L/MCO2,c,L | |  |  |  |  |  |

2.5.1.2.4. Fuel consumption (provide values for each reference fuel tested, for the phases: the measured values for the combined see paragraphs 1.2.3.8. and 1.2.3.9. of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1)**(as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,L/FCc,L |  |  |  |  |  | - |
| Final values FEp,L, FEc,L |  |  |  | - | - |  |

2.5.1.3. Vehicle M for NOVC-HEV (if applicable)

2.5.1.3.1. Cycle Energy Demand

2.5.1.3.1.1. 4 phase cycle: … J

2.5.1.3.1.2. 3 phase cycle: … J

2.5.1.3.2. Road load coefficients

2.5.1.3.2.1. f0, N: …

2.5.1.3.2.2. f1, N/(km/h): …

2.5.1.3.2.3. f2, N/(km/h) (2): …

2.5.1.3.3. CO2 mass emissions (provide values for each reference fuel tested, for the phases: the measured values for the combined see paragraphs 1.2.3.8. and 1.2.3.9. of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5/MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| average |  |  |  |  |  |
| Final MCO2,p,L/MCO2,c,L | |  |  |  |  |  |

2.5.1.3.4. Fuel consumption (provide values for each reference fuel tested, for the phases: the measured values for the combined see paragraphs 1.2.3.8. and 1.2.3.9. of Annex B6 to UN Regulation No. 154)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1)**(as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,L / FCc,L |  |  |  |  |  | - |
| Final values FEp,L, FEc,L |  |  |  | - | - |  |

2.5.1.4. For vehicles powered by an internal combustion engine which are equipped with periodically regenerating systems as defined in paragraph 3.8.1. of UN Regulation No. 154, the test results shall be adjusted by the Ki factor as specified in Appendix 1 to Annex B6 of UN Regulation No. 154.

2.5.1.4.1. Information about regeneration strategy for CO2 emissions and fuel consumption

D — number of operating cycles between 2 cycles where regenerative phases occur: …

d — number of operating cycles required for regeneration: …

Applicable Type 1 cycle (Annex B4 to UN Regulation No. 154) (14): …

|  |  |  |
| --- | --- | --- |
|  | Combined  4 phase cycle | Combined  3 phase cycle |
| Ki (additive / multiplicative) (1)  Values for CO2 and fuel consumption (10) |  |  |

2.5.2. Pure electric vehicles[[13]](#footnote-14)

2.5.2.1. Electric energy consumption

2.5.2.1.1. Vehicle High

2.5.2.1.1.1. Cycle Energy Demand

2.5.2.1.1.1.1. 4 phase cycle: … J

2.5.2.1.1.1.2. 3 phase cycle: … J

2.5.2.1.1.2. Road load coefficients

2.5.2.1.1.2.1. f0, N: …

2.5.2.1.1.2.2. f1, N/(km/h): …

2.5.2.1.1.2.3. f2, N/(km/h) (2): …

|  |  |  |
| --- | --- | --- |
| EAC(Wh) | Test | |
| 1 |  |
| 2 |  |
| 3 |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Test* | *(as applicable)* | | | | | | |
| *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated EC | 1 |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |
| average |  |  |  |  |  |  |  |
| Declared value | | — | — | — | — | — |  |  |

2.5.2.1.1.3. Total time out of tolerance for the conduct of the cycle: … sec

2.5.2.1.2. Vehicle Low (if applicable)

2.5.2.1.2.1. Cycle Energy Demand

2.5.2.1.2.1.1. 4 phase cycle: … J

2.5.2.1.2.1.2. 3 phase cycle: … J

2.5.2.1.2.2. Road load coefficients

2.5.2.1.2.2.1. f0, N: …

2.5.2.1.2.2.2. f1, N/(km/h): …

2.5.2.1.2.2.3. f2, N/(km/h) (2): …

|  |  |  |
| --- | --- | --- |
| EAC(Wh) | Test | |
| 1 |  |
| 2 |  |
| 3 |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Test* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated EC | 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| average |  |  |  |
| Declared value | | — |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Calculated EC | 1 |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |
| average |  |  |  |  |  |  |  |
| Declared value | | — | — | — | — | — |  |  |

2.5.2.1.2.3. Total time out of tolerance for the conduct of the cycle: … sec

2.5.2.2. Pure Electric Range

2.5.2.2.1. Vehicle High

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *PER (km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Measured Pure Electric Range | 1 |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |
| average |  |  |  |  |  |  |  |
| Declared value | | — | — | — | — | — |  |  |

2.5.2.2.2. Vehicle Low (if applicable)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *PER (km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Measured Pure Electric Range | 1 |  |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |  |
| average |  |  |  |  |  |  |  |
| Declared value | | — | — | — | — | — |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | |  |  |

2.5.3. Externally chargeable (OVC) Hybrid Electric Vehicle and Fuel Cell Hybrid Vehicle (as applicable):

2.5.3.1. CO2 mass emission charge sustaining (only applicable for OVC-HEVs)

2.5.3.1.1. Vehicle High

2.5.3.1.1.1. Cycle Energy Demand

2.5.3.1.1.1.1. 4 phase cycle: … J

2.5.3.1.1.1.2. 3 phase cycle: … J

2.5.3.1.1.2. Road load coefficients

2.5.3.1.1.2.1. f0, N: …

2.5.3.1.1.2.2. f1, N/(km/h): …

2.5.3.1.1.2.3. f2, N/(km/h) (2): …

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5/MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| Average |  |  |  |  |  |
| Final MCO2,p,H/MCO2,c,H | |  |  |  |  |  |

2.5.3.1.2. Vehicle Low (if applicable)

2.5.3.1.2.1. Cycle Energy Demand

2.5.3.1.2.1.1. 4 phase cycle: … J

2.5.3.1.2.1.2. 3 phase cycle: … J

2.5.3.1.2.2. Road load coefficients

2.5.3.1.2.2.1. f0, N: …

2.5.3.1.2.2.2. f1, N/(km/h): …

2.5.3.1.2.2.3. f2, N/(km/h) (2): …

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5/MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| Average |  |  |  |  |  |
| Final MCO2,p,L/MCO2,c,L | |  |  |  |  |  |

2.5.3.1.3. Vehicle M (if applicable)

2.5.3.1.3.1. Cycle Energy Demand:

2.5.3.1.3.1.1. 4 phase cycle: … J

2.5.3.1.3.1.2. 3 phase cycle: … J

2.5.3.1.3.2. Road load coefficients

2.5.3.1.3.2.1. f0, N: …

2.5.3.1.3.2.2. f1, N/(km/h): …

2.5.3.1.3.2.3. f2, N/(km/h) (2): …

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Low* | *Medium* | *High* | *Extra High* | *Combined*  *4 phase cycle* |
| MCO2,p,5/MCO2,c,5 | 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| Average |  |  |  |  |  |
| MCO2,p,M/MCO2,c,M | |  |  |  |  |  |

2.5.3.2. CO2 mass emission charge-depleting (only applicable for OVC-HEVs)

Vehicle High

|  |  |  |
| --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Combined*  *4 phase cycle* |
| MCO2,CD | 1 |  |
| 2 |  |
| 3 |  |
| Average |  |
| Final MCO2,CD,H | |  |

Vehicle Low (if applicable)

|  |  |  |
| --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Combined*  *4 phase cycle* |
| MCO2,CD | 1 |  |
| 2 |  |
| 3 |  |
| Average |  |
| Final MCO2,CD,L | |  |

Vehicle M (if applicable)

|  |  |  |
| --- | --- | --- |
| *CO2 Emission (g/km)* | *Test* | *Combined*  *4 phase cycle* |
| MCO2,CD | 1 |  |
| 2 |  |
| 3 |  |
| Average |  |
| Final MCO2,CD,M | |  |

2.5.3.3. CO2 mass emission (weighted, combined) [[14]](#footnote-15) (only applicable for OVC-HEVs):

Vehicle High: MCO2,weighted … g/km

Vehicle Low (if applicable): MCO2,weighted … g/km

Vehicle M (if applicable): MCO2,weighted … g/km

2.5.3.3.1. Minimum and maximum CO2 values within the interpolation family.

2.5.3.4. Fuel consumption Charge-Sustaining

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Vehicle High* | | | | | | |
| *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1) (as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,H / FCc,H or FEp,H, FEc,H |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Vehicle Low (if applicable)* | | | | | | |
| *Fuel consumption (l/100 km) or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1) (as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,L / FCc,L or FEp,L, FEc,L |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Vehicle M (if applicable)* | | | | | | |
| *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1) or fuel efficiency (km/l or km/kg) (1) (as applicable)* | *Low* | *Medium* | *High* | *Extra High* | *Combined FC*  *4 phase cycle* | *Combined FE*  *3 phase cycle* |
| Final values FCp,M / FCc,M or FEp,M, FEc,M |  |  |  |  |  |  |

2.5.3.5. Fuel consumption Charge-Depleting

Vehicle High

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1)*  *Combined*  *4 phase cycle* | *Fuel efficiency (km/l) (1)*  *Combined*  *3 phase cycle* |
| Final values FCCD,H or FECD,H |  |  |

Vehicle Low (if applicable)

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1)*  *Combined*  *4 phase cycle* | *Fuel efficiency (km/l) (1)*  *Combined*  *3 phase cycle* |
| Final values FCCD,L or FECD,L |  |  |

Vehicle M (if applicable)

|  |  |  |
| --- | --- | --- |
|  | *Fuel consumption (l/100 km or m3/100 km or kg/100 km) (1)*  *Combined*  *4 phase cycle* | *Fuel efficiency (km/l) (1)*  *Combined*  *3 phase cycle* |
| Final values FCCD,M or FECD,M |  |  |

2.5.3.6. Fuel consumption (weighted, combined) [[15]](#footnote-16) for 4 phase cycle

Vehicle High: FCweighted … l/100 km or kg/100 km

Vehicle Low (if applicable): FCweighted … l/100 km or kg/100 km

Vehicle M (if applicable): FCweighted … l/100 km or kg/100 km

2.5.3.7. Ranges:

2.5.3.7.1. All Electric Range AER

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *AER (km)* | *Test* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| AER values | 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| Average |  |  |  |
| Final values AER | |  |  |  |

2.5.3.7.2. Equivalent All Electric Range EAER (where applicable)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *EAER (km)* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Measured\* |  |  |  |  |  |  |  |
| Final EAER values |  |  |  |  |  |  |  |

\* For 3-phase WLTP test, the arithmetic average for all individual charge-depleting tests

2.5.3.7.3. Actual Charge Depleting Range RCDA

|  |  |  |
| --- | --- | --- |
| *RCDA (km)* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| RCDA values |  |  |

2.5.3.7.4. Charge-Depleting Cycle Range RCDC

|  |  |  |  |
| --- | --- | --- | --- |
| *RCDC (km)* | *Test* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| RCDC values | 1 |  |  |
| 2 |  |  |
| 3 |  |  |
| Average |  |  |
| Final values RCDC | |  |  |

2.5.3.8. Electric energy consumption

2.5.3.8.1. Electric Energy Consumption EC

|  |  |
| --- | --- |
| EAC(Wh) |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *EC (Wh/km)* | *Low* | *Medium* | *High* | *Extra High* | *City* | *Combined*  *4 phase cycle* | *Combined*  *3 phase cycle* |
| Electric energy consumption values |  |  |  |  |  |  |  |

2.5.3.8.2. UF-weighted charge-depleting electric energy consumption ECAC,CD (combined)

|  |  |  |
| --- | --- | --- |
| *ECAC,CD (Wh/km)* | *Test* | *Combined*  *4 phase cycle* |
| ECAC,CD values | 1 |  |
| 2 |  |
| 3 |  |
| Average |  |
| Final values ECAC,CD | |  |

2.5.3.8.3. UF-weighted electric energy consumption ECAC, weighted (combined)

|  |  |  |
| --- | --- | --- |
| *ECAC,weighted (Wh/km)* | *Test* | *Combined*  *4 phase cycle* |
| ECAC,weighted values | 1 |  |
| 2 |  |
| 3 |  |
| Average |  |
| Final values ECAC,weighted | |  |

Repeat 2.5.3. in case of base vehicle.

2.5.4. Not Off Vehicle Charging Fuel Cell Hybrid Vehicles (NOVC-FCHV)

|  |  |  |
| --- | --- | --- |
|  | *Fuel Consumption (kg/100 km)*  *Combined*  *4 phase cycle* | *Fuel Efficiency (km/kg)*  *Combined*  *3 phase cycle* |
| Final values FCc or FEc |  |  |

Repeat 2.5.4. in case of base vehicle.

2.5.5. Device for monitoring the consumption of fuel and/or electric energy: yes/not applicable …

**3. Remarks: …**

**Explanatory Notes**

(4) If the means of identification of type contains characters not relevant to describe the vehicle, component or separate technical unit types covered by this information, such characters shall be represented in the documentation by the symbol ‘?’ (e.g. ABC??123??)

(5) (Reserved)

(5a) (Reserved)

(6) (Reserved)

(8) Where applicable.

(9) Round to 2 decimal places

(10) Round to 4 decimal places

(10a) Round to 3 decimal places

(11) Not applicable

(12) Mean value calculated by adding mean values (M.Ki) calculated for THC and NOx.

(13) Round to 1 decimal place more than limit value.

(14) Indicate the applicable procedure.

(22) Applicable Type 1 cycle: Annex B1 of UN Regulation No. 154

(23) If modelling is applied instead of the type 1 test-cycle, this value shall be the one provided by the modelling methodology.

(a) Delete where not applicable (there are cases where nothing needs to be deleted when more than one entry is applicable)

Annex A3

**Arrangements of the approval mark**

In the approval mark issued and affixed to a vehicle in conformity with paragraph 5. of this Regulation, the type approval number shall be accompanied by an alphanumeric character reflecting the level that the approval is limited to.

This annex outlines the appearance of this mark and gives an example how it shall be composed.

The following schematic graphic presents the general lay-out, proportions and contents of the marking. The meaning of numbers and alphabetical character are identified, and sources to determine the corresponding alternatives for each approval case are also referred.

Number of country[[16]](#footnote-17) Letter according to

granting the approval Approval Level

Number of Regulation (Regulation No. 154)

Series of amendments No.

Section 3 of Approval number

**a**

E11

154R – 012439 – 02

**a/2**

**a/3**

**a/3**

a = 8 mm (minimum)

The following graphic is a practical example of how the marking should be composed.

E11

154 R – 012439 – 1A

The preceding approval mark affixed to a vehicle in conformity with paragraph 5. of this Regulation shows that the vehicle type concerned has been approved in the United Kingdom (E 11), pursuant to Regulation 154 under approval number 2439, as defined in Section 3 of paragraph 5.2.1. This mark indicates that the approval was given in accordance with the requirements of this Regulation with the 01 series of amendments incorporated. Furthermore, the accompanying code (1A) denotes that the vehicle is approved to Level 1A (Europe).

The following graphic is a practical example of how the marking should be composed.

E2

154 R – 012439 – 1A

83 R – 089876 – ZA

The preceding approval mark affixed to a vehicle in conformity with paragraph 5. of this Regulation shows that the vehicle type concerned has been approved in France (E 2), pursuant to:

1. UN Regulation No. 83 under section 3 of approval number 9876. This mark indicates that the approval was given in accordance with the requirements of this Regulation with the 08 series of amendments incorporated. Furthermore, the accompanying code (ZA) denotes that the vehicle is approved under a certain level of requirements associated with the ZA character.
2. This Regulation under approval number 2439, as defined in Section 3 of paragraph 5.2.1. This mark indicates that the approval was given in accordance with the requirements of this Regulation with the 01 series of amendments incorporated. Furthermore, the accompanying code (1A) denotes that the vehicle is approved to Level 1A (Europe).

# Table A3/1

**Characters with reference to approval level**

|  |  |
| --- | --- |
| *Code* | *Contracting Party on which the requirements are based* |
| 1A | European Union |
| 1B | Japan |
| 02 | Harmonized |

Annexes Part B

The annexes in Annexes Part B describe the procedures for determining the levels of emissions of gaseous compounds, particulate matter, particle number, CO2 emissions, fuel consumption, fuel efficiency, electric energy consumption and electric range from light-duty vehicles.

Annex B1

Worldwide light-duty test cycles (WLTC)

1. General requirements

The cycle to be driven depends on the ratio of the test vehicle’s rated power to mass in running order minus 75 kg, W/kg, and its maximum velocity, (as defined in paragraph 3.7.2. of this Regulation).

The cycle resulting from the requirements described in this annex shall be referred to in other parts of this Regulation as the "applicable cycle".

2. Vehicle classifications

2.1. Class 1 vehicles have a power to mass in running order minus 75 kg ratio W/kg.

2.2. Class 2 vehicles have a power to mass in running order minus 75 kg ratio > 22 but ≤ 34 W/kg.

2.3. Class 3 vehicles have a power to mass in running order minus 75 kg ratio > 34 W/kg.

2.3.1. Class 3 vehicles are divided into 2 subclasses according to their maximum speed, vmax.

2.3.1.1. Class 3a vehicles with vmax < 120 km/h.

2.3.1.2. Class 3b vehicles with vmax ≥ 120 km/h.

2.3.2. All vehicles tested according to Annex B8 shall be considered to be Class 3 vehicles.

3. Test cycles

3.1. Class 1 cycle

3.1.1. A complete Class 1 cycle shall consist of a low phase (Low1), a medium phase (Medium1) and an additional low phase (Low1).

3.1.2. The Low1 phase is described in Figure A1/1 and Table A1/1.

3.1.3. The Medium1 phase is described in Figure A1/2 and Table A1/2.

3.2. Class 2 cycle

3.2.1. A complete Class 2 cycle shall consist of a low phase (Low2), a medium phase (Medium2), a high phase (High2) and an extra high phase (Extra High2).

A 3-phase Class 2 cycle shall consist of a low phase (Low2), a medium phase (Medium2) and a high phase (High2).

3.2.2. The Low2 phase is described in Figure A1/3 and Table A1/3.

3.2.3. The Medium2 phase is described in Figure A1/4 and Table A1/4.

3.2.4. The High2 phase is described in Figure A1/5 and Table A1/5.

3.2.5. The Extra High2 phase is described in Figure A1/6 and Table A1/6.

3.3. Class 3 cycle

Class 3 cycles are divided into 2 subclasses to reflect the subdivision of Class 3 vehicles.

3.3.1. Class 3a cycle

3.3.1.1. A complete Class 3a cycle shall consist of a low phase (Low3), a medium phase (Medium3a), a high phase (High3a) and an extra high phase (Extra High3).

A 3-phase Class 3a cycle shall consist of a low phase (Low3), a medium phase (Medium3a) and a high phase (High3a).

3.3.1.2. The Low3 phase is described in Figure A1/7 and Table A1/7.

3.3.1.3. The Medium3a phase is described in Figure A1/8 and Table A1/8.

3.3.1.4. The High3a phase is described in Figure A1/10 and Table A1/10.

3.3.1.5. The Extra High3 phase is described in Figure A1/12 and Table A1/12.

3.3.2. Class 3b cycle

3.3.2.1. A complete Class 3b cycle shall consist of a low phase (Low3) phase, a medium phase (Medium3b), a high phase (High3b) and an extra high phase (Extra High3).

A 3-phase Class 3b cycle shall consist of a low phase (Low3) phase, a medium phase (Medium3b) and a high phase (High3b).

3.3.2.2. The Low3 phase is described in Figure A1/7 and Table A1/7.

3.3.2.3. The Medium3b phase is described in Figure A1/9 and Table A1/9.

3.3.2.4. The High3b phase is described in Figure A1/11 and Table A1/11.

3.3.2.5. The Extra High3 phase is described in Figure A1/12 and Table A1/12.

3.4. Duration of the cycle phases

3.4.1. Class 1 cycle.

The first low speed phase starts at second 0 (tstart\_low11) and ends at second 589 (tend\_low11, duration 589 s)

The medium speed phase starts at second 589 (tstart\_medium1) and ends at second 1022 (tend\_medium1, duration 433 s)

The second low speed phase starts at second 1022 (tstart\_low12) and ends at second 1611 (tend\_low12, duration 589 s)

3.4.2. Class 2 and class 3 cycles.

The low speed phase starts at second 0 (tstart\_low2, tstart\_low3) and ends at second 589 (tend\_low2, tend\_low3, duration 589 s)

The medium speed phase starts at second 589 (tstart\_medium2, tstart\_medium3) and ends at second 1022 (tend\_medium2, tend\_medium3, duration 433 s)

The high speed phase starts at second 1022 (tstart\_high2, tstart\_high3) and ends at second 1477 (tend\_high2, tend\_high3, duration 455 s)

The extra high speed phase starts at second 1477 (tstart\_exhigh2, tstart\_exhigh3) and ends at second 1800 (tend\_exhigh2, tend\_exhigh3, duration 323 s)

3.5. WLTC city cycles

The WLTC city cycle consists of the low and medium speed phases only.

4. WLTC Class 1 cycle

# Figure A1/1

**WLTC, Class 1 cycle, phase Low11**

# 

# Figure A1/2a

**WLTC, Class 1 cycle, phase Medium1**

# 

Figure A1/2b

**WLTC, Class 1 cycle, phase Low12**



# Table A1/1

# **WLTC, Class 1 cycle, phase Low11 (Second 589 is the end of phase Low11 and the start of phase Medium1)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 0 | 0.0 | 47 | 18.8 | 94 | 0.0 | 141 | 35.7 |
| 1 | 0.0 | 48 | 19.5 | 95 | 0.0 | 142 | 35.9 |
| 2 | 0.0 | 49 | 20.2 | 96 | 0.0 | 143 | 36.6 |
| 3 | 0.0 | 50 | 20.9 | 97 | 0.0 | 144 | 37.5 |
| 4 | 0.0 | 51 | 21.7 | 98 | 0.0 | 145 | 38.4 |
| 5 | 0.0 | 52 | 22.4 | 99 | 0.0 | 146 | 39.3 |
| 6 | 0.0 | 53 | 23.1 | 100 | 0.0 | 147 | 40.0 |
| 7 | 0.0 | 54 | 23.7 | 101 | 0.0 | 148 | 40.6 |
| 8 | 0.0 | 55 | 24.4 | 102 | 0.0 | 149 | 41.1 |
| 9 | 0.0 | 56 | 25.1 | 103 | 0.0 | 150 | 41.4 |
| 10 | 0.0 | 57 | 25.4 | 104 | 0.0 | 151 | 41.6 |
| 11 | 0.0 | 58 | 25.2 | 105 | 0.0 | 152 | 41.8 |
| 12 | 0.2 | 59 | 23.4 | 106 | 0.0 | 153 | 41.8 |
| 13 | 3.1 | 60 | 21.8 | 107 | 0.0 | 154 | 41.9 |
| 14 | 5.7 | 61 | 19.7 | 108 | 0.7 | 155 | 41.9 |
| 15 | 8.0 | 62 | 17.3 | 109 | 1.1 | 156 | 42.0 |
| 16 | 10.1 | 63 | 14.7 | 110 | 1.9 | 157 | 42.0 |
| 17 | 12.0 | 64 | 12.0 | 111 | 2.5 | 158 | 42.2 |
| 18 | 13.8 | 65 | 9.4 | 112 | 3.5 | 159 | 42.3 |
| 19 | 15.4 | 66 | 5.6 | 113 | 4.7 | 160 | 42.6 |
| 20 | 16.7 | 67 | 3.1 | 114 | 6.1 | 161 | 43.0 |
| 21 | 17.7 | 68 | 0.0 | 115 | 7.5 | 162 | 43.3 |
| 22 | 18.3 | 69 | 0.0 | 116 | 9.4 | 163 | 43.7 |
| 23 | 18.8 | 70 | 0.0 | 117 | 11.0 | 164 | 44.0 |
| 24 | 18.9 | 71 | 0.0 | 118 | 12.9 | 165 | 44.3 |
| 25 | 18.4 | 72 | 0.0 | 119 | 14.5 | 166 | 44.5 |
| 26 | 16.9 | 73 | 0.0 | 120 | 16.4 | 167 | 44.6 |
| 27 | 14.3 | 74 | 0.0 | 121 | 18.0 | 168 | 44.6 |
| 28 | 10.8 | 75 | 0.0 | 122 | 20.0 | 169 | 44.5 |
| 29 | 7.1 | 76 | 0.0 | 123 | 21.5 | 170 | 44.4 |
| 30 | 4.0 | 77 | 0.0 | 124 | 23.5 | 171 | 44.3 |
| 31 | 0.0 | 78 | 0.0 | 125 | 25.0 | 172 | 44.2 |
| 32 | 0.0 | 79 | 0.0 | 126 | 26.8 | 173 | 44.1 |
| 33 | 0.0 | 80 | 0.0 | 127 | 28.2 | 174 | 44.0 |
| 34 | 0.0 | 81 | 0.0 | 128 | 30.0 | 175 | 43.9 |
| 35 | 1.5 | 82 | 0.0 | 129 | 31.4 | 176 | 43.8 |
| 36 | 3.8 | 83 | 0.0 | 130 | 32.5 | 177 | 43.7 |
| 37 | 5.6 | 84 | 0.0 | 131 | 33.2 | 178 | 43.6 |
| 38 | 7.5 | 85 | 0.0 | 132 | 33.4 | 179 | 43.5 |
| 39 | 9.2 | 86 | 0.0 | 133 | 33.7 | 180 | 43.4 |
| 40 | 10.8 | 87 | 0.0 | 134 | 33.9 | 181 | 43.3 |
| 41 | 12.4 | 88 | 0.0 | 135 | 34.2 | 182 | 43.1 |
| 42 | 13.8 | 89 | 0.0 | 136 | 34.4 | 183 | 42.9 |
| 43 | 15.2 | 90 | 0.0 | 137 | 34.7 | 184 | 42.7 |
| 44 | 16.3 | 91 | 0.0 | 138 | 34.9 | 185 | 42.5 |
| 45 | 17.3 | 92 | 0.0 | 139 | 35.2 | 186 | 42.3 |
| 46 | 18.0 | 93 | 0.0 | 140 | 35.4 | 187 | 42.2 |
| 188 | 42.2 | 237 | 39.7 | 286 | 25.3 | 335 | 14.3 |
| 189 | 42.2 | 238 | 39.9 | 287 | 24.9 | 336 | 14.3 |
| 190 | 42.3 | 239 | 40.0 | 288 | 24.5 | 337 | 14.0 |
| 191 | 42.4 | 240 | 40.1 | 289 | 24.2 | 338 | 13.0 |
| 192 | 42.5 | 241 | 40.2 | 290 | 24.0 | 339 | 11.4 |
| 193 | 42.7 | 242 | 40.3 | 291 | 23.8 | 340 | 10.2 |
| 194 | 42.9 | 243 | 40.4 | 292 | 23.6 | 341 | 8.0 |
| 195 | 43.1 | 244 | 40.5 | 293 | 23.5 | 342 | 7.0 |
| 196 | 43.2 | 245 | 40.5 | 294 | 23.4 | 343 | 6.0 |
| 197 | 43.3 | 246 | 40.4 | 295 | 23.3 | 344 | 5.5 |
| 198 | 43.4 | 247 | 40.3 | 296 | 23.3 | 345 | 5.0 |
| 199 | 43.4 | 248 | 40.2 | 297 | 23.2 | 346 | 4.5 |
| 200 | 43.2 | 249 | 40.1 | 298 | 23.1 | 347 | 4.0 |
| 201 | 42.9 | 250 | 39.7 | 299 | 23.0 | 348 | 3.5 |
| 202 | 42.6 | 251 | 38.8 | 300 | 22.8 | 349 | 3.0 |
| 203 | 42.2 | 252 | 37.4 | 301 | 22.5 | 350 | 2.5 |
| 204 | 41.9 | 253 | 35.6 | 302 | 22.1 | 351 | 2.0 |
| 205 | 41.5 | 254 | 33.4 | 303 | 21.7 | 352 | 1.5 |
| 206 | 41.0 | 255 | 31.2 | 304 | 21.1 | 353 | 1.0 |
| 207 | 40.5 | 256 | 29.1 | 305 | 20.4 | 354 | 0.5 |
| 208 | 39.9 | 257 | 27.6 | 306 | 19.5 | 355 | 0.0 |
| 209 | 39.3 | 258 | 26.6 | 307 | 18.5 | 356 | 0.0 |
| 210 | 38.7 | 259 | 26.2 | 308 | 17.6 | 357 | 0.0 |
| 211 | 38.1 | 260 | 26.3 | 309 | 16.6 | 358 | 0.0 |
| 212 | 37.5 | 261 | 26.7 | 310 | 15.7 | 359 | 0.0 |
| 213 | 36.9 | 262 | 27.5 | 311 | 14.9 | 360 | 0.0 |
| 214 | 36.3 | 263 | 28.4 | 312 | 14.3 | 361 | 2.2 |
| 215 | 35.7 | 264 | 29.4 | 313 | 14.1 | 362 | 4.5 |
| 216 | 35.1 | 265 | 30.4 | 314 | 14.0 | 363 | 6.6 |
| 217 | 34.5 | 266 | 31.2 | 315 | 13.9 | 364 | 8.6 |
| 218 | 33.9 | 267 | 31.9 | 316 | 13.8 | 365 | 10.6 |
| 219 | 33.6 | 268 | 32.5 | 317 | 13.7 | 366 | 12.5 |
| 220 | 33.5 | 269 | 33.0 | 318 | 13.6 | 367 | 14.4 |
| 221 | 33.6 | 270 | 33.4 | 319 | 13.5 | 368 | 16.3 |
| 222 | 33.9 | 271 | 33.8 | 320 | 13.4 | 369 | 17.9 |
| 223 | 34.3 | 272 | 34.1 | 321 | 13.3 | 370 | 19.1 |
| 224 | 34.7 | 273 | 34.3 | 322 | 13.2 | 371 | 19.9 |
| 225 | 35.1 | 274 | 34.3 | 323 | 13.2 | 372 | 20.3 |
| 226 | 35.5 | 275 | 33.9 | 324 | 13.2 | 373 | 20.5 |
| 227 | 35.9 | 276 | 33.3 | 325 | 13.4 | 374 | 20.7 |
| 228 | 36.4 | 277 | 32.6 | 326 | 13.5 | 375 | 21.0 |
| 229 | 36.9 | 278 | 31.8 | 327 | 13.7 | 376 | 21.6 |
| 230 | 37.4 | 279 | 30.7 | 328 | 13.8 | 377 | 22.6 |
| 231 | 37.9 | 280 | 29.6 | 329 | 14.0 | 378 | 23.7 |
| 232 | 38.3 | 281 | 28.6 | 330 | 14.1 | 379 | 24.8 |
| 233 | 38.7 | 282 | 27.8 | 331 | 14.3 | 380 | 25.7 |
| 234 | 39.1 | 283 | 27.0 | 332 | 14.4 | 381 | 26.2 |
| 235 | 39.3 | 284 | 26.4 | 333 | 14.4 | 382 | 26.4 |
| 236 | 39.5 | 285 | 25.8 | 334 | 14.4 | 383 | 26.4 |
| 384 | 26.4 | 433 | 0.0 | 482 | 3.1 | 531 | 48.2 |
| 385 | 26.5 | 434 | 0.0 | 483 | 4.6 | 532 | 48.5 |
| 386 | 26.6 | 435 | 0.0 | 484 | 6.1 | 533 | 48.7 |
| 387 | 26.8 | 436 | 0.0 | 485 | 7.8 | 534 | 48.9 |
| 388 | 26.9 | 437 | 0.0 | 486 | 9.5 | 535 | 49.1 |
| 389 | 27.2 | 438 | 0.0 | 487 | 11.3 | 536 | 49.1 |
| 390 | 27.5 | 439 | 0.0 | 488 | 13.2 | 537 | 49.0 |
| 391 | 28.0 | 440 | 0.0 | 489 | 15.0 | 538 | 48.8 |
| 392 | 28.8 | 441 | 0.0 | 490 | 16.8 | 539 | 48.6 |
| 393 | 29.9 | 442 | 0.0 | 491 | 18.4 | 540 | 48.5 |
| 394 | 31.0 | 443 | 0.0 | 492 | 20.1 | 541 | 48.4 |
| 395 | 31.9 | 444 | 0.0 | 493 | 21.6 | 542 | 48.3 |
| 396 | 32.5 | 445 | 0.0 | 494 | 23.1 | 543 | 48.2 |
| 397 | 32.6 | 446 | 0.0 | 495 | 24.6 | 544 | 48.1 |
| 398 | 32.4 | 447 | 0.0 | 496 | 26.0 | 545 | 47.5 |
| 399 | 32.0 | 448 | 0.0 | 497 | 27.5 | 546 | 46.7 |
| 400 | 31.3 | 449 | 0.0 | 498 | 29.0 | 547 | 45.7 |
| 401 | 30.3 | 450 | 0.0 | 499 | 30.6 | 548 | 44.6 |
| 402 | 28.0 | 451 | 0.0 | 500 | 32.1 | 549 | 42.9 |
| 403 | 27.0 | 452 | 0.0 | 501 | 33.7 | 550 | 40.8 |
| 404 | 24.0 | 453 | 0.0 | 502 | 35.3 | 551 | 38.2 |
| 405 | 22.5 | 454 | 0.0 | 503 | 36.8 | 552 | 35.3 |
| 406 | 19.0 | 455 | 0.0 | 504 | 38.1 | 553 | 31.8 |
| 407 | 17.5 | 456 | 0.0 | 505 | 39.3 | 554 | 28.7 |
| 408 | 14.0 | 457 | 0.0 | 506 | 40.4 | 555 | 25.8 |
| 409 | 12.5 | 458 | 0.0 | 507 | 41.2 | 556 | 22.9 |
| 410 | 9.0 | 459 | 0.0 | 508 | 41.9 | 557 | 20.2 |
| 411 | 7.5 | 460 | 0.0 | 509 | 42.6 | 558 | 17.3 |
| 412 | 4.0 | 461 | 0.0 | 510 | 43.3 | 559 | 15.0 |
| 413 | 2.9 | 462 | 0.0 | 511 | 44.0 | 560 | 12.3 |
| 414 | 0.0 | 463 | 0.0 | 512 | 44.6 | 561 | 10.3 |
| 415 | 0.0 | 464 | 0.0 | 513 | 45.3 | 562 | 7.8 |
| 416 | 0.0 | 465 | 0.0 | 514 | 45.5 | 563 | 6.5 |
| 417 | 0.0 | 466 | 0.0 | 515 | 45.5 | 564 | 4.4 |
| 418 | 0.0 | 467 | 0.0 | 516 | 45.2 | 565 | 3.2 |
| 419 | 0.0 | 468 | 0.0 | 517 | 44.7 | 566 | 1.2 |
| 420 | 0.0 | 469 | 0.0 | 518 | 44.2 | 567 | 0.0 |
| 421 | 0.0 | 470 | 0.0 | 519 | 43.6 | 568 | 0.0 |
| 422 | 0.0 | 471 | 0.0 | 520 | 43.1 | 569 | 0.0 |
| 423 | 0.0 | 472 | 0.0 | 521 | 42.8 | 570 | 0.0 |
| 424 | 0.0 | 473 | 0.0 | 522 | 42.7 | 571 | 0.0 |
| 425 | 0.0 | 474 | 0.0 | 523 | 42.8 | 572 | 0.0 |
| 426 | 0.0 | 475 | 0.0 | 524 | 43.3 | 573 | 0.0 |
| 427 | 0.0 | 476 | 0.0 | 525 | 43.9 | 574 | 0.0 |
| 428 | 0.0 | 477 | 0.0 | 526 | 44.6 | 575 | 0.0 |
| 429 | 0.0 | 478 | 0.0 | 527 | 45.4 | 576 | 0.0 |
| 430 | 0.0 | 479 | 0.0 | 528 | 46.3 | 577 | 0.0 |
| 431 | 0.0 | 480 | 0.0 | 529 | 47.2 | 578 | 0.0 |
| 432 | 0.0 | 481 | 1.6 | 530 | 47.8 | 579 | 0.0 |
| 580 | 0.0 |  |  |  |  |  |  |
| 581 | 0.0 |  |  |  |  |  |  |
| 582 | 0.0 |  |  |  |  |  |  |
| 583 | 0.0 |  |  |  |  |  |  |
| 584 | 0.0 |  |  |  |  |  |  |
| 585 | 0.0 |  |  |  |  |  |  |
| 586 | 0.0 |  |  |  |  |  |  |
| 587 | 0.0 |  |  |  |  |  |  |
| 588 | 0.0 |  |  |  |  |  |  |
| 589 | 0.0 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

# Table A1/2a

# **WLTC, Class 1 cycle, phase Medium1 (The start of this phase is at second 589)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 590 | 0.0 | 637 | 18.4 | 684 | 56.2 | 731 | 57.9 |
| 591 | 0.0 | 638 | 19.0 | 685 | 56.7 | 732 | 58.8 |
| 592 | 0.0 | 639 | 20.1 | 686 | 57.3 | 733 | 59.6 |
| 593 | 0.0 | 640 | 21.5 | 687 | 57.9 | 734 | 60.3 |
| 594 | 0.0 | 641 | 23.1 | 688 | 58.4 | 735 | 60.9 |
| 595 | 0.0 | 642 | 24.9 | 689 | 58.8 | 736 | 61.3 |
| 596 | 0.0 | 643 | 26.4 | 690 | 58.9 | 737 | 61.7 |
| 597 | 0.0 | 644 | 27.9 | 691 | 58.4 | 738 | 61.8 |
| 598 | 0.0 | 645 | 29.2 | 692 | 58.1 | 739 | 61.8 |
| 599 | 0.0 | 646 | 30.4 | 693 | 57.6 | 740 | 61.6 |
| 600 | 0.6 | 647 | 31.6 | 694 | 56.9 | 741 | 61.2 |
| 601 | 1.9 | 648 | 32.8 | 695 | 56.3 | 742 | 60.8 |
| 602 | 2.7 | 649 | 34.0 | 696 | 55.7 | 743 | 60.4 |
| 603 | 5.2 | 650 | 35.1 | 697 | 55.3 | 744 | 59.9 |
| 604 | 7.0 | 651 | 36.3 | 698 | 55.0 | 745 | 59.4 |
| 605 | 9.6 | 652 | 37.4 | 699 | 54.7 | 746 | 58.9 |
| 606 | 11.4 | 653 | 38.6 | 700 | 54.5 | 747 | 58.6 |
| 607 | 14.1 | 654 | 39.6 | 701 | 54.4 | 748 | 58.2 |
| 608 | 15.8 | 655 | 40.6 | 702 | 54.3 | 749 | 57.9 |
| 609 | 18.2 | 656 | 41.6 | 703 | 54.2 | 750 | 57.7 |
| 610 | 19.7 | 657 | 42.4 | 704 | 54.1 | 751 | 57.5 |
| 611 | 21.8 | 658 | 43.0 | 705 | 53.8 | 752 | 57.2 |
| 612 | 23.2 | 659 | 43.6 | 706 | 53.5 | 753 | 57.0 |
| 613 | 24.7 | 660 | 44.0 | 707 | 53.0 | 754 | 56.8 |
| 614 | 25.8 | 661 | 44.4 | 708 | 52.6 | 755 | 56.6 |
| 615 | 26.7 | 662 | 44.8 | 709 | 52.2 | 756 | 56.6 |
| 616 | 27.2 | 663 | 45.2 | 710 | 51.9 | 757 | 56.7 |
| 617 | 27.7 | 664 | 45.6 | 711 | 51.7 | 758 | 57.1 |
| 618 | 28.1 | 665 | 46.0 | 712 | 51.7 | 759 | 57.6 |
| 619 | 28.4 | 666 | 46.5 | 713 | 51.8 | 760 | 58.2 |
| 620 | 28.7 | 667 | 47.0 | 714 | 52.0 | 761 | 59.0 |
| 621 | 29.0 | 668 | 47.5 | 715 | 52.3 | 762 | 59.8 |
| 622 | 29.2 | 669 | 48.0 | 716 | 52.6 | 763 | 60.6 |
| 623 | 29.4 | 670 | 48.6 | 717 | 52.9 | 764 | 61.4 |
| 624 | 29.4 | 671 | 49.1 | 718 | 53.1 | 765 | 62.2 |
| 625 | 29.3 | 672 | 49.7 | 719 | 53.2 | 766 | 62.9 |
| 626 | 28.9 | 673 | 50.2 | 720 | 53.3 | 767 | 63.5 |
| 627 | 28.5 | 674 | 50.8 | 721 | 53.3 | 768 | 64.2 |
| 628 | 28.1 | 675 | 51.3 | 722 | 53.4 | 769 | 64.4 |
| 629 | 27.6 | 676 | 51.8 | 723 | 53.5 | 770 | 64.4 |
| 630 | 26.9 | 677 | 52.3 | 724 | 53.7 | 771 | 64.0 |
| 631 | 26.0 | 678 | 52.9 | 725 | 54.0 | 772 | 63.5 |
| 632 | 24.6 | 679 | 53.4 | 726 | 54.4 | 773 | 62.9 |
| 633 | 22.8 | 680 | 54.0 | 727 | 54.9 | 774 | 62.4 |
| 634 | 21.0 | 681 | 54.5 | 728 | 55.6 | 775 | 62.0 |
| 635 | 19.5 | 682 | 55.1 | 729 | 56.3 | 776 | 61.6 |
| 636 | 18.6 | 683 | 55.6 | 730 | 57.1 | 777 | 61.4 |
| 778 | 61.2 | 827 | 49.7 | 876 | 53.2 | 925 | 44.4 |
| 779 | 61.0 | 828 | 50.6 | 877 | 53.1 | 926 | 44.5 |
| 780 | 60.7 | 829 | 51.6 | 878 | 53.0 | 927 | 44.6 |
| 781 | 60.2 | 830 | 52.5 | 879 | 53.0 | 928 | 44.7 |
| 782 | 59.6 | 831 | 53.3 | 880 | 53.0 | 929 | 44.6 |
| 783 | 58.9 | 832 | 54.1 | 881 | 53.0 | 930 | 44.5 |
| 784 | 58.1 | 833 | 54.7 | 882 | 53.0 | 931 | 44.4 |
| 785 | 57.2 | 834 | 55.3 | 883 | 53.0 | 932 | 44.2 |
| 786 | 56.3 | 835 | 55.7 | 884 | 52.8 | 933 | 44.1 |
| 787 | 55.3 | 836 | 56.1 | 885 | 52.5 | 934 | 43.7 |
| 788 | 54.4 | 837 | 56.4 | 886 | 51.9 | 935 | 43.3 |
| 789 | 53.4 | 838 | 56.7 | 887 | 51.1 | 936 | 42.8 |
| 790 | 52.4 | 839 | 57.1 | 888 | 50.2 | 937 | 42.3 |
| 791 | 51.4 | 840 | 57.5 | 889 | 49.2 | 938 | 41.6 |
| 792 | 50.4 | 841 | 58.0 | 890 | 48.2 | 939 | 40.7 |
| 793 | 49.4 | 842 | 58.7 | 891 | 47.3 | 940 | 39.8 |
| 794 | 48.5 | 843 | 59.3 | 892 | 46.4 | 941 | 38.8 |
| 795 | 47.5 | 844 | 60.0 | 893 | 45.6 | 942 | 37.8 |
| 796 | 46.5 | 845 | 60.6 | 894 | 45.0 | 943 | 36.9 |
| 797 | 45.4 | 846 | 61.3 | 895 | 44.3 | 944 | 36.1 |
| 798 | 44.3 | 847 | 61.5 | 896 | 43.8 | 945 | 35.5 |
| 799 | 43.1 | 848 | 61.5 | 897 | 43.3 | 946 | 35.0 |
| 800 | 42.0 | 849 | 61.4 | 898 | 42.8 | 947 | 34.7 |
| 801 | 40.8 | 850 | 61.2 | 899 | 42.4 | 948 | 34.4 |
| 802 | 39.7 | 851 | 60.5 | 900 | 42.0 | 949 | 34.1 |
| 803 | 38.8 | 852 | 60.0 | 901 | 41.6 | 950 | 33.9 |
| 804 | 38.1 | 853 | 59.5 | 902 | 41.1 | 951 | 33.6 |
| 805 | 37.4 | 854 | 58.9 | 903 | 40.3 | 952 | 33.3 |
| 806 | 37.1 | 855 | 58.4 | 904 | 39.5 | 953 | 33.0 |
| 807 | 36.9 | 856 | 57.9 | 905 | 38.6 | 954 | 32.7 |
| 808 | 37.0 | 857 | 57.5 | 906 | 37.7 | 955 | 32.3 |
| 809 | 37.5 | 858 | 57.1 | 907 | 36.7 | 956 | 31.9 |
| 810 | 37.8 | 859 | 56.7 | 908 | 36.2 | 957 | 31.5 |
| 811 | 38.2 | 860 | 56.4 | 909 | 36.0 | 958 | 31.0 |
| 812 | 38.6 | 861 | 56.1 | 910 | 36.2 | 959 | 30.6 |
| 813 | 39.1 | 862 | 55.8 | 911 | 37.0 | 960 | 30.2 |
| 814 | 39.6 | 863 | 55.5 | 912 | 38.0 | 961 | 29.7 |
| 815 | 40.1 | 864 | 55.3 | 913 | 39.0 | 962 | 29.1 |
| 816 | 40.7 | 865 | 55.0 | 914 | 39.7 | 963 | 28.4 |
| 817 | 41.3 | 866 | 54.7 | 915 | 40.2 | 964 | 27.6 |
| 818 | 41.9 | 867 | 54.4 | 916 | 40.7 | 965 | 26.8 |
| 819 | 42.7 | 868 | 54.2 | 917 | 41.2 | 966 | 26.0 |
| 820 | 43.4 | 869 | 54.0 | 918 | 41.7 | 967 | 25.1 |
| 821 | 44.2 | 870 | 53.9 | 919 | 42.2 | 968 | 24.2 |
| 822 | 45.0 | 871 | 53.7 | 920 | 42.7 | 969 | 23.3 |
| 823 | 45.9 | 872 | 53.6 | 921 | 43.2 | 970 | 22.4 |
| 824 | 46.8 | 873 | 53.5 | 922 | 43.6 | 971 | 21.5 |
| 825 | 47.7 | 874 | 53.4 | 923 | 44.0 | 972 | 20.6 |
| 826 | 48.7 | 875 | 53.3 | 924 | 44.2 | 973 | 19.7 |
| 974 | 18.8 |  |  |  |  |  |  |
| 975 | 17.7 |  |  |  |  |  |  |
| 976 | 16.4 |  |  |  |  |  |  |
| 977 | 14.9 |  |  |  |  |  |  |
| 978 | 13.2 |  |  |  |  |  |  |
| 979 | 11.3 |  |  |  |  |  |  |
| 980 | 9.4 |  |  |  |  |  |  |
| 981 | 7.5 |  |  |  |  |  |  |
| 982 | 5.6 |  |  |  |  |  |  |
| 983 | 3.7 |  |  |  |  |  |  |
| 984 | 1.9 |  |  |  |  |  |  |
| 985 | 1.0 |  |  |  |  |  |  |
| 986 | 0.0 |  |  |  |  |  |  |
| 987 | 0.0 |  |  |  |  |  |  |
| 988 | 0.0 |  |  |  |  |  |  |
| 989 | 0.0 |  |  |  |  |  |  |
| 990 | 0.0 |  |  |  |  |  |  |
| 991 | 0.0 |  |  |  |  |  |  |
| 992 | 0.0 |  |  |  |  |  |  |
| 993 | 0.0 |  |  |  |  |  |  |
| 994 | 0.0 |  |  |  |  |  |  |
| 995 | 0.0 |  |  |  |  |  |  |
| 996 | 0.0 |  |  |  |  |  |  |
| 997 | 0.0 |  |  |  |  |  |  |
| 998 | 0.0 |  |  |  |  |  |  |
| 999 | 0.0 |  |  |  |  |  |  |
| 1000 | 0.0 |  |  |  |  |  |  |
| 1001 | 0.0 |  |  |  |  |  |  |
| 1002 | 0.0 |  |  |  |  |  |  |
| 1003 | 0.0 |  |  |  |  |  |  |
| 1004 | 0.0 |  |  |  |  |  |  |
| 1005 | 0.0 |  |  |  |  |  |  |
| 1006 | 0.0 |  |  |  |  |  |  |
| 1007 | 0.0 |  |  |  |  |  |  |
| 1008 | 0.0 |  |  |  |  |  |  |
| 1009 | 0.0 |  |  |  |  |  |  |
| 1010 | 0.0 |  |  |  |  |  |  |
| 1011 | 0.0 |  |  |  |  |  |  |
| 1012 | 0.0 |  |  |  |  |  |  |
| 1013 | 0.0 |  |  |  |  |  |  |
| 1014 | 0.0 |  |  |  |  |  |  |
| 1015 | 0.0 |  |  |  |  |  |  |
| 1016 | 0.0 |  |  |  |  |  |  |
| 1017 | 0.0 |  |  |  |  |  |  |
| 1018 | 0.0 |  |  |  |  |  |  |
| 1019 | 0.0 |  |  |  |  |  |  |
| 1020 | 0.0 |  |  |  |  |  |  |
| 1021 | 0.0 |  |  |  |  |  |  |
| 1022 | 0.0 |  |  |  |  |  |  |

Table A1/2b

# **WLTC, Class 1 cycle, phase Low12 (Second 1022 is the end of phase Medium1 and the start of phase Low12)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1023 | 0.0 | 1070 | 19.5 | 1117 | 0.0 | 1164 | 35.9 |
| 1024 | 0.0 | 1071 | 20.2 | 1118 | 0.0 | 1165 | 36.6 |
| 1025 | 0.0 | 1072 | 20.9 | 1119 | 0.0 | 1166 | 37.5 |
| 1026 | 0.0 | 1073 | 21.7 | 1120 | 0.0 | 1167 | 38.4 |
| 1027 | 0.0 | 1074 | 22.4 | 1121 | 0.0 | 1168 | 39.3 |
| 1028 | 0.0 | 1075 | 23.1 | 1122 | 0.0 | 1169 | 40.0 |
| 1029 | 0.0 | 1076 | 23.7 | 1123 | 0.0 | 1170 | 40.6 |
| 1030 | 0.0 | 1077 | 24.4 | 1124 | 0.0 | 1171 | 41.1 |
| 1031 | 0.0 | 1078 | 25.1 | 1125 | 0.0 | 1172 | 41.4 |
| 1032 | 0.0 | 1079 | 25.4 | 1126 | 0.0 | 1173 | 41.6 |
| 1033 | 0.0 | 1080 | 25.2 | 1127 | 0.0 | 1174 | 41.8 |
| 1034 | 0.2 | 1081 | 23.4 | 1128 | 0.0 | 1175 | 41.8 |
| 1035 | 3.1 | 1082 | 21.8 | 1129 | 0.0 | 1176 | 41.9 |
| 1036 | 5.7 | 1083 | 19.7 | 1130 | 0.7 | 1177 | 41.9 |
| 1037 | 8.0 | 1084 | 17.3 | 1131 | 1.1 | 1178 | 42.0 |
| 1038 | 10.1 | 1085 | 14.7 | 1132 | 1.9 | 1179 | 42.0 |
| 1039 | 12.0 | 1086 | 12.0 | 1133 | 2.5 | 1180 | 42.2 |
| 1040 | 13.8 | 1087 | 9.4 | 1134 | 3.5 | 1181 | 42.3 |
| 1041 | 15.4 | 1088 | 5.6 | 1135 | 4.7 | 1182 | 42.6 |
| 1042 | 16.7 | 1089 | 3.1 | 1136 | 6.1 | 1183 | 43.0 |
| 1043 | 17.7 | 1090 | 0.0 | 1137 | 7.5 | 1184 | 43.3 |
| 1044 | 18.3 | 1091 | 0.0 | 1138 | 9.4 | 1185 | 43.7 |
| 1045 | 18.8 | 1092 | 0.0 | 1139 | 11.0 | 1186 | 44.0 |
| 1046 | 18.9 | 1093 | 0.0 | 1140 | 12.9 | 1187 | 44.3 |
| 1047 | 18.4 | 1094 | 0.0 | 1141 | 14.5 | 1188 | 44.5 |
| 1048 | 16.9 | 1095 | 0.0 | 1142 | 16.4 | 1189 | 44.6 |
| 1049 | 14.3 | 1096 | 0.0 | 1143 | 18.0 | 1190 | 44.6 |
| 1050 | 10.8 | 1097 | 0.0 | 1144 | 20.0 | 1191 | 44.5 |
| 1051 | 7.1 | 1098 | 0.0 | 1145 | 21.5 | 1192 | 44.4 |
| 1052 | 4.0 | 1099 | 0.0 | 1146 | 23.5 | 1193 | 44.3 |
| 1053 | 0.0 | 1100 | 0.0 | 1147 | 25.0 | 1194 | 44.2 |
| 1054 | 0.0 | 1101 | 0.0 | 1148 | 26.8 | 1195 | 44.1 |
| 1055 | 0.0 | 1102 | 0.0 | 1149 | 28.2 | 1196 | 44.0 |
| 1056 | 0.0 | 1103 | 0.0 | 1150 | 30.0 | 1197 | 43.9 |
| 1057 | 1.5 | 1104 | 0.0 | 1151 | 31.4 | 1198 | 43.8 |
| 1058 | 3.8 | 1105 | 0.0 | 1152 | 32.5 | 1199 | 43.7 |
| 1059 | 5.6 | 1106 | 0.0 | 1153 | 33.2 | 1200 | 43.6 |
| 1060 | 7.5 | 1107 | 0.0 | 1154 | 33.4 | 1201 | 43.5 |
| 1061 | 9.2 | 1108 | 0.0 | 1155 | 33.7 | 1202 | 43.4 |
| 1062 | 10.8 | 1109 | 0.0 | 1156 | 33.9 | 1203 | 43.3 |
| 1063 | 12.4 | 1110 | 0.0 | 1157 | 34.2 | 1204 | 43.1 |
| 1064 | 13.8 | 1111 | 0.0 | 1158 | 34.4 | 1205 | 42.9 |
| 1065 | 15.2 | 1112 | 0.0 | 1159 | 34.7 | 1206 | 42.7 |
| 1066 | 16.3 | 1113 | 0.0 | 1160 | 34.9 | 1207 | 42.5 |
| 1067 | 17.3 | 1114 | 0.0 | 1161 | 35.2 | 1208 | 42.3 |
| 1068 | 18.0 | 1115 | 0.0 | 1162 | 35.4 | 1209 | 42.2 |
| 1069 | 18.8 | 1116 | 0.0 | 1163 | 35.7 | 1210 | 42.2 |
| 1211 | 42.2 | 1260 | 39.9 | 1309 | 24.9 | 1358 | 14.3 |
| 1212 | 42.3 | 1261 | 40.0 | 1310 | 24.5 | 1359 | 14.0 |
| 1213 | 42.4 | 1262 | 40.1 | 1311 | 24.2 | 1360 | 13.0 |
| 1214 | 42.5 | 1263 | 40.2 | 1312 | 24.0 | 1361 | 11.4 |
| 1215 | 42.7 | 1264 | 40.3 | 1313 | 23.8 | 1362 | 10.2 |
| 1216 | 42.9 | 1265 | 40.4 | 1314 | 23.6 | 1363 | 8.0 |
| 1217 | 43.1 | 1266 | 40.5 | 1315 | 23.5 | 1364 | 7.0 |
| 1218 | 43.2 | 1267 | 40.5 | 1316 | 23.4 | 1365 | 6.0 |
| 1219 | 43.3 | 1268 | 40.4 | 1317 | 23.3 | 1366 | 5.5 |
| 1220 | 43.4 | 1269 | 40.3 | 1318 | 23.3 | 1367 | 5.0 |
| 1221 | 43.4 | 1270 | 40.2 | 1319 | 23.2 | 1368 | 4.5 |
| 1222 | 43.2 | 1271 | 40.1 | 1320 | 23.1 | 1369 | 4.0 |
| 1223 | 42.9 | 1272 | 39.7 | 1321 | 23.0 | 1370 | 3.5 |
| 1224 | 42.6 | 1273 | 38.8 | 1322 | 22.8 | 1371 | 3.0 |
| 1225 | 42.2 | 1274 | 37.4 | 1323 | 22.5 | 1372 | 2.5 |
| 1226 | 41.9 | 1275 | 35.6 | 1324 | 22.1 | 1373 | 2.0 |
| 1227 | 41.5 | 1276 | 33.4 | 1325 | 21.7 | 1374 | 1.5 |
| 1228 | 41.0 | 1277 | 31.2 | 1326 | 21.1 | 1375 | 1.0 |
| 1229 | 40.5 | 1278 | 29.1 | 1327 | 20.4 | 1376 | 0.5 |
| 1230 | 39.9 | 1279 | 27.6 | 1328 | 19.5 | 1377 | 0.0 |
| 1231 | 39.3 | 1280 | 26.6 | 1329 | 18.5 | 1378 | 0.0 |
| 1232 | 38.7 | 1281 | 26.2 | 1330 | 17.6 | 1379 | 0.0 |
| 1233 | 38.1 | 1282 | 26.3 | 1331 | 16.6 | 1380 | 0.0 |
| 1234 | 37.5 | 1283 | 26.7 | 1332 | 15.7 | 1381 | 0.0 |
| 1235 | 36.9 | 1284 | 27.5 | 1333 | 14.9 | 1382 | 0.0 |
| 1236 | 36.3 | 1285 | 28.4 | 1334 | 14.3 | 1383 | 2.2 |
| 1237 | 35.7 | 1286 | 29.4 | 1335 | 14.1 | 1384 | 4.5 |
| 1238 | 35.1 | 1287 | 30.4 | 1336 | 14.0 | 1385 | 6.6 |
| 1239 | 34.5 | 1288 | 31.2 | 1337 | 13.9 | 1386 | 8.6 |
| 1240 | 33.9 | 1289 | 31.9 | 1338 | 13.8 | 1387 | 10.6 |
| 1241 | 33.6 | 1290 | 32.5 | 1339 | 13.7 | 1388 | 12.5 |
| 1242 | 33.5 | 1291 | 33.0 | 1340 | 13.6 | 1389 | 14.4 |
| 1243 | 33.6 | 1292 | 33.4 | 1341 | 13.5 | 1390 | 16.3 |
| 1244 | 33.9 | 1293 | 33.8 | 1342 | 13.4 | 1391 | 17.9 |
| 1245 | 34.3 | 1294 | 34.1 | 1343 | 13.3 | 1392 | 19.1 |
| 1246 | 34.7 | 1295 | 34.3 | 1344 | 13.2 | 1393 | 19.9 |
| 1247 | 35.1 | 1296 | 34.3 | 1345 | 13.2 | 1394 | 20.3 |
| 1248 | 35.5 | 1297 | 33.9 | 1346 | 13.2 | 1395 | 20.5 |
| 1249 | 35.9 | 1298 | 33.3 | 1347 | 13.4 | 1396 | 20.7 |
| 1250 | 36.4 | 1299 | 32.6 | 1348 | 13.5 | 1397 | 21.0 |
| 1251 | 36.9 | 1300 | 31.8 | 1349 | 13.7 | 1398 | 21.6 |
| 1252 | 37.4 | 1301 | 30.7 | 1350 | 13.8 | 1399 | 22.6 |
| 1253 | 37.9 | 1302 | 29.6 | 1351 | 14.0 | 1400 | 23.7 |
| 1254 | 38.3 | 1303 | 28.6 | 1352 | 14.1 | 1401 | 24.8 |
| 1255 | 38.7 | 1304 | 27.8 | 1353 | 14.3 | 1402 | 25.7 |
| 1256 | 39.1 | 1305 | 27.0 | 1354 | 14.4 | 1403 | 26.2 |
| 1257 | 39.3 | 1306 | 26.4 | 1355 | 14.4 | 1404 | 26.4 |
| 1258 | 39.5 | 1307 | 25.8 | 1356 | 14.4 | 1405 | 26.4 |
| 1259 | 39.7 | 1308 | 25.3 | 1357 | 14.3 | 1406 | 26.4 |
| 1407 | 26.5 | 1456 | 0.0 | 1505 | 4.6 | 1554 | 48.5 |
| 1408 | 26.6 | 1457 | 0.0 | 1506 | 6.1 | 1555 | 48.7 |
| 1409 | 26.8 | 1458 | 0.0 | 1507 | 7.8 | 1556 | 48.9 |
| 1410 | 26.9 | 1459 | 0.0 | 1508 | 9.5 | 1557 | 49.1 |
| 1411 | 27.2 | 1460 | 0.0 | 1509 | 11.3 | 1558 | 49.1 |
| 1412 | 27.5 | 1461 | 0.0 | 1510 | 13.2 | 1559 | 49.0 |
| 1413 | 28.0 | 1462 | 0.0 | 1511 | 15.0 | 1560 | 48.8 |
| 1414 | 28.8 | 1463 | 0.0 | 1512 | 16.8 | 1561 | 48.6 |
| 1415 | 29.9 | 1464 | 0.0 | 1513 | 18.4 | 1562 | 48.5 |
| 1416 | 31.0 | 1465 | 0.0 | 1514 | 20.1 | 1563 | 48.4 |
| 1417 | 31.9 | 1466 | 0.0 | 1515 | 21.6 | 1564 | 48.3 |
| 1418 | 32.5 | 1467 | 0.0 | 1516 | 23.1 | 1565 | 48.2 |
| 1419 | 32.6 | 1468 | 0.0 | 1517 | 24.6 | 1566 | 48.1 |
| 1420 | 32.4 | 1469 | 0.0 | 1518 | 26.0 | 1567 | 47.5 |
| 1421 | 32.0 | 1470 | 0.0 | 1519 | 27.5 | 1568 | 46.7 |
| 1422 | 31.3 | 1471 | 0.0 | 1520 | 29.0 | 1569 | 45.7 |
| 1423 | 30.3 | 1472 | 0.0 | 1521 | 30.6 | 1570 | 44.6 |
| 1424 | 28.0 | 1473 | 0.0 | 1522 | 32.1 | 1571 | 42.9 |
| 1425 | 27.0 | 1474 | 0.0 | 1523 | 33.7 | 1572 | 40.8 |
| 1426 | 24.0 | 1475 | 0.0 | 1524 | 35.3 | 1573 | 38.2 |
| 1427 | 22.5 | 1476 | 0.0 | 1525 | 36.8 | 1574 | 35.3 |
| 1428 | 19.0 | 1477 | 0.0 | 1526 | 38.1 | 1575 | 31.8 |
| 1429 | 17.5 | 1478 | 0.0 | 1527 | 39.3 | 1576 | 28.7 |
| 1430 | 14.0 | 1479 | 0.0 | 1528 | 40.4 | 1577 | 25.8 |
| 1431 | 12.5 | 1480 | 0.0 | 1529 | 41.2 | 1578 | 22.9 |
| 1432 | 9.0 | 1481 | 0.0 | 1530 | 41.9 | 1579 | 20.2 |
| 1433 | 7.5 | 1482 | 0.0 | 1531 | 42.6 | 1580 | 17.3 |
| 1434 | 4.0 | 1483 | 0.0 | 1532 | 43.3 | 1581 | 15.0 |
| 1435 | 2.9 | 1484 | 0.0 | 1533 | 44.0 | 1582 | 12.3 |
| 1436 | 0.0 | 1485 | 0.0 | 1534 | 44.6 | 1583 | 10.3 |
| 1437 | 0.0 | 1486 | 0.0 | 1535 | 45.3 | 1584 | 7.8 |
| 1438 | 0.0 | 1487 | 0.0 | 1536 | 45.5 | 1585 | 6.5 |
| 1439 | 0.0 | 1488 | 0.0 | 1537 | 45.5 | 1586 | 4.4 |
| 1440 | 0.0 | 1489 | 0.0 | 1538 | 45.2 | 1587 | 3.2 |
| 1441 | 0.0 | 1490 | 0.0 | 1539 | 44.7 | 1588 | 1.2 |
| 1442 | 0.0 | 1491 | 0.0 | 1540 | 44.2 | 1589 | 0.0 |
| 1443 | 0.0 | 1492 | 0.0 | 1541 | 43.6 | 1590 | 0.0 |
| 1444 | 0.0 | 1493 | 0.0 | 1542 | 43.1 | 1591 | 0.0 |
| 1445 | 0.0 | 1494 | 0.0 | 1543 | 42.8 | 1592 | 0.0 |
| 1446 | 0.0 | 1495 | 0.0 | 1544 | 42.7 | 1593 | 0.0 |
| 1447 | 0.0 | 1496 | 0.0 | 1545 | 42.8 | 1594 | 0.0 |
| 1448 | 0.0 | 1497 | 0.0 | 1546 | 43.3 | 1595 | 0.0 |
| 1449 | 0.0 | 1498 | 0.0 | 1547 | 43.9 | 1596 | 0.0 |
| 1450 | 0.0 | 1499 | 0.0 | 1548 | 44.6 | 1597 | 0.0 |
| 1451 | 0.0 | 1500 | 0.0 | 1549 | 45.4 | 1598 | 0.0 |
| 1452 | 0.0 | 1501 | 0.0 | 1550 | 46.3 | 1599 | 0.0 |
| 1453 | 0.0 | 1502 | 0.0 | 1551 | 47.2 | 1600 | 0.0 |
| 1454 | 0.0 | 1503 | 1.6 | 1552 | 47.8 | 1601 | 0.0 |
| 1455 | 0.0 | 1504 | 3.1 | 1553 | 48.2 | 1602 | 0.0 |
| 1603 | 0.0 |  |  |  |  |  |  |
| 1604 | 0.0 |  |  |  |  |  |  |
| 1605 | 0.0 |  |  |  |  |  |  |
| 1606 | 0.0 |  |  |  |  |  |  |
| 1607 | 0.0 |  |  |  |  |  |  |
| 1608 | 0.0 |  |  |  |  |  |  |
| 1609 | 0.0 |  |  |  |  |  |  |
| 1610 | 0.0 |  |  |  |  |  |  |
| 1611 | 0.0 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

5. WLTC Class 2 cycle

# Figure A1/3

# **WLTC, Class 2 cycle, phase Low2**

# 

# Figure A1/4

# **WLTC, Class 2 cycle, phase Medium2**

# 


# Figure A1/5

# **WLTC, Class 2 cycle, phase High2**

# 

# Figure A1/6

# **WLTC, Class 2 cycle, phase Extra High2**



# Table A1/3

# **WLTC, Class 2 cycle, phase Low2 (Second 589 is the end of phase Low1 and the start of phase Medium1)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 0 | 0.0 | 47 | 11.6 | 94 | 0.0 | 141 | 36.8 |
| 1 | 0.0 | 48 | 12.4 | 95 | 0.0 | 142 | 35.1 |
| 2 | 0.0 | 49 | 13.2 | 96 | 0.0 | 143 | 32.2 |
| 3 | 0.0 | 50 | 14.2 | 97 | 0.0 | 144 | 31.1 |
| 4 | 0.0 | 51 | 14.8 | 98 | 0.0 | 145 | 30.8 |
| 5 | 0.0 | 52 | 14.7 | 99 | 0.0 | 146 | 29.7 |
| 6 | 0.0 | 53 | 14.4 | 100 | 0.0 | 147 | 29.4 |
| 7 | 0.0 | 54 | 14.1 | 101 | 0.0 | 148 | 29.0 |
| 8 | 0.0 | 55 | 13.6 | 102 | 0.0 | 149 | 28.5 |
| 9 | 0.0 | 56 | 13.0 | 103 | 0.0 | 150 | 26.0 |
| 10 | 0.0 | 57 | 12.4 | 104 | 0.0 | 151 | 23.4 |
| 11 | 0.0 | 58 | 11.8 | 105 | 0.0 | 152 | 20.7 |
| 12 | 0.0 | 59 | 11.2 | 106 | 0.0 | 153 | 17.4 |
| 13 | 1.2 | 60 | 10.6 | 107 | 0.8 | 154 | 15.2 |
| 14 | 2.6 | 61 | 9.9 | 108 | 1.4 | 155 | 13.5 |
| 15 | 4.9 | 62 | 9.0 | 109 | 2.3 | 156 | 13.0 |
| 16 | 7.3 | 63 | 8.2 | 110 | 3.5 | 157 | 12.4 |
| 17 | 9.4 | 64 | 7.0 | 111 | 4.7 | 158 | 12.3 |
| 18 | 11.4 | 65 | 4.8 | 112 | 5.9 | 159 | 12.2 |
| 19 | 12.7 | 66 | 2.3 | 113 | 7.4 | 160 | 12.3 |
| 20 | 13.3 | 67 | 0.0 | 114 | 9.2 | 161 | 12.4 |
| 21 | 13.4 | 68 | 0.0 | 115 | 11.7 | 162 | 12.5 |
| 22 | 13.3 | 69 | 0.0 | 116 | 13.5 | 163 | 12.7 |
| 23 | 13.1 | 70 | 0.0 | 117 | 15.0 | 164 | 12.8 |
| 24 | 12.5 | 71 | 0.0 | 118 | 16.2 | 165 | 13.2 |
| 25 | 11.1 | 72 | 0.0 | 119 | 16.8 | 166 | 14.3 |
| 26 | 8.9 | 73 | 0.0 | 120 | 17.5 | 167 | 16.5 |
| 27 | 6.2 | 74 | 0.0 | 121 | 18.8 | 168 | 19.4 |
| 28 | 3.8 | 75 | 0.0 | 122 | 20.3 | 169 | 21.7 |
| 29 | 1.8 | 76 | 0.0 | 123 | 22.0 | 170 | 23.1 |
| 30 | 0.0 | 77 | 0.0 | 124 | 23.6 | 171 | 23.5 |
| 31 | 0.0 | 78 | 0.0 | 125 | 24.8 | 172 | 24.2 |
| 32 | 0.0 | 79 | 0.0 | 126 | 25.6 | 173 | 24.8 |
| 33 | 0.0 | 80 | 0.0 | 127 | 26.3 | 174 | 25.4 |
| 34 | 1.5 | 81 | 0.0 | 128 | 27.2 | 175 | 25.8 |
| 35 | 2.8 | 82 | 0.0 | 129 | 28.3 | 176 | 26.5 |
| 36 | 3.6 | 83 | 0.0 | 130 | 29.6 | 177 | 27.2 |
| 37 | 4.5 | 84 | 0.0 | 131 | 30.9 | 178 | 28.3 |
| 38 | 5.3 | 85 | 0.0 | 132 | 32.2 | 179 | 29.9 |
| 39 | 6.0 | 86 | 0.0 | 133 | 33.4 | 180 | 32.4 |
| 40 | 6.6 | 87 | 0.0 | 134 | 35.1 | 181 | 35.1 |
| 41 | 7.3 | 88 | 0.0 | 135 | 37.2 | 182 | 37.5 |
| 42 | 7.9 | 89 | 0.0 | 136 | 38.7 | 183 | 39.2 |
| 43 | 8.6 | 90 | 0.0 | 137 | 39.0 | 184 | 40.5 |
| 44 | 9.3 | 91 | 0.0 | 138 | 40.1 | 185 | 41.4 |
| 45 | 10 | 92 | 0.0 | 139 | 40.4 | 186 | 42.0 |
| 46 | 10.8 | 93 | 0.0 | 140 | 39.7 | 187 | 42.5 |
| 188 | 43.2 | 237 | 33.5 | 286 | 32.5 | 335 | 25.0 |
| 189 | 44.4 | 238 | 35.8 | 287 | 30.9 | 336 | 24.6 |
| 190 | 45.9 | 239 | 37.6 | 288 | 28.6 | 337 | 23.9 |
| 191 | 47.6 | 240 | 38.8 | 289 | 25.9 | 338 | 23.0 |
| 192 | 49.0 | 241 | 39.6 | 290 | 23.1 | 339 | 21.8 |
| 193 | 50.0 | 242 | 40.1 | 291 | 20.1 | 340 | 20.7 |
| 194 | 50.2 | 243 | 40.9 | 292 | 17.3 | 341 | 19.6 |
| 195 | 50.1 | 244 | 41.8 | 293 | 15.1 | 342 | 18.7 |
| 196 | 49.8 | 245 | 43.3 | 294 | 13.7 | 343 | 18.1 |
| 197 | 49.4 | 246 | 44.7 | 295 | 13.4 | 344 | 17.5 |
| 198 | 48.9 | 247 | 46.4 | 296 | 13.9 | 345 | 16.7 |
| 199 | 48.5 | 248 | 47.9 | 297 | 15.0 | 346 | 15.4 |
| 200 | 48.3 | 249 | 49.6 | 298 | 16.3 | 347 | 13.6 |
| 201 | 48.2 | 250 | 49.6 | 299 | 17.4 | 348 | 11.2 |
| 202 | 47.9 | 251 | 48.8 | 300 | 18.2 | 349 | 8.6 |
| 203 | 47.1 | 252 | 48.0 | 301 | 18.6 | 350 | 6.0 |
| 204 | 45.5 | 253 | 47.5 | 302 | 19.0 | 351 | 3.1 |
| 205 | 43.2 | 254 | 47.1 | 303 | 19.4 | 352 | 1.2 |
| 206 | 40.6 | 255 | 46.9 | 304 | 19.8 | 353 | 0.0 |
| 207 | 38.5 | 256 | 45.8 | 305 | 20.1 | 354 | 0.0 |
| 208 | 36.9 | 257 | 45.8 | 306 | 20.5 | 355 | 0.0 |
| 209 | 35.9 | 258 | 45.8 | 307 | 20.2 | 356 | 0.0 |
| 210 | 35.3 | 259 | 45.9 | 308 | 18.6 | 357 | 0.0 |
| 211 | 34.8 | 260 | 46.2 | 309 | 16.5 | 358 | 0.0 |
| 212 | 34.5 | 261 | 46.4 | 310 | 14.4 | 359 | 0.0 |
| 213 | 34.2 | 262 | 46.6 | 311 | 13.4 | 360 | 1.4 |
| 214 | 34.0 | 263 | 46.8 | 312 | 12.9 | 361 | 3.2 |
| 215 | 33.8 | 264 | 47.0 | 313 | 12.7 | 362 | 5.6 |
| 216 | 33.6 | 265 | 47.3 | 314 | 12.4 | 363 | 8.1 |
| 217 | 33.5 | 266 | 47.5 | 315 | 12.4 | 364 | 10.3 |
| 218 | 33.5 | 267 | 47.9 | 316 | 12.8 | 365 | 12.1 |
| 219 | 33.4 | 268 | 48.3 | 317 | 14.1 | 366 | 12.6 |
| 220 | 33.3 | 269 | 48.3 | 318 | 16.2 | 367 | 13.6 |
| 221 | 33.3 | 270 | 48.2 | 319 | 18.8 | 368 | 14.5 |
| 222 | 33.2 | 271 | 48.0 | 320 | 21.9 | 369 | 15.6 |
| 223 | 33.1 | 272 | 47.7 | 321 | 25.0 | 370 | 16.8 |
| 224 | 33.0 | 273 | 47.2 | 322 | 28.4 | 371 | 18.2 |
| 225 | 32.9 | 274 | 46.5 | 323 | 31.3 | 372 | 19.6 |
| 226 | 32.8 | 275 | 45.2 | 324 | 34.0 | 373 | 20.9 |
| 227 | 32.7 | 276 | 43.7 | 325 | 34.6 | 374 | 22.3 |
| 228 | 32.5 | 277 | 42.0 | 326 | 33.9 | 375 | 23.8 |
| 229 | 32.3 | 278 | 40.4 | 327 | 31.9 | 376 | 25.4 |
| 230 | 31.8 | 279 | 39.0 | 328 | 30.0 | 377 | 27.0 |
| 231 | 31.4 | 280 | 37.7 | 329 | 29.0 | 378 | 28.6 |
| 232 | 30.9 | 281 | 36.4 | 330 | 27.9 | 379 | 30.2 |
| 233 | 30.6 | 282 | 35.2 | 331 | 27.1 | 380 | 31.2 |
| 234 | 30.6 | 283 | 34.3 | 332 | 26.4 | 381 | 31.2 |
| 235 | 30.7 | 284 | 33.8 | 333 | 25.9 | 382 | 30.7 |
| 236 | 32.0 | 285 | 33.3 | 334 | 25.5 | 383 | 29.5 |
| 384 | 28.6 | 433 | 0.0 | 482 | 2.5 | 531 | 26.0 |
| 385 | 27.7 | 434 | 0.0 | 483 | 5.2 | 532 | 26.5 |
| 386 | 26.9 | 435 | 0.0 | 484 | 7.9 | 533 | 26.9 |
| 387 | 26.1 | 436 | 0.0 | 485 | 10.3 | 534 | 27.3 |
| 388 | 25.4 | 437 | 0.0 | 486 | 12.7 | 535 | 27.9 |
| 389 | 24.6 | 438 | 0.0 | 487 | 15.0 | 536 | 30.3 |
| 390 | 23.6 | 439 | 0.0 | 488 | 17.4 | 537 | 33.2 |
| 391 | 22.6 | 440 | 0.0 | 489 | 19.7 | 538 | 35.4 |
| 392 | 21.7 | 441 | 0.0 | 490 | 21.9 | 539 | 38.0 |
| 393 | 20.7 | 442 | 0.0 | 491 | 24.1 | 540 | 40.1 |
| 394 | 19.8 | 443 | 0.0 | 492 | 26.2 | 541 | 42.7 |
| 395 | 18.8 | 444 | 0.0 | 493 | 28.1 | 542 | 44.5 |
| 396 | 17.7 | 445 | 0.0 | 494 | 29.7 | 543 | 46.3 |
| 397 | 16.6 | 446 | 0.0 | 495 | 31.3 | 544 | 47.6 |
| 398 | 15.6 | 447 | 0.0 | 496 | 33.0 | 545 | 48.8 |
| 399 | 14.8 | 448 | 0.0 | 497 | 34.7 | 546 | 49.7 |
| 400 | 14.3 | 449 | 0.0 | 498 | 36.3 | 547 | 50.6 |
| 401 | 13.8 | 450 | 0.0 | 499 | 38.1 | 548 | 51.4 |
| 402 | 13.4 | 451 | 0.0 | 500 | 39.4 | 549 | 51.4 |
| 403 | 13.1 | 452 | 0.0 | 501 | 40.4 | 550 | 50.2 |
| 404 | 12.8 | 453 | 0.0 | 502 | 41.2 | 551 | 47.1 |
| 405 | 12.3 | 454 | 0.0 | 503 | 42.1 | 552 | 44.5 |
| 406 | 11.6 | 455 | 0.0 | 504 | 43.2 | 553 | 41.5 |
| 407 | 10.5 | 456 | 0.0 | 505 | 44.3 | 554 | 38.5 |
| 408 | 9.0 | 457 | 0.0 | 506 | 45.7 | 555 | 35.5 |
| 409 | 7.2 | 458 | 0.0 | 507 | 45.4 | 556 | 32.5 |
| 410 | 5.2 | 459 | 0.0 | 508 | 44.5 | 557 | 29.5 |
| 411 | 2.9 | 460 | 0.0 | 509 | 42.5 | 558 | 26.5 |
| 412 | 1.2 | 461 | 0.0 | 510 | 39.5 | 559 | 23.5 |
| 413 | 0.0 | 462 | 0.0 | 511 | 36.5 | 560 | 20.4 |
| 414 | 0.0 | 463 | 0.0 | 512 | 33.5 | 561 | 17.5 |
| 415 | 0.0 | 464 | 0.0 | 513 | 30.4 | 562 | 14.5 |
| 416 | 0.0 | 465 | 0.0 | 514 | 27.0 | 563 | 11.5 |
| 417 | 0.0 | 466 | 0.0 | 515 | 23.6 | 564 | 8.5 |
| 418 | 0.0 | 467 | 0.0 | 516 | 21.0 | 565 | 5.6 |
| 419 | 0.0 | 468 | 0.0 | 517 | 19.5 | 566 | 2.6 |
| 420 | 0.0 | 469 | 0.0 | 518 | 17.6 | 567 | 0.0 |
| 421 | 0.0 | 470 | 0.0 | 519 | 16.1 | 568 | 0.0 |
| 422 | 0.0 | 471 | 0.0 | 520 | 14.5 | 569 | 0.0 |
| 423 | 0.0 | 472 | 0.0 | 521 | 13.5 | 570 | 0.0 |
| 424 | 0.0 | 473 | 0.0 | 522 | 13.7 | 571 | 0.0 |
| 425 | 0.0 | 474 | 0.0 | 523 | 16.0 | 572 | 0.0 |
| 426 | 0.0 | 475 | 0.0 | 524 | 18.1 | 573 | 0.0 |
| 427 | 0.0 | 476 | 0.0 | 525 | 20.8 | 574 | 0.0 |
| 428 | 0.0 | 477 | 0.0 | 526 | 21.5 | 575 | 0.0 |
| 429 | 0.0 | 478 | 0.0 | 527 | 22.5 | 576 | 0.0 |
| 430 | 0.0 | 479 | 0.0 | 528 | 23.4 | 577 | 0.0 |
| 431 | 0.0 | 480 | 0.0 | 529 | 24.5 | 578 | 0.0 |
| 432 | 0.0 | 481 | 1.4 | 530 | 25.6 | 579 | 0.0 |
| 580 | 0.0 |  |  |  |  |  |  |
| 581 | 0.0 |  |  |  |  |  |  |
| 582 | 0.0 |  |  |  |  |  |  |
| 583 | 0.0 |  |  |  |  |  |  |
| 584 | 0.0 |  |  |  |  |  |  |
| 585 | 0.0 |  |  |  |  |  |  |
| 586 | 0.0 |  |  |  |  |  |  |
| 587 | 0.0 |  |  |  |  |  |  |
| 588 | 0.0 |  |  |  |  |  |  |
| 589 | 0.0 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

# Table A1/4

# **WLTC, Class 2 cycle, phase Medium2 (The start of this phase is at second 589)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 590 | 0.0 | 637 | 38.6 | 684 | 59.3 | 731 | 55.3 |
| 591 | 0.0 | 638 | 39.8 | 685 | 60.2 | 732 | 55.1 |
| 592 | 0.0 | 639 | 40.6 | 686 | 61.3 | 733 | 54.8 |
| 593 | 0.0 | 640 | 41.1 | 687 | 62.4 | 734 | 54.6 |
| 594 | 0.0 | 641 | 41.9 | 688 | 63.4 | 735 | 54.5 |
| 595 | 0.0 | 642 | 42.8 | 689 | 64.4 | 736 | 54.3 |
| 596 | 0.0 | 643 | 44.3 | 690 | 65.4 | 737 | 53.9 |
| 597 | 0.0 | 644 | 45.7 | 691 | 66.3 | 738 | 53.4 |
| 598 | 0.0 | 645 | 47.4 | 692 | 67.2 | 739 | 52.6 |
| 599 | 0.0 | 646 | 48.9 | 693 | 68.0 | 740 | 51.5 |
| 600 | 0.0 | 647 | 50.6 | 694 | 68.8 | 741 | 50.2 |
| 601 | 1.6 | 648 | 52.0 | 695 | 69.5 | 742 | 48.7 |
| 602 | 3.6 | 649 | 53.7 | 696 | 70.1 | 743 | 47.0 |
| 603 | 6.3 | 650 | 55.0 | 697 | 70.6 | 744 | 45.1 |
| 604 | 9.0 | 651 | 56.8 | 698 | 71.0 | 745 | 43.0 |
| 605 | 11.8 | 652 | 58.0 | 699 | 71.6 | 746 | 40.6 |
| 606 | 14.2 | 653 | 59.8 | 700 | 72.2 | 747 | 38.1 |
| 607 | 16.6 | 654 | 61.1 | 701 | 72.8 | 748 | 35.4 |
| 608 | 18.5 | 655 | 62.4 | 702 | 73.5 | 749 | 32.7 |
| 609 | 20.8 | 656 | 63.0 | 703 | 74.1 | 750 | 30.0 |
| 610 | 23.4 | 657 | 63.5 | 704 | 74.3 | 751 | 27.5 |
| 611 | 26.9 | 658 | 63.0 | 705 | 74.3 | 752 | 25.3 |
| 612 | 30.3 | 659 | 62.0 | 706 | 73.7 | 753 | 23.4 |
| 613 | 32.8 | 660 | 60.4 | 707 | 71.9 | 754 | 22.0 |
| 614 | 34.1 | 661 | 58.6 | 708 | 70.5 | 755 | 20.8 |
| 615 | 34.2 | 662 | 56.7 | 709 | 68.9 | 756 | 19.8 |
| 616 | 33.6 | 663 | 55.0 | 710 | 67.4 | 757 | 18.9 |
| 617 | 32.1 | 664 | 53.7 | 711 | 66.0 | 758 | 18.0 |
| 618 | 30.0 | 665 | 52.7 | 712 | 64.7 | 759 | 17.0 |
| 619 | 27.5 | 666 | 51.9 | 713 | 63.7 | 760 | 16.1 |
| 620 | 25.1 | 667 | 51.4 | 714 | 62.9 | 761 | 15.5 |
| 621 | 22.8 | 668 | 51.0 | 715 | 62.2 | 762 | 14.4 |
| 622 | 20.5 | 669 | 50.7 | 716 | 61.7 | 763 | 14.9 |
| 623 | 17.9 | 670 | 50.6 | 717 | 61.2 | 764 | 15.9 |
| 624 | 15.1 | 671 | 50.8 | 718 | 60.7 | 765 | 17.1 |
| 625 | 13.4 | 672 | 51.2 | 719 | 60.3 | 766 | 18.3 |
| 626 | 12.8 | 673 | 51.7 | 720 | 59.9 | 767 | 19.4 |
| 627 | 13.7 | 674 | 52.3 | 721 | 59.6 | 768 | 20.4 |
| 628 | 16.0 | 675 | 53.1 | 722 | 59.3 | 769 | 21.2 |
| 629 | 18.1 | 676 | 53.8 | 723 | 59.0 | 770 | 21.9 |
| 630 | 20.8 | 677 | 54.5 | 724 | 58.6 | 771 | 22.7 |
| 631 | 23.7 | 678 | 55.1 | 725 | 58.0 | 772 | 23.4 |
| 632 | 26.5 | 679 | 55.9 | 726 | 57.5 | 773 | 24.2 |
| 633 | 29.3 | 680 | 56.5 | 727 | 56.9 | 774 | 24.3 |
| 634 | 32.0 | 681 | 57.1 | 728 | 56.3 | 775 | 24.2 |
| 635 | 34.5 | 682 | 57.8 | 729 | 55.9 | 776 | 24.1 |
| 636 | 36.8 | 683 | 58.5 | 730 | 55.6 | 777 | 23.8 |
| 778 | 23.0 | 827 | 59.9 | 876 | 46.9 | 925 | 49.0 |
| 779 | 22.6 | 828 | 60.7 | 877 | 47.1 | 926 | 48.5 |
| 780 | 21.7 | 829 | 61.4 | 878 | 47.5 | 927 | 48.0 |
| 781 | 21.3 | 830 | 62.0 | 879 | 47.8 | 928 | 47.5 |
| 782 | 20.3 | 831 | 62.5 | 880 | 48.3 | 929 | 47.0 |
| 783 | 19.1 | 832 | 62.9 | 881 | 48.8 | 930 | 46.9 |
| 784 | 18.1 | 833 | 63.2 | 882 | 49.5 | 931 | 46.8 |
| 785 | 16.9 | 834 | 63.4 | 883 | 50.2 | 932 | 46.8 |
| 786 | 16.0 | 835 | 63.7 | 884 | 50.8 | 933 | 46.8 |
| 787 | 14.8 | 836 | 64.0 | 885 | 51.4 | 934 | 46.9 |
| 788 | 14.5 | 837 | 64.4 | 886 | 51.8 | 935 | 46.9 |
| 789 | 13.7 | 838 | 64.9 | 887 | 51.9 | 936 | 46.9 |
| 790 | 13.5 | 839 | 65.5 | 888 | 51.7 | 937 | 46.9 |
| 791 | 12.9 | 840 | 66.2 | 889 | 51.2 | 938 | 46.9 |
| 792 | 12.7 | 841 | 67.0 | 890 | 50.4 | 939 | 46.8 |
| 793 | 12.5 | 842 | 67.8 | 891 | 49.2 | 940 | 46.6 |
| 794 | 12.5 | 843 | 68.6 | 892 | 47.7 | 941 | 46.4 |
| 795 | 12.6 | 844 | 69.4 | 893 | 46.3 | 942 | 46.0 |
| 796 | 13.0 | 845 | 70.1 | 894 | 45.1 | 943 | 45.5 |
| 797 | 13.6 | 846 | 70.9 | 895 | 44.2 | 944 | 45.0 |
| 798 | 14.6 | 847 | 71.7 | 896 | 43.7 | 945 | 44.5 |
| 799 | 15.7 | 848 | 72.5 | 897 | 43.4 | 946 | 44.2 |
| 800 | 17.1 | 849 | 73.2 | 898 | 43.1 | 947 | 43.9 |
| 801 | 18.7 | 850 | 73.8 | 899 | 42.5 | 948 | 43.7 |
| 802 | 20.2 | 851 | 74.4 | 900 | 41.8 | 949 | 43.6 |
| 803 | 21.9 | 852 | 74.7 | 901 | 41.1 | 950 | 43.6 |
| 804 | 23.6 | 853 | 74.7 | 902 | 40.3 | 951 | 43.5 |
| 805 | 25.4 | 854 | 74.6 | 903 | 39.7 | 952 | 43.5 |
| 806 | 27.1 | 855 | 74.2 | 904 | 39.3 | 953 | 43.4 |
| 807 | 28.9 | 856 | 73.5 | 905 | 39.2 | 954 | 43.3 |
| 808 | 30.4 | 857 | 72.6 | 906 | 39.3 | 955 | 43.1 |
| 809 | 32.0 | 858 | 71.8 | 907 | 39.6 | 956 | 42.9 |
| 810 | 33.4 | 859 | 71.0 | 908 | 40.0 | 957 | 42.7 |
| 811 | 35.0 | 860 | 70.1 | 909 | 40.7 | 958 | 42.5 |
| 812 | 36.4 | 861 | 69.4 | 910 | 41.4 | 959 | 42.4 |
| 813 | 38.1 | 862 | 68.9 | 911 | 42.2 | 960 | 42.2 |
| 814 | 39.7 | 863 | 68.4 | 912 | 43.1 | 961 | 42.1 |
| 815 | 41.6 | 864 | 67.9 | 913 | 44.1 | 962 | 42.0 |
| 816 | 43.3 | 865 | 67.1 | 914 | 44.9 | 963 | 41.8 |
| 817 | 45.1 | 866 | 65.8 | 915 | 45.6 | 964 | 41.7 |
| 818 | 46.9 | 867 | 63.9 | 916 | 46.4 | 965 | 41.5 |
| 819 | 48.7 | 868 | 61.4 | 917 | 47.0 | 966 | 41.3 |
| 820 | 50.5 | 869 | 58.4 | 918 | 47.8 | 967 | 41.1 |
| 821 | 52.4 | 870 | 55.4 | 919 | 48.3 | 968 | 40.8 |
| 822 | 54.1 | 871 | 52.4 | 920 | 48.9 | 969 | 40.3 |
| 823 | 55.7 | 872 | 50.0 | 921 | 49.4 | 970 | 39.6 |
| 824 | 56.8 | 873 | 48.3 | 922 | 49.8 | 971 | 38.5 |
| 825 | 57.9 | 874 | 47.3 | 923 | 49.6 | 972 | 37.0 |
| 826 | 59.0 | 875 | 46.8 | 924 | 49.3 | 973 | 35.1 |
| 974 | 33.0 |  |  |  |  |  |  |
| 975 | 30.6 |  |  |  |  |  |  |
| 976 | 27.9 |  |  |  |  |  |  |
| 977 | 25.1 |  |  |  |  |  |  |
| 978 | 22.0 |  |  |  |  |  |  |
| 979 | 18.8 |  |  |  |  |  |  |
| 980 | 15.5 |  |  |  |  |  |  |
| 981 | 12.3 |  |  |  |  |  |  |
| 982 | 8.8 |  |  |  |  |  |  |
| 983 | 6.0 |  |  |  |  |  |  |
| 984 | 3.6 |  |  |  |  |  |  |
| 985 | 1.6 |  |  |  |  |  |  |
| 986 | 0.0 |  |  |  |  |  |  |
| 987 | 0.0 |  |  |  |  |  |  |
| 988 | 0.0 |  |  |  |  |  |  |
| 989 | 0.0 |  |  |  |  |  |  |
| 990 | 0.0 |  |  |  |  |  |  |
| 991 | 0.0 |  |  |  |  |  |  |
| 992 | 0.0 |  |  |  |  |  |  |
| 993 | 0.0 |  |  |  |  |  |  |
| 994 | 0.0 |  |  |  |  |  |  |
| 995 | 0.0 |  |  |  |  |  |  |
| 996 | 0.0 |  |  |  |  |  |  |
| 997 | 0.0 |  |  |  |  |  |  |
| 998 | 0.0 |  |  |  |  |  |  |
| 999 | 0.0 |  |  |  |  |  |  |
| 1000 | 0.0 |  |  |  |  |  |  |
| 1001 | 0.0 |  |  |  |  |  |  |
| 1002 | 0.0 |  |  |  |  |  |  |
| 1003 | 0.0 |  |  |  |  |  |  |
| 1004 | 0.0 |  |  |  |  |  |  |
| 1005 | 0.0 |  |  |  |  |  |  |
| 1006 | 0.0 |  |  |  |  |  |  |
| 1007 | 0.0 |  |  |  |  |  |  |
| 1008 | 0.0 |  |  |  |  |  |  |
| 1009 | 0.0 |  |  |  |  |  |  |
| 1010 | 0.0 |  |  |  |  |  |  |
| 1011 | 0.0 |  |  |  |  |  |  |
| 1012 | 0.0 |  |  |  |  |  |  |
| 1013 | 0.0 |  |  |  |  |  |  |
| 1014 | 0.0 |  |  |  |  |  |  |
| 1015 | 0.0 |  |  |  |  |  |  |
| 1016 | 0.0 |  |  |  |  |  |  |
| 1017 | 0.0 |  |  |  |  |  |  |
| 1018 | 0.0 |  |  |  |  |  |  |
| 1019 | 0.0 |  |  |  |  |  |  |
| 1020 | 0.0 |  |  |  |  |  |  |
| 1021 | 0.0 |  |  |  |  |  |  |
| 1022 | 0.0 |  |  |  |  |  |  |

# Table A1/5

# **WLTC, Class 2 cycle, phase High2 (Second 1022 is the end of phase Medium2 and the start of phase High2)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1023 | 0.0 | 1070 | 46.0 | 1117 | 73.9 | 1164 | 71.7 |
| 1024 | 0.0 | 1071 | 46.4 | 1118 | 74.9 | 1165 | 69.9 |
| 1025 | 0.0 | 1072 | 47.0 | 1119 | 75.7 | 1166 | 67.9 |
| 1026 | 0.0 | 1073 | 47.4 | 1120 | 76.4 | 1167 | 65.7 |
| 1027 | 1.1 | 1074 | 48.0 | 1121 | 77.1 | 1168 | 63.5 |
| 1028 | 3.0 | 1075 | 48.4 | 1122 | 77.6 | 1169 | 61.2 |
| 1029 | 5.7 | 1076 | 49.0 | 1123 | 78.0 | 1170 | 59.0 |
| 1030 | 8.4 | 1077 | 49.4 | 1124 | 78.2 | 1171 | 56.8 |
| 1031 | 11.1 | 1078 | 50.0 | 1125 | 78.4 | 1172 | 54.7 |
| 1032 | 14.0 | 1079 | 50.4 | 1126 | 78.5 | 1173 | 52.7 |
| 1033 | 17.0 | 1080 | 50.8 | 1127 | 78.5 | 1174 | 50.9 |
| 1034 | 20.1 | 1081 | 51.1 | 1128 | 78.6 | 1175 | 49.4 |
| 1035 | 22.7 | 1082 | 51.3 | 1129 | 78.7 | 1176 | 48.1 |
| 1036 | 23.6 | 1083 | 51.3 | 1130 | 78.9 | 1177 | 47.1 |
| 1037 | 24.5 | 1084 | 51.3 | 1131 | 79.1 | 1178 | 46.5 |
| 1038 | 24.8 | 1085 | 51.3 | 1132 | 79.4 | 1179 | 46.3 |
| 1039 | 25.1 | 1086 | 51.3 | 1133 | 79.8 | 1180 | 46.5 |
| 1040 | 25.3 | 1087 | 51.3 | 1134 | 80.1 | 1181 | 47.2 |
| 1041 | 25.5 | 1088 | 51.3 | 1135 | 80.5 | 1182 | 48.3 |
| 1042 | 25.7 | 1089 | 51.4 | 1136 | 80.8 | 1183 | 49.7 |
| 1043 | 25.8 | 1090 | 51.6 | 1137 | 81.0 | 1184 | 51.3 |
| 1044 | 25.9 | 1091 | 51.8 | 1138 | 81.2 | 1185 | 53.0 |
| 1045 | 26.0 | 1092 | 52.1 | 1139 | 81.3 | 1186 | 54.9 |
| 1046 | 26.1 | 1093 | 52.3 | 1140 | 81.2 | 1187 | 56.7 |
| 1047 | 26.3 | 1094 | 52.6 | 1141 | 81.0 | 1188 | 58.6 |
| 1048 | 26.5 | 1095 | 52.8 | 1142 | 80.6 | 1189 | 60.2 |
| 1049 | 26.8 | 1096 | 52.9 | 1143 | 80.0 | 1190 | 61.6 |
| 1050 | 27.1 | 1097 | 53.0 | 1144 | 79.1 | 1191 | 62.2 |
| 1051 | 27.5 | 1098 | 53.0 | 1145 | 78.0 | 1192 | 62.5 |
| 1052 | 28.0 | 1099 | 53.0 | 1146 | 76.8 | 1193 | 62.8 |
| 1053 | 28.6 | 1100 | 53.1 | 1147 | 75.5 | 1194 | 62.9 |
| 1054 | 29.3 | 1101 | 53.2 | 1148 | 74.1 | 1195 | 63.0 |
| 1055 | 30.4 | 1102 | 53.3 | 1149 | 72.9 | 1196 | 63.0 |
| 1056 | 31.8 | 1103 | 53.4 | 1150 | 71.9 | 1197 | 63.1 |
| 1057 | 33.7 | 1104 | 53.5 | 1151 | 71.2 | 1198 | 63.2 |
| 1058 | 35.8 | 1105 | 53.7 | 1152 | 70.9 | 1199 | 63.3 |
| 1059 | 37.8 | 1106 | 55.0 | 1153 | 71.0 | 1200 | 63.5 |
| 1060 | 39.5 | 1107 | 56.8 | 1154 | 71.5 | 1201 | 63.7 |
| 1061 | 40.8 | 1108 | 58.8 | 1155 | 72.3 | 1202 | 63.9 |
| 1062 | 41.8 | 1109 | 60.9 | 1156 | 73.2 | 1203 | 64.1 |
| 1063 | 42.4 | 1110 | 63.0 | 1157 | 74.1 | 1204 | 64.3 |
| 1064 | 43.0 | 1111 | 65.0 | 1158 | 74.9 | 1205 | 66.1 |
| 1065 | 43.4 | 1112 | 66.9 | 1159 | 75.4 | 1206 | 67.9 |
| 1066 | 44.0 | 1113 | 68.6 | 1160 | 75.5 | 1207 | 69.7 |
| 1067 | 44.4 | 1114 | 70.1 | 1161 | 75.2 | 1208 | 71.4 |
| 1068 | 45.0 | 1115 | 71.5 | 1162 | 74.5 | 1209 | 73.1 |
| 1069 | 45.4 | 1116 | 72.8 | 1163 | 73.3 | 1210 | 74.7 |
| 1211 | 76.2 | 1260 | 35.4 | 1309 | 72.3 | 1358 | 70.8 |
| 1212 | 77.5 | 1261 | 32.7 | 1310 | 71.9 | 1359 | 70.8 |
| 1213 | 78.6 | 1262 | 30.0 | 1311 | 71.3 | 1360 | 70.9 |
| 1214 | 79.7 | 1263 | 29.9 | 1312 | 70.9 | 1361 | 70.9 |
| 1215 | 80.6 | 1264 | 30.0 | 1313 | 70.5 | 1362 | 70.9 |
| 1216 | 81.5 | 1265 | 30.2 | 1314 | 70.0 | 1363 | 70.9 |
| 1217 | 82.2 | 1266 | 30.4 | 1315 | 69.6 | 1364 | 71.0 |
| 1218 | 83.0 | 1267 | 30.6 | 1316 | 69.2 | 1365 | 71.0 |
| 1219 | 83.7 | 1268 | 31.6 | 1317 | 68.8 | 1366 | 71.1 |
| 1220 | 84.4 | 1269 | 33.0 | 1318 | 68.4 | 1367 | 71.2 |
| 1221 | 84.9 | 1270 | 33.9 | 1319 | 67.9 | 1368 | 71.3 |
| 1222 | 85.1 | 1271 | 34.8 | 1320 | 67.5 | 1369 | 71.4 |
| 1223 | 85.2 | 1272 | 35.7 | 1321 | 67.2 | 1370 | 71.5 |
| 1224 | 84.9 | 1273 | 36.6 | 1322 | 66.8 | 1371 | 71.7 |
| 1225 | 84.4 | 1274 | 37.5 | 1323 | 65.6 | 1372 | 71.8 |
| 1226 | 83.6 | 1275 | 38.4 | 1324 | 63.3 | 1373 | 71.9 |
| 1227 | 82.7 | 1276 | 39.3 | 1325 | 60.2 | 1374 | 71.9 |
| 1228 | 81.5 | 1277 | 40.2 | 1326 | 56.2 | 1375 | 71.9 |
| 1229 | 80.1 | 1278 | 40.8 | 1327 | 52.2 | 1376 | 71.9 |
| 1230 | 78.7 | 1279 | 41.7 | 1328 | 48.4 | 1377 | 71.9 |
| 1231 | 77.4 | 1280 | 42.4 | 1329 | 45.0 | 1378 | 71.9 |
| 1232 | 76.2 | 1281 | 43.1 | 1330 | 41.6 | 1379 | 71.9 |
| 1233 | 75.4 | 1282 | 43.6 | 1331 | 38.6 | 1380 | 72.0 |
| 1234 | 74.8 | 1283 | 44.2 | 1332 | 36.4 | 1381 | 72.1 |
| 1235 | 74.3 | 1284 | 44.8 | 1333 | 34.8 | 1382 | 72.4 |
| 1236 | 73.8 | 1285 | 45.5 | 1334 | 34.2 | 1383 | 72.7 |
| 1237 | 73.2 | 1286 | 46.3 | 1335 | 34.7 | 1384 | 73.1 |
| 1238 | 72.4 | 1287 | 47.2 | 1336 | 36.3 | 1385 | 73.4 |
| 1239 | 71.6 | 1288 | 48.1 | 1337 | 38.5 | 1386 | 73.8 |
| 1240 | 70.8 | 1289 | 49.1 | 1338 | 41.0 | 1387 | 74.0 |
| 1241 | 69.9 | 1290 | 50.0 | 1339 | 43.7 | 1388 | 74.1 |
| 1242 | 67.9 | 1291 | 51.0 | 1340 | 46.5 | 1389 | 74.0 |
| 1243 | 65.7 | 1292 | 51.9 | 1341 | 49.1 | 1390 | 73.0 |
| 1244 | 63.5 | 1293 | 52.7 | 1342 | 51.6 | 1391 | 72.0 |
| 1245 | 61.2 | 1294 | 53.7 | 1343 | 53.9 | 1392 | 71.0 |
| 1246 | 59.0 | 1295 | 55.0 | 1344 | 56.0 | 1393 | 70.0 |
| 1247 | 56.8 | 1296 | 56.8 | 1345 | 57.9 | 1394 | 69.0 |
| 1248 | 54.7 | 1297 | 58.8 | 1346 | 59.7 | 1395 | 68.0 |
| 1249 | 52.7 | 1298 | 60.9 | 1347 | 61.2 | 1396 | 67.7 |
| 1250 | 50.9 | 1299 | 63.0 | 1348 | 62.5 | 1397 | 66.7 |
| 1251 | 49.4 | 1300 | 65.0 | 1349 | 63.5 | 1398 | 66.6 |
| 1252 | 48.1 | 1301 | 66.9 | 1350 | 64.3 | 1399 | 66.7 |
| 1253 | 47.1 | 1302 | 68.6 | 1351 | 65.3 | 1400 | 66.8 |
| 1254 | 46.5 | 1303 | 70.1 | 1352 | 66.3 | 1401 | 66.9 |
| 1255 | 46.3 | 1304 | 71.0 | 1353 | 67.3 | 1402 | 66.9 |
| 1256 | 45.1 | 1305 | 71.8 | 1354 | 68.3 | 1403 | 66.9 |
| 1257 | 43.0 | 1306 | 72.8 | 1355 | 69.3 | 1404 | 66.9 |
| 1258 | 40.6 | 1307 | 72.9 | 1356 | 70.3 | 1405 | 66.9 |
| 1259 | 38.1 | 1308 | 73.0 | 1357 | 70.8 | 1406 | 66.9 |
| 1407 | 66.9 | 1456 | 0.0 |  |  |  |  |
| 1408 | 67.0 | 1457 | 0.0 |  |  |  |  |
| 1409 | 67.1 | 1458 | 0.0 |  |  |  |  |
| 1410 | 67.3 | 1459 | 0.0 |  |  |  |  |
| 1411 | 67.5 | 1460 | 0.0 |  |  |  |  |
| 1412 | 67.8 | 1461 | 0.0 |  |  |  |  |
| 1413 | 68.2 | 1462 | 0.0 |  |  |  |  |
| 1414 | 68.6 | 1463 | 0.0 |  |  |  |  |
| 1415 | 69.0 | 1464 | 0.0 |  |  |  |  |
| 1416 | 69.3 | 1465 | 0.0 |  |  |  |  |
| 1417 | 69.3 | 1466 | 0.0 |  |  |  |  |
| 1418 | 69.2 | 1467 | 0.0 |  |  |  |  |
| 1419 | 68.8 | 1468 | 0.0 |  |  |  |  |
| 1420 | 68.2 | 1469 | 0.0 |  |  |  |  |
| 1421 | 67.6 | 1470 | 0.0 |  |  |  |  |
| 1422 | 67.4 | 1471 | 0.0 |  |  |  |  |
| 1423 | 67.2 | 1472 | 0.0 |  |  |  |  |
| 1424 | 66.9 | 1473 | 0.0 |  |  |  |  |
| 1425 | 66.3 | 1474 | 0.0 |  |  |  |  |
| 1426 | 65.4 | 1475 | 0.0 |  |  |  |  |
| 1427 | 64.0 | 1476 | 0.0 |  |  |  |  |
| 1428 | 62.4 | 1477 | 0.0 |  |  |  |  |
| 1429 | 60.6 |  |  |  |  |  |  |
| 1430 | 58.6 |  |  |  |  |  |  |
| 1431 | 56.7 |  |  |  |  |  |  |
| 1432 | 54.8 |  |  |  |  |  |  |
| 1433 | 53.0 |  |  |  |  |  |  |
| 1434 | 51.3 |  |  |  |  |  |  |
| 1435 | 49.6 |  |  |  |  |  |  |
| 1436 | 47.8 |  |  |  |  |  |  |
| 1437 | 45.5 |  |  |  |  |  |  |
| 1438 | 42.8 |  |  |  |  |  |  |
| 1439 | 39.8 |  |  |  |  |  |  |
| 1440 | 36.5 |  |  |  |  |  |  |
| 1441 | 33.0 |  |  |  |  |  |  |
| 1442 | 29.5 |  |  |  |  |  |  |
| 1443 | 25.8 |  |  |  |  |  |  |
| 1444 | 22.1 |  |  |  |  |  |  |
| 1445 | 18.6 |  |  |  |  |  |  |
| 1446 | 15.3 |  |  |  |  |  |  |
| 1447 | 12.4 |  |  |  |  |  |  |
| 1448 | 9.6 |  |  |  |  |  |  |
| 1449 | 6.6 |  |  |  |  |  |  |
| 1450 | 3.8 |  |  |  |  |  |  |
| 1451 | 1.6 |  |  |  |  |  |  |
| 1452 | 0.0 |  |  |  |  |  |  |
| 1453 | 0.0 |  |  |  |  |  |  |
| 1454 | 0.0 |  |  |  |  |  |  |
| 1455 | 0.0 |  |  |  |  |  |  |

# Table A1/6

# **WLTC, Class 2 cycle, phase Extra High2 (Second 1477 is the end of phase High2 and the start of Extra High2)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1478 | 0.0 | 1525 | 63.4 | 1572 | 107.4 | 1619 | 113.7 |
| 1479 | 1.1 | 1526 | 64.5 | 1573 | 108.7 | 1620 | 114.1 |
| 1480 | 2.3 | 1527 | 65.7 | 1574 | 109.9 | 1621 | 114.4 |
| 1481 | 4.6 | 1528 | 66.9 | 1575 | 111.2 | 1622 | 114.6 |
| 1482 | 6.5 | 1529 | 68.1 | 1576 | 112.3 | 1623 | 114.7 |
| 1483 | 8.9 | 1530 | 69.1 | 1577 | 113.4 | 1624 | 114.7 |
| 1484 | 10.9 | 1531 | 70.0 | 1578 | 114.4 | 1625 | 114.7 |
| 1485 | 13.5 | 1532 | 70.9 | 1579 | 115.3 | 1626 | 114.6 |
| 1486 | 15.2 | 1533 | 71.8 | 1580 | 116.1 | 1627 | 114.5 |
| 1487 | 17.6 | 1534 | 72.6 | 1581 | 116.8 | 1628 | 114.5 |
| 1488 | 19.3 | 1535 | 73.4 | 1582 | 117.4 | 1629 | 114.5 |
| 1489 | 21.4 | 1536 | 74.0 | 1583 | 117.7 | 1630 | 114.7 |
| 1490 | 23.0 | 1537 | 74.7 | 1584 | 118.2 | 1631 | 115.0 |
| 1491 | 25.0 | 1538 | 75.2 | 1585 | 118.1 | 1632 | 115.6 |
| 1492 | 26.5 | 1539 | 75.7 | 1586 | 117.7 | 1633 | 116.4 |
| 1493 | 28.4 | 1540 | 76.4 | 1587 | 117.0 | 1634 | 117.3 |
| 1494 | 29.8 | 1541 | 77.2 | 1588 | 116.1 | 1635 | 118.2 |
| 1495 | 31.7 | 1542 | 78.2 | 1589 | 115.2 | 1636 | 118.8 |
| 1496 | 33.7 | 1543 | 78.9 | 1590 | 114.4 | 1637 | 119.3 |
| 1497 | 35.8 | 1544 | 79.9 | 1591 | 113.6 | 1638 | 119.6 |
| 1498 | 38.1 | 1545 | 81.1 | 1592 | 113.0 | 1639 | 119.7 |
| 1499 | 40.5 | 1546 | 82.4 | 1593 | 112.6 | 1640 | 119.5 |
| 1500 | 42.2 | 1547 | 83.7 | 1594 | 112.2 | 1641 | 119.3 |
| 1501 | 43.5 | 1548 | 85.4 | 1595 | 111.9 | 1642 | 119.2 |
| 1502 | 44.5 | 1549 | 87.0 | 1596 | 111.6 | 1643 | 119.0 |
| 1503 | 45.2 | 1550 | 88.3 | 1597 | 111.2 | 1644 | 118.8 |
| 1504 | 45.8 | 1551 | 89.5 | 1598 | 110.7 | 1645 | 118.8 |
| 1505 | 46.6 | 1552 | 90.5 | 1599 | 110.1 | 1646 | 118.8 |
| 1506 | 47.4 | 1553 | 91.3 | 1600 | 109.3 | 1647 | 118.8 |
| 1507 | 48.5 | 1554 | 92.2 | 1601 | 108.4 | 1648 | 118.8 |
| 1508 | 49.7 | 1555 | 93.0 | 1602 | 107.4 | 1649 | 118.9 |
| 1509 | 51.3 | 1556 | 93.8 | 1603 | 106.7 | 1650 | 119.0 |
| 1510 | 52.9 | 1557 | 94.6 | 1604 | 106.3 | 1651 | 119.0 |
| 1511 | 54.3 | 1558 | 95.3 | 1605 | 106.2 | 1652 | 119.1 |
| 1512 | 55.6 | 1559 | 95.9 | 1606 | 106.4 | 1653 | 119.2 |
| 1513 | 56.8 | 1560 | 96.6 | 1607 | 107.0 | 1654 | 119.4 |
| 1514 | 57.9 | 1561 | 97.4 | 1608 | 107.5 | 1655 | 119.6 |
| 1515 | 58.9 | 1562 | 98.1 | 1609 | 107.9 | 1656 | 119.9 |
| 1516 | 59.7 | 1563 | 98.7 | 1610 | 108.4 | 1657 | 120.1 |
| 1517 | 60.3 | 1564 | 99.5 | 1611 | 108.9 | 1658 | 120.3 |
| 1518 | 60.7 | 1565 | 100.3 | 1612 | 109.5 | 1659 | 120.4 |
| 1519 | 60.9 | 1566 | 101.1 | 1613 | 110.2 | 1660 | 120.5 |
| 1520 | 61.0 | 1567 | 101.9 | 1614 | 110.9 | 1661 | 120.5 |
| 1521 | 61.1 | 1568 | 102.8 | 1615 | 111.6 | 1662 | 120.5 |
| 1522 | 61.4 | 1569 | 103.8 | 1616 | 112.2 | 1663 | 120.5 |
| 1523 | 61.8 | 1570 | 105.0 | 1617 | 112.8 | 1664 | 120.4 |
| 1524 | 62.5 | 1571 | 106.1 | 1618 | 113.3 | 1665 | 120.3 |
| 1666 | 120.1 | 1715 | 120.4 | 1764 | 82.6 |  |  |
| 1667 | 119.9 | 1716 | 120.8 | 1765 | 81.9 |  |  |
| 1668 | 119.6 | 1717 | 121.1 | 1766 | 81.1 |  |  |
| 1669 | 119.5 | 1718 | 121.6 | 1767 | 80.0 |  |  |
| 1670 | 119.4 | 1719 | 121.8 | 1768 | 78.7 |  |  |
| 1671 | 119.3 | 1720 | 122.1 | 1769 | 76.9 |  |  |
| 1672 | 119.3 | 1721 | 122.4 | 1770 | 74.6 |  |  |
| 1673 | 119.4 | 1722 | 122.7 | 1771 | 72.0 |  |  |
| 1674 | 119.5 | 1723 | 122.8 | 1772 | 69.0 |  |  |
| 1675 | 119.5 | 1724 | 123.1 | 1773 | 65.6 |  |  |
| 1676 | 119.6 | 1725 | 123.1 | 1774 | 62.1 |  |  |
| 1677 | 119.6 | 1726 | 122.8 | 1775 | 58.5 |  |  |
| 1678 | 119.6 | 1727 | 122.3 | 1776 | 54.7 |  |  |
| 1679 | 119.4 | 1728 | 121.3 | 1777 | 50.9 |  |  |
| 1680 | 119.3 | 1729 | 119.9 | 1778 | 47.3 |  |  |
| 1681 | 119.0 | 1730 | 118.1 | 1779 | 43.8 |  |  |
| 1682 | 118.8 | 1731 | 115.9 | 1780 | 40.4 |  |  |
| 1683 | 118.7 | 1732 | 113.5 | 1781 | 37.4 |  |  |
| 1684 | 118.8 | 1733 | 111.1 | 1782 | 34.3 |  |  |
| 1685 | 119.0 | 1734 | 108.6 | 1783 | 31.3 |  |  |
| 1686 | 119.2 | 1735 | 106.2 | 1784 | 28.3 |  |  |
| 1687 | 119.6 | 1736 | 104.0 | 1785 | 25.2 |  |  |
| 1688 | 120.0 | 1737 | 101.1 | 1786 | 22.0 |  |  |
| 1689 | 120.3 | 1738 | 98.3 | 1787 | 18.9 |  |  |
| 1690 | 120.5 | 1739 | 95.7 | 1788 | 16.1 |  |  |
| 1691 | 120.7 | 1740 | 93.5 | 1789 | 13.4 |  |  |
| 1692 | 120.9 | 1741 | 91.5 | 1790 | 11.1 |  |  |
| 1693 | 121.0 | 1742 | 90.7 | 1791 | 8.9 |  |  |
| 1694 | 121.1 | 1743 | 90.4 | 1792 | 6.9 |  |  |
| 1695 | 121.2 | 1744 | 90.2 | 1793 | 4.9 |  |  |
| 1696 | 121.3 | 1745 | 90.2 | 1794 | 2.8 |  |  |
| 1697 | 121.4 | 1746 | 90.1 | 1795 | 0.0 |  |  |
| 1698 | 121.5 | 1747 | 90.0 | 1796 | 0.0 |  |  |
| 1699 | 121.5 | 1748 | 89.8 | 1797 | 0.0 |  |  |
| 1700 | 121.5 | 1749 | 89.6 | 1798 | 0.0 |  |  |
| 1701 | 121.4 | 1750 | 89.4 | 1799 | 0.0 |  |  |
| 1702 | 121.3 | 1751 | 89.2 | 1800 | 0.0 |  |  |
| 1703 | 121.1 | 1752 | 88.9 |  |  |  |  |
| 1704 | 120.9 | 1753 | 88.5 |  |  |  |  |
| 1705 | 120.6 | 1754 | 88.1 |  |  |  |  |
| 1706 | 120.4 | 1755 | 87.6 |  |  |  |  |
| 1707 | 120.2 | 1756 | 87.1 |  |  |  |  |
| 1708 | 120.1 | 1757 | 86.6 |  |  |  |  |
| 1709 | 119.9 | 1758 | 86.1 |  |  |  |  |
| 1710 | 119.8 | 1759 | 85.5 |  |  |  |  |
| 1711 | 119.8 | 1760 | 85.0 |  |  |  |  |
| 1712 | 119.9 | 1761 | 84.4 |  |  |  |  |
| 1713 | 120.0 | 1762 | 83.8 |  |  |  |  |
| 1714 | 120.2 | 1763 | 83.2 |  |  |  |  |

6. WLTC Class 3 cycle

# Figure A1/7

# **WLTC, Class 3 cycle, phase Low3**

# 


# Figure A1/8

# **WLTC, Class 3a cycle, phase Medium3a**

# 


# Figure A1/9

# **WLTC, Class 3b cycle, phase Medium3b**




# Figure A1/10

# **WLTC, Class 3a cycle, phase High3a**




# Figure A1/11

# **WLTC, Class 3b cycle, phase High3b**



# Figure A1/12

# **WLTC, Class 3 cycle, phase Extra High3**



# Table A1/7

# **WLTC, Class 3 cycle, phase Low3 (Second 589 is the end of phase Low3 and the start of phase Medium3)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 0 | 0.0 | 47 | 19.5 | 94 | 12.0 | 141 | 11.7 |
| 1 | 0.0 | 48 | 18.4 | 95 | 9.1 | 142 | 16.4 |
| 2 | 0.0 | 49 | 17.8 | 96 | 5.8 | 143 | 18.9 |
| 3 | 0.0 | 50 | 17.8 | 97 | 3.6 | 144 | 19.9 |
| 4 | 0.0 | 51 | 17.4 | 98 | 2.2 | 145 | 20.8 |
| 5 | 0.0 | 52 | 15.7 | 99 | 0.0 | 146 | 22.8 |
| 6 | 0.0 | 53 | 13.1 | 100 | 0.0 | 147 | 25.4 |
| 7 | 0.0 | 54 | 12.1 | 101 | 0.0 | 148 | 27.7 |
| 8 | 0.0 | 55 | 12.0 | 102 | 0.0 | 149 | 29.2 |
| 9 | 0.0 | 56 | 12.0 | 103 | 0.0 | 150 | 29.8 |
| 10 | 0.0 | 57 | 12.0 | 104 | 0.0 | 151 | 29.4 |
| 11 | 0.0 | 58 | 12.3 | 105 | 0.0 | 152 | 27.2 |
| 12 | 0.2 | 59 | 12.6 | 106 | 0.0 | 153 | 22.6 |
| 13 | 1.7 | 60 | 14.7 | 107 | 0.0 | 154 | 17.3 |
| 14 | 5.4 | 61 | 15.3 | 108 | 0.0 | 155 | 13.3 |
| 15 | 9.9 | 62 | 15.9 | 109 | 0.0 | 156 | 12.0 |
| 16 | 13.1 | 63 | 16.2 | 110 | 0.0 | 157 | 12.6 |
| 17 | 16.9 | 64 | 17.1 | 111 | 0.0 | 158 | 14.1 |
| 18 | 21.7 | 65 | 17.8 | 112 | 0.0 | 159 | 17.2 |
| 19 | 26.0 | 66 | 18.1 | 113 | 0.0 | 160 | 20.1 |
| 20 | 27.5 | 67 | 18.4 | 114 | 0.0 | 161 | 23.4 |
| 21 | 28.1 | 68 | 20.3 | 115 | 0.0 | 162 | 25.5 |
| 22 | 28.3 | 69 | 23.2 | 116 | 0.0 | 163 | 27.6 |
| 23 | 28.8 | 70 | 26.5 | 117 | 0.0 | 164 | 29.5 |
| 24 | 29.1 | 71 | 29.8 | 118 | 0.0 | 165 | 31.1 |
| 25 | 30.8 | 72 | 32.6 | 119 | 0.0 | 166 | 32.1 |
| 26 | 31.9 | 73 | 34.4 | 120 | 0.0 | 167 | 33.2 |
| 27 | 34.1 | 74 | 35.5 | 121 | 0.0 | 168 | 35.2 |
| 28 | 36.6 | 75 | 36.4 | 122 | 0.0 | 169 | 37.2 |
| 29 | 39.1 | 76 | 37.4 | 123 | 0.0 | 170 | 38.0 |
| 30 | 41.3 | 77 | 38.5 | 124 | 0.0 | 171 | 37.4 |
| 31 | 42.5 | 78 | 39.3 | 125 | 0.0 | 172 | 35.1 |
| 32 | 43.3 | 79 | 39.5 | 126 | 0.0 | 173 | 31.0 |
| 33 | 43.9 | 80 | 39.0 | 127 | 0.0 | 174 | 27.1 |
| 34 | 44.4 | 81 | 38.5 | 128 | 0.0 | 175 | 25.3 |
| 35 | 44.5 | 82 | 37.3 | 129 | 0.0 | 176 | 25.1 |
| 36 | 44.2 | 83 | 37.0 | 130 | 0.0 | 177 | 25.9 |
| 37 | 42.7 | 84 | 36.7 | 131 | 0.0 | 178 | 27.8 |
| 38 | 39.9 | 85 | 35.9 | 132 | 0.0 | 179 | 29.2 |
| 39 | 37.0 | 86 | 35.3 | 133 | 0.0 | 180 | 29.6 |
| 40 | 34.6 | 87 | 34.6 | 134 | 0.0 | 181 | 29.5 |
| 41 | 32.3 | 88 | 34.2 | 135 | 0.0 | 182 | 29.2 |
| 42 | 29.0 | 89 | 31.9 | 136 | 0.0 | 183 | 28.3 |
| 43 | 25.1 | 90 | 27.3 | 137 | 0.0 | 184 | 26.1 |
| 44 | 22.2 | 91 | 22.0 | 138 | 0.2 | 185 | 23.6 |
| 45 | 20.9 | 92 | 17.0 | 139 | 1.9 | 186 | 21.0 |
| 46 | 20.4 | 93 | 14.2 | 140 | 6.1 | 187 | 18.9 |
| 188 | 17.1 | 237 | 49.2 | 286 | 37.4 | 335 | 15.0 |
| 189 | 15.7 | 238 | 48.4 | 287 | 40.7 | 336 | 14.5 |
| 190 | 14.5 | 239 | 46.9 | 288 | 44.0 | 337 | 14.3 |
| 191 | 13.7 | 240 | 44.3 | 289 | 47.3 | 338 | 14.5 |
| 192 | 12.9 | 241 | 41.5 | 290 | 49.2 | 339 | 15.4 |
| 193 | 12.5 | 242 | 39.5 | 291 | 49.8 | 340 | 17.8 |
| 194 | 12.2 | 243 | 37.0 | 292 | 49.2 | 341 | 21.1 |
| 195 | 12.0 | 244 | 34.6 | 293 | 48.1 | 342 | 24.1 |
| 196 | 12.0 | 245 | 32.3 | 294 | 47.3 | 343 | 25.0 |
| 197 | 12.0 | 246 | 29.0 | 295 | 46.8 | 344 | 25.3 |
| 198 | 12.0 | 247 | 25.1 | 296 | 46.7 | 345 | 25.5 |
| 199 | 12.5 | 248 | 22.2 | 297 | 46.8 | 346 | 26.4 |
| 200 | 13.0 | 249 | 20.9 | 298 | 47.1 | 347 | 26.6 |
| 201 | 14.0 | 250 | 20.4 | 299 | 47.3 | 348 | 27.1 |
| 202 | 15.0 | 251 | 19.5 | 300 | 47.3 | 349 | 27.7 |
| 203 | 16.5 | 252 | 18.4 | 301 | 47.1 | 350 | 28.1 |
| 204 | 19.0 | 253 | 17.8 | 302 | 46.6 | 351 | 28.2 |
| 205 | 21.2 | 254 | 17.8 | 303 | 45.8 | 352 | 28.1 |
| 206 | 23.8 | 255 | 17.4 | 304 | 44.8 | 353 | 28.0 |
| 207 | 26.9 | 256 | 15.7 | 305 | 43.3 | 354 | 27.9 |
| 208 | 29.6 | 257 | 14.5 | 306 | 41.8 | 355 | 27.9 |
| 209 | 32.0 | 258 | 15.4 | 307 | 40.8 | 356 | 28.1 |
| 210 | 35.2 | 259 | 17.9 | 308 | 40.3 | 357 | 28.2 |
| 211 | 37.5 | 260 | 20.6 | 309 | 40.1 | 358 | 28.0 |
| 212 | 39.2 | 261 | 23.2 | 310 | 39.7 | 359 | 26.9 |
| 213 | 40.5 | 262 | 25.7 | 311 | 39.2 | 360 | 25.0 |
| 214 | 41.6 | 263 | 28.7 | 312 | 38.5 | 361 | 23.2 |
| 215 | 43.1 | 264 | 32.5 | 313 | 37.4 | 362 | 21.9 |
| 216 | 45.0 | 265 | 36.1 | 314 | 36.0 | 363 | 21.1 |
| 217 | 47.1 | 266 | 39.0 | 315 | 34.4 | 364 | 20.7 |
| 218 | 49.0 | 267 | 40.8 | 316 | 33.0 | 365 | 20.7 |
| 219 | 50.6 | 268 | 42.9 | 317 | 31.7 | 366 | 20.8 |
| 220 | 51.8 | 269 | 44.4 | 318 | 30.0 | 367 | 21.2 |
| 221 | 52.7 | 270 | 45.9 | 319 | 28.0 | 368 | 22.1 |
| 222 | 53.1 | 271 | 46.0 | 320 | 26.1 | 369 | 23.5 |
| 223 | 53.5 | 272 | 45.6 | 321 | 25.6 | 370 | 24.3 |
| 224 | 53.8 | 273 | 45.3 | 322 | 24.9 | 371 | 24.5 |
| 225 | 54.2 | 274 | 43.7 | 323 | 24.9 | 372 | 23.8 |
| 226 | 54.8 | 275 | 40.8 | 324 | 24.3 | 373 | 21.3 |
| 227 | 55.3 | 276 | 38.0 | 325 | 23.9 | 374 | 17.7 |
| 228 | 55.8 | 277 | 34.4 | 326 | 23.9 | 375 | 14.4 |
| 229 | 56.2 | 278 | 30.9 | 327 | 23.6 | 376 | 11.9 |
| 230 | 56.5 | 279 | 25.5 | 328 | 23.3 | 377 | 10.2 |
| 231 | 56.5 | 280 | 21.4 | 329 | 20.5 | 378 | 8.9 |
| 232 | 56.2 | 281 | 20.2 | 330 | 17.5 | 379 | 8.0 |
| 233 | 54.9 | 282 | 22.9 | 331 | 16.9 | 380 | 7.2 |
| 234 | 52.9 | 283 | 26.6 | 332 | 16.7 | 381 | 6.1 |
| 235 | 51.0 | 284 | 30.2 | 333 | 15.9 | 382 | 4.9 |
| 236 | 49.8 | 285 | 34.1 | 334 | 15.6 | 383 | 3.7 |
| 384 | 2.3 | 433 | 31.3 | 482 | 0.0 | 531 | 0.0 |
| 385 | 0.9 | 434 | 31.1 | 483 | 0.0 | 532 | 0.0 |
| 386 | 0.0 | 435 | 30.6 | 484 | 0.0 | 533 | 0.2 |
| 387 | 0.0 | 436 | 29.2 | 485 | 0.0 | 534 | 1.2 |
| 388 | 0.0 | 437 | 26.7 | 486 | 0.0 | 535 | 3.2 |
| 389 | 0.0 | 438 | 23.0 | 487 | 0.0 | 536 | 5.2 |
| 390 | 0.0 | 439 | 18.2 | 488 | 0.0 | 537 | 8.2 |
| 391 | 0.0 | 440 | 12.9 | 489 | 0.0 | 538 | 13 |
| 392 | 0.5 | 441 | 7.7 | 490 | 0.0 | 539 | 18.8 |
| 393 | 2.1 | 442 | 3.8 | 491 | 0.0 | 540 | 23.1 |
| 394 | 4.8 | 443 | 1.3 | 492 | 0.0 | 541 | 24.5 |
| 395 | 8.3 | 444 | 0.2 | 493 | 0.0 | 542 | 24.5 |
| 396 | 12.3 | 445 | 0.0 | 494 | 0.0 | 543 | 24.3 |
| 397 | 16.6 | 446 | 0.0 | 495 | 0.0 | 544 | 23.6 |
| 398 | 20.9 | 447 | 0.0 | 496 | 0.0 | 545 | 22.3 |
| 399 | 24.2 | 448 | 0.0 | 497 | 0.0 | 546 | 20.1 |
| 400 | 25.6 | 449 | 0.0 | 498 | 0.0 | 547 | 18.5 |
| 401 | 25.6 | 450 | 0.0 | 499 | 0.0 | 548 | 17.2 |
| 402 | 24.9 | 451 | 0.0 | 500 | 0.0 | 549 | 16.3 |
| 403 | 23.3 | 452 | 0.0 | 501 | 0.0 | 550 | 15.4 |
| 404 | 21.6 | 453 | 0.0 | 502 | 0.0 | 551 | 14.7 |
| 405 | 20.2 | 454 | 0.0 | 503 | 0.0 | 552 | 14.3 |
| 406 | 18.7 | 455 | 0.0 | 504 | 0.0 | 553 | 13.7 |
| 407 | 17.0 | 456 | 0.0 | 505 | 0.0 | 554 | 13.3 |
| 408 | 15.3 | 457 | 0.0 | 506 | 0.0 | 555 | 13.1 |
| 409 | 14.2 | 458 | 0.0 | 507 | 0.0 | 556 | 13.1 |
| 410 | 13.9 | 459 | 0.0 | 508 | 0.0 | 557 | 13.3 |
| 411 | 14.0 | 460 | 0.0 | 509 | 0.0 | 558 | 13.8 |
| 412 | 14.2 | 461 | 0.0 | 510 | 0.0 | 559 | 14.5 |
| 413 | 14.5 | 462 | 0.0 | 511 | 0.0 | 560 | 16.5 |
| 414 | 14.9 | 463 | 0.0 | 512 | 0.5 | 561 | 17.0 |
| 415 | 15.9 | 464 | 0.0 | 513 | 2.5 | 562 | 17.0 |
| 416 | 17.4 | 465 | 0.0 | 514 | 6.6 | 563 | 17.0 |
| 417 | 18.7 | 466 | 0.0 | 515 | 11.8 | 564 | 15.4 |
| 418 | 19.1 | 467 | 0.0 | 516 | 16.8 | 565 | 10.1 |
| 419 | 18.8 | 468 | 0.0 | 517 | 20.5 | 566 | 4.8 |
| 420 | 17.6 | 469 | 0.0 | 518 | 21.9 | 567 | 0.0 |
| 421 | 16.6 | 470 | 0.0 | 519 | 21.9 | 568 | 0.0 |
| 422 | 16.2 | 471 | 0.0 | 520 | 21.3 | 569 | 0.0 |
| 423 | 16.4 | 472 | 0.0 | 521 | 20.3 | 570 | 0.0 |
| 424 | 17.2 | 473 | 0.0 | 522 | 19.2 | 571 | 0.0 |
| 425 | 19.1 | 474 | 0.0 | 523 | 17.8 | 572 | 0.0 |
| 426 | 22.6 | 475 | 0.0 | 524 | 15.5 | 573 | 0.0 |
| 427 | 27.4 | 476 | 0.0 | 525 | 11.9 | 574 | 0.0 |
| 428 | 31.6 | 477 | 0.0 | 526 | 7.6 | 575 | 0.0 |
| 429 | 33.4 | 478 | 0.0 | 527 | 4.0 | 576 | 0.0 |
| 430 | 33.5 | 479 | 0.0 | 528 | 2.0 | 577 | 0.0 |
| 431 | 32.8 | 480 | 0.0 | 529 | 1.0 | 578 | 0.0 |
| 432 | 31.9 | 481 | 0.0 | 530 | 0.0 | 579 | 0.0 |
| 580 | 0.0 |  |  |  |  |  |  |
| 581 | 0.0 |  |  |  |  |  |  |
| 582 | 0.0 |  |  |  |  |  |  |
| 583 | 0.0 |  |  |  |  |  |  |
| 584 | 0.0 |  |  |  |  |  |  |
| 585 | 0.0 |  |  |  |  |  |  |
| 586 | 0.0 |  |  |  |  |  |  |
| 587 | 0.0 |  |  |  |  |  |  |
| 588 | 0.0 |  |  |  |  |  |  |
| 589 | 0.0 |  |  |  |  |  |  |

# Table A1/8

# **WLTC, Class 3a cycle, phase Medium3a (Second 589 is the end of phase Low3 and the start of phase Medium3a)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 590 | 0.0 | 637 | 53.0 | 684 | 18.9 | 731 | 41.9 |
| 591 | 0.0 | 638 | 53.0 | 685 | 18.9 | 732 | 42.0 |
| 592 | 0.0 | 639 | 52.9 | 686 | 21.3 | 733 | 42.2 |
| 593 | 0.0 | 640 | 52.7 | 687 | 23.9 | 734 | 42.4 |
| 594 | 0.0 | 641 | 52.6 | 688 | 25.9 | 735 | 42.7 |
| 595 | 0.0 | 642 | 53.1 | 689 | 28.4 | 736 | 43.1 |
| 596 | 0.0 | 643 | 54.3 | 690 | 30.3 | 737 | 43.7 |
| 597 | 0.0 | 644 | 55.2 | 691 | 30.9 | 738 | 44.0 |
| 598 | 0.0 | 645 | 55.5 | 692 | 31.1 | 739 | 44.1 |
| 599 | 0.0 | 646 | 55.9 | 693 | 31.8 | 740 | 45.3 |
| 600 | 0.0 | 647 | 56.3 | 694 | 32.7 | 741 | 46.4 |
| 601 | 1.0 | 648 | 56.7 | 695 | 33.2 | 742 | 47.2 |
| 602 | 2.1 | 649 | 56.9 | 696 | 32.4 | 743 | 47.3 |
| 603 | 5.2 | 650 | 56.8 | 697 | 28.3 | 744 | 47.4 |
| 604 | 9.2 | 651 | 56.0 | 698 | 25.8 | 745 | 47.4 |
| 605 | 13.5 | 652 | 54.2 | 699 | 23.1 | 746 | 47.5 |
| 606 | 18.1 | 653 | 52.1 | 700 | 21.8 | 747 | 47.9 |
| 607 | 22.3 | 654 | 50.1 | 701 | 21.2 | 748 | 48.6 |
| 608 | 26.0 | 655 | 47.2 | 702 | 21.0 | 749 | 49.4 |
| 609 | 29.3 | 656 | 43.2 | 703 | 21.0 | 750 | 49.8 |
| 610 | 32.8 | 657 | 39.2 | 704 | 20.9 | 751 | 49.8 |
| 611 | 36.0 | 658 | 36.5 | 705 | 19.9 | 752 | 49.7 |
| 612 | 39.2 | 659 | 34.3 | 706 | 17.9 | 753 | 49.3 |
| 613 | 42.5 | 660 | 31.0 | 707 | 15.1 | 754 | 48.5 |
| 614 | 45.7 | 661 | 26.0 | 708 | 12.8 | 755 | 47.6 |
| 615 | 48.2 | 662 | 20.7 | 709 | 12.0 | 756 | 46.3 |
| 616 | 48.4 | 663 | 15.4 | 710 | 13.2 | 757 | 43.7 |
| 617 | 48.2 | 664 | 13.1 | 711 | 17.1 | 758 | 39.3 |
| 618 | 47.8 | 665 | 12.0 | 712 | 21.1 | 759 | 34.1 |
| 619 | 47.0 | 666 | 12.5 | 713 | 21.8 | 760 | 29.0 |
| 620 | 45.9 | 667 | 14.0 | 714 | 21.2 | 761 | 23.7 |
| 621 | 44.9 | 668 | 19.0 | 715 | 18.5 | 762 | 18.4 |
| 622 | 44.4 | 669 | 23.2 | 716 | 13.9 | 763 | 14.3 |
| 623 | 44.3 | 670 | 28.0 | 717 | 12.0 | 764 | 12.0 |
| 624 | 44.5 | 671 | 32.0 | 718 | 12.0 | 765 | 12.8 |
| 625 | 45.1 | 672 | 34.0 | 719 | 13.0 | 766 | 16.0 |
| 626 | 45.7 | 673 | 36.0 | 720 | 16.3 | 767 | 20.4 |
| 627 | 46.0 | 674 | 38.0 | 721 | 20.5 | 768 | 24.0 |
| 628 | 46.0 | 675 | 40.0 | 722 | 23.9 | 769 | 29.0 |
| 629 | 46.0 | 676 | 40.3 | 723 | 26.0 | 770 | 32.2 |
| 630 | 46.1 | 677 | 40.5 | 724 | 28.0 | 771 | 36.8 |
| 631 | 46.7 | 678 | 39.0 | 725 | 31.5 | 772 | 39.4 |
| 632 | 47.7 | 679 | 35.7 | 726 | 33.4 | 773 | 43.2 |
| 633 | 48.9 | 680 | 31.8 | 727 | 36.0 | 774 | 45.8 |
| 634 | 50.3 | 681 | 27.1 | 728 | 37.8 | 775 | 49.2 |
| 635 | 51.6 | 682 | 22.8 | 729 | 40.2 | 776 | 51.4 |
| 636 | 52.6 | 683 | 21.1 | 730 | 41.6 | 777 | 54.2 |
| 778 | 56.0 | 827 | 37.1 | 876 | 75.8 | 925 | 62.3 |
| 779 | 58.3 | 828 | 38.9 | 877 | 76.6 | 926 | 62.7 |
| 780 | 59.8 | 829 | 41.4 | 878 | 76.5 | 927 | 62.0 |
| 781 | 61.7 | 830 | 44.0 | 879 | 76.2 | 928 | 61.3 |
| 782 | 62.7 | 831 | 46.3 | 880 | 75.8 | 929 | 60.9 |
| 783 | 63.3 | 832 | 47.7 | 881 | 75.4 | 930 | 60.5 |
| 784 | 63.6 | 833 | 48.2 | 882 | 74.8 | 931 | 60.2 |
| 785 | 64.0 | 834 | 48.7 | 883 | 73.9 | 932 | 59.8 |
| 786 | 64.7 | 835 | 49.3 | 884 | 72.7 | 933 | 59.4 |
| 787 | 65.2 | 836 | 49.8 | 885 | 71.3 | 934 | 58.6 |
| 788 | 65.3 | 837 | 50.2 | 886 | 70.4 | 935 | 57.5 |
| 789 | 65.3 | 838 | 50.9 | 887 | 70.0 | 936 | 56.6 |
| 790 | 65.4 | 839 | 51.8 | 888 | 70.0 | 937 | 56.0 |
| 791 | 65.7 | 840 | 52.5 | 889 | 69.0 | 938 | 55.5 |
| 792 | 66.0 | 841 | 53.3 | 890 | 68.0 | 939 | 55.0 |
| 793 | 65.6 | 842 | 54.5 | 891 | 67.3 | 940 | 54.4 |
| 794 | 63.5 | 843 | 55.7 | 892 | 66.2 | 941 | 54.1 |
| 795 | 59.7 | 844 | 56.5 | 893 | 64.8 | 942 | 54.0 |
| 796 | 54.6 | 845 | 56.8 | 894 | 63.6 | 943 | 53.9 |
| 797 | 49.3 | 846 | 57.0 | 895 | 62.6 | 944 | 53.9 |
| 798 | 44.9 | 847 | 57.2 | 896 | 62.1 | 945 | 54.0 |
| 799 | 42.3 | 848 | 57.7 | 897 | 61.9 | 946 | 54.2 |
| 800 | 41.4 | 849 | 58.7 | 898 | 61.9 | 947 | 55.0 |
| 801 | 41.3 | 850 | 60.1 | 899 | 61.8 | 948 | 55.8 |
| 802 | 43.0 | 851 | 61.1 | 900 | 61.5 | 949 | 56.2 |
| 803 | 45.0 | 852 | 61.7 | 901 | 60.9 | 950 | 56.1 |
| 804 | 46.5 | 853 | 62.3 | 902 | 59.7 | 951 | 55.1 |
| 805 | 48.3 | 854 | 62.9 | 903 | 54.6 | 952 | 52.7 |
| 806 | 49.5 | 855 | 63.3 | 904 | 49.3 | 953 | 48.4 |
| 807 | 51.2 | 856 | 63.4 | 905 | 44.9 | 954 | 43.1 |
| 808 | 52.2 | 857 | 63.5 | 906 | 42.3 | 955 | 37.8 |
| 809 | 51.6 | 858 | 63.9 | 907 | 41.4 | 956 | 32.5 |
| 810 | 49.7 | 859 | 64.4 | 908 | 41.3 | 957 | 27.2 |
| 811 | 47.4 | 860 | 65.0 | 909 | 42.1 | 958 | 25.1 |
| 812 | 43.7 | 861 | 65.6 | 910 | 44.7 | 959 | 27.0 |
| 813 | 39.7 | 862 | 66.6 | 911 | 46.0 | 960 | 29.8 |
| 814 | 35.5 | 863 | 67.4 | 912 | 48.8 | 961 | 33.8 |
| 815 | 31.1 | 864 | 68.2 | 913 | 50.1 | 962 | 37.0 |
| 816 | 26.3 | 865 | 69.1 | 914 | 51.3 | 963 | 40.7 |
| 817 | 21.9 | 866 | 70.0 | 915 | 54.1 | 964 | 43.0 |
| 818 | 18.0 | 867 | 70.8 | 916 | 55.2 | 965 | 45.6 |
| 819 | 17.0 | 868 | 71.5 | 917 | 56.2 | 966 | 46.9 |
| 820 | 18.0 | 869 | 72.4 | 918 | 56.1 | 967 | 47.0 |
| 821 | 21.4 | 870 | 73.0 | 919 | 56.1 | 968 | 46.9 |
| 822 | 24.8 | 871 | 73.7 | 920 | 56.5 | 969 | 46.5 |
| 823 | 27.9 | 872 | 74.4 | 921 | 57.5 | 970 | 45.8 |
| 824 | 30.8 | 873 | 74.9 | 922 | 59.2 | 971 | 44.3 |
| 825 | 33.0 | 874 | 75.3 | 923 | 60.7 | 972 | 41.3 |
| 826 | 35.1 | 875 | 75.6 | 924 | 61.8 | 973 | 36.5 |
| 974 | 31.7 |  |  |  |  |  |  |
| 975 | 27.0 |  |  |  |  |  |  |
| 976 | 24.7 |  |  |  |  |  |  |
| 977 | 19.3 |  |  |  |  |  |  |
| 978 | 16.0 |  |  |  |  |  |  |
| 979 | 13.2 |  |  |  |  |  |  |
| 980 | 10.7 |  |  |  |  |  |  |
| 981 | 8.8 |  |  |  |  |  |  |
| 982 | 7.2 |  |  |  |  |  |  |
| 983 | 5.5 |  |  |  |  |  |  |
| 984 | 3.2 |  |  |  |  |  |  |
| 985 | 1.1 |  |  |  |  |  |  |
| 986 | 0.0 |  |  |  |  |  |  |
| 987 | 0.0 |  |  |  |  |  |  |
| 988 | 0.0 |  |  |  |  |  |  |
| 989 | 0.0 |  |  |  |  |  |  |
| 990 | 0.0 |  |  |  |  |  |  |
| 991 | 0.0 |  |  |  |  |  |  |
| 992 | 0.0 |  |  |  |  |  |  |
| 993 | 0.0 |  |  |  |  |  |  |
| 994 | 0.0 |  |  |  |  |  |  |
| 995 | 0.0 |  |  |  |  |  |  |
| 996 | 0.0 |  |  |  |  |  |  |
| 997 | 0.0 |  |  |  |  |  |  |
| 998 | 0.0 |  |  |  |  |  |  |
| 999 | 0.0 |  |  |  |  |  |  |
| 1000 | 0.0 |  |  |  |  |  |  |
| 1001 | 0.0 |  |  |  |  |  |  |
| 1002 | 0.0 |  |  |  |  |  |  |
| 1003 | 0.0 |  |  |  |  |  |  |
| 1004 | 0.0 |  |  |  |  |  |  |
| 1005 | 0.0 |  |  |  |  |  |  |
| 1006 | 0.0 |  |  |  |  |  |  |
| 1007 | 0.0 |  |  |  |  |  |  |
| 1008 | 0.0 |  |  |  |  |  |  |
| 1009 | 0.0 |  |  |  |  |  |  |
| 1010 | 0.0 |  |  |  |  |  |  |
| 1011 | 0.0 |  |  |  |  |  |  |
| 1012 | 0.0 |  |  |  |  |  |  |
| 1013 | 0.0 |  |  |  |  |  |  |
| 1014 | 0.0 |  |  |  |  |  |  |
| 1015 | 0.0 |  |  |  |  |  |  |
| 1016 | 0.0 |  |  |  |  |  |  |
| 1017 | 0.0 |  |  |  |  |  |  |
| 1018 | 0.0 |  |  |  |  |  |  |
| 1019 | 0.0 |  |  |  |  |  |  |
| 1020 | 0.0 |  |  |  |  |  |  |
| 1021 | 0.0 |  |  |  |  |  |  |
| 1022 | 0.0 |  |  |  |  |  |  |

# Table A1/9

# **WLTC, Class 3b cycle, phase Medium3b (Second 589 is the end of phase Low3 and the start of phase Medium3b)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 590 | 0.0 | 637 | 53.0 | 684 | 18.9 | 731 | 41.9 |
| 591 | 0.0 | 638 | 53.0 | 685 | 18.9 | 732 | 42.0 |
| 592 | 0.0 | 639 | 52.9 | 686 | 21.3 | 733 | 42.2 |
| 593 | 0.0 | 640 | 52.7 | 687 | 23.9 | 734 | 42.4 |
| 594 | 0.0 | 641 | 52.6 | 688 | 25.9 | 735 | 42.7 |
| 595 | 0.0 | 642 | 53.1 | 689 | 28.4 | 736 | 43.1 |
| 596 | 0.0 | 643 | 54.3 | 690 | 30.3 | 737 | 43.7 |
| 597 | 0.0 | 644 | 55.2 | 691 | 30.9 | 738 | 44.0 |
| 598 | 0.0 | 645 | 55.5 | 692 | 31.1 | 739 | 44.1 |
| 599 | 0.0 | 646 | 55.9 | 693 | 31.8 | 740 | 45.3 |
| 600 | 0.0 | 647 | 56.3 | 694 | 32.7 | 741 | 46.4 |
| 601 | 1.0 | 648 | 56.7 | 695 | 33.2 | 742 | 47.2 |
| 602 | 2.1 | 649 | 56.9 | 696 | 32.4 | 743 | 47.3 |
| 603 | 4.8 | 650 | 56.8 | 697 | 28.3 | 744 | 47.4 |
| 604 | 9.1 | 651 | 56.0 | 698 | 25.8 | 745 | 47.4 |
| 605 | 14.2 | 652 | 54.2 | 699 | 23.1 | 746 | 47.5 |
| 606 | 19.8 | 653 | 52.1 | 700 | 21.8 | 747 | 47.9 |
| 607 | 25.5 | 654 | 50.1 | 701 | 21.2 | 748 | 48.6 |
| 608 | 30.5 | 655 | 47.2 | 702 | 21.0 | 749 | 49.4 |
| 609 | 34.8 | 656 | 43.2 | 703 | 21.0 | 750 | 49.8 |
| 610 | 38.8 | 657 | 39.2 | 704 | 20.9 | 751 | 49.8 |
| 611 | 42.9 | 658 | 36.5 | 705 | 19.9 | 752 | 49.7 |
| 612 | 46.4 | 659 | 34.3 | 706 | 17.9 | 753 | 49.3 |
| 613 | 48.3 | 660 | 31.0 | 707 | 15.1 | 754 | 48.5 |
| 614 | 48.7 | 661 | 26.0 | 708 | 12.8 | 755 | 47.6 |
| 615 | 48.5 | 662 | 20.7 | 709 | 12.0 | 756 | 46.3 |
| 616 | 48.4 | 663 | 15.4 | 710 | 13.2 | 757 | 43.7 |
| 617 | 48.2 | 664 | 13.1 | 711 | 17.1 | 758 | 39.3 |
| 618 | 47.8 | 665 | 12.0 | 712 | 21.1 | 759 | 34.1 |
| 619 | 47.0 | 666 | 12.5 | 713 | 21.8 | 760 | 29.0 |
| 620 | 45.9 | 667 | 14.0 | 714 | 21.2 | 761 | 23.7 |
| 621 | 44.9 | 668 | 19.0 | 715 | 18.5 | 762 | 18.4 |
| 622 | 44.4 | 669 | 23.2 | 716 | 13.9 | 763 | 14.3 |
| 623 | 44.3 | 670 | 28.0 | 717 | 12.0 | 764 | 12.0 |
| 624 | 44.5 | 671 | 32.0 | 718 | 12.0 | 765 | 12.8 |
| 625 | 45.1 | 672 | 34.0 | 719 | 13.0 | 766 | 16.0 |
| 626 | 45.7 | 673 | 36.0 | 720 | 16.0 | 767 | 19.1 |
| 627 | 46.0 | 674 | 38.0 | 721 | 18.5 | 768 | 22.4 |
| 628 | 46.0 | 675 | 40.0 | 722 | 20.6 | 769 | 25.6 |
| 629 | 46.0 | 676 | 40.3 | 723 | 22.5 | 770 | 30.1 |
| 630 | 46.1 | 677 | 40.5 | 724 | 24.0 | 771 | 35.3 |
| 631 | 46.7 | 678 | 39.0 | 725 | 26.6 | 772 | 39.9 |
| 632 | 47.7 | 679 | 35.7 | 726 | 29.9 | 773 | 44.5 |
| 633 | 48.9 | 680 | 31.8 | 727 | 34.8 | 774 | 47.5 |
| 634 | 50.3 | 681 | 27.1 | 728 | 37.8 | 775 | 50.9 |
| 635 | 51.6 | 682 | 22.8 | 729 | 40.2 | 776 | 54.1 |
| 636 | 52.6 | 683 | 21.1 | 730 | 41.6 | 777 | 56.3 |
| 778 | 58.1 | 827 | 37.1 | 876 | 72.7 | 925 | 64.1 |
| 779 | 59.8 | 828 | 38.9 | 877 | 71.3 | 926 | 62.7 |
| 780 | 61.1 | 829 | 41.4 | 878 | 70.4 | 927 | 62.0 |
| 781 | 62.1 | 830 | 44.0 | 879 | 70.0 | 928 | 61.3 |
| 782 | 62.8 | 831 | 46.3 | 880 | 70.0 | 929 | 60.9 |
| 783 | 63.3 | 832 | 47.7 | 881 | 69.0 | 930 | 60.5 |
| 784 | 63.6 | 833 | 48.2 | 882 | 68.0 | 931 | 60.2 |
| 785 | 64.0 | 834 | 48.7 | 883 | 68.0 | 932 | 59.8 |
| 786 | 64.7 | 835 | 49.3 | 884 | 68.0 | 933 | 59.4 |
| 787 | 65.2 | 836 | 49.8 | 885 | 68.1 | 934 | 58.6 |
| 788 | 65.3 | 837 | 50.2 | 886 | 68.4 | 935 | 57.5 |
| 789 | 65.3 | 838 | 50.9 | 887 | 68.6 | 936 | 56.6 |
| 790 | 65.4 | 839 | 51.8 | 888 | 68.7 | 937 | 56.0 |
| 791 | 65.7 | 840 | 52.5 | 889 | 68.5 | 938 | 55.5 |
| 792 | 66.0 | 841 | 53.3 | 890 | 68.1 | 939 | 55.0 |
| 793 | 65.6 | 842 | 54.5 | 891 | 67.3 | 940 | 54.4 |
| 794 | 63.5 | 843 | 55.7 | 892 | 66.2 | 941 | 54.1 |
| 795 | 59.7 | 844 | 56.5 | 893 | 64.8 | 942 | 54.0 |
| 796 | 54.6 | 845 | 56.8 | 894 | 63.6 | 943 | 53.9 |
| 797 | 49.3 | 846 | 57.0 | 895 | 62.6 | 944 | 53.9 |
| 798 | 44.9 | 847 | 57.2 | 896 | 62.1 | 945 | 54.0 |
| 799 | 42.3 | 848 | 57.7 | 897 | 61.9 | 946 | 54.2 |
| 800 | 41.4 | 849 | 58.7 | 898 | 61.9 | 947 | 55.0 |
| 801 | 41.3 | 850 | 60.1 | 899 | 61.8 | 948 | 55.8 |
| 802 | 42.1 | 851 | 61.1 | 900 | 61.5 | 949 | 56.2 |
| 803 | 44.7 | 852 | 61.7 | 901 | 60.9 | 950 | 56.1 |
| 804 | 48.4 | 853 | 62.3 | 902 | 59.7 | 951 | 55.1 |
| 805 | 51.4 | 854 | 62.9 | 903 | 54.6 | 952 | 52.7 |
| 806 | 52.7 | 855 | 63.3 | 904 | 49.3 | 953 | 48.4 |
| 807 | 53.0 | 856 | 63.4 | 905 | 44.9 | 954 | 43.1 |
| 808 | 52.5 | 857 | 63.5 | 906 | 42.3 | 955 | 37.8 |
| 809 | 51.3 | 858 | 64.5 | 907 | 41.4 | 956 | 32.5 |
| 810 | 49.7 | 859 | 65.8 | 908 | 41.3 | 957 | 27.2 |
| 811 | 47.4 | 860 | 66.8 | 909 | 42.1 | 958 | 25.1 |
| 812 | 43.7 | 861 | 67.4 | 910 | 44.7 | 959 | 26.0 |
| 813 | 39.7 | 862 | 68.8 | 911 | 48.4 | 960 | 29.3 |
| 814 | 35.5 | 863 | 71.1 | 912 | 51.4 | 961 | 34.6 |
| 815 | 31.1 | 864 | 72.3 | 913 | 52.7 | 962 | 40.4 |
| 816 | 26.3 | 865 | 72.8 | 914 | 54.0 | 963 | 45.3 |
| 817 | 21.9 | 866 | 73.4 | 915 | 57.0 | 964 | 49.0 |
| 818 | 18.0 | 867 | 74.6 | 916 | 58.1 | 965 | 51.1 |
| 819 | 17.0 | 868 | 76.0 | 917 | 59.2 | 966 | 52.1 |
| 820 | 18.0 | 869 | 76.6 | 918 | 59.0 | 967 | 52.2 |
| 821 | 21.4 | 870 | 76.5 | 919 | 59.1 | 968 | 52.1 |
| 822 | 24.8 | 871 | 76.2 | 920 | 59.5 | 969 | 51.7 |
| 823 | 27.9 | 872 | 75.8 | 921 | 60.5 | 970 | 50.9 |
| 824 | 30.8 | 873 | 75.4 | 922 | 62.3 | 971 | 49.2 |
| 825 | 33.0 | 874 | 74.8 | 923 | 63.9 | 972 | 45.9 |
| 826 | 35.1 | 875 | 73.9 | 924 | 65.1 | 973 | 40.6 |
| 974 | 35.3 |  |  |  |  |  |  |
| 975 | 30.0 |  |  |  |  |  |  |
| 976 | 24.7 |  |  |  |  |  |  |
| 977 | 19.3 |  |  |  |  |  |  |
| 978 | 16.0 |  |  |  |  |  |  |
| 979 | 13.2 |  |  |  |  |  |  |
| 980 | 10.7 |  |  |  |  |  |  |
| 981 | 8.8 |  |  |  |  |  |  |
| 982 | 7.2 |  |  |  |  |  |  |
| 983 | 5.5 |  |  |  |  |  |  |
| 984 | 3.2 |  |  |  |  |  |  |
| 985 | 1.1 |  |  |  |  |  |  |
| 986 | 0.0 |  |  |  |  |  |  |
| 987 | 0.0 |  |  |  |  |  |  |
| 988 | 0.0 |  |  |  |  |  |  |
| 989 | 0.0 |  |  |  |  |  |  |
| 990 | 0.0 |  |  |  |  |  |  |
| 991 | 0.0 |  |  |  |  |  |  |
| 992 | 0.0 |  |  |  |  |  |  |
| 993 | 0.0 |  |  |  |  |  |  |
| 994 | 0.0 |  |  |  |  |  |  |
| 995 | 0.0 |  |  |  |  |  |  |
| 996 | 0.0 |  |  |  |  |  |  |
| 997 | 0.0 |  |  |  |  |  |  |
| 998 | 0.0 |  |  |  |  |  |  |
| 999 | 0.0 |  |  |  |  |  |  |
| 1000 | 0.0 |  |  |  |  |  |  |
| 1001 | 0.0 |  |  |  |  |  |  |
| 1002 | 0.0 |  |  |  |  |  |  |
| 1003 | 0.0 |  |  |  |  |  |  |
| 1004 | 0.0 |  |  |  |  |  |  |
| 1005 | 0.0 |  |  |  |  |  |  |
| 1006 | 0.0 |  |  |  |  |  |  |
| 1007 | 0.0 |  |  |  |  |  |  |
| 1008 | 0.0 |  |  |  |  |  |  |
| 1009 | 0.0 |  |  |  |  |  |  |
| 1010 | 0.0 |  |  |  |  |  |  |
| 1011 | 0.0 |  |  |  |  |  |  |
| 1012 | 0.0 |  |  |  |  |  |  |
| 1013 | 0.0 |  |  |  |  |  |  |
| 1014 | 0.0 |  |  |  |  |  |  |
| 1015 | 0.0 |  |  |  |  |  |  |
| 1016 | 0.0 |  |  |  |  |  |  |
| 1017 | 0.0 |  |  |  |  |  |  |
| 1018 | 0.0 |  |  |  |  |  |  |
| 1019 | 0.0 |  |  |  |  |  |  |
| 1020 | 0.0 |  |  |  |  |  |  |
| 1021 | 0.0 |  |  |  |  |  |  |
| 1022 | 0.0 |  |  |  |  |  |  |

# Table A1/10

# **WLTC, Class 3a cycle, phase High3a (Second 1022 is the start of this phase)**

| *Time in s* | *Speed in km/h* |  | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1023 | 0.0 |  | 1070 | 29.0 | 1117 | 66.2 | 1164 | 52.6 |
| 1024 | 0.0 |  | 1071 | 32.0 | 1118 | 65.8 | 1165 | 54.5 |
| 1025 | 0.0 |  | 1072 | 34.8 | 1119 | 64.7 | 1166 | 56.6 |
| 1026 | 0.0 |  | 1073 | 37.7 | 1120 | 63.6 | 1167 | 58.3 |
| 1027 | 0.8 |  | 1074 | 40.8 | 1121 | 62.9 | 1168 | 60.0 |
| 1028 | 3.6 |  | 1075 | 43.2 | 1122 | 62.4 | 1169 | 61.5 |
| 1029 | 8.6 |  | 1076 | 46.0 | 1123 | 61.7 | 1170 | 63.1 |
| 1030 | 14.6 |  | 1077 | 48.0 | 1124 | 60.1 | 1171 | 64.3 |
| 1031 | 20.0 |  | 1078 | 50.7 | 1125 | 57.3 | 1172 | 65.7 |
| 1032 | 24.4 |  | 1079 | 52.0 | 1126 | 55.8 | 1173 | 67.1 |
| 1033 | 28.2 |  | 1080 | 54.5 | 1127 | 50.5 | 1174 | 68.3 |
| 1034 | 31.7 |  | 1081 | 55.9 | 1128 | 45.2 | 1175 | 69.7 |
| 1035 | 35.0 |  | 1082 | 57.4 | 1129 | 40.1 | 1176 | 70.6 |
| 1036 | 37.6 |  | 1083 | 58.1 | 1130 | 36.2 | 1177 | 71.6 |
| 1037 | 39.7 |  | 1084 | 58.4 | 1131 | 32.9 | 1178 | 72.6 |
| 1038 | 41.5 |  | 1085 | 58.8 | 1132 | 29.8 | 1179 | 73.5 |
| 1039 | 43.6 |  | 1086 | 58.8 | 1133 | 26.6 | 1180 | 74.2 |
| 1040 | 46.0 |  | 1087 | 58.6 | 1134 | 23.0 | 1181 | 74.9 |
| 1041 | 48.4 |  | 1088 | 58.7 | 1135 | 19.4 | 1182 | 75.6 |
| 1042 | 50.5 |  | 1089 | 58.8 | 1136 | 16.3 | 1183 | 76.3 |
| 1043 | 51.9 |  | 1090 | 58.8 | 1137 | 14.6 | 1184 | 77.1 |
| 1044 | 52.6 |  | 1091 | 58.8 | 1138 | 14.2 | 1185 | 77.9 |
| 1045 | 52.8 |  | 1092 | 59.1 | 1139 | 14.3 | 1186 | 78.5 |
| 1046 | 52.9 |  | 1093 | 60.1 | 1140 | 14.6 | 1187 | 79.0 |
| 1047 | 53.1 |  | 1094 | 61.7 | 1141 | 15.1 | 1188 | 79.7 |
| 1048 | 53.3 |  | 1095 | 63.0 | 1142 | 16.4 | 1189 | 80.3 |
| 1049 | 53.1 |  | 1096 | 63.7 | 1143 | 19.1 | 1190 | 81.0 |
| 1050 | 52.3 |  | 1097 | 63.9 | 1144 | 22.5 | 1191 | 81.6 |
| 1051 | 50.7 |  | 1098 | 63.5 | 1145 | 24.4 | 1192 | 82.4 |
| 1052 | 48.8 |  | 1099 | 62.3 | 1146 | 24.8 | 1193 | 82.9 |
| 1053 | 46.5 |  | 1100 | 60.3 | 1147 | 22.7 | 1194 | 83.4 |
| 1054 | 43.8 |  | 1101 | 58.9 | 1148 | 17.4 | 1195 | 83.8 |
| 1055 | 40.3 |  | 1102 | 58.4 | 1149 | 13.8 | 1196 | 84.2 |
| 1056 | 36.0 |  | 1103 | 58.8 | 1150 | 12.0 | 1197 | 84.7 |
| 1057 | 30.7 |  | 1104 | 60.2 | 1151 | 12.0 | 1198 | 85.2 |
| 1058 | 25.4 |  | 1105 | 62.3 | 1152 | 12.0 | 1199 | 85.6 |
| 1059 | 21.0 |  | 1106 | 63.9 | 1153 | 13.9 | 1200 | 86.3 |
| 1060 | 16.7 |  | 1107 | 64.5 | 1154 | 17.7 | 1201 | 86.8 |
| 1061 | 13.4 |  | 1108 | 64.4 | 1155 | 22.8 | 1202 | 87.4 |
| 1062 | 12.0 |  | 1109 | 63.5 | 1156 | 27.3 | 1203 | 88.0 |
| 1063 | 12.1 |  | 1110 | 62.0 | 1157 | 31.2 | 1204 | 88.3 |
| 1064 | 12.8 |  | 1111 | 61.2 | 1158 | 35.2 | 1205 | 88.7 |
| 1065 | 15.6 |  | 1112 | 61.3 | 1159 | 39.4 | 1206 | 89.0 |
| 1066 | 19.9 |  | 1113 | 61.7 | 1160 | 42.5 | 1207 | 89.3 |
| 1067 | 23.4 |  | 1114 | 62.0 | 1161 | 45.4 | 1208 | 89.8 |
| 1068 | 24.6 |  | 1115 | 64.6 | 1162 | 48.2 | 1209 | 90.2 |
| 1069 | 27.0 |  | 1116 | 66.0 | 1163 | 50.3 | 1210 | 90.6 |
| 1211 | 91.0 |  | 1260 | 95.7 | 1309 | 75.9 | 1358 | 68.2 |
| 1212 | 91.3 |  | 1261 | 95.5 | 1310 | 76.0 | 1359 | 66.1 |
| 1213 | 91.6 |  | 1262 | 95.3 | 1311 | 76.0 | 1360 | 63.8 |
| 1214 | 91.9 |  | 1263 | 95.2 | 1312 | 76.1 | 1361 | 61.6 |
| 1215 | 92.2 |  | 1264 | 95.0 | 1313 | 76.3 | 1362 | 60.2 |
| 1216 | 92.8 |  | 1265 | 94.9 | 1314 | 76.5 | 1363 | 59.8 |
| 1217 | 93.1 |  | 1266 | 94.7 | 1315 | 76.6 | 1364 | 60.4 |
| 1218 | 93.3 |  | 1267 | 94.5 | 1316 | 76.8 | 1365 | 61.8 |
| 1219 | 93.5 |  | 1268 | 94.4 | 1317 | 77.1 | 1366 | 62.6 |
| 1220 | 93.7 |  | 1269 | 94.4 | 1318 | 77.1 | 1367 | 62.7 |
| 1221 | 93.9 |  | 1270 | 94.3 | 1319 | 77.2 | 1368 | 61.9 |
| 1222 | 94.0 |  | 1271 | 94.3 | 1320 | 77.2 | 1369 | 60.0 |
| 1223 | 94.1 |  | 1272 | 94.1 | 1321 | 77.6 | 1370 | 58.4 |
| 1224 | 94.3 |  | 1273 | 93.9 | 1322 | 78.0 | 1371 | 57.8 |
| 1225 | 94.4 |  | 1274 | 93.4 | 1323 | 78.4 | 1372 | 57.8 |
| 1226 | 94.6 |  | 1275 | 92.8 | 1324 | 78.8 | 1373 | 57.8 |
| 1227 | 94.7 |  | 1276 | 92.0 | 1325 | 79.2 | 1374 | 57.3 |
| 1228 | 94.8 |  | 1277 | 91.3 | 1326 | 80.3 | 1375 | 56.2 |
| 1229 | 95.0 |  | 1278 | 90.6 | 1327 | 80.8 | 1376 | 54.3 |
| 1230 | 95.1 |  | 1279 | 90.0 | 1328 | 81.0 | 1377 | 50.8 |
| 1231 | 95.3 |  | 1280 | 89.3 | 1329 | 81.0 | 1378 | 45.5 |
| 1232 | 95.4 |  | 1281 | 88.7 | 1330 | 81.0 | 1379 | 40.2 |
| 1233 | 95.6 |  | 1282 | 88.1 | 1331 | 81.0 | 1380 | 34.9 |
| 1234 | 95.7 |  | 1283 | 87.4 | 1332 | 81.0 | 1381 | 29.6 |
| 1235 | 95.8 |  | 1284 | 86.7 | 1333 | 80.9 | 1382 | 28.7 |
| 1236 | 96.0 |  | 1285 | 86.0 | 1334 | 80.6 | 1383 | 29.3 |
| 1237 | 96.1 |  | 1286 | 85.3 | 1335 | 80.3 | 1384 | 30.5 |
| 1238 | 96.3 |  | 1287 | 84.7 | 1336 | 80.0 | 1385 | 31.7 |
| 1239 | 96.4 |  | 1288 | 84.1 | 1337 | 79.9 | 1386 | 32.9 |
| 1240 | 96.6 |  | 1289 | 83.5 | 1338 | 79.8 | 1387 | 35.0 |
| 1241 | 96.8 |  | 1290 | 82.9 | 1339 | 79.8 | 1388 | 38.0 |
| 1242 | 97.0 |  | 1291 | 82.3 | 1340 | 79.8 | 1389 | 40.5 |
| 1243 | 97.2 |  | 1292 | 81.7 | 1341 | 79.9 | 1390 | 42.7 |
| 1244 | 97.3 |  | 1293 | 81.1 | 1342 | 80.0 | 1391 | 45.8 |
| 1245 | 97.4 |  | 1294 | 80.5 | 1343 | 80.4 | 1392 | 47.5 |
| 1246 | 97.4 |  | 1295 | 79.9 | 1344 | 80.8 | 1393 | 48.9 |
| 1247 | 97.4 |  | 1296 | 79.4 | 1345 | 81.2 | 1394 | 49.4 |
| 1248 | 97.4 |  | 1297 | 79.1 | 1346 | 81.5 | 1395 | 49.4 |
| 1249 | 97.3 |  | 1298 | 78.8 | 1347 | 81.6 | 1396 | 49.2 |
| 1250 | 97.3 |  | 1299 | 78.5 | 1348 | 81.6 | 1397 | 48.7 |
| 1251 | 97.3 |  | 1300 | 78.2 | 1349 | 81.4 | 1398 | 47.9 |
| 1252 | 97.3 |  | 1301 | 77.9 | 1350 | 80.7 | 1399 | 46.9 |
| 1253 | 97.2 |  | 1302 | 77.6 | 1351 | 79.6 | 1400 | 45.6 |
| 1254 | 97.1 |  | 1303 | 77.3 | 1352 | 78.2 | 1401 | 44.2 |
| 1255 | 97.0 |  | 1304 | 77.0 | 1353 | 76.8 | 1402 | 42.7 |
| 1256 | 96.9 |  | 1305 | 76.7 | 1354 | 75.3 | 1403 | 40.7 |
| 1257 | 96.7 |  | 1306 | 76.0 | 1355 | 73.8 | 1404 | 37.1 |
| 1258 | 96.4 |  | 1307 | 76.0 | 1356 | 72.1 | 1405 | 33.9 |
| 1259 | 96.1 |  | 1308 | 76.0 | 1357 | 70.2 | 1406 | 30.6 |
| 1407 | 28.6 |  | 1456 | 0.0 |  |  |  |  |
| 1408 | 27.3 |  | 1457 | 0.0 |  |  |  |  |
| 1409 | 27.2 |  | 1458 | 0.0 |  |  |  |  |
| 1410 | 27.5 |  | 1459 | 0.0 |  |  |  |  |
| 1411 | 27.4 |  | 1460 | 0.0 |  |  |  |  |
| 1412 | 27.1 |  | 1461 | 0.0 |  |  |  |  |
| 1413 | 26.7 |  | 1462 | 0.0 |  |  |  |  |
| 1414 | 26.8 |  | 1463 | 0.0 |  |  |  |  |
| 1415 | 28.2 |  | 1464 | 0.0 |  |  |  |  |
| 1416 | 31.1 |  | 1465 | 0.0 |  |  |  |  |
| 1417 | 34.8 |  | 1466 | 0.0 |  |  |  |  |
| 1418 | 38.4 |  | 1467 | 0.0 |  |  |  |  |
| 1419 | 40.9 |  | 1468 | 0.0 |  |  |  |  |
| 1420 | 41.7 |  | 1469 | 0.0 |  |  |  |  |
| 1421 | 40.9 |  | 1470 | 0.0 |  |  |  |  |
| 1422 | 38.3 |  | 1471 | 0.0 |  |  |  |  |
| 1423 | 35.3 |  | 1472 | 0.0 |  |  |  |  |
| 1424 | 34.3 |  | 1473 | 0.0 |  |  |  |  |
| 1425 | 34.6 |  | 1474 | 0.0 |  |  |  |  |
| 1426 | 36.3 |  | 1475 | 0.0 |  |  |  |  |
| 1427 | 39.5 |  | 1476 | 0.0 |  |  |  |  |
| 1428 | 41.8 |  | 1477 | 0.0 |  |  |  |  |
| 1429 | 42.5 |  |  |  |  |  |  |  |
| 1430 | 41.9 |  |  |  |  |  |  |  |
| 1431 | 40.1 |  |  |  |  |  |  |  |
| 1432 | 36.6 |  |  |  |  |  |  |  |
| 1433 | 31.3 |  |  |  |  |  |  |  |
| 1434 | 26.0 |  |  |  |  |  |  |  |
| 1435 | 20.6 |  |  |  |  |  |  |  |
| 1436 | 19.1 |  |  |  |  |  |  |  |
| 1437 | 19.7 |  |  |  |  |  |  |  |
| 1438 | 21.1 |  |  |  |  |  |  |  |
| 1439 | 22.0 |  |  |  |  |  |  |  |
| 1440 | 22.1 |  |  |  |  |  |  |  |
| 1441 | 21.4 |  |  |  |  |  |  |  |
| 1442 | 19.6 |  |  |  |  |  |  |  |
| 1443 | 18.3 |  |  |  |  |  |  |  |
| 1444 | 18.0 |  |  |  |  |  |  |  |
| 1445 | 18.3 |  |  |  |  |  |  |  |
| 1446 | 18.5 |  |  |  |  |  |  |  |
| 1447 | 17.9 |  |  |  |  |  |  |  |
| 1448 | 15.0 |  |  |  |  |  |  |  |
| 1449 | 9.9 |  |  |  |  |  |  |  |
| 1450 | 4.6 |  |  |  |  |  |  |  |
| 1451 | 1.2 |  |  |  |  |  |  |  |
| 1452 | 0.0 |  |  |  |  |  |  |  |
| 1453 | 0.0 |  |  |  |  |  |  |  |
| 1454 | 0.0 |  |  |  |  |  |  |  |
| 1455 | 0.0 |  |  |  |  |  |  |  |

# Table A1/11

# **WLTC, Class 3b cycle, phase High3b (Second 1022 is the start of this phase)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1023 | 0.0 | 1070 | 26.4 | 1117 | 69.7 | 1164 | 52.6 |
| 1024 | 0.0 | 1071 | 28.8 | 1118 | 69.3 | 1165 | 54.5 |
| 1025 | 0.0 | 1072 | 31.8 | 1119 | 68.1 | 1166 | 56.6 |
| 1026 | 0.0 | 1073 | 35.3 | 1120 | 66.9 | 1167 | 58.3 |
| 1027 | 0.8 | 1074 | 39.5 | 1121 | 66.2 | 1168 | 60.0 |
| 1028 | 3.6 | 1075 | 44.5 | 1122 | 65.7 | 1169 | 61.5 |
| 1029 | 8.6 | 1076 | 49.3 | 1123 | 64.9 | 1170 | 63.1 |
| 1030 | 14.6 | 1077 | 53.3 | 1124 | 63.2 | 1171 | 64.3 |
| 1031 | 20.0 | 1078 | 56.4 | 1125 | 60.3 | 1172 | 65.7 |
| 1032 | 24.4 | 1079 | 58.9 | 1126 | 55.8 | 1173 | 67.1 |
| 1033 | 28.2 | 1080 | 61.2 | 1127 | 50.5 | 1174 | 68.3 |
| 1034 | 31.7 | 1081 | 62.6 | 1128 | 45.2 | 1175 | 69.7 |
| 1035 | 35.0 | 1082 | 63.0 | 1129 | 40.1 | 1176 | 70.6 |
| 1036 | 37.6 | 1083 | 62.5 | 1130 | 36.2 | 1177 | 71.6 |
| 1037 | 39.7 | 1084 | 60.9 | 1131 | 32.9 | 1178 | 72.6 |
| 1038 | 41.5 | 1085 | 59.3 | 1132 | 29.8 | 1179 | 73.5 |
| 1039 | 43.6 | 1086 | 58.6 | 1133 | 26.6 | 1180 | 74.2 |
| 1040 | 46.0 | 1087 | 58.6 | 1134 | 23.0 | 1181 | 74.9 |
| 1041 | 48.4 | 1088 | 58.7 | 1135 | 19.4 | 1182 | 75.6 |
| 1042 | 50.5 | 1089 | 58.8 | 1136 | 16.3 | 1183 | 76.3 |
| 1043 | 51.9 | 1090 | 58.8 | 1137 | 14.6 | 1184 | 77.1 |
| 1044 | 52.6 | 1091 | 58.8 | 1138 | 14.2 | 1185 | 77.9 |
| 1045 | 52.8 | 1092 | 59.1 | 1139 | 14.3 | 1186 | 78.5 |
| 1046 | 52.9 | 1093 | 60.1 | 1140 | 14.6 | 1187 | 79.0 |
| 1047 | 53.1 | 1094 | 61.7 | 1141 | 15.1 | 1188 | 79.7 |
| 1048 | 53.3 | 1095 | 63.0 | 1142 | 16.4 | 1189 | 80.3 |
| 1049 | 53.1 | 1096 | 63.7 | 1143 | 19.1 | 1190 | 81.0 |
| 1050 | 52.3 | 1097 | 63.9 | 1144 | 22.5 | 1191 | 81.6 |
| 1051 | 50.7 | 1098 | 63.5 | 1145 | 24.4 | 1192 | 82.4 |
| 1052 | 48.8 | 1099 | 62.3 | 1146 | 24.8 | 1193 | 82.9 |
| 1053 | 46.5 | 1100 | 60.3 | 1147 | 22.7 | 1194 | 83.4 |
| 1054 | 43.8 | 1101 | 58.9 | 1148 | 17.4 | 1195 | 83.8 |
| 1055 | 40.3 | 1102 | 58.4 | 1149 | 13.8 | 1196 | 84.2 |
| 1056 | 36.0 | 1103 | 58.8 | 1150 | 12.0 | 1197 | 84.7 |
| 1057 | 30.7 | 1104 | 60.2 | 1151 | 12.0 | 1198 | 85.2 |
| 1058 | 25.4 | 1105 | 62.3 | 1152 | 12.0 | 1199 | 85.6 |
| 1059 | 21.0 | 1106 | 63.9 | 1153 | 13.9 | 1200 | 86.3 |
| 1060 | 16.7 | 1107 | 64.5 | 1154 | 17.7 | 1201 | 86.8 |
| 1061 | 13.4 | 1108 | 64.4 | 1155 | 22.8 | 1202 | 87.4 |
| 1062 | 12.0 | 1109 | 63.5 | 1156 | 27.3 | 1203 | 88.0 |
| 1063 | 12.1 | 1110 | 62.0 | 1157 | 31.2 | 1204 | 88.3 |
| 1064 | 12.8 | 1111 | 61.2 | 1158 | 35.2 | 1205 | 88.7 |
| 1065 | 15.6 | 1112 | 61.3 | 1159 | 39.4 | 1206 | 89.0 |
| 1066 | 19.9 | 1113 | 62.6 | 1160 | 42.5 | 1207 | 89.3 |
| 1067 | 23.4 | 1114 | 65.3 | 1161 | 45.4 | 1208 | 89.8 |
| 1068 | 24.6 | 1115 | 68.0 | 1162 | 48.2 | 1209 | 90.2 |
| 1069 | 25.2 | 1116 | 69.4 | 1163 | 50.3 | 1210 | 90.6 |
| 1211 | 91.0 | 1260 | 95.7 | 1309 | 75.9 | 1358 | 68.2 |
| 1212 | 91.3 | 1261 | 95.5 | 1310 | 75.9 | 1359 | 66.1 |
| 1213 | 91.6 | 1262 | 95.3 | 1311 | 75.8 | 1360 | 63.8 |
| 1214 | 91.9 | 1263 | 95.2 | 1312 | 75.7 | 1361 | 61.6 |
| 1215 | 92.2 | 1264 | 95.0 | 1313 | 75.5 | 1362 | 60.2 |
| 1216 | 92.8 | 1265 | 94.9 | 1314 | 75.2 | 1363 | 59.8 |
| 1217 | 93.1 | 1266 | 94.7 | 1315 | 75.0 | 1364 | 60.4 |
| 1218 | 93.3 | 1267 | 94.5 | 1316 | 74.7 | 1365 | 61.8 |
| 1219 | 93.5 | 1268 | 94.4 | 1317 | 74.1 | 1366 | 62.6 |
| 1220 | 93.7 | 1269 | 94.4 | 1318 | 73.7 | 1367 | 62.7 |
| 1221 | 93.9 | 1270 | 94.3 | 1319 | 73.3 | 1368 | 61.9 |
| 1222 | 94.0 | 1271 | 94.3 | 1320 | 73.5 | 1369 | 60.0 |
| 1223 | 94.1 | 1272 | 94.1 | 1321 | 74.0 | 1370 | 58.4 |
| 1224 | 94.3 | 1273 | 93.9 | 1322 | 74.9 | 1371 | 57.8 |
| 1225 | 94.4 | 1274 | 93.4 | 1323 | 76.1 | 1372 | 57.8 |
| 1226 | 94.6 | 1275 | 92.8 | 1324 | 77.7 | 1373 | 57.8 |
| 1227 | 94.7 | 1276 | 92.0 | 1325 | 79.2 | 1374 | 57.3 |
| 1228 | 94.8 | 1277 | 91.3 | 1326 | 80.3 | 1375 | 56.2 |
| 1229 | 95.0 | 1278 | 90.6 | 1327 | 80.8 | 1376 | 54.3 |
| 1230 | 95.1 | 1279 | 90.0 | 1328 | 81.0 | 1377 | 50.8 |
| 1231 | 95.3 | 1280 | 89.3 | 1329 | 81.0 | 1378 | 45.5 |
| 1232 | 95.4 | 1281 | 88.7 | 1330 | 81.0 | 1379 | 40.2 |
| 1233 | 95.6 | 1282 | 88.1 | 1331 | 81.0 | 1380 | 34.9 |
| 1234 | 95.7 | 1283 | 87.4 | 1332 | 81.0 | 1381 | 29.6 |
| 1235 | 95.8 | 1284 | 86.7 | 1333 | 80.9 | 1382 | 27.3 |
| 1236 | 96.0 | 1285 | 86.0 | 1334 | 80.6 | 1383 | 29.3 |
| 1237 | 96.1 | 1286 | 85.3 | 1335 | 80.3 | 1384 | 32.9 |
| 1238 | 96.3 | 1287 | 84.7 | 1336 | 80.0 | 1385 | 35.6 |
| 1239 | 96.4 | 1288 | 84.1 | 1337 | 79.9 | 1386 | 36.7 |
| 1240 | 96.6 | 1289 | 83.5 | 1338 | 79.8 | 1387 | 37.6 |
| 1241 | 96.8 | 1290 | 82.9 | 1339 | 79.8 | 1388 | 39.4 |
| 1242 | 97.0 | 1291 | 82.3 | 1340 | 79.8 | 1389 | 42.5 |
| 1243 | 97.2 | 1292 | 81.7 | 1341 | 79.9 | 1390 | 46.5 |
| 1244 | 97.3 | 1293 | 81.1 | 1342 | 80.0 | 1391 | 50.2 |
| 1245 | 97.4 | 1294 | 80.5 | 1343 | 80.4 | 1392 | 52.8 |
| 1246 | 97.4 | 1295 | 79.9 | 1344 | 80.8 | 1393 | 54.3 |
| 1247 | 97.4 | 1296 | 79.4 | 1345 | 81.2 | 1394 | 54.9 |
| 1248 | 97.4 | 1297 | 79.1 | 1346 | 81.5 | 1395 | 54.9 |
| 1249 | 97.3 | 1298 | 78.8 | 1347 | 81.6 | 1396 | 54.7 |
| 1250 | 97.3 | 1299 | 78.5 | 1348 | 81.6 | 1397 | 54.1 |
| 1251 | 97.3 | 1300 | 78.2 | 1349 | 81.4 | 1398 | 53.2 |
| 1252 | 97.3 | 1301 | 77.9 | 1350 | 80.7 | 1399 | 52.1 |
| 1253 | 97.2 | 1302 | 77.6 | 1351 | 79.6 | 1400 | 50.7 |
| 1254 | 97.1 | 1303 | 77.3 | 1352 | 78.2 | 1401 | 49.1 |
| 1255 | 97.0 | 1304 | 77.0 | 1353 | 76.8 | 1402 | 47.4 |
| 1256 | 96.9 | 1305 | 76.7 | 1354 | 75.3 | 1403 | 45.2 |
| 1257 | 96.7 | 1306 | 76.0 | 1355 | 73.8 | 1404 | 41.8 |
| 1258 | 96.4 | 1307 | 76.0 | 1356 | 72.1 | 1405 | 36.5 |
| 1259 | 96.1 | 1308 | 76.0 | 1357 | 70.2 | 1406 | 31.2 |
| 1407 | 27.6 | 1456 | 0.0 |  |  |  |  |
| 1408 | 26.9 | 1457 | 0.0 |  |  |  |  |
| 1409 | 27.3 | 1458 | 0.0 |  |  |  |  |
| 1410 | 27.5 | 1459 | 0.0 |  |  |  |  |
| 1411 | 27.4 | 1460 | 0.0 |  |  |  |  |
| 1412 | 27.1 | 1461 | 0.0 |  |  |  |  |
| 1413 | 26.7 | 1462 | 0.0 |  |  |  |  |
| 1414 | 26.8 | 1463 | 0.0 |  |  |  |  |
| 1415 | 28.2 | 1464 | 0.0 |  |  |  |  |
| 1416 | 31.1 | 1465 | 0.0 |  |  |  |  |
| 1417 | 34.8 | 1466 | 0.0 |  |  |  |  |
| 1418 | 38.4 | 1467 | 0.0 |  |  |  |  |
| 1419 | 40.9 | 1468 | 0.0 |  |  |  |  |
| 1420 | 41.7 | 1469 | 0.0 |  |  |  |  |
| 1421 | 40.9 | 1470 | 0.0 |  |  |  |  |
| 1422 | 38.3 | 1471 | 0.0 |  |  |  |  |
| 1423 | 35.3 | 1472 | 0.0 |  |  |  |  |
| 1424 | 34.3 | 1473 | 0.0 |  |  |  |  |
| 1425 | 34.6 | 1474 | 0.0 |  |  |  |  |
| 1426 | 36.3 | 1475 | 0.0 |  |  |  |  |
| 1427 | 39.5 | 1476 | 0.0 |  |  |  |  |
| 1428 | 41.8 | 1477 | 0.0 |  |  |  |  |
| 1429 | 42.5 |  |  |  |  |  |  |
| 1430 | 41.9 |  |  |  |  |  |  |
| 1431 | 40.1 |  |  |  |  |  |  |
| 1432 | 36.6 |  |  |  |  |  |  |
| 1433 | 31.3 |  |  |  |  |  |  |
| 1434 | 26.0 |  |  |  |  |  |  |
| 1435 | 20.6 |  |  |  |  |  |  |
| 1436 | 19.1 |  |  |  |  |  |  |
| 1437 | 19.7 |  |  |  |  |  |  |
| 1438 | 21.1 |  |  |  |  |  |  |
| 1439 | 22.0 |  |  |  |  |  |  |
| 1440 | 22.1 |  |  |  |  |  |  |
| 1441 | 21.4 |  |  |  |  |  |  |
| 1442 | 19.6 |  |  |  |  |  |  |
| 1443 | 18.3 |  |  |  |  |  |  |
| 1444 | 18.0 |  |  |  |  |  |  |
| 1445 | 18.3 |  |  |  |  |  |  |
| 1446 | 18.5 |  |  |  |  |  |  |
| 1447 | 17.9 |  |  |  |  |  |  |
| 1448 | 15.0 |  |  |  |  |  |  |
| 1449 | 9.9 |  |  |  |  |  |  |
| 1450 | 4.6 |  |  |  |  |  |  |
| 1451 | 1.2 |  |  |  |  |  |  |
| 1452 | 0.0 |  |  |  |  |  |  |
| 1453 | 0.0 |  |  |  |  |  |  |
| 1454 | 0.0 |  |  |  |  |  |  |
| 1455 | 0.0 |  |  |  |  |  |  |

# Table A1/12

# **WLTC, Class 3 cycle, phase Extra High3 (Second 1477 is the start of this phase)**

| *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* | *Time in s* | *Speed in km/h* |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1478 | 0.0 | 1525 | 72.5 | 1572 | 120.7 | 1619 | 113.0 |
| 1479 | 2.2 | 1526 | 70.8 | 1573 | 121.8 | 1620 | 114.1 |
| 1480 | 4.4 | 1527 | 68.6 | 1574 | 122.6 | 1621 | 115.1 |
| 1481 | 6.3 | 1528 | 66.2 | 1575 | 123.2 | 1622 | 115.9 |
| 1482 | 7.9 | 1529 | 64.0 | 1576 | 123.6 | 1623 | 116.5 |
| 1483 | 9.2 | 1530 | 62.2 | 1577 | 123.7 | 1624 | 116.7 |
| 1484 | 10.4 | 1531 | 60.9 | 1578 | 123.6 | 1625 | 116.6 |
| 1485 | 11.5 | 1532 | 60.2 | 1579 | 123.3 | 1626 | 116.2 |
| 1486 | 12.9 | 1533 | 60.0 | 1580 | 123.0 | 1627 | 115.2 |
| 1487 | 14.7 | 1534 | 60.4 | 1581 | 122.5 | 1628 | 113.8 |
| 1488 | 17.0 | 1535 | 61.4 | 1582 | 122.1 | 1629 | 112.0 |
| 1489 | 19.8 | 1536 | 63.2 | 1583 | 121.5 | 1630 | 110.1 |
| 1490 | 23.1 | 1537 | 65.6 | 1584 | 120.8 | 1631 | 108.3 |
| 1491 | 26.7 | 1538 | 68.4 | 1585 | 120.0 | 1632 | 107.0 |
| 1492 | 30.5 | 1539 | 71.6 | 1586 | 119.1 | 1633 | 106.1 |
| 1493 | 34.1 | 1540 | 74.9 | 1587 | 118.1 | 1634 | 105.8 |
| 1494 | 37.5 | 1541 | 78.4 | 1588 | 117.1 | 1635 | 105.7 |
| 1495 | 40.6 | 1542 | 81.8 | 1589 | 116.2 | 1636 | 105.7 |
| 1496 | 43.3 | 1543 | 84.9 | 1590 | 115.5 | 1637 | 105.6 |
| 1497 | 45.7 | 1544 | 87.4 | 1591 | 114.9 | 1638 | 105.3 |
| 1498 | 47.7 | 1545 | 89.0 | 1592 | 114.5 | 1639 | 104.9 |
| 1499 | 49.3 | 1546 | 90.0 | 1593 | 114.1 | 1640 | 104.4 |
| 1500 | 50.5 | 1547 | 90.6 | 1594 | 113.9 | 1641 | 104.0 |
| 1501 | 51.3 | 1548 | 91.0 | 1595 | 113.7 | 1642 | 103.8 |
| 1502 | 52.1 | 1549 | 91.5 | 1596 | 113.3 | 1643 | 103.9 |
| 1503 | 52.7 | 1550 | 92.0 | 1597 | 112.9 | 1644 | 104.4 |
| 1504 | 53.4 | 1551 | 92.7 | 1598 | 112.2 | 1645 | 105.1 |
| 1505 | 54.0 | 1552 | 93.4 | 1599 | 111.4 | 1646 | 106.1 |
| 1506 | 54.5 | 1553 | 94.2 | 1600 | 110.5 | 1647 | 107.2 |
| 1507 | 55.0 | 1554 | 94.9 | 1601 | 109.5 | 1648 | 108.5 |
| 1508 | 55.6 | 1555 | 95.7 | 1602 | 108.5 | 1649 | 109.9 |
| 1509 | 56.3 | 1556 | 96.6 | 1603 | 107.7 | 1650 | 111.3 |
| 1510 | 57.2 | 1557 | 97.7 | 1604 | 107.1 | 1651 | 112.7 |
| 1511 | 58.5 | 1558 | 98.9 | 1605 | 106.6 | 1652 | 113.9 |
| 1512 | 60.2 | 1559 | 100.4 | 1606 | 106.4 | 1653 | 115.0 |
| 1513 | 62.3 | 1560 | 102.0 | 1607 | 106.2 | 1654 | 116.0 |
| 1514 | 64.7 | 1561 | 103.6 | 1608 | 106.2 | 1655 | 116.8 |
| 1515 | 67.1 | 1562 | 105.2 | 1609 | 106.2 | 1656 | 117.6 |
| 1516 | 69.2 | 1563 | 106.8 | 1610 | 106.4 | 1657 | 118.4 |
| 1517 | 70.7 | 1564 | 108.5 | 1611 | 106.5 | 1658 | 119.2 |
| 1518 | 71.9 | 1565 | 110.2 | 1612 | 106.8 | 1659 | 120.0 |
| 1519 | 72.7 | 1566 | 111.9 | 1613 | 107.2 | 1660 | 120.8 |
| 1520 | 73.4 | 1567 | 113.7 | 1614 | 107.8 | 1661 | 121.6 |
| 1521 | 73.8 | 1568 | 115.3 | 1615 | 108.5 | 1662 | 122.3 |
| 1522 | 74.1 | 1569 | 116.8 | 1616 | 109.4 | 1663 | 123.1 |
| 1523 | 74.0 | 1570 | 118.2 | 1617 | 110.5 | 1664 | 123.8 |
| 1524 | 73.6 | 1571 | 119.5 | 1618 | 111.7 | 1665 | 124.4 |
| 1666 | 125.0 | 1715 | 127.7 | 1764 | 82.0 |  |  |
| 1667 | 125.4 | 1716 | 128.1 | 1765 | 81.3 |  |  |
| 1668 | 125.8 | 1717 | 128.5 | 1766 | 80.4 |  |  |
| 1669 | 126.1 | 1718 | 129.0 | 1767 | 79.1 |  |  |
| 1670 | 126.4 | 1719 | 129.5 | 1768 | 77.4 |  |  |
| 1671 | 126.6 | 1720 | 130.1 | 1769 | 75.1 |  |  |
| 1672 | 126.7 | 1721 | 130.6 | 1770 | 72.3 |  |  |
| 1673 | 126.8 | 1722 | 131.0 | 1771 | 69.1 |  |  |
| 1674 | 126.9 | 1723 | 131.2 | 1772 | 65.9 |  |  |
| 1675 | 126.9 | 1724 | 131.3 | 1773 | 62.7 |  |  |
| 1676 | 126.9 | 1725 | 131.2 | 1774 | 59.7 |  |  |
| 1677 | 126.8 | 1726 | 130.7 | 1775 | 57.0 |  |  |
| 1678 | 126.6 | 1727 | 129.8 | 1776 | 54.6 |  |  |
| 1679 | 126.3 | 1728 | 128.4 | 1777 | 52.2 |  |  |
| 1680 | 126.0 | 1729 | 126.5 | 1778 | 49.7 |  |  |
| 1681 | 125.7 | 1730 | 124.1 | 1779 | 46.8 |  |  |
| 1682 | 125.6 | 1731 | 121.6 | 1780 | 43.5 |  |  |
| 1683 | 125.6 | 1732 | 119.0 | 1781 | 39.9 |  |  |
| 1684 | 125.8 | 1733 | 116.5 | 1782 | 36.4 |  |  |
| 1685 | 126.2 | 1734 | 114.1 | 1783 | 33.2 |  |  |
| 1686 | 126.6 | 1735 | 111.8 | 1784 | 30.5 |  |  |
| 1687 | 127.0 | 1736 | 109.5 | 1785 | 28.3 |  |  |
| 1688 | 127.4 | 1737 | 107.1 | 1786 | 26.3 |  |  |
| 1689 | 127.6 | 1738 | 104.8 | 1787 | 24.4 |  |  |
| 1690 | 127.8 | 1739 | 102.5 | 1788 | 22.5 |  |  |
| 1691 | 127.9 | 1740 | 100.4 | 1789 | 20.5 |  |  |
| 1692 | 128.0 | 1741 | 98.6 | 1790 | 18.2 |  |  |
| 1693 | 128.1 | 1742 | 97.2 | 1791 | 15.5 |  |  |
| 1694 | 128.2 | 1743 | 95.9 | 1792 | 12.3 |  |  |
| 1695 | 128.3 | 1744 | 94.8 | 1793 | 8.7 |  |  |
| 1696 | 128.4 | 1745 | 93.8 | 1794 | 5.2 |  |  |
| 1697 | 128.5 | 1746 | 92.8 | 1795 | 0.0 |  |  |
| 1698 | 128.6 | 1747 | 91.8 | 1796 | 0.0 |  |  |
| 1699 | 128.6 | 1748 | 91.0 | 1797 | 0.0 |  |  |
| 1700 | 128.5 | 1749 | 90.2 | 1798 | 0.0 |  |  |
| 1701 | 128.3 | 1750 | 89.6 | 1799 | 0.0 |  |  |
| 1702 | 128.1 | 1751 | 89.1 | 1800 | 0.0 |  |  |
| 1703 | 127.9 | 1752 | 88.6 |  |  |  |  |
| 1704 | 127.6 | 1753 | 88.1 |  |  |  |  |
| 1705 | 127.4 | 1754 | 87.6 |  |  |  |  |
| 1706 | 127.2 | 1755 | 87.1 |  |  |  |  |
| 1707 | 127.0 | 1756 | 86.6 |  |  |  |  |
| 1708 | 126.9 | 1757 | 86.1 |  |  |  |  |
| 1709 | 126.8 | 1758 | 85.5 |  |  |  |  |
| 1710 | 126.7 | 1759 | 85.0 |  |  |  |  |
| 1711 | 126.8 | 1760 | 84.4 |  |  |  |  |
| 1712 | 126.9 | 1761 | 83.8 |  |  |  |  |
| 1713 | 127.1 | 1762 | 83.2 |  |  |  |  |
| 1714 | 127.4 | 1763 | 82.6 |  |  |  |  |

7. Cycle identification

In order to confirm if the correct cycle version was chosen or if the correct cycle was implemented into the test bench operation system, checksums of the vehicle speed values for cycle phases and the whole cycle are listed in Table A1/13.

Table A1/13

# **1Hz checksums (as applicable)**

|  |  |  |
| --- | --- | --- |
| *Cycle class* | *Cycle phase* | *Checksum of 1 Hz target vehicle speeds* |
| Class 1 | Low | 11988.4 |
| Medium | 17162.8 |
| Low | 11988.4 |
| Total | 41139.6 |
| Class 2 | Low | 11162.2 |
| Medium | 17054.3 |
| High | 24450.6 |
| Extra High | 28869.8 |
| Total | 81536.9 |
| Class 3a | Low | 11140.3 |
| Medium | 16995.7 |
| High | 25646.0 |
| Extra High | 29714.9 |
| Total | 83496.9 |
| Class 3b | Low | 11140.3 |
| Medium | 17121.2 |
| High | 25782.2 |
| Extra High | 29714.9 |
| Total | 83758.6 |

8. Cycle modification

This paragraph shall not apply to OVC-HEVs, NOVC-HEVs and NOVC-FCHVs.

However, at the request of the manufacturer and with approval of the responsible authority, the downscaling procedure described in paragraph 8.2. of this annex may be applied for a NOVC-HEV using the maximum rated engine power as the maximum vehicle power rating on the applicable WLTP test cycle where the electric machine does not impact the maximum vehicle power.

In the case that the voltage of the traction REESS of a NOVC-HEV is less than 60V, the manufacturer shall supply technical evidence to the responsible authority that the electric machine does not impact the maximum vehicle power on the applicable WLTP test cycle .

In the case that the voltage of the traction REESS of a NOVC-HEV is equal to or greater than 60V, the manufacturer shall demonstrate to the responsible authority that the electric machine does not impact the maximum vehicle power on the applicable WLTP test cycle . Examples of such demonstration could include: torque/power profiles delivered from the engine and electric machine; electric machine operating envelopes; power curves; or other appropriate information to demonstrate the power delivery.

8.1. General remarks

Driveability problems may occur for vehicles with power to mass ratios close to the borderlines between Class 1 and Class 2 vehicles, or between Class 2 and Class 3 vehicles, or for very low powered vehicles in Class 1.

Since these problems are related mainly to cycle phases with a combination of high vehicle speed and high accelerations rather than to the maximum speed of the cycle, the downscaling procedure shall be applied to improve driveability.

8.2. This paragraph describes the method to modify the cycle profile using the downscaling procedure. The modified vehicle speed values calculated according to paragraphs 8.2.1. to 8.2.3. shall be rounded according to paragraph 6.1.8. of this Regulation to 1 place of decimal in a final step.

8.2.1. Downscaling procedure for Class 1 cycles

Figure A1/14 shows an example of a downscaled medium speed phase of the Class 1 WLTC.

# Figure A1/14

# **Downscaled medium speed phase of the Class 1 WLTC**



For the Class 1 cycle, the downscaling period is the time period between second 651 and second 906. Within this time period, the acceleration for the original cycle shall be calculated using the following equation:

where:

is the vehicle speed, km/h;

i is the time between second 651 and second 906.

The downscaling shall be applied first in the time period between second 651 and second 848. The downscaled speed trace shall be subsequently calculated using the following equation:

with .

For , .

In order to meet the original vehicle speed at second 907, a correction factor for the deceleration shall be calculated using the following equation:

where 36.7 km/h is the original vehicle speed at second 907.

The downscaled vehicle speed between second 849 and second 906 shall be subsequently calculated using the following equation:

For .

8.2.2. Downscaling procedure for Class 2 cycles

Since the driveability problems are exclusively related to the extra high speed phases of the Class 2 and Class 3 cycles, the downscaling is related to those time periods of the extra high speed phases where driveability problems are expected to occur (see Figures A1/15 and A1/16).

# Figure A1/15

# **Downscaled extra high speed phase of the Class 2 WLTC**



For the Class 2 cycle, the downscaling period is the time period between second 1520 and second 1742. Within this time period, the acceleration for the original cycle shall be calculated using the following equation:

where:

is the vehicle speed, km/h;

i is the time between second 1520 and second 1742.

The downscaling shall be applied first to the time period between second 1520 and second 1725. Second 1725 is the time when the maximum speed of the extra high speed phase is reached. The downscaled speed trace shall be subsequently calculated using the following equation:

for .

For , .

In order to meet the original vehicle speed at second 1743, a correction factor for the deceleration shall be calculated using the following equation:

90.4 km/h is the original vehicle speed at second 1743.

The downscaled vehicle speed between second 1726 and second 1742 shall be calculated using the following equation:

for .

8.2.3. Downscaling procedure for Class 3 cycles

Figure A1/16 shows an example for a downscaled extra high speed phase of the Class 3 WLTC.

# Figure A1/16

# **Downscaled extra high speed phase of the Class 3 WLTC**



For the Class 3 cycle, the downscaling period is the time period between second 1533 and second 1762. Within this time period, the acceleration for the original cycle shall be calculated using the following equation:

where:

is the vehicle speed, km/h;

i is the time between second 1533 and second 1762.

The downscaling shall be applied first in the time period between second 1533 and second 1724. Second 1724 is the time when the maximum speed of the extra high speed phase is reached. The downscaled speed trace shall be subsequently calculated using the following equation:

For .

For , .

In order to meet the original vehicle speed at second 1763, a correction factor for the deceleration shall be calculated using the following equation:

82.6 km/h is the original vehicle speed at second 1763.

The downscaled vehicle speed between second 1725 and second 1762 shall be subsequently calculated using the following equation:

For .

8.3. Determination of the downscaling factor (as applicable)

The downscaling factor is a function of the ratio between the maximum required power of the cycle phases where the downscaling is to be applied and the rated power of the vehicle, .

The maximum required power (in kW) is related to a specific time i and the corresponding vehicle speed vi in the cycle trace and is calculated using the following equation:

where:

, , are the applicable road load coefficients, N, N/(km/h), and N/(km/h)² respectively;

is the applicable test mass, kg;

vi is the speed at time i, km/h;

ai is the acceleration at time i, m/s².

The cycle time i at which maximum power or power values close to maximum power is required is second 764 for the Class 1 cycle, second 1574 for the Class 2 cycle and second 1566 for the Class 3 cycle.

The corresponding vehicle speed values, and acceleration values, , are as follows:

 km/h,  m/s² for Class 1,

 km/h,  m/s² for Class 2,

 km/h,  m/s² for Class 3.

shall be calculated using the following equation:

The downscaling factor, , shall be calculated using the following equations:

if , then

and no downscaling shall be applied.

If , then .

The calculation parameter/coefficients, , and , are as follows:

Class 1 , ,

Class 2 , , .

Class 3 , .

The resulting shall be rounded according to paragraph 6.1.8. of this Regulation to 3 places of decimal and shall be applied only if it exceeds 0.010.

The following data shall be recorded:

(a) fdsc;

(b) vmax;

(c) dcycle (distance driven), m.

The distance shall be calculated using the following equation:

dcycle = (, for

i = tstart + 1 to tend

tstart is the time at which the applicable test cycle starts (see paragraph 3 of this annex), s;

tend is the time at which the applicable test cycle ends (see paragraph 3 of this annex), s.

8.4. Additional requirements (as applicable)

For different vehicle configurations in terms of test mass and driving resistance coefficients, downscaling shall be applied individually.

If, after application of downscaling, the vehicle’s maximum speed is lower than the maximum speed of the cycle, the process described in paragraph 9. of this annex shall be applied with the applicable cycle.

If the vehicle cannot follow the speed trace of the applicable cycle within the tolerance at speeds lower than its maximum speed, it shall be driven with the accelerator control fully activated during these periods. During such periods of operation, speed trace violations shall be permitted.

9. Cycle modifications for vehicles with a maximum speed lower than the maximum speed of the cycle specified in the previous paragraphs of this annex

9.1. General remarks

This paragraph applies to vehicles that are technically able to follow the speed trace of the applicable cycle specified in paragraph 1. of this annex (base cycle) at speeds lower than its maximum speed, but whose maximum speed is limited to a value lower than the maximum speed of the base cycle for other reasons. For the purposes of this paragraph, the applicable cycle specified in paragraph 1. shall be referred to as the "base cycle" and is used to determine the capped speed cycle.

In the cases where downscaling according to paragraph 8.2. of this annex is applied, the downscaled cycle shall be used as the base cycle.

The maximum speed of the base cycle shall be referred to as vmax,cycle.

The maximum speed of the vehicle shall be referred to as its capped speed vcap.

If vcap is applied to a Class 3b vehicle, the Class 3b cycle as defined in paragraph 3.3.2. of this annex shall be used as the base cycle. This shall apply even if vcap is lower than 120 km/h.

In the cases where vcap is applied, the base cycle shall be modified as described in paragraph 9.2. of this annex in order to achieve the same cycle distance for the capped speed cycle as for the base cycle.

9.2. Calculation steps

9.2.1. Determination of the distance difference per cycle phase

An interim capped speed cycle shall be derived by replacing all vehicle speed samples vi where vi > vcap by vcap.

9.2.1.1. If vcap < vmax,medium, the distance of the medium speed phases of the base cycle dbase,medium and the interim capped speed cycle dcap,medium shall be calculated using the following equation for both cycles:

dmedium = (, for i = 590 to 1022

where:

vmax,medium is the maximum vehicle speed of the medium speed phase as listed in Table A1/2 for the Class 1 cycle, in Table A1/4 for the Class 2 cycle, in Table A1/8 for the Class 3a cycle and in Table A1/9 for the Class 3b cycle.

9.2.1.2. If vcap < vmax,high, the distances of the high speed phases of the base cycle dbase,high and the interim capped speed cycle dcap,high shall be calculated using the following equation for both cycles:

dhigh = (, for i = 1023 to 1477

vmax,high is the maximum vehicle speed of the high speed phase as listed in Table A1/5 for the Class 2 cycle, in Table A1/10 for the Class 3a cycle and in Table A1/11 for the Class 3b cycle.

9.2.1.3. The distances of the extra high speed phase of the base cycle dbase,exhigh and the interim capped speed cycle dcap,exhigh shall be calculated applying the following equation to the extra high speed phase of both cycles:

dexhigh = (, for i = 1478 to 1800

9.2.2. Determination of the time periods to be added to the interim capped speed cycle in order to compensate for distance differences

In order to compensate for a difference in distance between the base cycle and the interim capped speed cycle, corresponding time periods with vi = vcap shall be added to the interim capped speed cycle as described in paragraphs 9.2.2.1. to 9.2.2.3. inclusive of this annex.

9.2.2.1. Additional time period for the medium speed phase

If vcap < vmax,medium, the additional time period to be added to the medium speed phase of the interim capped speed cycle shall be calculated using the following equation:

Δtmedium =

The number of time samples nadd,medium with vi = vcap to be added to the medium speed phase of the interim capped speed cycle equals Δtmedium, rounded according to paragraph 6.1.8. of this Regulation to the nearest integer.

9.2.2.2. Additional time period for the high speed phase

If vcap < vmax,high, the additional time period to be added to the high speed phases of the interim capped speed cycle shall be calculated using the following equation:

Δthigh =

The number of time samples nadd,high with vi = vcap to be added to the high speed phase of the interim capped speed cycle equals Δthigh, rounded according to paragraph 6.1.8. of this Regulation to the nearest integer.

9.2.2.3. The additional time period to be added to the extra high speed phase of the interim capped speed cycle shall be calculated using the following equation:

Δtexhigh =

The number of time samples nadd,exhigh with vi = vcap to be added to the extra high speed phase of the interim capped speed cycle equals Δtexhigh, rounded according to paragraph 6.1.8. of this Regulation to the nearest integer.

9.2.3. Construction of the final capped speed cycle

9.2.3.1. Class 1 cycle

The first part of the final capped speed cycle consists of the vehicle speed trace of the interim capped speed cycle up to the last sample in the medium speed phase where v = vcap. The time of this sample is referred to as tmedium.

Then nadd,medium samples with vi = vcap shall be added, so that the time of the last sample is (tmedium + nadd,medium).

The remaining part of the medium speed phase of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1022 + nadd,medium).

9.2.3.2. Class 2 and Class 3 cycles

9.2.3.2.1. vcap < vmax,medium

The first part of the final capped speed cycle consists of the vehicle speed trace of the interim capped speed cycle up to the last sample in the medium speed phase where v = vcap. The time of this sample is referred to as tmedium.

Then nadd,medium samples with vi = vcap shall be added, so that the time of the last sample is (tmedium + nadd,medium).

The remaining part of the medium speed phase of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1022 + nadd,medium).

In a next step, the first part of the high speed phase of the interim capped speed cycle up to the last sample in the high speed phase where v = vcap shall be added. The time of this sample in the interim capped speed is referred to as thigh, so that the time of this sample in the final capped speed cycle is (thigh + nadd,medium).

Then, nadd,high samples with vi = vcap shall be added, so that the time of the last sample becomes (thigh + nadd,medium + nadd,high).

The remaining part of the high speed phase of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1477 + nadd,medium + nadd,high).

In a next step, the first part of the extra high speed phase (if applicable) of the interim capped speed cycle up to the last sample in the extra high speed phase where v = vcap shall be added. The time of this sample in the interim capped speed is referred to as texhigh, so that the time of this sample in the final capped speed cycle is (texhigh + nadd,medium + nadd,high).

Then nadd,exhigh samples with vi = vcap shall be added, so that the time of the last sample is (texhigh + nadd,medium + nadd,high + nadd,exhigh).

The remaining part of the extra high speed phase (if applicable) of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1800 + nadd,medium + nadd,high+ nadd,exhigh).

The length of the final capped speed cycle is equivalent to the length of the base cycle except for differences caused by the rounding process according to paragraph 6.1.8. of this Regulation for nadd,medium, nadd,high and nadd,exhigh.

9.2.3.2.2. vmax, medium ≤ vcap < vmax, high

The first part of the final capped speed cycle consists of the vehicle speed trace of the interim capped speed cycle up to the last sample in the high speed phase where v = vcap. The time of this sample is referred to as thigh.

Then, nadd,high samples with vi = vcap shall be added, so that the time of the last sample is (thigh + nadd,high).

The remaining part of the high speed phase of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1477 + nadd,high).

In a next step, the first part of the extra high speed phase (if applicable) of the interim capped speed cycle up to the last sample in the extra high speed phase where v = vcap shall be added. The time of this sample in the interim capped speed is referred to as texhigh, so that the time of this sample in the final capped speed cycle is (texhigh + nadd,high).

Then nadd,exhigh samples with vi = vcap shall be added, so that the time of the last sample is (texhigh + nadd,high + nadd,exhigh).

The remaining part of the extra high speed phase (if applicable) of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1800 + nadd,high+ nadd,exhigh).

The length of the final capped speed cycle is equivalent to the length of the base cycle except for differences caused by the rounding process according to paragraph 6.1.8. of this Regulation for nadd,high and nadd,exhigh.

9.2.3.2.3. vmax, high ≤ vcap < vmax, exhigh

The first part of the final capped speed cycle consists of the vehicle speed trace of the interim capped speed cycle up to the last sample in the extra high speed phase where v = vcap. The time of this sample is referred to as texhigh.

Then, nadd,exhigh samples with vi = vcap shall be added, so that the time of the last sample is (texhigh + nadd,exhigh).

The remaining part of the extra high speed phase of the interim capped speed cycle, which is identical with the same part of the base cycle, shall then be added, so that the time of the last sample is (1800 + nadd,exhigh).

The length of the final capped speed cycle is equivalent to the length of the base cycle except for differences caused by the rounding process according to paragraph 6.1.8. of this Regulation for nadd,exhigh.

10. Allocation of cycles to vehicles

10.1. A vehicle of a certain class shall be tested on the cycle of the same class, i.e. Class 1 vehicles on the Class 1 cycle, Class 2 vehicles on the Class 2 cycle, Class 3a vehicles on the Class 3a cycle, and Class 3b vehicles on the Class 3b cycle. However, at the request of the manufacturer and with approval of the responsible authority, a vehicle may be tested on a numerically higher cycle class, e.g. a Class 2 vehicle may be tested on a Class 3 cycle. In this case the differences between Classes 3a and 3b shall be respected and the cycle may be downscaled according to paragraphs 8. to 8.4. inclusive of this annex.

Annex B2

Gear selection and shift point determination for vehicles equipped with manual transmissions

1. General approach

1.1. The shifting procedures described in this annex shall apply to vehicles equipped with manual shift transmissions.

1.2. The prescribed gears and shifting points are based on the balance between the power required to overcome driving resistance and acceleration, and the power provided by the engine in all possible gears at a specific cycle phase.

1.3. The calculation to determine the gears to use shall be based on engine speeds and full load power curves versus engine speed.

1.4. For vehicles equipped with a dual-range transmission (low and high), only the range designed for normal on-road operation shall be considered for gear use determination.

1.5. The prescriptions for clutch operation shall not be applied if the clutch is operated automatically without the need of an engagement or disengagement of the driver.

1.6. This annex shall not apply to vehicles tested according to Annex B8.

2. Required data and precalculations

The following data are required and calculations shall be performed in order to determine the gears to be used when driving the cycle on a chassis dynamometer:

(a) , the maximum rated engine power as declared by the manufacturer, kW;

(b) nrated, the rated engine speed declared by the manufacturer as the engine speed at which the engine develops its maximum power, min-1;

(c) , idling speed, min-1.

nidle shall be measured over a period of at least 1 minute at a sampling rate of at least 1 Hz with the engine running in warm condition, the gear lever placed in neutral, and the clutch engaged. The conditions for temperature, peripheral and auxiliary devices, etc. shall be the same as described in Annex B6 for the Type 1 test.

The value to be used in this annex shall be the arithmetic average over the measuring period and rounded according to paragraph 6.1.8. of this Regulation to the nearest 10 min-1;

(d) ng, the number of forward gears.

The forward gears in the transmission range designed for normal on-road operation shall be numbered in descending order of the ratio between engine speed in min-1 and vehicle speed in km/h. Gear 1 is the gear with the highest ratio, gear ng is the gear with the lowest ratio. ng determines the number of forward gears;

(e) (n/v)i, the ratio obtained by dividing the engine speed n by the vehicle speed v for each gear i, for i = 1 to ng, min-1/(km/h). (n/v)i shall be calculated according to the equations in paragraph 8. of Annex B7;

(f) , , , road load coefficients selected for testing, N, N/(km/h), and N/(km/h)² respectively;

(g) nmax

nmax1 = n95\_high, the maximum engine speed where 95 per cent of rated power is reached, min – 1;

If n95\_high cannot be determined because the engine speed is limited to a lower value nlim for all gears and the corresponding full load power is higher than 95 per cent of rated power, n95\_high shall be set to nlim.

nmax2 = (n/v)( ngvmax) × vmax,cycle

nmax3 = (n/v)( ngvmax) × vmax,vehicle

where:

vmax,cycle is the maximum speed of the vehicle speed trace according to Annex B1, km/h;

vmax,vehicle is the maximum speed of the vehicle according to paragraph 2.(i) of this annex, km/h;

(n/v)(ngvmax) is the ratio obtained by dividing engine speed n by the vehicle speed v for the gear ngvmax, min-1/(km/h );

ngvmax is defined in paragraph 2.(i) of this annex;

nmax is the maximum of nmax1, nmax2 and nmax3, min-1.

(h) Pwot(n), the full load power curve over the engine speed range

The power curve shall consist of a sufficient number of data sets (n, Pwot) so that the calculation of interim points between consecutive data sets can be performed by linear interpolation. Deviation of the linear interpolation from the full load power curve according to UN Regulation No. 85 shall not exceed 2 per cent. The first data set shall be at nmin\_drive\_set (see (k)(3) below) or lower. The last data set shall be at nmax or higher engine speed. Data sets need not be spaced equally but all data sets shall be reported.

The data sets and the values Prated and nrated shall be taken from the power curve as declared by the manufacturer.

The full load power at engine speeds not covered by UN Regulation No. 85 shall be determined according to the method described in UN Regulation No. 85;

(i) Determination of ngvmax and vmax

ngvmax, the gear in which the maximum vehicle speed is reached and shall be determined as follows:

If vmax(ng) ≥ vmax(ng-1) and vmax(ng-1) ≥ vmax(ng-2), then:

ngvmax = ng and vmax = vmax(ng).

If vmax(ng) < vmax(ng-1) and vmax(ng-1) ≥ vmax(ng-2), then:

ngvmax = ng-1 and vmax = vmax(ng-1),

otherwise, ngvmax = ng -2 and vmax = vmax(ng-2)

where:

vmax(ng) is the vehicle speed at which the required road load power equals the available power Pwot in gear ng (see Figure A2/1a).

vmax(ng-1) is the vehicle speed at which the required road load power equals the available power Pwot in the next lower gear (gear ng-1). See Figure A2/1b.

vmax(ng-2) is the vehicle speed at which the required road load power equals the available power Pwot in the gear ng-2.

Vehicle speed values rounded according to paragraph 6.1.8. of this Regulation to one place of decimal shall be used for the determination of vmax and ngvmax.

The required road load power, kW, shall be calculated using the following equation:

where:

vis the vehicle speed specified above, km/h.

The available power at vehicle speed vmax in gear ng, gear ng - 1 or gear ng-2 shall be determined from the full load power curve, Pwot(n), by using the following equations:

nng = (n/v)ng × vmax(ng);

nng-1 = (n/v)ng-1 × vmax(ng-1);

nng-2 = (n/v)ng-2 × vmax(ng-2),

and by reducing the power values of the full load power curve by 10 per cent.

The method described above shall be extended to even lower gears, i.e. ng- 3, ng-4, etc. if necessary.

If, for the purpose of limiting maximum vehicle speed, the maximum engine speed is limited to nlim which is lower than the engine speed corresponding to the intersection of the road load power curve and the available power curve, then:

ngvmax = ng and vmax = nlim / (n/v)(ng).

Figure A2/1a

**An example where ngvmax is the highest gear**



Figure A2/1b

**An example where ngvmax is the 2nd highest gear**



(j) Exclusion of a crawler gear

Gear 1 may be excluded at the request of the manufacturer if all of the following conditions are fulfilled:

(1) The vehicle family is homologated to tow a trailer;

(2) (n/v)1 × (vmax / n95\_high) > 6.74;

(3) (n/v)2 × (vmax / n95\_high) > 3.85;

(4) The vehicle, having a mass mt as defined in the equation below, is able to pull away from standstill within 4 seconds, on an uphill gradient of at least 12 per cent, on five separate occasions within a period of 5 minutes.

mt = mr0 + 25 kg + (MC – mr0 – 25 kg) × 0.28

(factor 0.28 in the above equation shall be used for category 2 vehicles with a gross vehicle mass up to 3.5 tons and shall be replaced by factor 0.15 in the case of category 1 vehicles),

where:

vmax is the maximum vehicle speed as specified in paragraph 2. (i) of this annex. Only the vmax value resulting from the intersection of the required road load power curve and the available power curve of the relevant gear shall be used for the conditions in (2) and (3) above. A vmax value resulting from a limitation of the engine speed which prevents this intersection of curves shall not be used;

(n/v)(ngvmax) is the ratio obtained by dividing the engine speed n by the vehicle speed v for gear ngvmax, min-1/(km/h);

mr0 is the mass in running order, kg;

MC is the technically permissible maximum laden mass of the combination (see paragraph 3.2.27. of this Regulation), kg.

In this case, gear 1 shall not be used when driving the cycle on a chassis dynamometer and the gears shall be renumbered starting with the second gear as gear 1.

(k) Definition of nmin\_drive

nmin\_drive is the minimum engine speed when the vehicle is in motion, min-1;

(1) For ngear = 1, nmin\_drive = nidle,

(2) For ngear = 2,

(i) for transitions from first to second gear:

nmin\_drive = 1.15 ×nidle,

(ii) for decelerations to standstill:

nmin\_drive = nidle,

(iii) for all other driving conditions:

nmin\_drive = 0.9 × nidle.

(3) For ngear > 2, nmin\_drive shall be determined by:

nmin\_drive = nidle + 0.125 × (nrated -nidle).

This value shall be referred to as nmin\_drive\_set.

nmin\_drive\_set shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest integer.

Values higher than nmin\_drive\_set may be used for ngear > 2 if requested by the manufacturer. In this case, the manufacturer may specify one value for acceleration/constant speed phases (nmin\_drive\_up) and a different value for deceleration phases (nmin\_drive\_down).

Samples which have acceleration values ≥ -0.1389 m/s² shall belong to the acceleration/constant speed phases. This phase specification shall only be used for the determination of the initial gear according to paragraph 3.5. of this annex and shall not be applied to the requirements specified in paragraph 4. of this annex.

In addition, for an initial period of time (tstart\_phase), the manufacturer may specify higher values (nmin\_drive\_start or nmin\_drive\_up\_start and nmin\_drive\_down\_start) for the values nmin\_drive or nmin\_drive\_up and nmin\_drive\_down for ngear > 2 than specified above.

The initial time period shall be specified by the manufacturer but shall not exceed the low speed phase of the cycle and shall end in a stop phase so that there is no change of nmin\_drive within a short trip.

All individually chosen nmin\_drive values shall be equal to or higher than nmin\_drive\_set but shall not exceed (2 × nmin\_drive\_set).

All individually chosen nmin\_drive values and tstart\_phase shall be recorded.

Only nmin\_drive\_set shall be used as the lower limit for the full load power curve according to paragraph 2(h) above.

(l) , test mass of the vehicle, kg.

3. Calculations of required power, engine speeds, available power, and possible gear to be used

3.1. Calculation of required power

For each second j of the cycle trace, the power required to overcome driving resistance and to accelerate shall be calculated using the following equation:

where:

is the required power at second j, kW;

is the vehicle acceleration at second j, m/s², and is calculated as follows:

;

j = tstart to tend – 1,

tstart is the time at which the applicable test cycle starts (see paragraph 3 of Annex B1 of this Regulation), s;

tend is the time at which the applicable test cycle ends (see paragraph 3 of Annex B1 of this Regulation), s;

The acceleration value at second tend (second 1611 for class 1 cycle and second 1800 for class 2 and 3 cycles) may be set to 0 in order to avoid empty cells.

is a factor taking the inertial resistances of the drivetrain during acceleration into account and is set to 1.03.

3.2. Determination of engine speeds

For any  km/h, it shall be assumed that the vehicle is standing still and the engine speed shall be set to .The gear lever shall be placed in neutral with the clutch engaged except 1 second before beginning an acceleration from standstill where first gear shall be selected with the clutch disengaged.

For each  km/h of the cycle trace and each gear i, to ng the engine speed, , shall be calculated using the following equation:

The calculation shall be performed with floating point numbers; the results shall not be rounded.

3.3. Selection of possible gears with respect to engine speed

The following gears may be selected for driving the speed trace at vj:

(a) All gears i < ngvmax where nmin\_drive ≤ ni,j ≤ nmax1;

(b) All gears i ≥ ngvmax where nmin\_drive ≤ ni,j ≤ nmax2;

(c) Gear 1, if n1,j < nmin\_drive.

If aj < 0 and ni,j ≤ nidle, ni,j shall be set to nidle and the clutch shall be disengaged.

If aj ≥ 0 and ni,j < max(1.15 × nidle ; min. engine speed of the Pwot(n) curve), ni,j shall be set to the maximum of (1.15 × nidle) or the min. engine speed of the Pwot(n) curve, and the clutch shall be set to “undefined”.

“Undefined” covers any status of the clutch between disengaged and engaged, depending on the individual engine and transmission design. In such a case, the real engine speed may deviate from the calculated engine speed.

With regard to the definition of nmin\_drive in paragraph 2 (k) the requirements (a) to (c) specified above can be expressed as follows for deceleration phases:

During a deceleration phase, gears with ngear > 2 shall be used as long as the engine speed does not drop below nmin\_drive.

Gear 2 shall be used during a deceleration phase within a short trip of the cycle (not at the end of a short trip) as long as the engine speed does not drop below (0.9 × nidle).

If the engine speed drops below nidle, the clutch shall be disengaged.

If the deceleration phase is the last part of a short trip shortly before a stop phase, the second gear shall be used as long as the engine speed does not drop below nidle. This requirement shall be applied to the whole deceleration phase ending at standstill.

A deceleration phase is a time period of more than 2 seconds with a vehicle speed ≥ 1.0 km/h and with strictly monotonic decrease of vehicle speed (see paragraph 4. of this annex).

3.4. Calculation of available power

For each engine speed value nk of the full load power curve as specified in paragraph 2 (h) of this annex the available power, Pavailable\_k, shall be calculated using the following equation:

where:

is the power available at nk at full load condition from the full load power curve;

is a safety margin accounting for the difference between the stationary full load condition power curve and the power available during transition conditions. SM shall be set to 10 per cent;

ASM is an additional power safety margin which may be applied at the request of the manufacturer.

When requested, the manufacturer shall provide the ASM values (in per cent reduction of the wot power) together with data sets for Pwot(n) as shown by the example in Table A2/1. Linear interpolation shall be used between consecutive data points. ASM is limited to 50 per cent.

The application of an ASM requires the approval of the responsible authority.

Table A2/1

| *n* | *Pwot* | *SM*  *per cent* | *ASM*  *per cent* | *Pavailable* |
| --- | --- | --- | --- | --- |
| *min-1* | *kW* | *kW* |
| 700 | 6.3 | 10.0 | 20.0 | 4.4 |
| 1000 | 15.7 | 10.0 | 20.0 | 11.0 |
| 1500 | 32.3 | 10.0 | 15.0 | 24.2 |
| 1800 | 56.6 | 10.0 | 10.0 | 45.3 |
| 1900 | 59.7 | 10.0 | 5.0 | 50.8 |
| 2000 | 62.9 | 10.0 | 0.0 | 56.6 |
| 3000 | 94.3 | 10.0 | 0.0 | 84.9 |
| 4000 | 125.7 | 10.0 | 0.0 | 113.2 |
| 5000 | 157.2 | 10.0 | 0.0 | 141.5 |
| 5700 | 179.2 | 10.0 | 0.0 | 161.3 |
| 5800 | 180.1 | 10.0 | 0.0 | 162.1 |
| 6000 | 174.7 | 10.0 | 0.0 | 157.3 |
| 6200 | 169.0 | 10.0 | 0.0 | 152.1 |
| 6400 | 164.3 | 10.0 | 0.0 | 147.8 |
| 6600 | 156.4 | 10.0 | 0.0 | 140.8 |

For each possible gear i and each vehicle speed value of the cycle trace (j as specified in paragraph 3.1 of this annex) and each engine speed value ni,j ≥ nmin of the full load power curve the available power shall be calculated from adjacent nk, Pavailable\_k values of the full load power curve by linear interpolation.

3.5. Determination of possible gears to be used

The possible gears to be used shall be determined by the following conditions:

(a) The conditions of paragraph 3.3. of this annex are fulfilled, and

(b) For ngear > 2, if

The initial gear to be used for each second of the cycle trace is the highest final possible gear, imax. When starting from standstill, only the first gear shall be used.

The lowest final possible gear is imin.

4. Additional requirements for corrections and/or modifications of gear use

The initial gear selection shall be checked and modified in order to avoid too frequent gearshifts and to ensure driveability and practicality.

An acceleration phase is a time period of more than 2 seconds with a vehicle speed ≥ 1.0 km/h and with strictly monotonic increase of vehicle speed. A deceleration phase is a time period of more than 2 seconds with a vehicle speed ≥ 1.0 km/h and with strictly monotonic decrease of vehicle speed. A constant speed phase is a time period of more than 2 seconds with a constant vehicle speed ≥ 1.0 km/h.

The end of an acceleration/deceleration phase is determined by the last time sample in which the vehicle speed is higher/lower than the vehicle speed of the previous time sample. In this context the end of a deceleration phase could be the beginning of an acceleration phase. In this case the requirements for acceleration phases overrule the requirements for deceleration phases.

Corrections and/or modifications shall be made according to the following requirements:

The modification check described in paragraph 4.(a) of this annex shall be applied to the complete cycle trace twice prior to the application of paragraphs 4.(b) to 4.(f) of this annex.

(a) If a one step higher gear (n+1) is required for only 1 second and the gears before and after are the same (n) or one of them is one step lower (n – 1), gear (n + 1) shall be corrected to gear n.

Examples:

Gear sequence i - 1, i, i - 1 shall be replaced by:

i - 1, i - 1, i - 1;

Gear sequence i - 1, i, i - 2 shall be replaced by:

i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1.

If, during acceleration or constant speed phases or transitions from constant speed to acceleration or acceleration to constant speed phases where these phases only contain upshifts, a gear is used for only one second, the gear in the following second shall be corrected to the gear before, so that a gear is used for at least 2 seconds.

Examples:

Gear sequence 1, 2, 3, 3, 3, 3, 3 shall be replaced by:

1, 1, 2, 2, 3, 3, 3.

Gear sequence 1, 2, 3, 4, 5, 5, 6, 6, 6, 6, 6 shall be replaced by:

1, 1, 2, 2, 3, 3, 4, 4, 5, 5, 6.

This requirement shall not be applied to downshifts during an acceleration phase or if the use of a gear for just one second follows immediately after such a downshift or if the downshift occurs right at the beginning of an acceleration phase. In these cases, the downshifts shall be first corrected according to paragraph 4.(b) of this annex.

Example:

Gear sequence 4, 4, 3, 4, 5, 5, 5, where the first second or the third second determines the start of an acceleration phase and where paragraph 4.(b) does not apply in the further course of the acceleration phase, shall be replaced by:

4, 4, 4, 4, 5, 5, 5.

However, if the gear at the beginning of an acceleration phase is one step lower than the gear in the previous second and the gears in the following (up to five) seconds are the same as the gear in the previous second but followed by a downshift, so that the application of paragraph 4.(c) would correct them to the same gear as at the beginning of the acceleration phase, the application of paragraph 4.(c) should be performed instead.

Example:

For a speed trace sequence

19.6 18.3 18.0 18.3 18.5 17.9 15.0 km/h

with an initial gear use of

3 3 2 3 3 2 2,

the gears in the fourth and fifth second shall be corrected to a one step lower gear (which would be done by an application of paragraph 4.(c)) instead of a correction of the gear at the beginning of the acceleration phase (second three), so that the correction results in the following gear sequence

3 3 2 2 2 2 2

Furthermore, if the gear in the first second of an acceleration phase is the same as the gear in the previous second and the gear in the following seconds is one step higher, the gear in the 2nd second of the acceleration phase shall be replaced by the gear used in the first second of the acceleration phase.

Example:

For a speed trace sequence

30.9 25.5 21.4 20.2 22.9 26.6 30.2 km/h

with an initial gear use of

3 3 2 2 3 3 3,

the gear in the fifth second (the 2nd second of the acceleration phase) shall be corrected to a one step lower gear in order to ensure the use of a gear within the acceleration phase for at least two seconds, so that the correction results in the following gear sequence

3 3 2 2 2 3 3

Gears shall not be skipped during upshifts within acceleration phases.

However, an upshift by two gears is permitted at the transition from an acceleration phase to a constant speed phase if the duration of the constant speed phase exceeds 5 seconds.

(b) If a downshift is required during an acceleration phase or at the beginning of the acceleration phase, the gear required during this downshift shall be noted (iDS). The starting point of a correction procedure is defined by either the last previous second when iDS was identified or by the starting point of the acceleration phase if all time samples before have gears > iDS. The highest gear of the time samples before the downshift determines the reference gear iref for the downshift. A downshift where iDS = iref – 1 is referred to as a one step downshift, a downshift where iDS = iref – 2 is referred to as a two step downshift, a downshift where iDS = iref – 3 is referred to as a three step downshift. The following check shall then be applied.

(i) One step downshifts

Working forward from the starting point of the correction procedure to the end of the acceleration phase, the latest occurrence of a 10 second window containing iDS for either 2 or more consecutive seconds, or 2 or more individual seconds, shall be identified. The last usage of iDS in this window defines the end point of the correction procedure. Between the start and end of the correction period, all requirements for gears greater than iDS shall be corrected to a requirement of iDS.

From the end of the correction period (in case of 10 second windows containing iDS for either 2 or more consecutive seconds, or 2 or more individual seconds) or from the starting point of the correction procedure (in case that all 10 second windows contain iDS only for one second or some 10 second windows contain no iDS at all) to the end of the acceleration phase all downshifts with a duration of only one second shall be removed.

(ii) Two or three step downshifts

Working forward from the starting point of the correction procedure to the end of the acceleration phase, the latest occurrence of iDS shall be identified. From the starting point of the correction procedure all requirements for gears greater than or equal to iDS up to the latest occurrence of iDS shall be corrected to (iDS + 1).

(iii) One step downshifts and two step and/or three step downshifts

If one step downshifts as well as two step and/or three step downshifts occur during an acceleration phase, three step downshifts shall be corrected before two or one step downshifts are corrected and two step downshifts shall be corrected before one step downshifts are corrected. In such cases, the starting point of the correction procedure for the two or one step downshifts is the second immediately following the end of the correction period for the three step downshifts and the starting point of the correction procedure for the one step downshifts is the second immediately following the end of the correction period for the two step downshifts. If a three step downshift occurs after a one or two step downshift, it shall overrule these downshifts in the time period before the three step downshift. If a two step downshift occurs after a one step downshift, it shall overrule the one step downshift in the time period before the two step downshift.

Examples are shown in Tables A2/2 to A2/6.

Table A2/2




Table A2/3




Table A2/4




Table A2/5





Table A2/6



This correction shall not be performed for gear 1. The requirements of the 3rd sub-paragraph of paragraph 3.3. (If aj ≥ 0…..) shall not be applied for gear corrections described in this paragraph for gears > 2.

The modification check described in paragraph 4.(c) of this annex shall be applied to the complete cycle trace twice prior to the application of paragraphs 4.(d) to 4.(f) of this annex.

(c) If gear is used for a time sequence of 1 to 5 seconds and the gear prior to this sequence is one step lower and the gear after this sequence is one or two steps lower than within this sequence or the gear prior to this sequence is two steps lower and the gear after this sequence is one step lower than within the sequence, the gear for the sequence shall be corrected to the maximum of the gears before and after the sequence.

Examples:

(i) Gear sequence i -1, , i -1 shall be replaced by:

i -1, i -1, i -1;

Gear sequence i - 1, i, i - 2 shall be replaced by:

i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1.

(ii) Gear sequence i - 1, , , i - 1 shall be replaced by:

i - 1, i - 1, i - 1, i - 1;

Gear sequence i - 1, i, i, i - 2 shall be replaced by:

i- 1, i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1, i - 1.

(iii) Gear sequence i - 1, , ,, i - 1shall be replaced by:

i – 1, i – 1, i – 1, i – 1, i - 1;

Gear sequence i-1, i, i, i, i - 2 shall be replaced by:

i - 1, i - 1, i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1, i - 1, i - 1.

(iv) Gear sequence i - 1, ,, , , i - 1 shall be replaced by:

i - 1, i - 1, i - 1, i - 1, i - 1, i - 1;

Gear sequence i - 1, i, i, i, i, i - 2 shall be replaced by:

i - 1, i - 1, i - 1, i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i, i, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1, i - 1, i - 1, i - 1.

(v) Gear sequence i - 1, ,,, , , i - 1 shall be replaced by:

i - 1, i - 1, i - 1, i - 1, i - 1, i – 1, i - 1;

Gear sequence i-1, i, i, i, i, i, i - 2 shall be replaced by:

i - 1, i - 1, i - 1, i - 1, i - 1, i - 1, i - 2;

Gear sequence i - 2, i, i, i, i, i, i - 1 shall be replaced by:

i - 2, i - 1, i - 1, i - 1, i - 1, i - 1, i - 1.

In all cases (i) to (v), i-1 ≥ imin shall be fulfilled.

(d) No upshift to a higher gear shall be performed within a deceleration phase.

(e) No upshift to a higher gear at the transition from an acceleration or constant speed phase to a deceleration phase shall be performed if one of the gears in the first two seconds following the end of the deceleration phase is lower than the upshifted gear or is gear 0.

Example:

If vi ≤ vi+1 and vi+2 < vi+1 and gear i = 4 and gear (i + 1 = 5) and gear (i + 2 = 5), then gear (i + 1) and gear (i + 2) shall be set to 4 if the gear for the phase following the deceleration phase is gear 4 or lower. For all following cycle trace points with gear 5 within the deceleration phase, the gear shall also be set to 4. If the gear following the deceleration phase is gear 5, an upshift shall be performed.

If there is an upshift during the transition and the initial deceleration phase by 2 gears, an upshift by 1 gear shall be performed instead. In this case, no further modifications shall be performed in the following gear use checks.

(f) Other gear modifications for deceleration phases

A downshift to first gear is not permitted during deceleration phases. If such a downshift would be necessary in the last part of a short trip just before a stop phase, since the engine speed would drop below nidle in 2nd gear, gear 0 shall be used instead and the gear lever shall be placed in neutral and the clutch shall be engaged.

If the first gear is required in a time period of at least 2 seconds immediately before a deceleration to stop, this gear should be used until the first sample of the deceleration phase. For the rest of the deceleration phase, gear 0 shall be used and the gear lever shall be placed in neutral and the clutch shall be engaged.

If during a deceleration phase the duration of a gear period (a time sequence with constant gear) between two gear periods of 3 seconds or more is only 1 second, it shall be replaced by gear 0 and the clutch shall be disengaged.

If during a deceleration phase the duration of a gear period between two gear periods of 3 seconds or more is 2 seconds, it shall be replaced by gear 0 for the 1st second and for the 2nd second with the gear that follows after the 2 second period. The clutch shall be disengaged for the 1st second.

Example: A gear sequence 5, 4, 4, 2 shall be replaced by 5, 0, 2, 2.

This requirement shall only be applied if the gear that follows after the 2 second period is > 0.

If several gear periods with durations of 1 or 2 seconds follow one another, corrections shall be performed as follows:

A gear sequence i, i, i, i - 1, i - 1, i - 2 or i, i, i, i - 1, i - 2, i - 2 shall be changed to i, i, i, 0, i - 2, i - 2.

A gear sequence such as i, i, i, i - 1, i - 2, i - 3 or i, i, i, i - 2, i - 2, i - 3 or other possible combinations shall be changed to i, i, i, 0, i - 3, i - 3.

This change shall also be applied to gear sequences where the acceleration is ≥ 0 for the first 2 seconds and < 0 for the 3rd second or where the acceleration is ≥ 0 for the last 2 seconds.

For extreme transmission designs, it is possible that gear periods with durations of 1 or 2 seconds following one another may last up to 7 seconds. In such cases, the correction above shall be complemented by the following correction requirements in a second step.

A gear sequence j, 0, i, i, i - 1, k with j > (i + 1) and k ≤ (i – 1) but k > 0 shall be changed to j, 0, i - 1, i - 1, i - 1, k, if gear (i – 1) is one or two steps below imax for second 3 of this sequence (one after gear 0).

If gear (i – 1) is more than two steps below imax for second 3 of this sequence, a gear sequence j, 0, i, i, i - 1, k with j > (i + 1) and   
k ≤ (i –1) but k > 0 shall be changed to j, 0, 0, k, k, k.

A gear sequence j, 0, i, i, i-2, k with j > (i + 1) and k ≤ (i – 2) but k > 0 shall be changed to j, 0, i - 2, i - 2 , i - 2, k, if gear (i – 2) is one or two steps below imax for second 3 of this sequence (one after gear 0).

If gear (i – 2) is more than two steps below imax for second 3 of this sequence, a gear sequence j, 0, i, i, i - 2, k with j > (i + 1) and   
k ≤ (i – 2) but k > 0 shall be changed to j, 0, 0, k, k, k.

In all cases specified above in this sub-paragraph (paragraph 4.(f) of this annex), the clutch disengagement (gear 0) for 1 second is used in order to avoid too high engine speeds for this second. If this is not an issue and, if requested by the manufacturer, it is allowed to use the lower gear of the following second directly instead of gear 0 for downshifts of up to 3 steps. The use of this option shall be recorded.

If the deceleration phase is the last part of a short trip shortly before a stop phase and the last gear > 0 before the stop phase is used only for a period of up to 2 seconds, gear 0 shall be used instead and the gear lever shall be placed in neutral and the clutch shall be engaged.

Examples: A gear sequence of 4, 0, 2, 2, 0 for the last 5 seconds before a stop phase shall be replaced by 4, 0, 0, 0, 0. A gear sequence of 4, 3, 3, 0 for the last 4 seconds before a stop phase shall be replaced by 4, 0, 0, 0.

5. Final requirements

(a) Paragraphs 4.(a) to 4.(f) inclusive of this annex shall be applied sequentially, scanning the complete cycle trace in each case. Since modifications to paragraphs 4.(a) to 4.(f) inclusive of this annex may create new gear use sequences, these new gear sequences shall be checked twice and modified if necessary.

(b) After the application of paragraph 4.(b) of this annex, a downshift by more than one gear could occur at the transition from a deceleration or constant speed phase to an acceleration phase.

In this case, the gear for the last sample of the deceleration or constant speed phase shall be replaced by gear 0 and the clutch shall be disengaged. If the “suppress gear 0 during downshifts” option according to paragraph 4.(f) of this annex is chosen, the gear of the following second (first second of the acceleration phase) shall be used instead of gear 0.

1. In order to enable the assessment of the correctness of the calculation, the checksum of v\*gear for v ≥ 1.0 km/h, rounded according to paragraph 6.1.8. of this Regulation to four places of decimal, shall be calculated and recorded.

6. Calculation tools

Examples of gear shift calculating tools can be found in the UN GTR No. 15 webpage on the UNECE website.[[17]](#footnote-18)

The following tools are provided:

(a) ACCESS based tool;

(b) Matlab code tool;

(c) .NET framework tool;

(d) Python based tool.

These tools were validated by the comparison of calculation results between the ACCESS tool, the Matlab code, the .NET framework code and the Python based tool for 115 different vehicle configurations supplemented by additional calculations for 7 of them with additional options like "apply speed cap", "suppress downscaling", "choose other vehicle class cycle" and "choose individual nmin\_drive values".

The 115 vehicle configurations cover extreme technical designs for transmission and engines and all vehicle classes.

All four tools deliver identical results with respect to gear use and clutch operation and although only the text in Annexes B1 and B2 is legally binding the tools have achieved a status that qualifies them as reference tools.

Annex B3

Specifications of reference fuels

1. This annex provides information relating to the specification for the reference fuels to be used when conducting Type 1 tests.

2. (Reserved)

3. Technical data on liquid fuels for testing vehicles with positive-ignition engines

3.1. (Reserved)

# 3.2. (Reserved)

# 3.3. (Reserved)

3.4. (Reserved)

# 3.5. (Reserved)

3.6. Gasoline/petrol

Table A3/6

# **Gasoline/petrol (E10H)**

| *Parameter* | *Unit* | *Limits (*a*)* | | | *Test method (*b*)* |
| --- | --- | --- | --- | --- | --- |
| *Minimum* | | *Maximum* |
| Research octane number, RON (c) |  | 95.0 | | 98.0 | EN ISO 5164  JIS K2280 |
| Motor octane number, MON (c) |  | 85.0 | | 89.0 | EN ISO 5163  JIS K2280 |
| Density at 15 °C | kg/m3 | 743.0 | | 756.0 | EN ISO 12185  JIS K2249-1,2,3 |
| Vapour pressure | kPa | 56.0 | | 60.0 | EN 13016-1  JIS K2258 |
| Water content | % v/v |  | | 0.05 | EN 12937 |
| Appearance at -7 °C |  | clear and bright | | |  |
| Distillation: |  |  | |  |  |
| — evaporated at 70 °C | % v/v | 34.0 | | 46.0 | EN-ISO 3405 |
| — evaporated at 100 °C | % v/v | 54.0 | | 62.0 | EN-ISO 3405 |
| — evaporated at 150 °C | % v/v | 86.0 | | 94.0 | EN-ISO 3405 |
| — final boiling point | °C | 170 | | 195 | EN-ISO 3405 |
| Residue | % v/v |  | | 2.0 | EN-ISO 3405 |
| Hydrocarbon analysis: |  |  | |  |  |
| — olefins | % v/v | 6.0 | | 13.0 | EN 22854  JIS K2536-1,2 |
| — aromatics | % v/v | 25.0 | | 32.0 | EN 22854  JIS K2536-1,2,3 |
| — benzene | % v/v |  | | 1.00 | EN 22854  EN 238  JIS K2536-2,3,4 |
| — saturates | % v/v | To be recorded | | | EN 22854 |
| Carbon/hydrogen ratio |  | To be recorded | | |  |
| Carbon/oxygen ratio |  | To be recorded | | |  |
| Induction period (d) | minutes | 480 |  | | EN-ISO 7536 |
| Oxygen content (e) | % m/m | 3.3 | 3.7 | | EN 22854  JIS K2536-2,4,6 |
| Solvent washed gum  (Existent gum content) | mg/100ml |  | 4 | | EN-ISO 6246  JIS K2261 |
| Sulphur content (f) | mg/kg |  | 10 | | EN ISO 20846  EN ISO 20884  JIS K2541-1,2,6,7, |
| Copper corrosion |  |  | Class 1 | | EN-ISO 2160 |
| Lead content | mg/l |  | 5 | | EN 237  JIS K2255 |
| Phosphorus content (g) | mg/l |  | 1.3 | | ASTM D 3231 |
| Ethanol (e) | % v/v | 9.0 | 10.0 | | EN 22854  JIS K2536-2,4,6 |
| (a) The values quoted in the specifications are ‘true values’. In establishing of their limit values the terms of ISO 4259 "Petroleum products - Determination and application of precision data in relation to methods of test" have been applied and in fixing a minimum value, a minimum difference of 2R above zero has been taken into account; in fixing a maximum and minimum value, the minimum difference is 4R (R = reproducibility).  Notwithstanding this measure, which is necessary for technical reasons, the manufacturer of fuels shall nevertheless aim at a zero value where the stipulated maximum value is 2R and at the mean value in the case of quotations of maximum and minimum limits. Should it be necessary to clarify whether a fuel meets the requirements of the specifications, the terms of ISO 4259 shall be applied.  (b) Equivalent EN/ISO methods will be adopted when issued for properties listed above.  (c) A correction factor of 0.2 for MON and RON shall be subtracted for the calculation of the final result in accordance with EN 228:2008.  (d) The fuel may contain oxidation inhibitors and metal deactivators normally used to stabilise refinery gasoline streams, but detergent/dispersive additives and solvent oils shall not be added.  (e) Ethanol is the only oxygenate that shall be intentionally added to the reference fuel. The Ethanol used shall conform to EN 15376.  (f) The actual sulphur content of the fuel used for the Type 1 test shall be recorded.  (g) There shall be no intentional addition of compounds containing phosphorus, iron, manganese, or lead to this reference fuel. | | | | | |

3.7. Ethanol (nominal 95 RON, E85)

# Table A3/7

# **Ethanol (nominal 95 RON, E85)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Parameter* | *Unit* | *Limits (*a*)* | | *Test method (*b*)* |
| *Minimum* | *Maximum* |
| Research octane number, RON |  | 95 |  | EN ISO 5164 |
| Motor octane number, MON |  | 85 |  | EN ISO 5163 |
| Density at 15 °C | kg/m3 | To be recorded | | ISO 3675 |
| Vapour pressure | kPa | 40 | 60 | EN ISO 13016-1 (DVPE) |
| Sulphur content (c)(d) | mg/kg |  | 10 | EN ISO 20846 EN ISO 20884 |
| Oxidation stability | minutes | 360 |  | EN ISO 7536 |
| Existent gum content (solvent washed) | mg/100ml |  | 5 | EN-ISO 6246 |
| Appearance: This shall be determined at ambient temperature or 15 °C whichever is higher. |  | Clear and bright, visibly free of suspended or precipitated contaminants | | Visual inspection |
| Ethanol and higher alcohols (g) | % v/v | 83 | 85 | EN 1601  EN 13132  EN 14517 |
| Higher alcohols (C3-C8) | % v/v |  | 2 |  |
| Methanol | % v/v |  | 0.5 |  |
| Petrol (e) | % v/v | Balance | | EN 228 |
| Phosphorus | mg/l | 0.3 (f) | | ASTM D 3231 |
| Water content | % v/v |  | 0.3 | ASTM E 1064 |
| Inorganic chloride content | mg/l |  | 1 | ISO 6227 |
| pHe |  | 6.5 | 9 | ASTM D 6423 |
| Copper strip corrosion (3h at 50 °C) | Rating | Class 1 |  | EN ISO 2160 |
| Acidity, (as acetic acid CH3COOH) | % (m/m)  (mg/l) |  | 0.005-40 | ASTM D 1613 |
| Carbon/hydrogen ratio |  | Record | |  |
| Carbon/oxygen ratio |  | Record | |  |
| (a) The values quoted in the specifications are ‘true values’. In establishing of their limit values the terms of ISO 4259 "Petroleum products — Determination and application of precision data in relation to methods of test" have been applied and in fixing a minimum value, a minimum difference of 2R above zero has been taken into account; in fixing a maximum and minimum value, the minimum difference is 4R (R = reproducibility). Notwithstanding this measure, which is necessary for technical reasons, the manufacturer of fuels shall nevertheless aim at a zero value where the stipulated maximum value is 2R and at the mean value in the case of quotations of maximum and minimum limits. Should it be necessary to clarify whether a fuel meets the requirements of the specifications, the terms of ISO 4259 shall be applied.  (b) In cases of dispute, the procedures for resolving the dispute and interpretation of the results based on test method precision, described in EN ISO 4259 shall be used.  (c) In cases of national dispute concerning sulphur content, either EN ISO 20846 or EN ISO 20884 shall be called up (similar to the reference in the national Annex of EN 228).  (d) The actual sulphur content of the fuel used for the Type 1 test shall be recorded.  (e) The unleaded petrol content can be determined as 100 minus the sum of the percentage content of water and alcohols.  (f) There shall be no intentional addition of compounds containing phosphorus, iron, manganese, or lead to this reference fuel.  (g) Ethanol to meet specification of EN 15376 is the only oxygenate that shall be intentionally added to this reference fuel. | | | | |

4. Technical data on gaseous fuels for testing vehicles with positive-ignition engines

4.1. LPG (A and B)

# Table A3/8

# **LPG (A and B)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| *Parameter* | *Unit* | *Fuel E1* | *Fuel E2* | *Fuel J* | *Fuel K* | *Test method* |
| Composition: |  |  |  |  |  | ISO 7941 |
| C3-content | % vol | 30 ±2 | 85 ±2 |  | Winter:  min. 15,  max. 35  Summer:  max. 10 | KS M ISO 7941 |
| Propane and propylene content | % mole |  |  | Min 20,  max 30 |  | JIS K2240 |
| C4-content | % vol | Balance | |  | Winter:  min.60,  Summer:  min. 85 | KS M ISO 7941 |
| Butane and butylene content |  |  |  | Min 70,  max 80 |  | JIS K2240 |
| Butadiene |  |  |  |  | max. 0.5 | KS M ISO 7941 |
| < C3, > C4 | % vol | Max. 2 | Max. 2 |  |  |  |
| Olefins | % vol | Max. 12 | Max. 15 |  |  |  |
| Evaporation residue | mg/kg | Max. 50 | Max. 50 |  |  | EN 15470 |
| Evaporation residue (100ml) | ml | - |  |  | 0.05 | ASTM D2158 |
| Water at 0 °C |  | Free | |  |  | EN 15469 |
| Total sulphur content | mg/kg | Max. 10 | Max 10 |  |  | ASTM 6667 |
|  |  |  |  | Max 40 | KS M 2150, ASTM D4486,  ASTM D5504 |
| Hydrogen sulphide |  | None | None |  |  | ISO 8819 |
| Copper strip corrosion | rating | Class 1 | Class 1 |  |  | ISO 6251 (a) |
| Copper corrosion | 40 ℃, 1h | - |  |  | 1 | KS M ISO 6251 |
| Odour |  | Characteristic | |  |  |  |
| Motor octane number |  | Min. 89 | Min. 89 |  |  | EN 589  Annex B |
| Vapour pressure (40 ℃) | MPa | - | 1.27 |  |  | KS M ISO 4256  KS M ISO 8973 |
| Density (15 ℃) | kg/m³ | 500 |  |  | 620 | KS M 2150,  KS M ISO 3993  KS M ISO 8973 |
| (a) This method may not accurately determine the presence of corrosive materials if the sample contains corrosion inhibitors or other chemicals which diminish the corrosivity of the sample to the copper strip. Therefore, the addition of such compounds for the sole purpose of biasing the test method is prohibited. | | | | | | |

4.2. NG/biomethane

4.2.1. "G20""High Gas" (nominal 100 per cent Methane)

# Table A3/9

# **"G20" "High Gas" (nominal 100 per cent methane)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Characteristics* | *Units* | *Basis* | *Limits* | | *Test method* |
| *Minimum* | *Maximum* |
| Composition: |  |  |  |  |  |
| Methane | % mole | 100 | 99 | 100 | ISO 6974 |
| Balance (a) | % mole | — | — | 1 | ISO 6974 |
| N2 | % mole |  |  |  | ISO 6974 |
| Sulphur content | mg/m3 (b) | — | — | 10 | ISO 6326-5 |
| Wobbe Index (net) | MJ/m3 (c) | 48.2 | 47.2 | 49.2 |  |
| (a) Inerts (different from N2) + C2 + C2+.  (b) Value to be determined at 293.15 K (20 °C) and 101.325 kPa.  (c) Value to be determined at 273.15 K (0 °C) and 101.325 kPa. | | | | | |

# 4.2.2. (Reserved)

4.2.3. "G25""Low Gas" (nominal 86 per cent Methane)

# Table A3/11

# **"G25" "Low Gas" (nominal 86 per cent methane)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Characteristics* | *Units* | *Basis* | *Limits* | | *Test method* |
| *Minimum* | *Maximum* |
| Composition: |  |  |  |  |  |
| Methane | % mole | 86 | 84 | 88 | ISO 6974 |
| Balance (a) | % mole | — | — | 1 | ISO 6974 |
| N2 | % mole | 14 | 12 | 16 | ISO 6974 |
| Sulphur content | mg/m3 (b) | — | — | 10 | ISO 6326-5 |
| Wobbe Index (net) | MJ/m3 (c) | 39.4 | 38.2 | 40.6 |  |
| (a) Inerts (different from N2) + C2 + C2+.  (b) Value to be determined at 293.15 K (20 °C) and 101.325 kPa.  (c) Value to be determined at 273.15 K (0 °C) and 101.325 kPa. | | | | | |

4.2.4. "J-Gas" (nominal 85 per cent Methane)

# Table A3/12

# **"J-Gas" (nominal 85 per cent methane)**

|  |  |  |  |
| --- | --- | --- | --- |
| *Characteristics* | *Units* | *Limits* | |
| *Minimum* | *Maximum* |
| Methane | % mole | 85 |  |
| Ethane | % mole |  | 10 |
| Propane | % mole |  | 6 |
| Butane | % mole |  | 4 |
| HC of C3+C4 | % mole |  | 8 |
| HC of C5 or more | % mole |  | 0.1 |
| Other gases (H2+O2+N2+CO+CO2) | % mole |  | 1.0 |
| Sulphur content | mg/Nm3 |  | 10 |
| Wobbe Index | WI | 13.260 | 13.730 |
| Gross Calorific value | kcal/Nm3 | 10.410 | 11.050 |
| Maximum combustion speed | MCP | 36.8 | 37.5 |

4.2.5. Hydrogen

This paragraph is only applicable for the 4-phase WLTP test

For ICE vehicles fuelled by hydrogen, the reference fuel described in Table A3/18 shall be used.

5. Technical data on liquid fuels for testing vehicles with compression ignition engines

5.1. J-Diesel (nominal 53 Cetane, B0)

# 5.2. (Reserved)

# 5.3. (Reserved)

5.4. Diesel

# Table A3/17

# **Diesel (B5H)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Parameter* | *Unit* | *Limits (a)* | | *Test method (as applicable)* |
| *Minimum* | *Maximum* |
| Cetane Index |  | 46.0 |  | EN-ISO 4264  JIS K2280 |
| Cetane number (b) |  | 52.0 | 56.0 | EN-ISO 5165 |
| Density at 15 °C | kg/m³ | 833.0 | 837.0 | EN-ISO 12185  JIS K2249 |
| Distillation: |  |  |  |  |
| — 50 % point | °C | 245.0 | — | EN-ISO 3405  JIS K2254 |
| — 95 % point | °C | 345.0 | 360.0 | EN-ISO 3405  JIS K2254 |
| — final boiling point | °C | — | 370.0 | EN-ISO 3405  JIS K2254 |
| Flash point | °C | 55 | — | EN ISO 2719  JIS K2265-3 |
| Cloud point | °C | — | -10 | EN ISO 3015 |
| Viscosity at 40 °C | mm²/s | 2.30 | 3.30 | EN-ISO 3104  JIS K2283 |
| Polycyclic aromatic hydrocarbons | % m/m | 2.0 | 4.0 | EN 12916  JIS method HPLC |
| Sulphur content | mg/kg | — | 10.0 | EN ISO 20846/  EN ISO 20884  JIS K2541-1,2,6,7 |
| Copper corrosion (3 hours, 50 °C) |  | — | Class 1 | EN-ISO 2160 |
| Conradson carbon residue (10 % DR) | % m/m | — | 0.20 | EN-ISO10370 |
| Ash content | % m/m | — | 0.010 | EN-ISO 6245 |
| Total contamination | mg/kg |  | 24 | EN 12662 |
| Water content | mg/kg | — | 200 | EN-ISO12937 |
| Acid number | mg KOH/g | — | 0.10 | EN ISO 6618 |
| Lubricity (HFRR wear scan diameter at 60 °C) | μm | — | 400 | EN ISO 12156 |
| Oxidation stability at 110 °C (c) | h | 20.0 |  | EN 15751 |
| FAME (d) | % v/v | 4.5 | 5.0 | EN 14078 |
| (a) The values quoted in the specifications are 'true values'. In establishing of their limit values the terms of ISO 4259 Petroleum products – Determination and application of precision data in relation to methods of test have been applied and in fixing a minimum value, a minimum difference of 2R above zero has been taken into account; in fixing a maximum and minimum value, the minimum difference is 4R (R = reproducibility).  Notwithstanding this measure, which is necessary for technical reasons, the manufacturer of fuels shall nevertheless aim at a zero value where the stipulated maximum value is 2R and at the mean value in the case of quotations of maximum and minimum limits. Should it be necessary to clarify whether a fuel meets the requirements of the specifications, the terms of ISO 4259 shall be applied.  (b) The range for cetane number is not in accordance with the requirements of a minimum range of 4R. However, in the case of a dispute between fuel supplier and fuel user, the terms of ISO 4259 may be used to resolve such disputes provided replicate measurements, of sufficient number to achieve the necessary precision, are made in preference to single determinations.  (c) Even though oxidation stability is controlled, it is likely that shelf life will be limited. Advice shall be sought from the supplier as to storage conditions and life.  (d) FAME content to meet the specification of EN 14214. | | | | |

6. Technical data on fuels for testing fuel cell vehicles

6.1. Compressed hydrogen gas for fuel cell vehicles

Table A3/18

# **Hydrogen for fuel cell vehicles**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | *Characteristics* | *Units* | *Limits* | | *Test Method* | | *Minimum* | *Maximum* | | Hydrogen fuel index | % mole fraction | 99.97 |  | (a) | | Total non-hydrogen gases | μmol/mol |  | 300 |  | | Lists of non-hydrogen gases and the specification of each contaminant **(f)** | | | |  | | Water (H2O) | μmol/mol |  | 5 | (e) | | Total hydrocarbons(b) except methane (C1 equivalent) | μmol/mol |  | 2 | (e) | | Methane (CH4) | μmol/mol |  | 100 | (e) | | Oxygen (O2) | μmol/mol |  | 5 | (e) | | Helium (He) | μmol/mol |  | 300 | (e) | | Total Nitrogen (N2) and Argon (Ar) (b) | μmol/mol |  | 300 | (e) | | Carbon dioxide (CO2) | μmol/mol |  | 2 | (e) | | Carbon monoxide (CO) (c) | μmol/mol |  | 0.2 | (e) | | Total sulfur compounds (d) (H2S basis) | μmol/mol |  | 0.004 | (e) | | Formaldehyde (HCHO) | μmol/mol |  | 0.2 | (e) | | Formic acid (HCOOH) | μmol/mol |  | 0.2 | (e) | | Ammonia (NH3) | μmol/mol |  | 0.1 | (e) | | Total halogenated compounds (e)  (Halogenate ion basis) | μmol/mol |  | 0.05 | (e) | | (a)  The hydrogen fuel index is determined by subtracting the “total non-hydrogen gases” in this table, expressed in mole per cent, from 100 mole per cent.  (b) Total hydrocarbons except methane include oxygenated organic species.  (c) The sum of measured CO, HCHO and HCOOH shall not exceed 0.2 µmol/mol  (d)  As a minimum, total sulphur compounds include H2S, COS, CS2 and mercaptans, which are typically found in natural gas.  (e) Test method shall be documented. Test methods defined in ISO21087 are preferable.  (f) The analysis of specific contaminants depending on the production process shall be exempted. A vehicle manufacturer shall provide the responsible authority reasons for exempting specific contaminants. | | | | | |

7. Technical data on fuels for Type 4 test on evaporative emissions

Table A3/19

**Petrol reference fuel for Type 4 test**

| *Parameter* | *Unit* | *Limits* | | *Test method* |
| --- | --- | --- | --- | --- |
| *Minimum* | *Maximum* |
| Research octane number, RON |  | 95.0 | 98.0 | EN ISO 5164  JIS K2280 |
| Density at 15 °C | kg/m3 | 743.0 | 756.0 | EN ISO 12185  JIS K2249-1,2,3 |
| Vapour pressure | kPa | 56.0 | 60.0 | EN 13016-1  JIS K2258-1,2 |
| Distillation: |  |  |  |  |
| – evaporated at 70 °C | % v/v | 34.0 | 46.0 | EN ISO 3405 |
| – evaporated at 100 °C | % v/v | 54.0 | 62.0 | EN ISO 3405 |
| – evaporated at 150 °C | % v/v | 86.0 | 94.0 | EN ISO 3405 |
| Hydrocarbon analysis: |  |  |  |  |
| – olefins | % v/v | 6.0 | 13.0 | EN 22854  JIS K2536-1,2 |
| – aromatics | % v/v | 25.0 | 32.0 | EN 22854  JIS K2536-1,2,3 |
| – benzene | % v/v | - | 1.00 | EN 22854 EN 238  JIS K2536-2,3,4 |
| Oxygen content | % m/m | 3.3 | 3.7 | EN 22854  JIS K2536-2,4,6 |
| Sulphur content | mg/kg | — | 10 | EN ISO 20846  EN ISO 20884  JIS K2541-1,2,6,7 |
| Lead content | mg/l | Not detected | | EN 237  JIS K2255 |
| Ethanol | % v/v | 9.0 | 10.0 | EN 22854  JIS K2536-2,4,6 |
| MTBE |  | Not detected | | JIS K2536-2,4,5,6a |
| Methanol |  | Not detected | | JIS K2536-2,4,5,6a |
| Kerosene |  | Not detected | | JIS K2536-2,4(a) |
| a Other method that is traceable to national or international standard may be used. | | | | |

Annex B4

Road load and dynamometer setting

1. Scope

This annex describes the determination of the road load of a test vehicle and the transfer of that road load to a chassis dynamometer.

2. Terms and definitions

2.1. For the purpose of this document, the terms and definitions given in paragraph 3. of this Regulation shall have primacy. Where definitions are not provided in paragraph 3. of this Regulation, definitions given in ISO 3833:1977 "Road vehicles -- Types -- Terms and definitions" shall apply.

2.2. Reference speed points shall start at 20 km/h in incremental steps of 10 km/h and with the highest reference speed according to the following provisions:

(a) The highest reference speed point shall be 130 km/h or the reference speed point immediately above the maximum speed of the applicable test cycle if this value is less than 130 km/h. In the case that the applicable test cycle contains less than the 4 cycle phases (Low, Medium, High and Extra High) and at the request of the manufacturer and with approval of the responsible authority, the highest reference speed may be increased to the reference speed point immediately above the maximum speed of the next higher phase, but no higher than 130 km/h; in this case road load determination and chassis dynamometer setting shall be done with the same reference speed points;

(b) If a reference speed point applicable for the cycle plus 14 km/h is more than or equal to the maximum vehicle speed vmax, this reference speed point shall be excluded from the coastdown test and from chassis dynamometer setting. The next lower reference speed point shall become the highest reference speed point for the vehicle.

2.3. Unless otherwise specified, a cycle energy demand shall be calculated according to paragraph 5. of Annex B7 over the target speed trace of the applicable drive cycle.

2.4. f0, f1, f2 are the road load coefficients of the road load equation F = f0+ f1× v + f2× v2 determined according to this annex.

is the constant road load coefficient and shall be rounded according to paragraph 6.1.8. of this Regulation to one place of decimal, N;

is the first order road load coefficient and shall be rounded according to paragraph 6.1.8. of this Regulation to three places of decimal, N/(km/h);

is the second order road load coefficient and shall be rounded according to paragraph 6.1.8. of this Regulation to five places of decimal, N/(km/h)².

Unless otherwise stated, the road load coefficients shall be calculated with a least square regression analysis over the range of the reference speed points.

2.5. Rotational mass

2.5.1. Determination of mr

mr is the equivalent effective mass of all the wheels and vehicle components rotating with the wheels on the road while the gearbox is placed in neutral, in kilograms (kg). mr shall be measured or calculated using an appropriate technique agreed upon by the responsible authority. Alternatively, mr may be estimated to be 3 per cent of the sum of the mass in running order and 25 kg.

2.5.2. Application of rotational mass to the road load

Coastdown times shall be transferred to forces and vice versa by taking into account the applicable test mass plus mr. This shall apply to measurements on the road as well as on a chassis dynamometer.

2.5.3. Application of rotational mass for the inertia setting

If the vehicle is tested on a dynamometer in 4WD operation, the equivalent inertia mass of the chassis dynamometer shall be set to the applicable test mass.'

Otherwise, the equivalent inertia mass of the chassis dynamometer shall be set to the test mass plus either the equivalent effective mass of the wheels not influencing the measurement results or 50 per cent of mr.

2.6. Additional masses for setting the test mass shall be applied such that the weight distribution of that vehicle is approximately the same as that of the vehicle with its mass in running order. In the case of Category N vehicles or passenger vehicles derived from Category N vehicles, the additional masses shall be located in a representative manner and shall be justified to the responsible authority upon their request. The weight distribution of the vehicle shall be recorded and shall be used for any subsequent road load determination testing.

3. General requirements

The manufacturer shall be responsible for the accuracy of the road load coefficients and shall ensure this for each production vehicle within the road load family. Tolerances within the road load determination, simulation and calculation methods shall not be used to underestimate the road load of production vehicles. At the request of the responsible authority, the accuracy of the road load coefficients of an individual vehicle shall be demonstrated.

3.1. Overall measurement accuracy, precision, resolution and frequency

The required overall measurement accuracy shall be as follows:

(a) Vehicle speed accuracy: ±0.2 km/h with a measurement frequency of at least 10 Hz;

(b) Time: min. accuracy: ±10 ms; min. precision and resolution:10 ms;

(c) Wheel torque accuracy: ±6 Nm or ±0.5 per cent of the maximum measured total torque, whichever is greater, for the whole vehicle, with a measurement frequency of at least 10 Hz;

(d) Wind speed accuracy: ±0.3 m/s, with a measurement frequency of at least 1 Hz;

(e) Wind direction accuracy: ±3°, with a measurement frequency of at least 1 Hz;

(f) Atmospheric temperature accuracy: ±1 °C, with a measurement frequency of at least 0.1 Hz;

(g) Atmospheric pressure accuracy: ±0.3 kPa, with a measurement frequency of at least 0.1 Hz;

(h) Vehicle mass accuracy measured on the same weighing scale before and after the test: ±10 kg (±20 kg for vehicles > 4,000 kg);

(i) Tyre pressure accuracy: ±5 kPa;

(j) Wheel rotational speed accuracy: ±0.05 s-1 or 1 per cent, whichever is greater.

3.2. Wind tunnel criteria

3.2.1. Wind velocity

The wind velocity during a measurement shall remain within ±2 km/h at the centre of the test section. The possible wind velocity shall be at least 140 km/h.

3.2.2. Air temperature


The air temperature during a measurement shall remain within ±3 °C at the centre of the test section. The air temperature distribution at the nozzle outlet shall remain within ±3 °C.

3.2.3. Turbulence

For an equally-spaced 3 by 3 grid over the entire nozzle outlet, the turbulence intensity, , shall not exceed 1 per cent. See Figure A4/1.

Figure A4/1

**Turbulence intensity**



where:

is the turbulence intensity;

is the turbulent velocity fluctuation, m/s;

is the free flow velocity, m/s.

3.2.4. Solid blockage ratio

The vehicle blockage ratio expressed as the quotient of the vehicle frontal area and the area of the nozzle outlet as calculated using the following equation, shall not exceed 0.35.

where:

is the vehicle blockage ratio;

is the frontal area of the vehicle, m²;

is the nozzle outlet area, m².

3.2.5. Rotating wheels

To properly determine the aerodynamic influence of the wheels, the wheels of the test vehicle shall rotate at such a speed that the resulting vehicle velocity is within ±3 km/h of the wind velocity.

3.2.6. Moving belt

To simulate the fluid flow at the underbody of the test vehicle, the wind tunnel shall have a moving belt extending from the front to the rear of the vehicle. The speed of the moving belt shall be within ±3 km/h of the wind velocity.

3.2.7. Fluid flow angle

At nine equally distributed points over the nozzle area, the root mean square deviation of both the pitch angle α and the yaw angle β (Y-, Z-plane) at the nozzle outlet shall not exceed 1°.

3.2.8. Air pressure

At nine equally distributed points over the nozzle outlet area, the standard deviation of the total pressure at the nozzle outlet shall be less than or equal to 0.02.

where:

is the standard deviation of the pressure ratio ;

is the variation of total pressure between the measurement points, N/m2;

is the dynamic pressure, N/ m².

The absolute difference of the pressure coefficient over a distance 3 metres ahead and 3 metres behind the centre of the balance in the empty test section and at a height of the centre of the nozzle outlet shall not deviate more than ±0.02.

≤ 0.02

where:

is the pressure coefficient.

3.2.9. Boundary layer thickness

At (balance center point), the wind velocity shall have at least 99 per cent of the inflow velocity 30 mm above the wind tunnel floor.

 mm

where:

is the distance perpendicular to the road where 99 per cent of free stream velocity is reached (boundary layer thickness).

3.2.10. Restraint blockage ratio

The restraint system mounting shall not be in front of the vehicle. The relative blockage ratio of the vehicle frontal area due to the restraint system, , shall not exceed 0.10.

where:

is the relative blockage ratio of the restraint system;

is the frontal area of the restraint system projected on the nozzle face, m²;

is the frontal area of the vehicle, m².

3.2.11. Measurement accuracy of the balance in the x-direction

The inaccuracy of the resulting force in the x-direction shall not exceed ±5 N. The resolution of the measured force shall be within ±3 N.

3.2.12. Measurement precision

The precision of the measured force shall be within ±3 N.

4. Road load measurement on road

4.1. Requirements for road test

4.1.1. Atmospheric conditions for road test

Atmospheric conditions (wind conditions, atmospheric temperature and atmospheric pressure) shall be measured according to paragraph 3.1. of this annex. Only those atmospheric conditions measured during coastdown time measurements and/or torque measurement shall be used for checking data validity and corrections.

4.1.1.1. Permissible wind conditions when using stationary anemometry and on-board anemometry

4.1.1.1.1. Permissible wind conditions when using stationary anemometry

The wind speed shall be measured at a location and height above the road level alongside the test road where the most representative wind conditions will be experienced. In cases where tests in opposite directions cannot be performed at the same part of the test track (e.g. on an oval test track with an obligatory driving direction), the wind speed and direction shall be measured at the opposite parts of the test track.

The wind conditions during run pairs shall meet all of the following criteria:

(a) Wind speed shall be less than 5 m/s over a 5 second moving average period;

(b) Peak wind speeds shall not exceed 8 m/s for more than 2 consecutive seconds;

(c) The arithmetic average of the vector component of the wind speed across the test road shall be less than 2 m/s.

The wind correction shall be calculated according to paragraph 4.5.3. of this annex.

4.1.1.1.2. Permissible wind conditions when using on-board anemometry

For testing with an on-board anemometer, a device as described in paragraph 4.3.2. of this annex shall be used.

The wind conditions during run pairs shall meet all of the following criteria:

(a) The arithmetic average of the wind speed shall be less than 7 m/s;

(b) Peak wind speeds shall not exceed 10 m/s for more than 2 consecutive seconds;

(c) The arithmetic average of the vector component of the wind speed across the test road shall be less than 4 m/s.

4.1.1.2. Atmospheric temperature

The atmospheric temperature should be within the range of 5 °C up to and including 40 °C.

At the option of the manufacturer, coastdowns may be performed between 1 °C and 40 °C.

If the difference between the highest and the lowest measured temperature during the coastdown test is more than 5 °C, the temperature correction shall be applied separately for each run with the arithmetic average of the ambient temperature of that run.

In that case, the values of the road load coefficients f0, f1 and f2 shall be determined and corrected for each run pair. The final set of f0, f1 and f2 values shall be the arithmetic average of the individually corrected coefficients f0, f1 and f2 respectively.

4.1.2. Test road

The road surface shall be flat, even, clean, dry and free of obstacles or wind barriers that might impede the measurement of the road load, and its texture and composition shall be representative of current urban and highway road surfaces, i.e. no airstrip-specific surface. The longitudinal slope of the test road shall not exceed ±1 per cent. The local slope between any points 3 metres apart shall not deviate more than ±0.5 per cent from this longitudinal slope. If tests in opposite directions cannot be performed at the same part of the test track (e.g. on an oval test track with an obligatory driving direction), the sum of the longitudinal slopes of the parallel test track segments shall be between 0 and an upward slope of 0.1 per cent. The maximum camber of the test road shall be 1.5 per cent.

4.2. Preparation

4.2.1. Test vehicle

Each test vehicle shall conform in all its components with the production series, (e.g. side mirrors shall be same position as during normal vehicle operation, body gaps shall not be sealed), or, if the vehicle is different from the production vehicle, a full description shall be recorded.

4.2.1.1. Requirements for test vehicle selection

4.2.1.1.1. Without using the interpolation method

A test vehicle (vehicle H) with the combination of road load relevant characteristics (i.e. mass, aerodynamic drag and tyre rolling resistance) producing the highest cycle energy demand shall be selected from the family (see paragraphs 6.3.2. and 6.3.3. of this Regulation).

If the aerodynamic influence of the different wheels within one interpolation family is not known, the selection shall be based on the highest expected aerodynamic drag. As a guideline, the highest aerodynamic drag may be expected for wheels with (a) the largest width, (b) the largest diameter, and (c) the most open structure design (in that order of importance).

The wheel selection shall be performed additional to the requirement of the highest cycle energy demand.

4.2.1.1.2. Using an interpolation method

At the request of the manufacturer, an interpolation method may be applied.

In this case, two test vehicles shall be selected from the family complying with the respective family requirement.

Test vehicle H shall be the vehicle producing the higher, and preferably highest, cycle energy demand of that selection, test vehicle L the one producing the lower, and preferably lowest, cycle energy demand of that selection.

All items of optional equipment and/or body shapes that are chosen not to be considered when applying the interpolation method shall be identical for both test vehicles H and L such that these items of optional equipment produce the highest combination of the cycle energy demand due to their road load relevant characteristics (i.e. mass, aerodynamic drag and tyre rolling resistance).

In the case where individual vehicles can be supplied with a complete set of standard wheels and tyres and in addition a complete set of snow tyres (marked with 3 Peaked Mountain and Snowflake – 3PMS) with or without wheels, the additional wheels/tyres shall not be considered as optional equipment.

4.2.1.1.2.1. The following requirements between vehicles H and L shall be fulfilled for the road load relevant characteristics:

(a) To allow extrapolating road load coefficients:

(i) If f0\_ind is below f\*0\_L or above f0\_H as defined in paragraph 3.2.3.2.2.4. of Annex B7 while performing the calculation in paragraph 3.2.3.2.2.4. of Annex B7, the following minimum differences between H and L are required:

Rolling resistance of at least 1.0 kg/tonne and a mass of at least 30 kg; in case of RR between 0 and 1.0, the minimum of the mass difference is replaced with 100 kg instead of 30 kg;

(ii) If f2\_ind is below f\*2\_L or above f2\_H as defined in paragraph 3.2.3.2.2.4. of Annex B7 while performing the calculation in paragraph 3.2.3.2.2.4. of Annex B7, the following minimum difference between H and L is required:

Aerodynamic drag (CD × Af) of at least 0.05 m². If the manufacturer can demonstrate that the results after an extrapolation are still rational, the minimum criteria in points (i) to (iii) above can be waived.

(b) For each road load characteristic (i.e. mass, aerodynamic drag and tyre rolling resistance) as well as for the road load coefficients f0 and f2, the value of vehicle H shall be higher than that of vehicle L, otherwise the worst case shall be applied for that road load relevant characteristic. At the request of the manufacturer and upon approval by the responsible authority the requirements of this point can be waived.

4.2.1.1.2.2. To achieve a sufficient difference between vehicle H and vehicle L on a particular road load relevant characteristic, or in order to fulfil criteria of paragraph 4.2.1.1.2.1. of this annex, the manufacturer may artificially worsen vehicle H, e.g. by applying a higher test mass.

4.2.1.2. Requirements for families

4.2.1.2.1. Requirements for applying the interpolation family without using the interpolation method

For the criteria defining an interpolation family, see paragraph 6.3.2. of this Regulation.

4.2.1.2.2. Requirements for applying the interpolation family using the interpolation method are:

(a) Fulfilling the interpolation family criteria listed in paragraph 6.3.2. of this Regulation;

(b) Fulfilling the requirements in paragraphs 2.3.1. and 2.3.2. of Annex B6;

(c) Performing the calculations in paragraph 3.2.3.2. of Annex B7.

4.2.1.2.3. Requirements for applying the road load family

4.2.1.2.3.1. At the request of the manufacturer and upon fulfilling the criteria of paragraph 6.3.3. of this Regulation, the road load values for vehicles H and L of an interpolation family shall be calculated.

4.2.1.2.3.2. Test vehicles H and L as defined in paragraph 4.2.1.1.2. of this annex shall be referred to as HR and LR for the purpose of the road load family.

4.2.1.2.3.3. The difference in cycle energy demand between HR and LR of the road load family shall be at least 4 per cent and shall not exceed 35 per cent based on HR over a complete WLTC Class 3 cycle.

If more than one transmission is included in the road load family, a transmission with the highest power losses shall be used for road load determination.

4.2.1.2.3.4. If the road load delta of the vehicle option causing the friction difference is determined according to paragraph 6.8. of this annex, a new road load family shall be calculated which includes the road load delta in both vehicle L and vehicle H of that new road load family.

where:

N refers to the road load coefficients of the new road load family;

R refers to the road load coefficients of the reference road load family; Delta refers to the delta road load coefficients determined in paragraph 6.8.1. of this annex.

4.2.1.3. Allowable combinations of test vehicle selection and family requirements

Table A4/1 shows the permissible combinations of test vehicle selection and family requirements as described in paragraphs 4.2.1.1. and 4.2.1.2. of this annex.

Table A4/1

**Permissible combinations of test vehicle selection and family requirements**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Requirements to be fulfilled:* | *(1) w/o interpolation method* | *(2) Interpolation method w/o road load family* | *(3) Applying the road load family* | *(4) Interpolation method using one or more road load families* |
| Road load test vehicle | Paragraph 4.2.1.1.1. of this annex. | Paragraph 4.2.1.1.2. of this annex. | Paragraph 4.2.1.1.2. of this annex. | n.a. |
| Family | Paragraph 4.2.1.2.1. of this annex. | Paragraph 4.2.1.2.2. of this annex. | Paragraph 4.2.1.2.3. of this annex. | Paragraph 4.2.1.2.2. of this annex. |
| Additional | none | none | none | Application of column (3) "Applying the road load family" and application of paragraph 4.2.1.3.1. of this annex. |

4.2.1.3.1. Deriving road loads of an interpolation family from a road load family

Road loads HR and/or LR shall be determined according to this annex.

The road load of vehicle H (and L) of an interpolation family within the road load family shall be calculated according to paragraphs 3.2.3.2.2. to 3.2.3.2.2.4. inclusive of Annex B7 by:

(a) Using HR and LR of the road load family instead of H and L as inputs for the equations;

(b) Using the road load parameters (i.e. test mass, Δ(CD ×Af) compared to vehicle LR, and tyre rolling resistance) of vehicle H (or L) of the interpolation family as inputs for the individual vehicle;

(c) Repeating this calculation for each H and L vehicle of every interpolation family within the road load family.

The road load interpolation shall only be applied on those road load-relevant characteristics that were identified to be different between test vehicle LR and HR. For other road load-relevant characteristic(s), the value of vehicle HR shall apply.

H and L of the interpolation family may be derived from different road load families. If that difference between these road load families comes from applying the delta method, refer to paragraph 4.2.1.2.3.4. of this annex.

4.2.1.4. Application of the road load matrix family

A vehicle that fulfils the criteria of paragraph 6.3.4. of this Regulation that is:

(a) Representative of the intended series of complete vehicles to be covered by the road load matrix family in terms of estimated worst CD value and body shape; and

(b) Representative of the intended series of vehicles to be covered by the road load matrix family in terms of estimated average of the mass of optional equipment

shall be used to determine the road load.

In the case that no representative body shape for a complete vehicle can be determined, the test vehicle shall be equipped with a square box with rounded corners with radii of maximum of 25 mm and a width equal to the maximum width of the vehicles covered by the road load matrix family, and a total height of the test vehicle of 3.0 m ±0.1 m, including the box.

The manufacturer and the responsible authority shall agree which vehicle test model is representative.

The values of the vehicle parameters test mass, tyre rolling resistance and frontal area of both a vehicle HM and LM shall be determined in such a way that vehicle HM produces the highest cycle energy demand and vehicle LM the lowest cycle energy from the road load matrix family. The manufacturer and the responsible authority shall agree on the vehicle parameters for vehicles HM and LM.

The road load of all individual vehicles of the road load matrix family, including HM and LM, shall be calculated according to paragraph 5.1. of this annex.

4.2.1.5. Movable aerodynamic body parts

Movable aerodynamic body parts on the test vehicles shall operate during road load determination as intended under WLTP Type 1 test conditions (test temperature, vehicle speed and acceleration range, engine load, etc.).

Every vehicle system that dynamically modifies the vehicle’s aerodynamic drag (e.g. vehicle height control) shall be considered to be a movable aerodynamic body part. Appropriate requirements shall be added if future vehicles are equipped with movable aerodynamic items of optional equipment whose influence on aerodynamic drag justifies the need for further requirements.

4.2.1.6. Weighing

Before and after the road load determination procedure, the selected vehicle shall be weighed, including the test driver and equipment, to determine the arithmetic average mass . The mass of the vehicle shall be greater than or equal to the test mass of vehicle H or of vehicle L at the start of the road load determination procedure.

4.2.1.7. Test vehicle configuration

The test vehicle configuration shall be recorded and shall be used for any subsequent coastdown testing.

4.2.1.8. Test vehicle condition

4.2.1.8.1. Run-in

The test vehicle shall be suitably run-in for the purpose of the subsequent test for at least 10,000 but no more than 80,000 km.

At the request of the manufacturer, the following may be used:

(a) a vehicle with a minimum of 3,000 km;

(b) a vehicle with run-in according to paragraph 2.2. or 2.3. of Annex B8 of this Regulation.

4.2.1.8.2. Manufacturer's specifications

The vehicle shall conform to the manufacturer’s intended production vehicle specifications regarding:

(a) tyre pressures described in paragraph 4.2.2.3. of this annex;

(b) wheel alignment described in paragraph 4.2.1.8.3. of this annex;

(c) ground clearance;

(d) vehicle height;

(e) drivetrain and wheel bearing lubricants; and

(f) to avoid unrepresentative parasitic drag, brake adjustment.

4.2.1.8.3. Wheel alignment

Toe and camber shall be set to the maximum deviation from the longitudinal axis of the vehicle in the range defined by the manufacturer. If a manufacturer prescribes values for toe and camber for the vehicle, these values shall be used. At the request of the manufacturer, values with higher deviations from the longitudinal axis of the vehicle than the prescribed values may be used. The prescribed values shall be the reference for all maintenance during the lifetime of the vehicle.

Other adjustable wheel alignment parameters (such as caster) shall be set to the values recommended by the manufacturer. In the absence of recommended values, they shall be set to the arithmetic average of the range defined by the manufacturer.

Such adjustable parameters and set values shall be recorded.

4.2.1.8.4. Closed panels

During the road load determination, the engine compartment cover, luggage compartment cover, manually-operated movable panels and all windows shall be closed.

4.2.1.8.5. Vehicle coastdown mode

If the determined dynamometer settings cannot meet the criteria described in paragraphs 8.1.3. or 8.2.3. of this annex due to non-reproducible forces, the vehicle shall be equipped with a vehicle coastdown mode. The vehicle coastdown mode shall be approved and its use shall be recorded by the responsible authority.

If a vehicle is equipped with a vehicle coastdown mode, it shall be engaged both during road load determination and on the chassis dynamometer.

4.2.2. Tyres

4.2.2.1. Tyre rolling resistance

Tyre rolling resistances shall be measured according to Annex 6 to UN Regulation No. 117 – series of amendments 02, or an internationally-accepted equivalent. The rolling resistance coefficients shall be aligned according to the respective regional procedures (e.g. EU 1235/2011), and categorised according to the rolling resistance classes in Table A4/2.

Table A4/2

**Energy efficiency classes according to rolling resistance coefficients (RRC) for C1, C2 and C3 tyres and the RRC values to be used for those energy efficiency classes in the interpolation, kg/tonne**

|  |  |  |  |
| --- | --- | --- | --- |
| *Energy efficiency class* | *Range of RRC for C1 tyres* | *Range of RRC for C2 tyres* | *Range of RRC for C3 tyres* |
| 1 | RRC ≤ 6.5 | RRC ≤ 5.5 | RRC ≤ 4.0 |
| 2 | 6.6 ≤ RRC ≤ 7.7 | 5.6 ≤ RRC ≤ 6.7 | 4.1 ≤ RRC ≤ 5.0 |
| 3 | 7.8 ≤ RRC ≤ 9.0 | 6.8 ≤ RRC ≤ 8.0 | 5.1 ≤ RRC ≤ 6.0 |
| 4 | 9.1 ≤ RRC ≤ 10.5 | 8.1 ≤ RRC ≤ 9.0 | 6.1 ≤ RRC ≤ 7.0 |
| 5 | RRC ≥10.6 | RRC ≥ 9.1 | RRC ≥ 7.1 |
| *Energy efficiency class* | *Value of RRC to be used for interpolation for C1 tyres* | *Value of RRC to be used for interpolation for C2 tyres* | *Value of RRC to be used for interpolation for C3 tyres* |
| 1 | RRC = 5.9\* | RRC = 4.9\* | RRC = 3.5\* |
| 2 | RRC = 7.1 | RRC = 6.1 | RRC = 4.5 |
| 3 | RRC = 8.4 | RRC = 7.4 | RRC = 5.5 |
| 4 | RRC = 9.8 | RRC = 8.6 | RRC = 6.5 |
| 5 | RRC = 11.3 | RRC = 9.9 | RRC = 7.5 |

\* Only for 4 phase WLTP calculation of individual vehicles: In case the actual RRC value is lower than this value, the actual rolling resistance value of the tyre or any higher value up to the RRC value indicated here shall be used for interpolation.

If the interpolation method is applied to rolling resistance, the actual rolling resistance values for the tyres fitted to the test vehicles L and H shall be used as input for the interpolation method. For an individual vehicle within an interpolation family, the RRC value for the energy efficiency class of the tyres fitted shall be used.

In the case where individual vehicles can be supplied with a complete set of standard wheels and tyres and in addition a complete set of snow tyres (marked with 3 Peaked Mountain and Snowflake – 3PMS) with or without wheels, the additional wheels/tyres shall not be considered as optional equipment.

4.2.2.2. Tyre condition

Tyres used for the test shall:

(a) Not be older than 2 years after the production date;

(b) Not be specially conditioned or treated (e.g. heated or artificially aged), with the exception of grinding in the original shape of the tread;

(c) Be run-in on a road for at least 200 km before road load determination;

(d) Have a constant tread depth before the test between 100 and 80 per cent of the original tread depth at any point over the full tread width of the tyre.

After measurement of tread depth, the driving distance shall be limited to 500 km. If 500 km are exceeded, the tread depth shall be measured again.

4.2.2.3. Tyre pressure

The front and rear tyres shall be inflated to the lower limit of the tyre pressure range for the respective axle for the selected tyre at the coastdown test mass, as specified by the vehicle manufacturer.

4.2.2.3.1. Tyre pressure adjustment

If the difference between ambient and soak temperature is more than 5 °C, the tyre pressure shall be adjusted as follows:

(a) The tyres shall be soaked for more than 1 hour at 10 per cent above the target pressure;

(b) Prior to testing, the tyre pressure shall be reduced to the inflation pressure as specified in paragraph 4.2.2.3. of this annex, adjusted for difference between the soaking environment temperature and the ambient test temperature at a rate of 0.8 kPa per 1 °C using the following equation:

where:

is the tyre pressure adjustment added to the tyre pressure defined in paragraph 4.2.2.3. of this annex, kPa;

0.8 is the pressure adjustment factor, kPa/°C;

is the tyre soaking temperature, °C;

is the test ambient temperature, °C.

(c) Between the pressure adjustment and the vehicle warm-up, the tyres shall be shielded from external heat sources including sun radiation.

4.2.3. Instrumentation

Any instruments shall be installed in such a manner as to minimise their effects on the aerodynamic characteristics of the vehicle.

If the effect of the installed instrument on (CD × Af) is expected to be greater than 0.015 m2,the difference in the value of (CD × Af) of the vehicle with and without the instrument shall be measured in a wind tunnel fulfilling the criteria in paragraph 3.2. of this annex. The corresponding difference shall be subtracted from f2. At the request of the manufacturer, and with approval of the responsible authority, the determined value may be used for similar vehicles where the influence of the equipment is expected to be the same.

4.2.4. Vehicle warm-up

4.2.4.1. On the road

Warming up shall only be performed by driving the vehicle.

4.2.4.1.1. Before warm-up, the vehicle shall be decelerated with the clutch disengaged or an automatic transmission placed in neutral by moderate braking from 80 to 20 km/h within 5 to 10 seconds. After this braking, there shall be no further actuation or manual adjustment of the braking system.

At the request of the manufacturer and upon approval of the responsible authority, the brakes may also be activated after the warm-up with the same deceleration as described in this paragraph and only if necessary.

4.2.4.1.2. Warming up and stabilization

All vehicles shall be driven at 90 per cent of the maximum speed of the applicable WLTC. The vehicle may be driven at 90 per cent of the maximum speed of the next higher phase (see Table A4/3) if this phase is added to the applicable WLTC warm-up procedure as defined in paragraph 7.3.4. of this annex. The vehicle shall be warmed up for at least 20 minutes until stable conditions are reached.

Table A4/3

**Warming-up and stabilization across phases (as applicable)**

| *Cycle class* | *Applicable WLTC* | *90 per cent of maximum speed* | *Next higher phase* |
| --- | --- | --- | --- |
| Class 1 | Low1 + Medium1 | 58 km/h | NA |
| Class 2 | Low2 + Medium2 + High2 + Extra High2 | 111 km/h | NA |
| Low2 + Medium2 + High2 | 77 km/h | Extra High (111 km/h) |
| Class 3 | Low3 + Medium3 + High3 + Extra High3 | 118 km/h | NA |
| Low3 + Medium3 + High3 | 88 km/h | Extra High (118 km/h) |

4.2.4.1.3. Criterion for stable condition

Refer to paragraph 4.3.1.4.2. of this annex.

4.3. Measurement and calculation of road load using the coastdown method

The road load shall be determined by using either the stationary anemometry (paragraph 4.3.1. of this annex) or the on-board anemometry (paragraph 4.3.2. of this annex) method.

4.3.1. Coastdown method using stationary anemometry

4.3.1.1. Selection of reference speeds for road load curve determination

Reference speeds for road load determination shall be selected according to paragraph 2.2. of this annex.

4.3.1.2. Data collection

During the test, elapsed time and vehicle speed shall be measured at a minimum frequency of 10 Hz.

4.3.1.3. Vehicle coastdown procedure

4.3.1.3.1. Following the vehicle warm-up procedure described in paragraph 4.2.4. of this annex and immediately prior to each coastdown run, the vehicle shall be accelerated to 10 to 15 km/h above the highest reference speed and shall be driven at that speed for a maximum of 1 minute. After that, the coastdown run shall be started immediately.

4.3.1.3.2. During a coastdown run, the transmission shall be in neutral. Any movement of the steering wheel shall be avoided as much as possible, and the vehicle brakes shall not be operated.

4.3.1.3.3. The test shall be repeated until the coastdown data satisfy the statistical precision requirements as specified in paragraph 4.3.1.4.2. of this annex.

4.3.1.3.4. Although it is recommended that each coastdown run should be performed without interruption, if data cannot be collected in a single run for all the reference speed points, the coastdown test may be performed with coastdown runs where the first and last reference speeds are not necessarily the highest and lowest reference speeds. In this case, the following additional requirements shall apply:

(a) At least one reference speed in each coastdown run shall overlap with the immediately higher speed range coastdown run. This reference speed shall be referred to as a split point;

(b) At each overlapped reference speed, the average force of the immediately lower speed coastdown run shall not deviate from the average force of the immediately higher speed coastdown run by ±10 N or ± 5 per cent, whichever is greater;

(c) Overlapped reference speed data of the lower speed coastdown run shall be used only for checking criterion (b) and shall be excluded from evaluation of the statistical precision as defined in paragraph 4.3.1.4.2. of this annex;

(d) The overlapped speed may be less than 10 km/h but shall not be less than 5 km/h. In this case, overlap criterion (b) shall be checked by either extrapolating the polynomial curves for the lower and higher speed segment to a 10 km/h overlap, or by comparing the average force in the specific speed range.

4.3.1.3.5. It is recommended that coastdown runs should be conducted successively without undue delay between runs. If there is a delay between runs (e.g. for a driver break, checking vehicle integrity, etc.), the vehicle shall be warmed up again as described in paragraph 4.2.4. and the coastdown runs shall be re-commenced from this point.

4.3.1.4. Coastdown time measurement

4.3.1.4.1. The coastdown time corresponding to reference speed as the elapsed time from vehicle speed () to () shall be measured.

4.3.1.4.2. These measurements shall be carried out in opposite directions until a minimum of three pairs of measurements have been obtained that satisfy the statistical precision pj defined in the following equation:

where:

is the statistical precision of the measurements made at reference speed vj;

is the number of pairs of measurements;

is the harmonic average of the coastdown time at reference speed vj in seconds given by the following equation:

where:

is the harmonic average coastdown time of the ith pair of measurements at velocity vj, seconds, s, given by the following equation:

where:

and are the coastdown times of the ith measurement at reference speed vj, in seconds, s, in the respective directions a and b;

is the standard deviation, expressed in seconds, s, defined by:

σj

is a coefficient given in Table A4/4.

Table A4/4

**Coefficient h as a function of n**

|  |  |  |  |
| --- | --- | --- | --- |
| *n* | *h* | *n* | *h* |
| 3 | 4.3 | 17 | 2.1 |
| 4 | 3.2 | 18 | 2.1 |
| 5 | 2.8 | 19 | 2.1 |
| 6 | 2.6 | 20 | 2.1 |
| 7 | 2.5 | 21 | 2.1 |
| 8 | 2.4 | 22 | 2.1 |
| 9 | 2.3 | 23 | 2.1 |
| 10 | 2.3 | 24 | 2.1 |
| 11 | 2.2 | 25 | 2.1 |
| 12 | 2.2 | 26 | 2.1 |
| 13 | 2.2 | 27 | 2.1 |
| 14 | 2.2 | 28 | 2.1 |
| 15 | 2.2 | 29 | 2.0 |
| 16 | 2.1 | 30 | 2.0 |

4.3.1.4.3. If during a measurement in one direction any external factor or driver action occurs that obviously influences the road load test, that measurement and the corresponding measurement in the opposite direction shall be rejected. All the rejected data and the reason for rejection shall be recorded, and the number of rejected pairs of measurement shall not exceed 1/3 of the total number of measurement pairs. In the case of split runs, the rejection criteria shall be applied at each split run speed range.

Due to uncertainty of data validity and for practical reasons, more than the minimum number of run pairs required in paragraph 4.3.1.4.2. of this annex may be performed, but the total number of run pairs shall not exceed 30 runs including the rejected pairs as described in this paragraph. In this case, data evaluation shall be carried out as described in paragraph 4.3.1.4.2. of this annex starting from the first run pair, then including as many consecutive run pairs as needed to reach the statistical precision on a data set containing no more than 1/3 of rejected pairs. The remaining run pairs shall be disregarded.

4.3.1.4.4. The following equation shall be used to compute the arithmetic average of the road load where the harmonic average of the alternate coastdown times shall be used:

where:

Δv is 5 km/h;

is the harmonic average of alternate coastdown time measurements at velocity , seconds, s, given by:

where:

and are the harmonic average coastdown times in directions a and b, respectively, corresponding to reference speed , in seconds, s, given by the following two equations:

and:

.

where:

is the arithmetic average of the test vehicle masses at the beginning and end of road load determination, kg;

is the equivalent effective mass of rotating components according to paragraph 2.5.1. of this annex;

The coefficients, , and in the road load equation shall be calculated with a least squares regression analysis.

In the case that the tested vehicle is the representative vehicle of a road load matrix family, the coefficient f1 shall be set to zero and the coefficients f0 and f2 shall be recalculated with a least squares regression analysis.

4.3.1.4.5. Correction to reference conditions

The curve determined in paragraph 4.3.1.4.4. of this annex shall be corrected to reference conditions as specified in paragraph 4.5. of this annex.

4.3.2. Coastdown method using on-board anemometry

The vehicle shall be warmed up and stabilised according to paragraph 4.2.4. of this annex.

4.3.2.1. Additional instrumentation for on-board anemometry

The on-board anemometer and instrumentation shall be calibrated by means of operation on the test vehicle where such calibration occurs during the warm-up for the test.

4.3.2.1.1. Relative wind speed shall be measured at a minimum frequency of 1 Hz and to an accuracy of 0.3 m/s. Vehicle blockage shall be accounted for in the calibration of the anemometer.

4.3.2.1.2. Wind direction shall be relative to the direction of the vehicle. The relative wind direction (yaw) shall be measured with a resolution of 1 degree and an accuracy of 3 degrees; the dead band of the instrument shall not exceed 10 degrees and shall be directed towards the rear of the vehicle.

4.3.2.1.3. Before the coastdown, the anemometer shall be calibrated for speed and yaw offset as specified in ISO 10521-1:2006(E) Annex A.

4.3.2.1.4. Anemometer blockage shall be corrected for in the calibration procedure as described in ISO 10521-1:2006(E) Annex A in order to minimise its effect.

4.3.2.2. Selection of vehicle speed range for road load curve determination

The test vehicle speed range shall be selected according to paragraph 2.2. of this annex.

4.3.2.3. Data collection

During the procedure, elapsed time, vehicle speed, and air velocity (speed, direction) relative to the vehicle, shall be measured at a minimum frequency of 5 Hz. Ambient temperature shall be synchronised and sampled at a minimum frequency of 0.1 Hz.

4.3.2.4. Vehicle coastdown procedure

The measurements shall be carried out in run pairs in opposite directions until a minimum of ten consecutive runs (five pairs) have been obtained. Should an individual run fail to satisfy the required on-board anemometry test conditions, that pair, i.e. that run and the corresponding run in the opposite direction, shall be rejected. All valid pairs shall be included in the final analysis with a minimum of 5 pairs of coastdown runs. See paragraph 4.3.2.6.10. of this annex for statistical validation criteria.

The anemometer shall be installed in a position such that the effect on the operating characteristics of the vehicle is minimised.

The anemometer shall be installed according to one of the options below:

(a) Using a boom approximately 2 metres in front of the vehicle’s forward aerodynamic stagnation point;

(b) On the roof of the vehicle at its centreline. If possible, the anemometer shall be mounted within 30 cm from the top of the windshield;

(c) On the engine compartment cover of the vehicle at its centreline, mounted at the midpoint position between the vehicle front and the base of the windshield.

In all cases, the anemometer shall be mounted parallel to the road surface. In the event that positions (b) or (c) are used, the coastdown results shall be analytically adjusted for the additional aerodynamic drag induced by the anemometer. The adjustment shall be made by testing the coastdown vehicle in a wind tunnel both with and without the anemometer installed in the same position as used on the track, The calculated difference shall be the incremental aerodynamic drag coefficient combined with the frontal area, which shall be used to correct the coastdown results.

4.3.2.4.1. Following the vehicle warm-up procedure described in paragraph 4.2.4. of this annex and immediately prior to each coastdown run, the vehicle shall be accelerated to 10 to 15 km/h above the highest reference speed and shall be driven at that speed for a maximum of 1 minute. After that, the coastdown run shall be started immediately.

4.3.2.4.2. During a coastdown run, the transmission shall be in neutral. Any steering wheel movement shall be avoided as much as possible, and the vehicle’s brakes shall not be operated.

4.3.2.4.3. Although it is recommended that each coastdown run be performed without interruption, if data cannot be collected in a single run for all the reference speed points the coastdown test may be performed with coastdown runs where the first and last reference speeds are not necessarily the highest and lowest reference speeds. For split runs, the following additional requirements shall apply:

(a) At least one reference speed in each coastdown run shall overlap with the immediately higher speed range coastdown run. This reference speed shall be referred to as a split point;

(b) At each overlapped reference speed, the average force of the immediately lower speed coastdown run shall not deviate from the average force of the immediately higher speed range coastdown run by ±10 N or ±5 per cent, whichever is greater;

(c) Overlapped reference speed data of the lower speed coastdown run shall be used only for checking criterion (b) and shall be excluded from evaluation of the statistical precision as defined in paragraph 4.3.1.4.2. of this annex;

(d) The overlapped speed may be less than 10 km/h but shall not be less than 5 km/h. In this case, overlap criterion (b) shall be checked by either extrapolating the polynomial curves for the lower and higher speed segment to a 10 km/h overlap, or by comparing the average force in the specific speed range.

4.3.2.4.4. It is recommended that coastdown runs should be conducted successively without undue delay between runs. If there is a delay between runs (e.g. for a driver break, checking vehicle integrity, etc.), the vehicle shall be warmed up again as described in paragraph 4.2.4. and the coastdown runs shall be re-commenced from this point.

4.3.2.5. Determination of the equation of motion

Symbols used in the on-board anemometer equations of motion are listed in Table A4/5.

Table A4/5

**Symbols used in the on-board anemometer equations of motion**

| *Symbol* | *Units* | *Description* |
| --- | --- | --- |
|  | m2 | frontal area of the vehicle |
| … | degrees-1 | aerodynamic drag coefficients as a function of yaw angle |
|  | N | mechanical drag coefficient |
|  | N/(km/h) | mechanical drag coefficient |
|  | N/(km/h)2 | mechanical drag coefficient |
|  |  | aerodynamic drag coefficient at yaw angle Y |
|  | N | drag |
|  | N | aerodynamic drag |
|  | N | front axle drag (including driveline) |
|  | N | gravitational drag |
|  | N | mechanical drag |
|  | N | rear axle drag (including driveline) |
|  | N | tyre rolling resistance |
|  | - | sine of the slope of the track in the direction of travel (+ indicates ascending) |
|  | m/s2 | acceleration |
|  | m/s2 | gravitational constant |
|  | kg | arithmetic average mass of the test vehicle before and after road load determination |
| me | kg | effective vehicle mass including rotating components |
|  | kg/m3 | air density |
|  | s | time |
|  | K | temperature |
|  | km/h | vehicle speed |
|  | km/h | relative wind speed |
|  | degrees | yaw angle of apparent wind relative to direction of vehicle travel |

4.3.2.5.1. General form

The general form of the equation of motion is as follows:

where:

;

;

In the case that the slope of the test track is equal to or less than 0.1 per cent over its length, Dgrav may be set to zero.

4.3.2.5.2. Mechanical drag modelling

Mechanical drag consisting of separate components representing tyre and front and rear axle frictional losses and (including transmission losses) shall be modelled as a three-term polynomial as a function of vehicle speed v as in the equation below:

where , , and are determined in the data analysis using the least squares method. These constants reflect the combined driveline and tyre drag.

In the case that the tested vehicle is the representative vehicle of a road load matrix family, the coefficient Bm shall be set to zero and the coefficients Am and Cm shall be recalculated with a least squares regression analysis.

4.3.2.5.3. Aerodynamic drag modelling

The aerodynamic drag coefficient (Y) shall be modelled as a five-term polynomial as a function of yaw angle Y as in the equation below:

to are constant coefficients whose values are determined in the data analysis.

The aerodynamic drag shall be determined by combining the drag coefficient with the vehicle’s frontal area Af and the relative wind velocity .

4.3.2.5.4. Final equation of motion

Through substitution, the final form of the equation of motion becomes:

-

4.3.2.6. Data reduction

A three-term equation shall be generated to describe the road load force as a function of velocity, , corrected to standard ambient temperature and pressure conditions, and in still air. The method for this analysis process is described in paragraphs 4.3.2.6.1. to 4.3.2.6.10. inclusive of this annex.

4.3.2.6.1. Determining calibration coefficients

If not previously determined, calibration factors to correct for vehicle blockage shall be determined for relative wind speed and yaw angle. Vehicle speed , relative wind velocityand yaw measurements during the warm-up phase of the test procedure shall be recorded. Paired runs in alternate directions on the test track at a constant velocity of 80 km/h shall be performed, and the arithmetic average values of , and for each run shall be determined. Calibration factors that minimize the total errors in head and cross winds over all the run pairs, i.e. the sum of , etc., shall be selected where and refer to wind speed and wind direction from the paired test runs in opposing directions during the vehicle warm-up/stabilization prior to testing.

4.3.2.6.2. Deriving second by second observations

From the data collected during the coastdown runs, values for , , , and shall be determined by applying calibration factors obtained in paragraphs 4.3.2.1.3. and 4.3.2.1.4. of this annex. Data filtering shall be used to adjust samples to a frequency of 1 Hz.

4.3.2.6.3. Preliminary analysis

Using a linear least squares regression technique, all data points shall be analysed at once to determine , , , , , , and given and .

4.3.2.6.4. Data outliers

A predicted force shall be calculated and compared to the observed data points. Data points with excessive deviations, e.g., over three standard deviations, shall be flagged.

4.3.2.6.5. Data filtering (optional)

Appropriate data filtering techniques may be applied and the remaining data points shall be smoothed out.

4.3.2.6.6. Data elimination

Data points gathered where yaw angles are greater than ±20 degrees from the direction of vehicle travel shall be flagged. Data points gathered where relative wind is less than + 5 km/h (to avoid conditions where tailwind speed is higher than vehicle speed) shall also be flagged. Data analysis shall be restricted to vehicle speeds within the speed range selected according to paragraph 4.3.2.2. of this annex.

4.3.2.6.7. Final data analysis

All data that has not been flagged shall be analysed using a linear least squares regression technique. Given and , Am, Bm, Cm, a0, a1, a2, a3 and a4 shall be determined.

4.3.2.6.8. Constrained analysis (optional)

To better separate the vehicle aerodynamic and mechanical drag, a constrained analysis may be applied such that the vehicle’s frontal area and the drag coefficient may be fixed if they have been previously determined.

4.3.2.6.9. Correction to reference conditions

Equations of motion shall be corrected to reference conditions as specified in paragraph 4.5. of this annex.

4.3.2.6.10. Statistical criteria for on-board anemometry

The exclusion of each single pair of coastdown runs shall change the calculated road load for each coastdown reference speed less than the convergence requirement, for all and :

where:

is the difference between the calculated road load with all coastdown runs and the calculated road load with the ith pair of coastdown runs excluded, N;

is the calculated road load with all coastdown runs included, N;

is the reference speed, km/h;

is the number of pairs of coastdown runs, all valid pairs are included.

In the case that the convergence requirement is not met, pairs shall be removed from the analysis, starting with the pair giving the highest change in calculated road load, until the convergence requirement is met, as long as a minimum of 5 valid pairs are used for the final road load determination.

4.4. Measurement and calculation of running resistance using the torque meter method

As an alternative to the coastdown methods, the torque meter method may also be used in which the running resistance is determined by measuring wheel torque on the driven wheels at the reference speed points for time periods of at least 5 seconds.

4.4.1. Installation of torque meters

Wheel torque meters shall be installed between the wheel hub and the wheel of each driven wheel, measuring the required torque to keep the vehicle at a constant speed.

The torque meter shall be calibrated on a regular basis, at least once a year, traceable to national or international standards, in order to meet the required accuracy and precision.

4.4.2. Procedure and data sampling

4.4.2.1. Selection of reference speeds for running resistance curve determination

Reference speed points for running resistance determination shall be selected according to paragraph 2.2. of this annex.

The reference speeds shall be measured in descending order. At the request of the manufacturer, there may be stabilization periods between measurements but the stabilization speed shall not exceed the speed of the next reference speed.

4.4.2.2. Data collection

Data sets consisting of actual speed actual torque and time over a period of at least 5 seconds shall be measured for every at a sampling frequency of at least 10 Hz. The data sets collected over one time period for a reference speed shall be referred to as one measurement.

4.4.2.3. Vehicle torque meter measurement procedure

Prior to the torque meter method test measurement, a vehicle warm-up shall be performed according to paragraph 4.2.4. of this annex.

During test measurement, steering wheel movement shall be avoided as much as possible, and the vehicle brakes shall not be operated.

The test shall be repeated until the running resistance data satisfy the measurement precision requirements as specified in paragraph 4.4.3.2. of this annex.

4.4.2.4. Velocity deviation

During a measurement at a single reference speed point, the velocity deviation from the arithmetic average velocity (vji-vjm) calculated according to paragraph 4.4.3. of this annex, shall be within the values in Table A4/6.

Additionally, the arithmetic average velocity vjm at every reference speed point shall not deviate from the reference speed vj by more than ±1 km/h or 2 per cent of the reference speed vj, whichever is greater.

Table A4/6

**Velocity deviation**

| *Time period, s* | *Velocity deviation, km/h* |
| --- | --- |
| 5 - 10 | ±0.2 |
| 10 - 15 | ±0.4 |
| 15 - 20 | ±0.6 |
| 20 - 25 | ±0.8 |
| 25 - 30 | ±1.0 |
| ≥ 30 | ±1.2 |

4.4.2.5. Atmospheric temperature

Tests shall be performed under the same temperature conditions as defined in paragraph 4.1.1.2. of this annex.

4.4.3. Calculation of arithmetic average velocity and arithmetic average torque

4.4.3.1. Calculation process

Arithmetic average velocity , km/h, and arithmetic average torque , in Nm, of each measurement shall be calculated from the data sets collected according to the requirements of paragraph 4.4.2.2. of this annex using the following equations:

and

where:

is the actual vehicle speed of the ith data set at reference speed point j, km/h;

is the number of data sets in a single measurement;

is the actual torque of the ith data set, Nm;

is the compensation term for speed drift, Nm, given by the following equation:

.

shall be no greater than 0.05 and may be disregarded if is not greater than ±0.005 m/s2;

is the test vehicle mass at the start of the measurements and shall be measured immediately before the warm-up procedure and no earlier, kg;

mr is the equivalent effective mass of rotating components according to paragraph 2.5.1. of this annex, kg;

is the dynamic radius of the tyre determined at a reference point of 80 km/h or at the highest reference speed point of the vehicle if this speed is lower than 80 km/h, calculated using the following equation:

where:

is the rotational frequency of the driven tyre, s-1;

is the arithmetic average acceleration, m/s2, calculated using the following equation:

where:

is the time at which the ith data set was sampled, s.

4.4.3.2. Measurement precision

The measurements shall be carried out in opposite directions until a minimum of three pairs of measurements at each reference speed have been obtained, for which satisfies the precision ρj according to the following equation:

where:

is the number pairs of measurements for ;

is the running resistance at the speed , Nm, given by the equation:

where:

is the arithmetic average torque of the ith pair of measurements at speed , Nm, and given by:

where:

and are the arithmetic average torques of the ith measurement at speed determined in paragraph 4.4.3.1. of this annex for each direction, a and b respectively, Nm;

is the standard deviation, Nm, calculated using the following equation:

is a coefficient as a function of n as given in Table A4/4 in paragraph 4.3.1.4.2. of this annex.

4.4.4. Running resistance curve determination

The arithmetic average speed and arithmetic average torque at each reference speed point shall be calculated using the following equations:

Vjm = ½ × (vjma + vjmb)

Cjm = ½ × (Cjma +Cjmb)

The following least squares regression curve of arithmetic average running resistance shall be fitted to all the data pairs (, ) at all reference speeds described in paragraph 4.4.2.1. of this annex to determine the coefficients c0, c1 and c2.

The coefficients, , and as well as the coastdown times measured on the chassis dynamometer (see paragraph 8.2.4. of this annex) shall be recorded.

In the case that the tested vehicle is the representative vehicle of a road load matrix family, the coefficient c1 shall be set to zero and the coefficients c0 and c2 shall be recalculated with a least squares regression analysis.

4.4.5. Correction to reference conditions

Equations of motion shall be corrected to reference conditions as specified in paragraph 4.5.of this annex.

4.5. Correction to reference conditions and measurement equipment

4.5.1. Air resistance correction factor

The correction factor for air resistance K2 shall be determined using the following equation:

where:

is the arithmetic average atmospheric temperature of all individual runs, Kelvin (K);

is the arithmetic average atmospheric pressure, kPa.

4.5.2. Rolling resistance correction factor

The correction factor for rolling resistance, in Celsius-1 (°C-1), may be determined based on empirical data and approved by the responsible authority for the particular vehicle and tyre combination to be tested, or may be assumed to be as follows:

4.5.3. Wind correction

4.5.3.1. Wind correction when using stationary anemometry

Wind correction may be waived when the arithmetic average wind speed for each valid run pair is 2 m/s or less. In the case that wind speed is measured at more than one part of the test track, such as when the test is performed on an oval test track (see paragraph 4.1.1.1.1. of this annex), the wind speed shall be averaged at each measurement location and the higher of two average wind speeds shall be used to determine whether a wind speed correction is to be applied or may be waived.

4.5.3.1.1. The wind resistance correction for the coastdown method or for the torque meter method shall be calculated using the following equations:

or:

where:

is the wind resistance correction for the coastdown method, N;

is the coefficient of the aerodynamic term determined according to paragraph 4.3.1.4.4. of this annex;

in the case that wind speed is measured at only one point, vw is the arithmetic average vector component of the wind speed parallel to the test road during all valid run pairs, m/s;

in the case that the wind speed is measured at two points, vw is the lower of the two arithmetic average vector components of the wind speed parallel to the test road during all valid run pairs, m/s;

is the wind resistance correction for the torque meter method, Nm;

is the coefficient of the aerodynamic term for the torque meter method determined according to paragraph 4.4.4. of this annex.

4.5.3.2. Wind correction when using on-board anemometry

In the case that the coastdown method is based on on-board anemometry, w1 and w2 in the equations in paragraph 4.5.3.1.1. of this annex shall be set to zero, as the wind correction is already applied according to paragraph 4.3.2. of this annex.

4.5.4. Test mass correction factor

The correction factor for the test mass of the test vehicle shall be determined using the following equation:

where:

is the test mass of the test vehicle, kg;

is the arithmetic average of the test vehicle masses at the beginning and end of road load determination, kg.

4.5.5. Road load curve correction

4.5.5.1. The curve determined in paragraph 4.3.1.4.4. of this annex shall be corrected to reference conditions as follows:

where:

is the corrected road load, N;

is the constant road load coefficient, N;

is the first order road load coefficient, N/(km/h);

is the second order road load coefficient, N/(km/h)2;

is the correction factor for rolling resistance as defined in paragraph 4.5.2. of this annex;

is the test mass correction as defined in paragraph 4.5.4. of this annex;

is the correction factor for air resistance as defined in paragraph 4.5.1. of this annex;

is the arithmetic average atmospheric temperature during all valid run pairs, °C;

is vehicle velocity, km/h;

is the wind resistance correction as defined in paragraph 4.5.3. of this annex, N.

The result of the calculation below shall be used as the target road load coefficient At in the calculation of the chassis dynamometer load setting described in paragraph 8.1. of this annex:

The result of the calculation below shall be used as the target road load coefficient Bt in the calculation of the chassis dynamometer load setting described in paragraph 8.1. of this annex:

(f1 × (1 + K0 × (T-20))).

The result of the calculation below shall be used as the target road load coefficient Ct in the calculation of the chassis dynamometer load setting described in paragraph 8.1. of this annex:

(K2 × f2).

4.5.5.2. The curve determined in paragraph 4.4.4. of this annex shall be corrected to reference conditions and measurement equipment installed according to the following procedure.

4.5.5.2.1. Correction to reference conditions

where:

is the corrected running resistance, Nm;

is the constant term as determined in paragraph 4.4.4. of this annex, Nm;

is the coefficient of the first order term as determined in paragraph 4.4.4. of this annex, Nm/(km/h);

is the coefficient of the second order term as determined in paragraph 4.4.4. of this annex, Nm/(km/h)2;

is the correction factor for rolling resistance as defined in paragraph 4.5.2. of this annex;

is the test mass correction as defined in paragraph 4.5.4. of this annex;

is the correction factor for air resistance as defined in paragraph 4.5.1. of this annex;

is the vehicle velocity, km/h;

T is the arithmetic average atmospheric temperature during all valid run pairs, °C;

is the wind resistance correction as defined in paragraph 4.5.3. of this annex.

4.5.5.2.2. Correction for installed torque meters

If the running resistance is determined according to the torque meter method, the running resistance shall be corrected for effects of the torque measurement equipment installed outside the vehicle on its aerodynamic characteristics.

The running resistance coefficient c2 shall be corrected using the following equation:

c2corr = K2 × c2 × (1 + (∆(CD × Af))/(CD’ × Af’))

where:

∆(CD × Af) = (CD × Af) - (CD’ × Af’) ;

CD’ × Af’ is the product of the aerodynamic drag coefficient multiplied by the frontal area of the vehicle with the torque meter measurement equipment installed measured in a wind tunnel fulfilling the criteria of paragraph 3.2. of this annex, m²;

CD × Af is the product of the aerodynamic drag coefficient multiplied by the frontal area of the vehicle with the torque meter measurement equipment not installed measured in a wind tunnel fulfilling the criteria of paragraph 3.2. of this annex, m².

4.5.5.2.3. Target running resistance coefficients

The result of the calculation below shall be used as the target running resistance coefficient at in the calculation of the chassis dynamometer load setting described in paragraph 8.2. of this annex:

The result of the calculation below shall be used as the target running resistance coefficient bt in the calculation of the chassis dynamometer load setting described in paragraph 8.2. of this annex:

(c1 × (1 + K0 × (T-20))).

The result of the calculation below shall be used as the target running resistance coefficient ct in the calculation of the chassis dynamometer load setting described in paragraph 8.2. of this annex:

(c2corr × r).

5. Method for the calculation of road load or running resistance based on vehicle parameters

5.1. Calculation of road load and running resistance for vehicles based on a representative vehicle of a road load matrix family

If the road load of the representative vehicle is determined according to a coastdown method described in paragraph 4.3. of this annex or according to the wind tunnel method described in paragraph 6. of this annex, the road load of an individual vehicle shall be calculated according to paragraph 5.1.1. of this annex considering vehicle parameters in paragraph 4.2.1.4.

If the running resistance of the representative vehicle is determined according to the torque meter method described in paragraph 4.4. of this annex, the running resistance of an individual vehicle shall be calculated according to paragraph 5.1.2. of this annex considering vehicle parameters in paragraph 4.2.1.4.

5.1.1. The road load force for an individual vehicle shall be calculated using the following equation:

where:

Fc is the calculated road load force as a function of vehicle velocity, N;

f0 is the constant road load coefficient, N, defined by the equation:

f0 = Max((0.05 × f0r + 0.95 × (f0r × TM/TMr + () × 9.81 × TM));

(0.2 × f0r + 0.8 × (f0r × TM/TMr + () × 9.81 × TM)))

f0r is the constant road load coefficient of the representative vehicle of the road load matrix family, N;

f1 is the first order road load coefficient, N/(km/h), and shall be set to zero;

f2 is the second order road load coefficient, N/(km/h)², defined by the equation:

f2 = Max((0.05 × f2r + 0.95 × f2r × Af / Afr); (0.2 × f2r + 0.8 × f2r × Af / Afr))

f2r is the second order road load coefficient of the representative vehicle of the road load matrix family, N/(km/h)²;

v is the vehicle speed, km/h;

TM is the actual test mass of the individual vehicle of the road load matrix family, kg;

TMr is the test mass of the representative vehicle of the road load matrix family, kg;

Af is the frontal area of the individual vehicle of the road load matrix family, m²,

Afr is the frontal area of the representative vehicle of the road load matrix family, m2;

RR is the tyre rolling resistance of the individual vehicle of the road load matrix family, kg/tonne;

RRr is the tyre rolling resistance of the representative vehicle of the road load matrix family, kg/tonne.

For the tyres fitted to an individual vehicle, the value of the rolling resistance RR shall be set to the class value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4.

If the tyres on the front and rear axles belong to different energy efficiency classes, the weighted mean shall be used, calculated using the equation in paragraph 3.2.3.2.2.2. of Annex B7.

If the same tyres were fitted to test vehicles L and H, the value of RRind when using the interpolation method shall be set to RRH.

5.1.2. The running resistance for an individual vehicle shall be calculated using the following equation:

where:

Cc is the calculated running resistance as a function of vehicle velocity, Nm;

c0 is the constant running resistance coefficient, Nm, defined by the equation:

c0 = r’/1.02 × Max((0.05 × 1.02 × c0r/r’ + 0.95 × (1.02 × c0r/r’ × TM/TMr + () × 9.81 × TM));

(0.2 × 1.02 × c0r/r’ + 0.8 × (1.02 × c0r/r’ × TM/TMr + () × 9.81 × TM)))

c0r is the constant running resistance coefficient of the representative vehicle of the road load matrix family, Nm;

c1 is the first order running resistance coefficient, Nm/(km/h), and shall be set to zero;

c2 is the second order running resistance coefficient, Nm/(km/h)², defined by the equation:

c2 = r’/1.02 × Max((0.05 × 1.02 × c2r/r’ + 0.95 × 1.02 × c2r/r’ × Af / Afr); (0.2 × 1.02 × c2r/r’ + 0.8 × 1.02 ×c2r/r’ × Af / Afr))

c2r is the second order running resistance coefficient of the representative vehicle of the road load matrix family, N/(km/h)2;

v is the vehicle speed, km/h;

TM is the actual test mass of the individual vehicle of the road load matrix family, kg;

TMr is the test mass of the representative vehicle of the road load matrix family, kg;

Af is the frontal area of the individual vehicle of the road load matrix family, m²;

Afr is the frontal area of the representative vehicle of the road load matrix family, m2;

RR is the tyre rolling resistance of the individual vehicle of the road load matrix family, kg/tonne;

RRr is the tyre rolling resistance of the representative vehicle of the road load matrix family, kg/tonne;

r’ is the dynamic radius of the tyre on the chassis dynamometer obtained at 80 km/h, m;

1.02 is an approximate coefficient compensating for drivetrain losses.

5.2. Calculation of the default road load based on vehicle parameters

5.2.1. As an alternative for determining road load with the coastdown or torque meter method, a calculation method for default road load may be used.

For the calculation of a default road load based on vehicle parameters, several parameters such as test mass, width and height of the vehicle shall be used. The default road load Fc shall be calculated for the reference speed points.

5.2.2. The default road load force shall be calculated using the following equation:

where:

is the calculated default road load force as a function of vehicle velocity, N;

is the constant road load coefficient, N, defined by the following equation:

;

is the first order road load coefficient, N/(km/h), and shall be set to zero;

is the second order road load coefficient, N/(km/h)2, defined by the following equation:

;

is vehicle velocity, km/h;

test mass, kg;

vehicle width as defined in term No. 6.2. of Standard ISO 612:1978, m;

vehicle height as defined in term No. 6.3. of Standard ISO 612:1978, m.

6. Wind tunnel method

The wind tunnel method is a road load measurement method using a combination of a wind tunnel and a chassis dynamometer or of a wind tunnel and a flat belt dynamometer. The test benches may be separate facilities or integrated with one another.

6.1. Measurement method

6.1.1. The road load shall be determined by:

(a) Adding the road load forces measured in a wind tunnel and those measured using a flat belt dynamometer; or

(b) Adding the road load forces measured in a wind tunnel and those measured on a chassis dynamometer.

6.1.2. Aerodynamic drag shall be measured in the wind tunnel.

6.1.3. Rolling resistance and drivetrain losses shall be measured using a flat belt or a chassis dynamometer, measuring the front and rear axles simultaneously.

6.2. Approval of the facilities by the responsible authority

The results of the wind tunnel method shall be compared to those obtained using the coastdown method to demonstrate qualification of the facilities and recorded.

6.2.1. Three vehicles shall be selected by the responsible authority. The vehicles shall cover the range of vehicles (e.g. size, weight) planned to be measured with the facilities concerned.

6.2.2. Two separate coastdown tests shall be performed with each of the three vehicles according to paragraph 4.3. of this annex, and the resulting road load coefficients, f0, f1 and f2, shall be determined according to that paragraph and corrected according to paragraph 4.5.5. of this annex. The coastdown test result of a test vehicle shall be the arithmetic average of the road load coefficients of its two separate coastdown tests. If more than two coastdown tests are necessary to fulfil the approval of facilities' criteria, all valid tests shall be averaged.

6.2.3. Measurement with the wind tunnel method according to paragraphs 6.3. to 6.7. inclusive of this annex shall be performed on the same three vehicles as selected in paragraph 6.2.1. of this annex and in the same conditions, and the resulting road load coefficients, f0, f1 and f2, shall be determined.

If the manufacturer chooses to use one or more of the available alternative procedures within the wind tunnel method (i.e. paragraph 6.5.2.1. on preconditioning, paragraphs 6.5.2.2. and 6.5.2.3. on the procedure, including paragraph 6.5.2.3.3. on dynamometer setting), these procedures shall also be used also for the approval of the facilities.

6.2.4. Approval criteria

The facility or combination of facilities used shall be approved if both of the following two criteria are fulfilled:

1. The difference in cycle energy, expressed as εk, between the wind tunnel method and the coastdown method shall be within ±0.05 for each of the three vehicles k according to the following equation:

where:

εk is the difference in cycle energy over a complete Class 3 WLTC for vehicle k between the wind tunnel method and the coastdown method, per cent;

Ek,WTM is the cycle energy over a complete Class 3 WLTC for vehicle k, calculated with the road load derived from the wind tunnel method (WTM) calculated according to paragraph 5. of Annex B7, J;

Ek,coastdown is the cycle energy over a complete Class 3 WLTC for vehicle k, calculated with the road load derived from the coastdown method calculated according to paragraph 5. of Annex B7, J.; and

1. The arithmetic average of the three differences shall be within 0.02.

The approval shall be recorded by the responsible authority including measurement data and the facilities concerned.

The facility may be used for road load determination for a maximum of two years after the approval has been granted.

Each combination of roller chassis dynamometer or moving belt and wind tunnel shall be approved separately.

Every combination of wind speeds (see paragraph 6.4.3. of this annex) used for the determination of road load values shall be validated separately.

6.3. Vehicle preparation and temperature

Conditioning and preparation of the vehicle shall be performed according to paragraphs 4.2.1. and 4.2.2. of this annex and applies to both the flat belt or roller chassis dynamometers and the wind tunnel measurements.

In the case that the alternative warm-up procedure described in paragraph 6.5.2.1. of this annex is applied, the target test mass adjustment, the weighing of the vehicle and the measurement shall all be performed without the driver in the vehicle.

The flat belt or the chassis dynamometer test cells shall have a temperature set point of 20 °C with a tolerance of ±3 °C. At the request of the manufacturer, the set point may also be 23 °C with a tolerance of ±3 °C.

6.4. Wind tunnel procedure

6.4.1. Wind tunnel criteria

The wind tunnel design, test methods and the corrections shall provide a value of (CD × Af) representative of the on-road (CD × Af) value and with a repeatability of ±0.015 m².

For all (CD × Af) measurements, the wind tunnel criteria listed in paragraph 3.2. of this annex shall be met with the following modifications:

(a) The solid blockage ratio described in paragraph 3.2.4. of this annex shall be less than 25 per cent;

(b) The belt surface contacting any tyre shall exceed the length of that tyre's contact area by at least 20 per cent and shall be at least as wide as that contact patch;

(c) The standard deviation of total air pressure at the nozzle outlet described in paragraph 3.2.8. of this annex shall be less than 1 per cent;

(d) The restraint system blockage ratio described in paragraph 3.2.10. of this annex shall be less than 3 per cent;

(e) Additionally to the requirement defined in paragraph 3.2.11. of this annex, when measuring Class 1 vehicles, the precision of the measured force shall not exceed ±2.0 N.

6.4.2. Wind tunnel measurement

The vehicle shall be in the condition described in paragraph 6.3. of this annex.

The vehicle shall be placed parallel to the longitudinal centre line of the tunnel with a maximum tolerance of ±10 mm.

The vehicle shall be placed with a yaw angle of 0 ° within a tolerance of ±0.1°.

Aerodynamic drag shall be measured for at least for 60 seconds and at a minimum frequency of 5 Hz. Alternatively, the drag may be measured at a minimum frequency of 1 Hz and with at least 300 subsequent samples. The result shall be the arithmetic average of the drag.

Prior to a test it shall be checked that at the aerodynamic force measured at a wind speed of 0 km/h yields a result equal to 0 Newtons.

In the case that the vehicle has movable aerodynamic body parts, paragraph 4.2.1.5. of this annex shall apply. Where movable parts are velocity-dependent, every applicable position shall be measured in the wind tunnel and evidence shall be provided to the responsible authority indicating the relationship between reference speed, movable part position, and the corresponding (CD × Af).

6.4.3. Wind speeds for wind tunnel measurement

The aerodynamic force shall be measured at two wind speeds under the following speed conditions:

(a) Class 1 vehicles

Lower wind speed *vlow* to measure aerodynamic force shall be *vlow* < 80 km/h;

Higher wind speed *vhigh* shall be (*vlow*+ 40 km/h*≤* *vhigh* *≤* 150 km/h).

(b) Class 2 and 3 vehicles

Lower wind speed *vlow* to measure aerodynamic force shall be 80 km/h*≤* *vlow* *≤* 100 km/h;

Higher wind speed shall be (*vlow*+ 40 km/h*≤* *vhigh* *≤* 150 km/h).

6.5. Flat belt applied for the wind tunnel method

6.5.1. Flat belt criteria

6.5.1.1. Description of the flat belt test bench

The wheels shall rotate on flat belts that do not change the rolling characteristics of the wheels compared to those on the road. The measured forces in the x-direction shall include the frictional forces in the drivetrain.

6.5.1.2. Vehicle restraint system

The dynamometer shall be equipped with a centring device aligning the vehicle within a tolerance of ±0.5 degrees of rotation around the z-axis. The restraint system shall maintain the centred drive wheel position throughout the coastdown runs of the road load determination within the following limits:

6.5.1.2.1. Lateral position (y-axis)

The vehicle shall remain aligned in the y-direction and lateral movement shall be minimised.

6.5.1.2.2. Front and rear position (x-axis)

Additional to the requirement of paragraph 6.5.1.2.1. of this annex, both wheel axes shall be within ±10 mm of the belt’s lateral centre lines.

6.5.1.2.3. Vertical force

The restraint system shall be designed so as to impose no vertical force on the drive wheels.

6.5.1.3. Accuracy of measured forces

Only the reaction force for turning the wheels shall be measured. No external forces shall be included in the result (e.g. force of the cooling fan air, vehicle restraints, aerodynamic reaction forces of the flat belt, dynamometer losses, etc.).

The force in the x-direction shall be measured with an accuracy of ±5 N.

6.5.1.4. Flat belt speed control

The belt speed shall be controlled with an accuracy of ±0.1 km/h.

6.5.1.5. Flat belt surface

The flat belt surface shall be clean, dry and free from foreign material that might cause tyre slippage.

6.5.1.6. Cooling

A current of air of variable speed shall be blown towards the vehicle. The set point of the linear velocity of the air at the blower outlet shall be equal to the corresponding dynamometer speed above measurement speeds of 5 km/h. The linear velocity of the air at the blower outlet shall be within ±5 km/h or ±10 per cent of the corresponding measurement speed, whichever is greater.

6.5.2. Flat belt measurement

The measurement procedure may be performed according to either paragraph 6.5.2.2. or paragraph 6.5.2.3. of this annex.

6.5.2.1. Preconditioning

The vehicle shall be conditioned on the dynamometer as described in paragraphs 4.2.4.1.1. to 4.2.4.1.3. inclusive of this annex.

The dynamometer load setting Fd for the preconditioning shall be:

where in the case of applying paragraph 6.7.2.1:

ad = 0

bd = f1a;

or, where in the case of applying paragraph 6.7.2.2.:

*ad = 0*

*bd = 0*

The equivalent inertia of the dynamometer shall be the test mass.

The aerodynamic drag used for the load setting shall be determined in accordance with paragraph 6.7.2. of this annex and may be set directly as input. Otherwise, ad, bd, and cd from this paragraph shall be used.

At the request of the manufacturer, as an alternative to paragraph 4.2.4.1.2. of this annex, the warm-up may be conducted by driving the vehicle with the flat belt.

In this case, the warm-up speed shall be 110 per cent of the maximum speed of the applicable WLTC. The warm up is considered complete when the vehicle has been driven for at least 1,200 seconds and the change of measured force over a period of 200 seconds is less than 5 N.

6.5.2.2. Measurement procedure with stabilised speeds

6.5.2.2.1. The test shall be conducted from the highest to the lowest reference speed point.

6.5.2.2.2. Immediately after the measurement at the previous speed point, the deceleration from the current to the next applicable reference speed point shall be performed in a smooth transition of approximately 1 m/s².

6.5.2.2.3. The reference speed shall be stabilised for at least 4 seconds and for a maximum of 10 seconds. The measurement equipment shall ensure that the signal of the measured force is stabilised after that period.

6.5.2.2.4. The force at each reference speed shall be measured for at least 6 seconds while the vehicle speed is kept constant. The resulting force for that reference speed point FjDyno shall be the arithmetic average of the force during the measurement.

6.5.2.2.5. The steps in paragraphs 6.5.2.2.2. to 6.5.2.2.4. inclusive of this annex shall be repeated for each reference speed.

6.5.2.3. Measurement procedure by deceleration

6.5.2.3.1. Preconditioning and dynamometer setting shall be performed according to paragraph 6.5.2.1. of this annex. Prior to each coastdown, the vehicle shall be driven at the highest reference speed or, in the case that the alternative warm-up procedure is used at 110 per cent of the highest reference speed, for at least 1 minute. The vehicle shall be subsequently accelerated to at least 10 km/h above the highest reference speed and the coastdown shall be started immediately.

6.5.2.3.2. The measurement shall be performed according to paragraphs 4.3.1.3.1. to 4.3.1.4.4. inclusive of this annex but excluding paragraph 4.3.1.4.2., where and are replaced by . The measurement shall be stopped after two decelerations if the force of both coastdowns at each reference speed point is within ±10 N, otherwise at least three coastdowns shall be performed using the criteria set out in paragraph 4.3.1.4.2. of this annex.

6.5.2.3.3. The force fjDyno at each reference speed vj shall be calculated by removing the dynamometer set force:

where:

fjDecel is the force determined according to the equation calculating Fj in paragraph 4.3.1.4.4. of this annex at reference speed point j, N;

is the force determined to the equation calculating Fd in paragraph 6.5.2.1. of this annex at reference speed point j, N.

Alternatively, at the request of the manufacturer, bd and cd may be set to zero during the coastdown and for calculating fjDyno.

6.5.2.4. Measurement conditions

The vehicle shall be in the condition described in paragraph 4.3.1.3.2. of this annex.

6.5.3. Measurement result of the flat belt method

The result of the flat belt dynamometer fjDyno shall be referred to as fj for the further calculations in paragraph 6.7. of this annex.

6.6. Chassis dynamometer applied for the wind tunnel method

6.6.1. Criteria

In addition to the descriptions in paragraphs 1. and 2. of Annex B5, the criteria described in paragraphs 6.6.1.1. to 6.6.1.6. shall apply.

6.6.1.1. Description of a chassis dynamometer

The front and rear axles shall be equipped with a single roller with a diameter of not less than 1.2 metres.

6.6.1.2. Vehicle restraint system

The dynamometer shall be equipped with a centring device aligning the vehicle. The restraint system shall maintain the centred drive wheel position within the following recommended limits throughout the coastdown runs of the road load determination:

6.6.1.2.1. Vehicle position

The vehicle to be tested shall be installed on the chassis dynamometer roller as defined in paragraph 7.3.3. of this annex.

6.6.1.2.2. Vertical force

The restraint system shall fulfil the requirements of paragraph 6.5.1.2.3. of this annex.

6.6.1.3. Accuracy of measured forces

The accuracy of measured forces shall be as described in paragraph 6.5.1.3. of this annex apart from the force in the x-direction that shall be measured with an accuracy as described in paragraph 2.4.1. of Annex B5.

6.6.1.4. Dynamometer speed control

The roller speeds shall be controlled with an accuracy of ±0.2 km/h.

6.6.1.5. Roller surface

The roller surface shall be clean, dry and free from foreign material that might cause tyre slippage.

6.6.1.6. Cooling

The cooling fan shall be as described in paragraph 6.5.1.6. of this annex.

6.6.2. Dynamometer measurement

The measurement shall be performed as described in paragraph 6.5.2. of this annex.

6.6.3. Correcting measured chassis dynamometer forces to those on a flat surface

The measured forces on the chassis dynamometer shall be corrected to a reference equivalent to the road (flat surface) and the result shall be referred to as fj.

where:

c1 is the tyre rolling resistance fraction of fjDyno;

c2 is a chassis dynamometer-specific radius correction factor;

fjDyno is the force calculated in paragraph 6.5.2.3.3. of this annex for each reference speed j, N;

RWheel is one-half of the nominal design tyre diameter, m;

RDyno is the radius of the chassis dynamometer roller, m.

The manufacturer and the responsible authority shall agree on the factors c1 and c2 to be used, based on correlation test evidence provided by the manufacturer for the range of tyre characteristics intended to be tested on the chassis dynamometer.

As an alternative the following conservative equation may be used:

C2 shall be 0.2 except that 2.0 shall be used if the road load delta method (see paragraph 6.8. of this annex) is used and the road load delta calculated according to paragraph 6.8.1. of this annex is negative.

6.7. Calculations

6.7.1. Correction of the flat belt and chassis dynamometer results

The measured forces determined in paragraphs 6.5. and 6.6. of this annex shall be corrected to reference conditions using the following equation:

where:

is the corrected resistance measured at the flat belt or chassis dynamometer at reference speed j, N;

is the measured force at reference speed j, N;

is the correction factor for rolling resistance as defined in paragraph 4.5.2. of this annex, K-1;

is the test mass correction as defined in paragraph 4.5.4. of this annex, N;

T is the arithmetic average temperature in the test cell during the measurement, K.

6.7.2. Calculation of the aerodynamic force

The calculation in paragraph 6.7.2.1. shall be applied considering the results of both wind speeds. However, if the difference of the product of the drag coefficient and frontal area measured at the wind speeds vlow and vhigh is less than 0.015 m², the calculation in paragraph 6.7.2.2. may be applied at the request of the manufacturer.

6.7.2.1. The aerodynamic force of each wind speed , , and shall be calculated using the equation below.

where:

is the product of the drag coefficient and frontal area measured in the wind tunnel at a certain reference speed point j, if applicable, m²;

is the dry air density defined in paragraph 3.2.10. of this Regulation, kg/m³;

is the aerodynamic force calculated at wind speed w, N;

vw is the applicable wind speed, km/h.

is the reference to the applicable wind speed "0wind", "low" and "high";

is the aerodynamic force at 0 km/h, N;

is the aerodynamic force at vlow, N;

is the aerodynamic force at vhigh, N.

The aerodynamic force coefficients and shall be calculated with a least square regression analysis using , , and and the equation below:

The final result for the aerodynamic force FAj shall be calculated with the equation below at each reference speed point vj. If the vehicle is equipped with velocity-dependent movable aerodynamic body parts, the corresponding aerodynamic force shall be applied for the reference speed points concerned.

6.7.2.2. The aerodynamic force shall be calculated using the equation below, where the final of that wind speed shall be used that is also used for determination of optional equipment within the interpolation method. If the vehicle is equipped with velocity-dependent movable aerodynamic body parts, the corresponding (CD × Af) values shall be applied for the reference speed points concerned.

where:

is the aerodynamic force calculated at reference speed j, N;

is the product of the drag coefficient and frontal area measured in the wind tunnel at a certain reference speed point j, if applicable, m²;

is the dry air density defined in paragraph 3.2.10. of this Regulation, kg/m³;

vj is the reference speed j, km/h.

6.7.3. Calculation of road load values

The total road load as a sum of the results of paragraphs 6.7.1 and 6.7.2. of this annex shall be calculated using the following equation:

for all applicable reference speed points j, N.

For all calculated, the coefficients f0, f1 and f2 in the road load equation shall be calculated with a least squares regression analysis and shall be used as the target coefficients in paragraph 8.1.1. of this annex.

In the case that the vehicle tested according to the wind tunnel method is the representative vehicle of a road load matrix family, the coefficient f1 shall be set to zero and the coefficients f0 and f2 shall be recalculated with a least squares regression analysis.

6.8. Road load delta method

For the purpose of including options when using the interpolation method which are not incorporated in the road load interpolation (i.e. aerodynamics, rolling resistance and mass), a delta in vehicle friction may be measured by the road load delta method (e.g. friction difference between brake systems). The following steps shall be performed:

(a) The friction of reference vehicle R shall be measured;

(b) The friction of the vehicle with the option (vehicle N) causing the difference in friction shall be measured;

(c) The difference shall be calculated according to paragraph 6.8.1. of this annex.

These measurements shall be performed on a flat belt according to paragraph 6.5. of this annex or on a chassis dynamometer according to paragraph 6.6. of this annex, and the correction of the results (excluding aerodynamic force) calculated according to paragraph 6.7.1. of this annex.

The application of this method is permitted only if the following criterion is fulfilled:

where:

FDj,R is the corrected resistance of vehicle R measured on the flat belt or chassis dynamometer at reference speed j calculated according to paragraph 6.7.1. of this annex, N;

FDj,N is the corrected resistance of vehicle N measured on the flat belt or chassis dynamometer at reference speed j calculated according to paragraph 6.7.1. of this annex, N;

n is the total number of speed points.

This alternative road load determination method may only be applied if vehicles R and N have identical aerodynamic resistance and if the measured delta appropriately covers the entire influence on the vehicle's energy consumption. This method shall not be applied if the overall accuracy of the absolute road load of vehicle N is compromised in any way.

6.8.1. Determination of delta flat belt or chassis dynamometer coefficients

The delta road load shall be calculated using the following equation:

where:

is the delta road load at reference speed j, N;

is the corrected resistance measured on the flat belt or chassis dynamometer at reference speed j calculated according to paragraph 6.7.1. of this annex for vehicle N, N;

is the corrected resistance of the reference vehicle measured on the flat belt or chassis dynamometer at reference speed j calculated according to paragraph 6.7.1. of this annex for reference vehicle R, N.

For all calculated FDj,Delta, the coefficients f0,Delta, f1,Delta and f2,Delta in the road load equation shall be calculated with a least squares regression analysis.

6.8.2. Determination of total road load

If the interpolation method (see paragraph 3.2.3.2. of Annex B7) is not used, the road load coefficients for vehicle N shall be calculated according to the following equations:

where:

N refers to the road load coefficients of vehicle N;

R refers to the road load coefficients of reference vehicle R;

Delta refers to the delta road load coefficients determined in paragraph 6.8.1. of this annex.

7. Transferring road load to a chassis dynamometer

7.1. Preparation for chassis dynamometer test

7.1.0. Selection of dynamometer operation

The test shall be carried out in accordance with paragraph 2.4.2.4. of Annex B6.

7.1.1. Laboratory conditions

7.1.1.1. Roller(s)

The chassis dynamometer roller(s) shall be clean, dry and free from foreign material that might cause tyre slippage. The dynamometer shall be run in the same coupled or uncoupled state as the subsequent Type 1 test. Chassis dynamometer speed shall be measured from the roller coupled to the power absorption unit.

7.1.1.1.1. Tyre slippage

Additional weight may be placed on or in the vehicle to eliminate tyre slippage. The manufacturer shall perform the load setting on the chassis dynamometer with the additional weight. The additional weight shall be present for both load setting and the emissions and fuel consumption tests. The use of any additional weight shall be recorded.

7.1.1.2. Room temperature

The laboratory atmospheric temperature shall be at a set point of 23 °C and shall not deviate by more than ±5 °C during the test unless otherwise required by any subsequent test.

7.2. Preparation of chassis dynamometer

7.2.1. Inertia mass setting

The equivalent inertia mass of the chassis dynamometer shall be set according to paragraph 2.5.3. of this annex. If the chassis dynamometer is not capable to meet the inertia setting exactly, the next higher inertia setting shall be applied with a maximum increase of 10 kg.

7.2.2. Chassis dynamometer warm-up

The chassis dynamometer shall be warmed up in accordance with the dynamometer manufacturer’s recommendations, or as appropriate, so that the frictional losses of the dynamometer may be stabilized.

7.3. Vehicle preparation

7.3.1. Tyre pressure adjustment

The tyre pressure at the soak temperature of a Type 1 test shall be set to no more than 50 per cent above the lower limit of the tyre pressure range for the selected tyre, as specified by the vehicle manufacturer (see paragraph 4.2.2.3. of this annex), and shall be recorded.

7.3.2. If the determination of dynamometer settings cannot meet the criteria described in paragraph 8.1.3. of this annex due to non-reproducible forces, the vehicle shall be equipped with a vehicle coastdown mode. The coastdown mode shall be approved by the responsible authority and its use shall be included in all relevant test reports.

If a vehicle is equipped with a vehicle coastdown mode, it shall be engaged both during road load determination and on the chassis dynamometer.

7.3.3. Vehicle placement on the dynamometer

The tested vehicle shall be placed on the chassis dynamometer in a straight ahead position and restrained in a safe manner.

7.3.3.1. In the case that a single roller chassis dynamometer is used, the vehicle shall be positioned and stay positioned throughout the procedure according to the requirements in 7.3.3.1.1. to 7.3.3.1.3.

7.3.3.1.1. Rotational alignment (rotation around z-axis)

The vehicle shall be positioned in line with the x-axis in order to minimise rotation around the z-axis

7.3.3.1.2. Lateral position (y-axis)

The vehicle shall remain aligned in the y-direction and lateral movement shall be minimised.

7.3.3.1.3. Front and rear position (x-axis)

For all rotating wheels the centre of the tyre’s contact patch on the roller shall be within ±25 mm or ±2 per cent of the roller diameter, whichever is smaller, from the top of the roller.

7.3.3.1.4. The tested vehicle shall be restrained with a system compliant with paragraph 2.3.2. of Annex B5 .

If the torque meter method is used, the tyre pressure shall be adjusted such that the dynamic radius is within 0.5 per cent of the dynamic radius rj calculated using the equations in paragraph 4.4.3.1. of this annex at the 80 km/h reference speed point. The dynamic radius on the chassis dynamometer shall be calculated according to the procedure described in paragraph 4.4.3.1. of this annex.

If this adjustment is outside the range defined in paragraph 7.3.1. of this annex, the torque meter method shall not apply.

7.3.4. Vehicle warm-up

7.3.4.1. The vehicle shall be warmed up with the applicable WLTC. In the case that the vehicle was warmed up at 90 per cent of the maximum speed of the next higher phase during the procedure defined in paragraph 4.2.4.1.2. of this annex, this higher phase shall be added to the applicable WLTC.

Table A4/7

**Vehicle warm-up**

| *Vehicle class* | *Applicable WLTC* | *Adopt next higher phase* | *Warm-up cycle* |
| --- | --- | --- | --- |
| Class 1 | Low1+ Medium1 | NA | Low1+ Medium1 |
| Class 2 | Low2 + Medium2 + High2 + Extra High2 | NA | Low2 + Medium2 + High2 + Extra High2 |
| Low2 + Medium2 + High2 | Yes (Extra High2) |
| No | Low2+ Medium2+ High2 |
| Class 3 | Low3 + Medium3 + High3 + Extra High3 | Low3 + Medium3 + High3 + Extra High3 | Low3 + Medium3 + High3 + Extra High3 |
| Low3 + Medium3 + High3 | Yes (Extra High3) |
| No | Low3 + Medium3 + High3 |

7.3.4.2. If the vehicle is already warmed up, the WLTC phase applied in paragraph 7.3.4.1. of this annex, with the highest speed, shall be driven.

7.3.4.3. Alternative warm-up procedure

7.3.4.3.1. At the request of the vehicle manufacturer and with approval of the responsible authority, an alternative warm-up procedure may be used. The approved alternative warm-up procedure may be used for vehicles within the same road load family and shall satisfy the requirements outlined in paragraphs 7.3.4.3.2. to 7.3.4.3.5. inclusive of this annex.

7.3.4.3.2. At least one vehicle representing the road load family shall be selected.

7.3.4.3.3. The cycle energy demand calculated according to paragraph 5. of Annex B7 with corrected road load coefficients f0a, f1a and f2a, for the alternative warm-up procedure shall be equal to or higher than the cycle energy demand calculated with the target road load coefficients f0, f1, and f2, for each applicable phase.

The corrected road load coefficients f0a, f1a and f2a, shall be calculated according to the following equations:

where:

Ad\_alt, Bd\_alt and Cd\_alt are the chassis dynamometer setting coefficients after the alternative warm-up procedure;

Ad\_WLTC, Bd\_WLTC

and Cd\_WLTC are the chassis dynamometer setting coefficients after a WLTC warm-up procedure described in paragraph 7.3.4.1. of this annex and a valid chassis dynamometer load setting according to paragraph 8. of this annex.

7.3.4.3.4. The corrected road load coefficients f0a, f1a and f2a, shall be used only for the purpose of paragraph 7.3.4.3.3. of this annex. For other purposes, the target road load coefficients f0, f1 and f2, shall be used as the target road load coefficients.

7.3.4.3.5. Details of the procedure and of its equivalency shall be provided to the responsible authority.

8. Chassis dynamometer load setting

8.1. Chassis dynamometer load setting using the coastdown method

This method is applicable when the road load coefficients f0, f1 and f2 have been determined.

In the case of a road load matrix family, this method shall be applied when the road load of the representative vehicle is determined using the coastdown method described in paragraph 4.3. of this annex. The target road load values are the values calculated using the method described in paragraph 5.1. of this annex.

8.1.1. Initial load setting

For a chassis dynamometer with coefficient control, the chassis dynamometer power absorption unit shall be adjusted with the arbitrary initial coefficients, , and , of the following equation:

where:

is the chassis dynamometer setting load, N;

is the speed of the chassis dynamometer roller, km/h.

The following are recommended coefficients to be used for the initial load setting:

(a)

for single-axis chassis dynamometers, or

for dual-axis chassis dynamometers, where , and are the target road load coefficients;

(b) Empirical values, such as those used for the setting for a similar type of vehicle.

For a chassis dynamometer of polygonal control, adequate load values at each reference speed shall be set to the chassis dynamometer power absorption unit.

8.1.2. Coastdown

The coastdown test on the chassis dynamometer shall be performed with the procedure given in paragraphs 8.1.3.4.1. or 8.1.3.4.2. of this annex and shall start no later than 120 seconds after completion of the warm-up procedure. Consecutive coastdown runs shall be started immediately. At the request of the manufacturer and with approval of the responsible authority, the time between the warm-up procedure and coastdowns using the iterative method may be extended to ensure a proper vehicle setting for the coastdown. The manufacturer shall provide the responsible authority with evidence for requiring additional time and evidence that the chassis dynamometer load setting parameters (e.g. coolant and/or oil temperature, force on a dynamometer) are not affected.

8.1.3. Verification

8.1.3.1. The target road load value shall be calculated using the target road load coefficient, , and for each reference speed, :

where:

At, Bt and Ct are the target road load parameters;

is the target road load at reference speed , N;

is the jth reference speed, km/h.

8.1.3.2. The measured road load shall be calculated using the following equation:

where:

Δv is 5 km/h;

Fmj is the measured road load for each reference speed vj, N;

TM is the test mass of the vehicle, kg;

mr is the equivalent effective mass of rotating components according to paragraph 2.5.1. of this annex, kg;

∆tj is the coastdown time corresponding to speed vj, s.

8.1.3.3. The coefficients As, Bs and Cs in the road load equation of the simulated road load on the chassis dynamometer shall be calculated using a least squares regression analysis:

The simulated road load for each reference speed vj shall be determined using the following equation, using the calculated As, Bs and Cs:

)

8.1.3.4. For dynamometer load setting, two different methods may be used. If the vehicle is accelerated by the dynamometer, the methods described in paragraph 8.1.3.4.1. of this annex shall be used. If the vehicle is accelerated under its own power, the methods in paragraphs 8.1.3.4.1. or 8.1.3.4.2. of this annex shall be used and the minimum acceleration multiplied by speed shall be 6 m²/sec³. Vehicles which are unable to achieve 6 m2/s3 shall be driven with the acceleration control fully applied.

8.1.3.4.1. Fixed run method

8.1.3.4.1.1. The dynamometer software shall perform a total of four coastdowns. From the first coastdown, the dynamometer setting coefficients for the second run shall be calculated according to paragraph 8.1.4. of this annex. Following the first coastdown, the software shall perform three additional coastdowns with either the fixed dynamometer setting coefficients determined after the first coastdown or the adjusted dynamometer setting coefficients according to paragraph 8.1.4. of this annex.

8.1.3.4.1.2. The final dynamometer setting coefficients A, B and C shall be calculated using the following equations:

where:

At, Bt and Ct are the target road load parameters;

, and are the simulated road load coefficients of the nth run;

, and are the dynamometer setting coefficients of the nth run;

n is the index number of coastdowns including the first stabilisation run.

8.1.3.4.2. Iterative method

The calculated forces in the specified speed ranges shall either be within ±10 N after a least squares regression of the forces for two consecutive coastdowns when compared with the target values, or additional coastdowns shall be performed after adjusting the chassis dynamometer load setting according to paragraph 8.1.4. of this annex until the tolerance is satisfied.

8.1.4. Adjustment

The chassis dynamometer setting load shall be adjusted according to the following equations:

Therefore:

where:

Fdj is the initial chassis dynamometer setting load, N;

is the adjusted chassis dynamometer setting load, N;

Fj is the adjustment road load equal to , N;

Fsj is the simulated road load at reference speed vj, N;

Ftj is the target road load at reference speed vj, N;

, and are the new chassis dynamometer setting coefficients.

8.1.5. At, Bt and Ct shall be used as the final values of f0, f1 and f2, and shall be used for the following purposes:

(a) Determination of downscaling, paragraph 8. of Annex B1;

(b) Determination of gearshift points, Annex B2;

(c) Interpolation of CO2 and fuel consumption, paragraph 3.2.3. of Annex B7;

(d) Calculation of results of electric and hybrid-electric vehicles, paragraph 4. of Annex B8.

8.2. Chassis dynamometer load setting using the torque meter method

This method is applicable when the running resistance is determined using the torque meter method described in paragraph 4.4. of this annex.

In the case of a road load matrix family, this method shall be applied when the running resistance of the representative vehicle is determined using the torque meter method as specified in paragraph 4.4. of this annex. The target running resistance values are the values calculated using the method specified in paragraph 5.1. of this annex.

8.2.1. Initial load setting

For a chassis dynamometer of coefficient control, the chassis dynamometer power absorption unit shall be adjusted with the arbitrary initial coefficients, , and , of the following equation:

where:

is the chassis dynamometer setting load, N;

is the speed of the chassis dynamometer roller, km/h.

The following coefficients are recommended for the initial load setting:

(a)

For single-axis chassis dynamometers, or

For dual-axis chassis dynamometers, where:

, and are the target running resistance coefficients; and

is the dynamic radius of the tyre on the chassis dynamometer obtained at 80 km/h, m, or

(b) Empirical values, such as those used for the setting for a similar type of vehicle.

For a chassis dynamometer of polygonal control, adequate load values at each reference speed shall be set for the chassis dynamometer power absorption unit.

8.2.2. Wheel torque measurement

The torque measurement test on the chassis dynamometer shall be performed with the procedure defined in paragraph 4.4.2. of this annex. The torque meter(s) shall be identical to the one(s) used in the preceding road test.

8.2.3. Verification

8.2.3.1. The target running resistance (torque) curve shall be determined using the equation in paragraph 4.5.5.2.1. of this annex and may be written as follows:

8.2.3.2. The simulated running resistance (torque) curve on the chassis dynamometer shall be calculated according to the method described and the measurement precision specified in paragraph 4.4.3.2. of this annex, and the running resistance (torque) curve determination as described in paragraph 4.4.4. of this annex with applicable corrections according to paragraph 4.5. of this annex, all with the exception of measuring in opposite directions, resulting in a simulated running resistance curve:

The simulated running resistance (torque) shall be within a tolerance of ±10 N×r’ from the target running resistance at every speed reference point where r’ is the dynamic radius of the tyre in metres on the chassis dynamometer obtained at 80 km/h.

If the tolerance at any reference speed does not satisfy the criterion of the method described in this paragraph, the procedure specified in paragraph 8.2.3.3. of this annex shall be used to adjust the chassis dynamometer load setting.

8.2.3.3. Adjustment

The chassis dynamometer load setting shall be adjusted using the following equation:

therefore:

where:

is the new chassis dynamometer setting load, N;

Fej is the adjustment road load equal to (Fsj-Ftj), Nm;

is the simulated road load at reference speed vj, Nm;

is the target road load at reference speed vj, Nm;

, and are the new chassis dynamometer setting coefficients;

r’ is the dynamic radius of the tyre on the chassis dynamometer obtained at 80 km/h, m.

Paragraphs 8.2.2. and 8.2.3. of this annex shall be repeated until the tolerance in paragraph 8.2.3.2. of this annex is met.

8.2.3.4. The mass of the driven axle(s), tyre specifications and chassis dynamometer load setting shall be recorded when the requirement of paragraph 8.2.3.2. of this annex is fulfilled.

8.2.4. Transforming running resistance coefficients to road load coefficients f0, f1, f2

8.2.4.1. If the vehicle does not coast down in a repeatable manner and a vehicle coastdown mode according to paragraph 4.2.1.8.5. of this annex is not feasible, the coefficients f0, f1 and f2 in the road load equation shall be calculated using the equations in paragraph 8.2.4.1.1. of this annex. In any other case, the procedure described in paragraphs 8.2.4.2. to 8.2.4.4. inclusive of this annex shall be performed.

8.2.4.1.1.

where:

c0, c1, c2 are the running resistance coefficients determined in paragraph 4.4.4. of this annex, Nm, Nm/(km/h), Nm/(km/h)²;

r is the dynamic tyre radius of the vehicle with which the running resistance was determined, m;

1.02 is an approximate coefficient compensating for drivetrain losses.

8.2.4.1.2. The determined f0, f1, f2 values shall not be used for a chassis dynamometer setting or any emission or range testing. They shall be used only in the following cases:

(a) Determination of downscaling, paragraph 8. of Annex B1;

(b) Determination of gearshift points, Annex B2;

(c) Interpolation of CO2 and fuel consumption, paragraph 3.2.3 of Annex B7;

(d) Calculation of results of electric and hybrid-electric vehicles, paragraph 4. of Annex B8.

8.2.4.2. Once the chassis dynamometer has been set within the specified tolerances, a vehicle coastdown procedure shall be performed on the chassis dynamometer as outlined in paragraph 4.3.1.3. of this annex. The coastdown times shall be recorded.

8.2.4.3. The road load Fj at reference speed vj, N, shall be determined using the following equation:

where:

Fj is the road load at reference speed vj, N;

TM is the test mass of the vehicle, kg;

mr is the equivalent effective mass of rotating components according to paragraph 2.5.1. of this annex, kg;

∆v = 5 km/h

∆tj is the coastdown time corresponding to speed vj, s.

8.2.4.4. The coefficients f0, f1 and f2 in the road load equation shall be calculated with a least squares regression analysis over the reference speed range.

Annex B5

Test equipment and calibrations

1. Test bench specifications and settings

1.1. Cooling fan specifications

1.1.1. A variable speed current of air shall be blown towards the vehicle. The set point of the linear velocity of the air at the blower outlet shall be equal to the corresponding roller speed above roller speeds of 5 km/h. The linear velocity of the air at the blower outlet shall be within ±5 km/h or ±10 per cent of the corresponding roller speed, whichever is greater.

1.1.2. The above-mentioned air velocity shall be determined as an averaged value of a number of measuring points that:

(a) For fans with rectangular outlets, are located at the centre of each rectangle dividing the whole of the fan outlet into 9 areas (dividing both horizontal and vertical sides of the fan outlet into 3 equal parts). The centre area shall not be measured (as shown in Figure A5/1);

Figure A5/1

**Fan with rectangular outlet**



(b) For fans with circular outlets, the outlet shall be divided into 8 equal sectors by vertical, horizontal and 45° lines. The measurement points shall lie on the radial centre line of each sector (22.5°) at two-thirds of the outlet radius (as shown in Figure A5/2).

Figure A5/2

**Fan with circular outlet**



These measurements shall be made with no vehicle or other obstruction in front of the fan. The device used to measure the linear velocity of the air shall be located between 0 and 20 cm from the air outlet.

1.1.3. The outlet of the fan shall have the following characteristics:

(a) An area of at least 0.3 m2; and

(b) A width/diameter of at least 0.8 metre.

1.1.4. The position of the fan shall be as follows:

(a) Height of the lower edge above ground: approximately 20 cm;

(b) Distance from the front of the vehicle: approximately 30 cm;

(c) Approximately on the longitudinal centreline of the vehicle.

1.1.5. At the request of the manufacturer and if considered appropriate by the responsible authority, the height, lateral position and distance from the vehicle of the cooling fan may be modified.

If the specified fan configuration is impractical for special vehicle designs, such as vehicles with rear-mounted engines or side air intakes, or it does not provide adequate cooling to properly represent in-use operation, at the request of the manufacturer and if considered appropriate by the responsible authority, the height, capacity, longitudinal and lateral position of the cooling fan may be modified and additional fans which may have different specifications (including constant speed fans) may be used.

1.1.6. In the cases described in paragraph 1.1.5. of this annex, the position and capacity of the cooling fan(s) and details of the justification supplied to the responsible authority shall be recorded. For any subsequent testing, similar positions and specifications shall be used in consideration of the justification to avoid non-representative cooling characteristics.

2. Chassis dynamometer

2.1. General requirements

2.1.1. The dynamometer shall be capable of simulating road load with three road load coefficients that can be adjusted to shape the load curve.

2.1.2. The chassis dynamometer may have a single or twin-roller configuration. In the case that twin-roller chassis dynamometers are used, the rollers shall be permanently coupled or the front roller shall drive, directly or indirectly, any inertial masses and the power absorption device.

2.2. Specific requirements

The following specific requirements relate to the dynamometer manufacturer's specifications.

2.2.1. The roller run-out shall be less than 0.25 mm at all measured locations.

2.2.2. The roller diameter shall be within ±1.0 mm of the specified nominal value at all measurement locations.

2.2.3. The dynamometer shall have a time measurement system for use in determining acceleration rates and for measuring vehicle/dynamometer coastdown times. This time measurement system shall not exceed an accuracy of ±0.001 per cent after at least 1,000 seconds of operation. This shall be verified upon initial installation.

2.2.4. The dynamometer shall have a speed measurement system with an accuracy of at least ±0.080 km/h. This shall be verified upon initial installation.

2.2.5. The dynamometer shall have a response time (90 per cent response to a tractive effort step change) of less than 100 ms with instantaneous accelerations that are at least 3 m/s2. This shall be verified upon initial installation and after major maintenance.

2.2.6. The base inertia of the dynamometer shall be stated by the dynamometer manufacturer and shall be confirmed to within 0.5 per cent or 7.5 kg whichever is the greater for each measured base inertia and ±0.2 per cent relative to any arithmetic average value by dynamic derivation from trials at constant acceleration, deceleration and force.

2.2.7. Roller speed shall be measured at a frequency of not less than 10 Hz.

2.3. Additional specific requirements for a chassis dynamometer in 4WD operation

2.3.1. For testing in 4WD operation, the chassis dynamometer shall have a single roller configuration. The 4WD control system shall be designed such that the following requirements are fulfilled when tested with a vehicle driven over the WLTC.

2.3.1.1. Road load simulation shall be applied such that the dynamometer in 4WD operation reproduces the same proportioning of forces as would be encountered when driving the vehicle on a smooth, dry, level road surface.

2.3.1.2. Upon initial installation and after major maintenance, the requirements of paragraph 2.3.1.2.1. of this annex and of either paragraph 2.3.1.2.2. or 2.3.1.2.3. of this annex shall be satisfied. The speed difference between the front and rear rollers shall be assessed by applying a 1 second moving average filter to roller speed data acquired at a minimum frequency of 20 Hz.

2.3.1.2.1. The difference in distance covered by the front and rear rollers shall be less than 0.2 per cent of the distance driven over the WLTC. The absolute number shall be integrated for the calculation of the total difference in distance over the WLTC.

2.3.1.2.2. The difference in distance covered by the front and rear rollers shall be less than 0.1 m in any 200 ms time period.

2.3.1.2.3. The speed difference of all roller speeds shall be within ±0.16 km/h.

2.3.1.3. The usage of twin roller dynamometers with 4WD configuration shall be accepted if the following conditions are met:

(a) The separation distance between the front and rear sets of twin rollers of the dynamometer (X in diagram below) is set as closely as possible to match the manufacturer’s declared wheelbase of the vehicle to be tested, and

(b) It shall be ensured that the setting of the separation distance between the roller sets used for dyno load setting is reproduced for vehicle testing.



2.3.2. Vehicle restraint system for single roller chassis dynamometers

2.3.2.1. Vertical force

In addition to the requirement of paragraph 7.3.3.1.3. of Annex B4, the restraint system shall be designed so that the vertical force imposed to the vehicle is minimized and is the same during the chassis dynamometer setting and all tests. This criteria is fulfilled, if either the restraint system is designed such that it cannot impose any different vertical force, or if a procedure to demonstrate how this requirement can be met is agreed between the responsible authority and the manufacturer.

2.3.2.2. Restraint stiffness

The restraint system shall exhibit sufficient stiffness in order to minimize any movements and rotations. Only limited movements along the z-axis and rotations over the y-axis are allowed to avoid non-negligible effects towards the test results and to fulfil the requirements of paragraph 2.3.2.1. of this annex.

2.4. Chassis dynamometer calibration

2.4.1. Force measurement system

The accuracy of the force transducer shall be at least ±10 N for all measured increments. This shall be verified upon initial installation, after major maintenance and within 370 days before testing.

2.4.2. Dynamometer parasitic loss calibration

The dynamometer's parasitic losses shall be measured and updated if any measured value differs from the current loss curve by more than 9.0 N. This shall be verified upon initial installation, after major maintenance and within 35 days before testing.

2.4.3. Verification of road load simulation without a vehicle

The dynamometer performance shall be verified by performing an unloaded coastdown test upon initial installation, after major maintenance, and within 7 days before testing. The arithmetic average coastdown force error shall be less than 10 N or 2 per cent, whichever is greater, at each reference speed point.

3. Exhaust gas dilution system

3.1. System specification

3.1.1. Overview

3.1.1.1. A full flow exhaust dilution system shall be used. The total vehicle exhaust shall be continuously diluted with ambient air under controlled conditions using a constant volume sampler. A critical flow venturi (CFV) or multiple critical flow venturis arranged in parallel, a positive displacement pump (PDP), a subsonic venturi (SSV), or an ultrasonic flow meter (UFM) may be used. The total volume of the mixture of exhaust and dilution air shall be measured and a continuously proportional sample of the volume shall be collected for analysis. The quantities of exhaust gas compounds shall be determined from the sample concentrations, corrected for their respective content of the dilution air and the totalised flow over the test period.

3.1.1.2. The exhaust dilution system shall consist of a connecting tube, a mixing device and dilution tunnel, dilution air conditioning, a suction device and a flow measurement device. Sampling probes shall be fitted in the dilution tunnel as specified in paragraphs 4.1., 4.2. and 4.3. of this annex.

3.1.1.3. The mixing device referred to in paragraph 3.1.1.2. of this annex shall be a vessel such as that illustrated in Figure A5/3 in which vehicle exhaust gases and the dilution air are combined so as to produce a homogeneous mixture at the sampling position.

3.2. General requirements

3.2.1. The vehicle exhaust gases shall be diluted with a sufficient amount of ambient air to prevent any water condensation in the sampling and measuring system at all conditions that may occur during a test.

3.2.2. The mixture of air and exhaust gases shall be homogeneous at the point where the sampling probes are located (see paragraph 3.3.3. of this annex). The sampling probes shall extract representative samples of the diluted exhaust gas.

3.2.3. The system shall enable the total volume of the diluted exhaust gases to be measured.

3.2.4. The sampling system shall be gas-tight. The design of the variable dilution sampling system and the materials used in its construction shall be such that the concentration of any compound in the diluted exhaust gases is not affected. If any component in the system (heat exchanger, cyclone separator, suction device, etc.) changes the concentration of any of the exhaust gas compounds and the systematic error cannot be corrected, sampling for that compound shall be carried out upstream from that component.

3.2.5. All parts of the dilution system in contact with raw or diluted exhaust gas shall be designed to minimise deposition or alteration of the particulate or particles. All parts shall be made of electrically conductive materials that do not react with exhaust gas components, and shall be electrically grounded to prevent electrostatic effects.

3.2.6. If the vehicle being tested is equipped with an exhaust pipe comprising several branches, the connecting tubes shall be connected as near as possible to the vehicle without adversely affecting their operation.

3.3. Specific requirements

3.3.1. Connection to vehicle exhaust

3.3.1.1. The start of the connecting tube is the exit of the tailpipe. The end of the connecting tube is the sample point, or first point of dilution.

For multiple tailpipe configurations where all the tailpipes are combined, the start of the connecting tube shall be taken at the last joint of where all the tailpipes are combined. In this case, the tube between the exit of the tailpipe and the start of the connecting tube may or may not be insulated or heated.

3.3.1.2. The connecting tube between the vehicle and dilution system shall be designed so as to minimize heat loss.

3.3.1.3. The connecting tube shall satisfy the following requirements:

(a) Be less than 3.6 metres long, or less than 6.1 metres long if heat-insulated. Its internal diameter shall not exceed 105 mm; the insulating materials shall have a thickness of at least 25 mm and thermal conductivity shall not exceed 0.1 W/m-1K-1 at 400 °C. Optionally, the tube may be heated to a temperature above the dew point. This may be assumed to be achieved if the tube is heated to 70 °C;

(b) Not cause the static pressure at the exhaust outlets on the vehicle being tested to differ by more than ±0.75 kPa at 50 km/h, or more than ±1.25 kPa for the duration of the test from the static pressures recorded when nothing is connected to the vehicle exhaust pipes. The pressure shall be measured in the exhaust outlet or in an extension having the same diameter and as near as possible to the end of the tailpipe. Sampling systems capable of maintaining the static pressure to within ±0.25 kPa may be used if a written request from a manufacturer to the responsible authority substantiates the need for the tighter tolerance;

(c) No component of the connecting tube shall be of a material that might affect the gaseous or solid composition of the exhaust gas. To avoid generation of any particles from elastomer connectors, elastomers employed shall be as thermally stable as possible and have minimum exposure to the exhaust gas. It is recommended not to use elastomer connectors to bridge the connection between the vehicle exhaust and the connecting tube.

3.3.2. Dilution air conditioning

3.3.2.1. The dilution air used for the primary dilution of the exhaust in the CVS tunnel shall pass through a medium capable of reducing particles of the most penetrating particle size in the filter material by ≥ 99.95 per cent, or through a filter of at least Class H13 of EN 1822:2019. This represents the specification of High Efficiency Particulate Air (HEPA) filters. The dilution air may optionally be charcoal-scrubbed before being passed to the HEPA filter. It is recommended that an additional coarse particle filter be situated before the HEPA filter and after the charcoal scrubber, if used.

3.3.2.2. At the vehicle manufacturer's request, the dilution air may be sampled according to good engineering practice to determine the tunnel contribution to background particulate and, if PN measurement is required particle levels, which can be subsequently subtracted from the values measured in the diluted exhaust. See paragraph 2.1.3. of Annex B6.

3.3.3. Dilution tunnel

3.3.3.1. Provision shall be made for the vehicle exhaust gases and the dilution air to be mixed. A mixing device may be used.

3.3.3.2. The homogeneity of the mixture in any cross-section at the location of the sampling probe shall not vary by more than ±2 per cent from the arithmetic average of the values obtained for at least five points located at equal intervals on the diameter of the gas stream.

3.3.3.3. For PM and PN (if PN measurement is required) emissions sampling, a dilution tunnel shall be used that:

(a) Consists of a straight tube of electrically-conductive material that is grounded;

(b) Causes turbulent flow (Reynolds number ≥ 4,000) and be of sufficient length to cause complete mixing of the exhaust and dilution air;

(c) Is at least 200 mm in diameter;

(d) May be insulated and/or heated.

3.3.4. Suction device

3.3.4.1. This device may have a range of fixed speeds to ensure sufficient flow to prevent any water condensation. This result is obtained if the flow is either:

(a) Twice as high as the maximum flow of exhaust gas produced by accelerations of the driving cycle; or

(b) Sufficient to ensure that the CO2 concentration in the dilute exhaust sample bag is less than 3 per cent by volume for petrol and diesel, less than 2.2 per cent by volume for LPG and less than 1.5 per cent by volume for NG/biomethane.

3.3.4.2. Compliance with the requirements in paragraph 3.3.4.1. of this annex may not be necessary if the CVS system is designed to inhibit condensation by such techniques, or combination of techniques, as:

(a) Reducing water content in the dilution air (dilution air dehumidification);

(b) Heating of the CVS dilution air and of all components up to the diluted exhaust flow measurement device and, optionally, the bag sampling system including the sample bags and also the system for the measurement of the bag concentrations.

In such cases, the selection of the CVS flow rate for the test shall be justified by showing that condensation of water cannot occur at any point within the CVS, bag sampling or analytical system.

3.3.5. Volume measurement in the primary dilution system

3.3.5.1. The method of measuring total dilute exhaust volume incorporated in the constant volume sampler shall be such that measurement is accurate to ±2 per cent under all operating conditions. If the device cannot compensate for variations in the temperature of the mixture of exhaust gases and dilution air at the measuring point, a heat exchanger shall be used to maintain the temperature to within ±6 °C of the specified operating temperature for a PDP CVS, ±11 °C for a CFV CVS, ±6 °C for a UFM CVS, and ±11 °C for an SSV CVS.

3.3.5.2. If necessary, some form of protection for the volume measuring device may be used e.g. a cyclone separator, bulk stream filter, etc.

3.3.5.3. A temperature sensor shall be installed immediately before the volume measuring device. This temperature sensor shall have an accuracy of ±1 °C and a response time of 1 second or less at 62 per cent of a given temperature variation (value measured in water or silicone oil).

3.3.5.4. Measurement of the pressure difference from atmospheric pressure shall be taken upstream from and, if necessary, downstream from the volume measuring device.

3.3.5.5. The pressure measurements shall have a precision and an accuracy of ±0.4 kPa during the test. See Table A5/5.

3.3.6. Recommended system description

Figure A5/3 is a schematic drawing of exhaust dilution systems that meet the requirements of this annex.

The following components are recommended:

(a) A dilution air filter, which may be pre-heated if necessary. This filter shall consist of the following filters in sequence: an optional activated charcoal filter (inlet side), and a HEPA filter (outlet side). It is recommended that an additional coarse particle filter be situated before the HEPA filter and after the charcoal filter, if used. The purpose of the charcoal filter is to reduce and stabilize the hydrocarbon concentrations of ambient emissions in the dilution air;

(b) A connecting tube by which vehicle exhaust is admitted into a dilution tunnel;

(c) An optional heat exchanger as described in paragraph 3.3.5.1. of this annex;

(d) A mixing device in which exhaust gas and dilution air are mixed homogeneously, and which may be located close to the vehicle so that the length of the connecting tube is minimized;

(e) A dilution tunnel from which particulate and, if applicable, particles are sampled;

(f) Some form of protection for the measurement system may be used e.g. a cyclone separator, bulk stream filter, etc.;

(g) A suction device of sufficient capacity to handle the total volume of diluted exhaust gas.

Exact conformity with these figures is not essential. Additional components such as instruments, valves, solenoids and switches may be used to provide additional information and co-ordinate the functions of the component system.

# Figure A5/3

# **Exhaust dilution system**

Dilution air

filters

Vehicle

exhaust

Dilution tunnel

Heat exchanger

(optional)

Vent

MC

Flow meter and suction device

Mixing device

Dilution air

PDP, CFV, SSV, UFM

Connecting tube

3.3.6.1. Positive displacement pump (PDP)

A positive displacement pump (PDP) full flow exhaust dilution system satisfies the requirements of this annex by metering the flow of gas through the pump at constant temperature and pressure. The total volume is measured by counting the revolutions made by the calibrated positive displacement pump. The proportional sample is achieved by sampling with pump, flow meter and flow control valve at a constant flow rate.

3.3.6.2. Critical flow venturi (CFV)

3.3.6.2.1. The use of a CFV for the full flow exhaust dilution system is based on the principles of flow mechanics for critical flow. The variable mixture flow rate of dilution and exhaust gas is maintained at sonic velocity that is directly proportional to the square root of the gas temperature. Flow is continually monitored, computed and integrated throughout the test.

3.3.6.2.2. The use of an additional critical flow sampling venturi ensures the proportionality of the gas samples taken from the dilution tunnel. As both pressure and temperature are equal at the two venturi inlets, the volume of the gas flow diverted for sampling is proportional to the total volume of diluted exhaust gas mixture produced, and thus the requirements of this annex are fulfilled.

3.3.6.2.3. A measuring CFV tube shall measure the flow volume of the diluted exhaust gas.


**3.3.6.3. Subsonic flow venturi (SSV)**

**3.3.6.3.1. The use of an SSV (Figure A5/4) for a full flow exhaust dilution system is based on the principles of flow mechanics. The variable mixture flow rate of dilution and exhaust gas is maintained at a subsonic velocity that is calculated from the physical dimensions of the subsonic venturi and measurement of the absolute temperature (T) and pressure (P) at the venturi inlet and the pressure in the throat of the venturi. Flow is continually monitored, computed and integrated throughout the test.**

**3.3.6.3.2. An SSV shall measure the flow volume of the diluted exhaust gas.**

# Figure A5/4

# **Schematic of a subsonic venturi tube (SSV)**



Suction device

3.3.6.4. Ultrasonic flow meter (UFM)

3.3.6.4.1. A UFM measures the velocity of the diluted exhaust gas in the CVS piping using the principle of ultrasonic flow detection by means of a pair, or multiple pairs, of ultrasonic transmitters/receivers mounted within the pipe as in Figure A5/5. The velocity of the flowing gas is determined by the difference in the time required for the ultrasonic signal to travel from transmitter to receiver in the upstream direction and the downstream direction. The gas velocity is converted to standard volumetric flow using a calibration factor for the tube diameter with real time corrections for the diluted exhaust temperature and absolute pressure.

3.3.6.4.2. Components of the system include:

(a) A suction device fitted with speed control, flow valve or other method for setting the CVS flow rate and also for maintaining constant volumetric flow at standard conditions;

(b) A UFM;

(c) Temperature and pressure measurement devices, T and P, required for flow correction;

(d) An optional heat exchanger for controlling the temperature of the diluted exhaust to the UFM. If installed, the heat exchanger shall be capable of controlling the temperature of the diluted exhaust to that specified in paragraph 3.3.5.1. of this annex. Throughout the test, the temperature of the air/exhaust gas mixture measured at a point immediately upstream of the suction device shall be within ±6 °C of the arithmetic average operating temperature during the test.

# Figure A5/5

# **Schematic of an ultrasonic flow meter (UFM)**

Heat

Exchanger

(

option

)

Ultrasonic

Flow Meter

Suction

Device

P

T

3.3.6.4.3. The following conditions shall apply to the design and use of the UFM type CVS:

(a) The velocity of the diluted exhaust gas shall provide a Reynolds number higher than 4,000 in order to maintain a consistent turbulent flow before the ultrasonic flow meter;

(b) An ultrasonic flow meter shall be installed in a pipe of constant diameter with a length of 10 times the internal diameter upstream and 5 times the diameter downstream;

(c) A temperature sensor (T) for the diluted exhaust shall be installed immediately before the ultrasonic flow meter. This sensor shall have an accuracy of ±1 °C and a response time of 0.1 seconds at 62 per cent of a given temperature variation (value measured in silicone oil);

(d) The absolute pressure (P) of the diluted exhaust shall be measured immediately before the ultrasonic flow meter to within ±0.3 kPa;

(e) If a heat exchanger is not installed upstream of the ultrasonic flow meter, the flow rate of the diluted exhaust, corrected to standard conditions, shall be maintained at a constant level during the test. This may be achieved by control of the suction device, flow valve or other method.

3.4. CVS calibration procedure

3.4.1. General requirements

3.4.1.1. The CVS system shall be calibrated by using an accurate flow meter and a restricting device and at the intervals listed in Table A5/4. The flow through the system shall be measured at various pressure readings and the control parameters of the system measured and related to the flows. The flow metering device (e.g. calibrated venturi, laminar flow element (LFE), calibrated turbine meter) shall be dynamic and suitable for the high flow rate encountered in constant volume sampler testing. The device shall be of certified accuracy.

3.4.1.2. The following paragraphs describe methods for calibrating PDP, CFV, SSV and UFM units using a laminar flow meter, which gives the required accuracy, along with a statistical check on the calibration validity.

3.4.2. Calibration of a positive displacement pump (PDP)

3.4.2.1. The following calibration procedure outlines the equipment, the test configuration and the various parameters that are measured to establish the flow rate of the CVS pump. All the parameters related to the pump are simultaneously measured with the parameters related to the flow meter that is connected in series with the pump. The calculated flow rate (given in m3/min at pump inlet for the measured absolute pressure and temperature) shall be subsequently plotted versus a correlation function that includes the relevant pump parameters. The linear equation that relates the pump flow and the correlation function shall be subsequently determined. In the case that a CVS has a multiple speed drive, a calibration for each range used shall be performed.

3.4.2.2. This calibration procedure is based on the measurement of the absolute values of the pump and flow meter parameters relating the flow rate at each point. The following conditions shall be maintained to ensure the accuracy and integrity of the calibration curve:

3.4.2.2.1. The pump pressures shall be measured at tappings on the pump rather than at the external piping on the pump inlet and outlet. Pressure taps that are mounted at the top centre and bottom centre of the pump drive head plate are exposed to the actual pump cavity pressures, and therefore reflect the absolute pressure differentials.

3.4.2.2.2. Temperature stability shall be maintained during the calibration. The laminar flow meter is sensitive to inlet temperature oscillations that cause data points to be scattered. Gradual changes of ±1 °C in temperature are acceptable as long as they occur over a period of several minutes.

3.4.2.2.3. All connections between the flow meter and the CVS pump shall be free of leakage.

3.4.2.3. During an exhaust emissions test, the measured pump parameters shall be used to calculate the flow rate from the calibration equation.

3.4.2.4. Figure A5/6 of this annex shows an example of a calibration set-up. Variations are permissible, provided that the responsible authority approves them as being of comparable accuracy. If the set-up shown in Figure A5/6 is used, the following data shall be found within the limits of accuracy given:

Barometric pressure (corrected), ±0.03 kPa

Ambient temperature, ±0.2 °C

Air temperature at LFE, ETI ±0.15 °C

Pressure depression upstream of LFE, EPI ±0.01 kPa

Pressure drop across the LFE matrix, EDP ±0.0015 kPa

Air temperature at CVS pump inlet, PTI ±0.2 °C

Air temperature at CVS pump outlet, PTO ±0.2 °C

Pressure depression at CVS pump inlet, PPI ±0.22 kPa

Pressure head at CVS pump outlet, PPO ±0.22 kPa

Pump revolutions during test period, ±1 min-1

Elapsed time for period (minimum 250 s), t ±0.1 s

Figure A5/6

**PDP calibration configuration**

Manometer

Surge control valve (scrubber)

PPI

PPO

Revolutions

Elapsed time

n

t

Temperature indicator

PTI

PTO

Variable-flow restrictor

Laminar flow element, LFE

ETI

EPI

EDP

Filter

3.4.2.5. After the system has been connected as shown in Figure A5/6, the variable restrictor shall be set in the wide-open position and the CVS pump shall run for 20 minutes before starting the calibration.

3.4.2.5.1. The restrictor valve shall be reset to a more restricted condition in increments of pump inlet depression (about 1 kPa) that will yield a minimum of six data points for the total calibration. The system shall be allowed to stabilize for 3 minutes before the data acquisition is repeated.

3.4.2.5.2. The air flow rate at each test point shall be calculated in standard m3/min from the flow meter data using the manufacturer's prescribed method.

3.4.2.5.3. The air flow rate shall be subsequently converted to pump flow in m3/rev at absolute pump inlet temperature and pressure.

where:

is the pump flow rate at and ,m3/rev;

is the air flow at 101.325 kPa and 273.15 K (0 °C), m3/min;

is the pump inlet temperature, Kelvin (K);

is the absolute pump inlet pressure, kPa;

is the pump speed, min-1.

3.4.2.5.4. To compensate for the interaction of pump speed pressure variations at the pump and the pump slip rate, the correlation function between the pump speed , the pressure differential from pump inlet to pump outlet and the absolute pump outlet pressure shall be calculated using the following equation:

where:

is the correlation function;

is the pressure differential from pump inlet to pump outlet, kPa;

absolute outlet pressure , kPa.

A linear least squares fit shall be performed to generate the calibration equations having the following form:

where B and M are the slopes, and A and D0 are the intercepts of the lines.

3.4.2.6. A CVS system having multiple speeds shall be calibrated at each speed used. The calibration curves generated for the ranges shall be approximately parallel and the intercept values shall increase as the pump flow range decreases.

3.4.2.7. The calculated values from the equation shall be within 0.5 per cent of the measured value of . Values of will vary from one pump to another. A calibration shall be performed at initial installation and after major maintenance.

3.4.3. Calibration of a critical flow venturi (CFV)

3.4.3.1. Calibration of a CFV is based upon the flow equation for a critical venturi:

where:

is the flow, m³/min;

is the calibration coefficient;

is the absolute pressure, kPa;

is the absolute temperature, Kelvin (K).

Gas flow is a function of inlet pressure and temperature.

The calibration procedure described in paragraphs 3.4.3.2. to 3.4.3.3.3.4. inclusive of this annex establishes the value of the calibration coefficient at measured values of pressure, temperature and air flow.

3.4.3.2. Measurements for flow calibration of a critical flow venturi are required and the following data shall be within the limits of accuracy given:

Barometric pressure (corrected), ±0.03 kPa,

LFE air temperature, flow meter, ETI ±0.15 °C,

Pressure depression upstream of LFE, EPI ±0.01 kPa,

Pressure drop across LFE matrix, EDP ±0.0015 kPa,

Air flow, Qs ±0.5 per cent,

CFV inlet depression, PPI ±0.02 kPa,

Temperature at venturi inlet, ±0.2 °C.

3.4.3.3. The equipment shall be set up as shown in Figure A5/7 and checked for leaks. Any leaks between the flow-measuring device and the critical flow venturi will seriously affect the accuracy of the calibration and shall therefore be prevented.

# Figure A5/7

# **CFV calibration configuration**

Variable-flow restrictor

LFE

Thermometer

Filter

EDP

ETI

EPI

CFV

Tv

PPI

3.4.3.3.1. The variable-flow restrictor shall be set to the open position, the suction device shall be started and the system stabilized. Data from all instruments shall be collected.

3.4.3.3.2. The flow restrictor shall be varied and at least eight readings across the critical flow range of the venturi shall be made.

3.4.3.3.3. The data recorded during the calibration shall be used in the following calculation:

3.4.3.3.3.1. The air flow rate Qs at each test point shall be calculated from the flow meter data using the manufacturer's prescribed method.

Values of the calibration coefficient shall be calculated for each test point:

where:

is the flow rate, m3/min at 273.15 K (0 °C) and 101.325, kPa;

is the temperature at the venturi inlet, Kelvin (K);

is the absolute pressure at the venturi inlet, kPa.

3.4.3.3.3.2. shall be plotted as a function of venturi inlet pressure Pv. For sonic flow  will have a relatively constant value. As pressure decreases (vacuum increases), the venturi becomes unchoked and decreases. These values of shall not be used for further calculations.

3.4.3.3.3.3. For a minimum of eight points in the critical region, an arithmetic average and the standard deviation shall be calculated.

3.4.3.3.3.4. If the standard deviation exceeds 0.3 per cent of the arithmetic average , corrective action shall be taken.

3.4.4. Calibration of a subsonic venturi (SSV)

3.4.4.1. Calibration of the SSV is based upon the flow equation for a subsonic venturi. Gas flow is a function of inlet pressure and temperature, and the pressure drop between the SSV inlet and throat.

3.4.4.2. Data analysis

3.4.4.2.1. The airflow rate, , at each restriction setting (minimum 16 settings) shall be calculated in standard m3/s from the flow meter data using the manufacturer's prescribed method. The discharge coefficient shall be calculated from the calibration data for each setting using the following equation:

where:

QSSV is the airflow rate at standard conditions (101.325 kPa, 273.15 K (0 °C)), m3/s;

T is the temperature at the venturi inlet, Kelvin (K);

is the diameter of the SSV throat, m;

rp is the ratio of the SSV throat pressure to inlet absolute static pressure, ;

is the ratio of the SSV throat diameter dV to the inlet pipe inner diameter ;

is the discharge coefficient of the SSV;

is the absolute pressure at venturi inlet, kPa.

To determine the range of subsonic flow, shall be plotted as a function of Reynolds number at the SSV throat. The Reynolds number at the SSV throat shall be calculated using the following equation:

where:

is 25.55152 in SI, ;

is the airflow rate at standard conditions (101.325 kPa, 273.15 K (0 °C)), m3/s;

is the diameter of the SSV throat, m;

is the absolute or dynamic viscosity of the gas, kg/ms;

is (empirical constant), kg/ms K0.5;

is 110.4 (empirical constant), Kelvin (K).

3.4.4.2.2. Because QSSV is an input to the Re equation, the calculations shall be started with an initial estimate for QSSV or Cd of the calibration venturi, and repeated until QSSV converges. The convergence method shall be accurate to at least 0.1 per cent.

3.4.4.2.3. For a minimum of sixteen points in the region of subsonic flow, the calculated values of Cd from the resulting calibration curve fit equation shall be within ±0.5 per cent of the measured Cd for each calibration point.

3.4.5. Calibration of an ultrasonic flow meter (UFM)

3.4.5.1. The UFM shall be calibrated against a suitable reference flow meter.

3.4.5.2. The UFM shall be calibrated in the CVS configuration that will be used in the test cell (diluted exhaust piping, suction device) and checked for leaks. See Figure A5/8.

3.4.5.3. A heater shall be installed to condition the calibration flow in the event that the UFM system does not include a heat exchanger.

3.4.5.4. For each CVS flow setting that will be used, the calibration shall be performed at temperatures from room temperature to the maximum that will be experienced during vehicle testing.

3.4.5.5. The manufacturer's recommended procedure shall be followed for calibrating the electronic portions (temperature (T) and pressure (P) sensors) of the UFM.

3.4.5.6. Measurements for flow calibration of the ultrasonic flow meter are required and the following data (in the case that a laminar flow element is used) shall be found within the limits of accuracy given:

Barometric pressure (corrected), ±0.03 kPa,

LFE air temperature, flow meter, ETI ±0.15 °C,

Pressure depression upstream of LFE, EPI ±0.01 kPa,

Pressure drop across (EDP) LFE matrix ±0.0015 kPa,

Air flow, ±0.5 per cent,

UFM inlet depression, ±0.02 kPa,

Temperature at UFM inlet, ±0.2 °C.

3.4.5.7. Procedure

3.4.5.7.1. The equipment shall be set up as shown in Figure A5/8 and checked for leaks. Any leaks between the flow-measuring device and the UFM will seriously affect the accuracy of the calibration.

# Figure A5/8

# **UFM calibration configuration**

Calibration flow meter (LFE, SSV)

Heater

UFM

Suction device

Including the necessary temperature and pressure sensors

P

T

Flow valve

The flow rate through the UFM can be set and controlled by speed control of the flow and/or flow valve

3.4.5.7.2. The suction device shall be started. Its speed and/or the position of the flow valve shall be adjusted to provide the set flow for the validation and the system stabilised. Data from all instruments shall be collected.

3.4.5.7.3. For UFM systems without a heat exchanger, the heater shall be operated to increase the temperature of the calibration air, allowed to stabilise and data from all the instruments recorded. The temperature shall be increased in reasonable steps until the maximum diluted exhaust temperature expected during the emissions test is reached.

3.4.5.7.4. The heater shall be subsequently turned off and the suction device speed and/or flow valve shall be adjusted to the next flow setting that will be used for vehicle emissions testing after which the calibration sequence shall be repeated.

3.4.5.8. The data recorded during the calibration shall be used in the following calculations. The air flow rate Qs at each test point shall be calculated from the flow meter data using the manufacturer's prescribed method.

where:

is the air flow rate at standard conditions (101.325 kPa, 273.15 K (0 °C)), m3/s;

is the air flow rate of the calibration flow meter at standard conditions (101.325 kPa, 273.15 K (0 °C)), m3/s;

is the calibration coefficient.

For UFM systems without a heat exchanger, shall be plotted as a function of Tact.

The maximum variation in shall not exceed 0.3 per cent of the arithmetic average value of all the measurements taken at the different temperatures.

3.5. System verification procedure

3.5.1. General requirements

3.5.1.1. The total accuracy of the CVS sampling system and analytical system shall be determined by introducing a known mass of an emissions gas compound into the system whilst it is being operated under normal test conditions and subsequently analysing and calculating the emission gas compounds according to the equations of Annex B7. The CFO method described in paragraph 3.5.1.1.1. of this annex and the gravimetric method described in paragraph 3.5.1.1.2. of this annex are both known to give sufficient accuracy.

The maximum permissible deviation between the quantity of gas introduced and the quantity of gas measured is ±2 per cent.

3.5.1.1.1. Critical flow orifice (CFO) method

The CFO method meters a constant flow of pure gas (CO, CO2, or C3H8) using a critical flow orifice device.

A known mass of pure carbon monoxide, carbon dioxide or propane gas shall be introduced into the CVS system through the calibrated critical orifice. If the inlet pressure is high enough, the flow rate which is restricted by means of the critical flow orifice, is independent of orifice outlet pressure (critical flow). The CVS system shall be operated as in a normal exhaust emissions test and enough time shall be allowed for subsequent analysis. The gas collected in the sample bag shall be analysed by the usual equipment (see paragraph 4.1. of this annex) and the results compared to the concentration of the known gas samples. If deviations exceed ±2 per cent, the cause of the malfunction shall be determined and corrected.

3.5.1.1.2. Gravimetric method

The gravimetric method weighs a quantity of pure gas (CO, CO2, or C3H8).

The weight of a small cylinder filled with either pure carbon monoxide, carbon dioxide or propane shall be determined with a precision of ±0.01 g. The CVS system shall operate under normal exhaust emissions test conditions while the pure gas is injected into the system for a time sufficient for subsequent analysis. The quantity of pure gas involved shall be determined by means of differential weighing. The gas accumulated in the bag shall be analysed by means of the equipment normally used for exhaust gas analysis as described in paragraph 4.1. of this annex. The results shall be subsequently compared to the concentration figures computed previously. If deviations exceed ±2 per cent, the cause of the malfunction shall be determined and corrected.

4. Emissions measurement equipment

4.1. Gaseous emissions measurement equipment

4.1.1. System overview

4.1.1.1. A continuously proportional sample of the diluted exhaust gases and the dilution air shall be collected for analysis.

4.1.1.2. The mass of gaseous emissions shall be determined from the proportional sample concentrations and the total volume measured during the test. Sample concentrations shall be corrected to take into account the respective compound concentrations in dilution air.

4.1.2. Sampling system requirements

4.1.2.1. The sample of diluted exhaust gases shall be taken upstream from the suction device.

With the exception of paragraphs 4.1.3.1. (hydrocarbon sampling system), paragraph 4.2. (PM measurement equipment) and paragraph 4.3 (PN measurement equipment) of this annex, the dilute exhaust gas sample may be taken downstream of the conditioning devices (if any).

4.1.2.2. The bag sampling flow rate shall be set to provide sufficient volumes of dilution air and diluted exhaust in the CVS bags to allow concentration measurement and shall not exceed 0.3 per cent of the flow rate of the dilute exhaust gases, unless the diluted exhaust bag fill volume is added to the integrated CVS volume.

4.1.2.3. A sample of the dilution air shall be taken near the dilution air inlet (after the filter if one is fitted).

4.1.2.4. The dilution air sample shall not be contaminated by exhaust gases from the mixing area.

4.1.2.5. The sampling rate for the dilution air shall be comparable to that used for the dilute exhaust gases.

4.1.2.6. The materials used for the sampling operations shall be such as not to change the concentration of the emissions compounds.

4.1.2.7. Filters may be used in order to extract the solid particles from the sample.

4.1.2.8. Any valve used to direct the exhaust gases shall be of a quick-adjustment, quick-acting type.

4.1.2.9. Quick-fastening, gas-tight connections may be used between three-way valves and the sample bags, the connections sealing themselves automatically on the bag side. Other systems may be used for conveying the samples to the analyser (e.g. three-way stop valves).

4.1.2.10. Sample storage

4.1.2.10.1. The gas samples shall be collected in sample bags of sufficient capacity so as not to impede the sample flow.

4.1.2.10.2. The bag material shall be such as to affect neither the measurements themselves nor the chemical composition of the gas samples by more than ±2 per cent after 30 minutes (e.g., laminated polyethylene/polyamide films, or fluorinated polyhydrocarbons).

4.1.3. Sampling systems

4.1.3.1. Hydrocarbon sampling system (heated flame ionisation detector, HFID)

4.1.3.1.1. The hydrocarbon sampling system shall consist of a heated sampling probe, line, filter and pump. The sample shall be taken upstream of the heat exchanger (if fitted). The sampling probe shall be installed at the same distance from the exhaust gas inlet as the particulate sampling probe and in such a way that neither interferes with samples taken by the other. It shall have a minimum internal diameter of 4 mm.

4.1.3.1.2. All heated parts shall be maintained at a temperature of 190 °C ±10 °C by the heating system.

4.1.3.1.3. The arithmetic average concentration of the measured hydrocarbons shall be determined by integration of the second-by-second data divided by the phase or test duration.

4.1.3.1.4. The heated sampling line shall be fitted with a heated filter FH having a 99 per cent efficiency for particles ≥ 0.3 μm to extract any solid particles from the continuous flow of gas required for analysis.

4.1.3.1.5. The sampling system delay time (from the probe to the analyser inlet) shall be no more than 4 seconds.

4.1.3.1.6. The HFID shall be used with a constant mass flow (heat exchanger) system to ensure a representative sample, unless compensation for varying CVS volume flow is made.

4.1.4. Analysers

4.1.4.1. General requirements for gas analysis

4.1.4.1.1. The analysers shall have a measuring range compatible with the accuracy required to measure the concentrations of the exhaust gas sample compounds.

4.1.4.1.2. If not defined otherwise, measurement errors shall not exceed ±2 per cent (intrinsic error of analyser) disregarding the reference value for the calibration gases.

4.1.4.1.3. The ambient air sample shall be measured on the same analyser with the same range.

4.1.4.1.4. No gas drying device shall be used before the analysers unless it is shown to have no effect on the content of the compound in the gas stream.

4.1.4.2. Carbon monoxide (CO) and carbon dioxide (CO2) analysis

The analysers shall be of the non-dispersive infrared (NDIR) absorption type.

4.1.4.3. Hydrocarbons (HC) analysis for all fuels other than diesel fuel

The analyser shall be of the flame ionization (FID) type calibrated with propane gas expressed in equivalent carbon atoms (C1).

4.1.4.4. Hydrocarbons (HC) analysis for diesel fuel and optionally for other fuels

The analyser shall be of the heated flame ionization type with detector, valves, pipework, etc., heated to 190 °C ± 10 °C. It shall be calibrated with propane gas expressed equivalent to carbon atoms (C1).

4.1.4.5. Methane (CH4) analysis

The analyser shall be either a gas chromatograph combined with a flame ionization detector (FID), or a flame ionization detector (FID) combined with a non-methane cutter (NMC-FID), calibrated with methane or propane gas expressed equivalent to carbon atoms (C1).

4.1.4.6. Nitrogen oxides (NOx) analysis

The analysers shall be of chemiluminescent (CLA) or non-dispersive ultra-violet resonance absorption (NDUV) types.

4.1.4.7. (Reserved)

4.1.4.8. (Reserved)

4.1.4.9. (Reserved)

4.1.4.10. (Reserved)

4.1.4.11. Hydrogen (H2) analysis (if applicable)

The analyser shall be of the sector field mass spectrometry type, calibrated with hydrogen.

4.1.4.12. Water (H2O) analysis (if applicable)

The analyser shall be of the non-dispersive infrared analyzer (NDIR) absorption type. The NDIR shall be calibrated either with water vapour or with propylene (C3H6). If the NDIR is calibrated with water vapour, it shall be ensured that no water condensation can occur in tubes and connections during the calibration process. If the NDIR is calibrated with propylene, the manufacturer of the analyzer shall provide the information for converting the concentration of propylene to its corresponding concentration of water vapour. The values for conversion shall be periodically checked by the manufacturer of the analyzer, and at least once per year.

4.1.5. Recommended system descriptions

4.1.5.1. Figure A5/9 is a schematic drawing of the gaseous emissions sampling system.

# Figure A5/9

# **Full flow exhaust dilution system schematic**

Dilution airfilters

Dilution air sample to:

- CVS bags

- PM sampling (optional)

- other devices

Vehicle exhaust

Dilution tunnel

HFID

Heat exchanger

(optional)

Vent

- CVS bag sampling

- other sampling systems

MC

Flow meter and suction device

Mixing device

Dilution air

PN

PDP, CFV, SSV, UFM

- continuous diluted exhaust analysers

- other sampling systems

- CVS bag sample (optional)

PM

4.1.5.2. Examples of system components are as listed below.

4.1.5.2.1. Two sampling probes for continuous sampling of the dilution air and of the diluted exhaust gas/air mixture.

4.1.5.2.2. A filter to extract solid particles from the flows of gas collected for analysis.

4.1.5.2.3. Pumps and flow controller to ensure constant uniform flow of diluted exhaust gas and dilution air samples taken during the course of the test from sampling probes and flow of the gas samples shall be such that, at the end of each test, the quantity of the samples is sufficient for analysis.

4.1.5.2.4. Quick-acting valves to divert a constant flow of gas samples into the sample bags or to the outside vent.

4.1.5.2.5. Gas-tight, quick-lock coupling elements between the quick-acting valves and the sample bags. The coupling shall close automatically on the sampling bag side. As an alternative, other methods of transporting the samples to the analyser may be used (three-way stopcocks, for instance).

4.1.5.2.6. Bags for collecting samples of the diluted exhaust gas and of the dilution air during the test.

4.1.5.2.7. A sampling critical flow venturi to take proportional samples of the diluted exhaust gas (CFV-CVS only).

4.1.5.3. Additional components required for hydrocarbon sampling using a heated flame ionization detector (HFID) as shown in Figure A5/10.

4.1.5.3.1. Heated sample probe in the dilution tunnel located in the same vertical plane as the particulate and, if applicable, particle sample probes.

4.1.5.3.2. Heated filter located after the sampling point and before the HFID.


4.1.5.3.3. Heated selection valves between the zero/calibration gas supplies and the HFID.

4.1.5.3.4. Means of integrating and recording instantaneous hydrocarbon concentrations.

4.1.5.3.5. Heated sampling lines and heated components from the heated probe to the HFID.

Figure A5/10

**Components required for hydrocarbon sampling using an HFID**



4.2. PM measurement equipment

4.2.1. Specification


4.2.1.1. System overview

4.2.1.1.1. The particulate sampling unit shall consist of a sampling probe (PSP), located in the dilution tunnel, a particle transfer tube (PTT), a filter holder(s) (FH), pump(s), flow rate regulators and measuring units. See Figures A5/11, A5/12 and A5/13.

4.2.1.1.2. A particle size pre-classifier (PCF), (e.g. cyclone or impactor) may be used. In such case, it is recommended that it be employed upstream of the filter holder.

# Figure A5/11

**Alternative particulate sampling probe configuration**



4.2.1.2. General requirements

4.2.1.2.1. The sampling probe for the test gas flow for particulate shall be arranged within the dilution tunnel so that a representative sample gas flow can be taken from the homogeneous air/exhaust mixture and shall be upstream of a heat exchanger (if any).

4.2.1.2.2. The particulate sample flow rate shall be proportional to the total mass flow of diluted exhaust gas in the dilution tunnel to within a tolerance of ±5 per cent of the particulate sample flow rate. The verification of the proportionality of the particulate sampling shall be made during the commissioning of the system and as required by the responsible authority.

4.2.1.2.3. The sampled dilute exhaust gas shall be maintained at a temperature above 20 °C and below 52 °C within 20 cm upstream or downstream of the particulate sampling filter face. Heating or insulation of components of the particulate sampling system to achieve this is permitted.

In the event that the 52 °C limit is exceeded during a test where periodic regeneration event does not occur, the CVS flow rate shall be increased or double dilution shall be applied (assuming that the CVS flow rate is already sufficient so as not to cause condensation within the CVS, sample bags or analytical system).

4.2.1.2.4. The particulate sample shall be collected on a single filter mounted within a holder in the sampled dilute exhaust gas flow.

4.2.1.2.5. All parts of the dilution system and the sampling system from the exhaust pipe up to the filter holder that are in contact with raw and diluted exhaust gas shall be designed to minimise deposition or alteration of the particulate. All parts shall be made of electrically conductive materials that do not react with exhaust gas components, and shall be electrically grounded to prevent electrostatic effects.

4.2.1.2.6. If it is not possible to compensate for variations in the flow rate, provision shall be made for a heat exchanger and a temperature control device as specified in paragraphs 3.3.5.1. or 3.3.6.4.2. of this annex, so as to ensure that the flow rate in the system is constant and the sampling rate accordingly proportional.

4.2.1.2.7. Temperatures required for the measurement of PM shall be measured with an accuracy of ±1 °C and a response time () of 15 seconds or less.

4.2.1.2.8. The sample flow from the dilution tunnel shall be measured with an accuracy of ±2.5 per cent of reading or ±1.5 per cent full scale, whichever is the least.

The accuracy specified above of the sample flow from the CVS tunnel is also applicable where double dilution is used. Consequently, the measurement and control of the secondary dilution air flow and diluted exhaust flow rates through the filter shall be of a higher accuracy.

4.2.1.2.9. All data channels required for the measurement of PM shall be logged at a frequency of 1 Hz or faster. Typically, these would include:

(a) Diluted exhaust temperature at the particulate sampling filter;

(b) Sampling flow rate;

(c) Secondary dilution air flow rate (if secondary dilution is used);

(d) Secondary dilution air temperature (if secondary dilution is used).

4.2.1.2.10. For double dilution systems, the accuracy of the diluted exhaust transferred from the dilution tunnel Vep defined in paragraph 3.3.2. of Annex B7 in the equation is not measured directly but determined by differential flow measurement.

The accuracy of the flow meters used for the measurement and control of the double diluted exhaust passing through the particulate sampling filters and for the measurement/control of secondary dilution air shall be sufficient so that the differential volume Vep shall meet the accuracy and proportional sampling requirements specified for single dilution.

The requirement that no condensation of the exhaust gas occur in the CVS dilution tunnel, diluted exhaust flow rate measurement system, CVS bag collection or analysis systems shall also apply in the case that double dilution systems are used.

4.2.1.2.11. Each flow meter used in a particulate sampling and double dilution system shall be subjected to a linearity verification as required by the instrument manufacturer.

Figure A5/12

**Particulate sampling system**





Figure A5/13

**Double dilution particulate sampling system**



4.2.1.3. Specific requirements

4.2.1.3.1. Sample probe

4.2.1.3.1.1. The sample probe shall deliver the particle size classification performance specified in paragraph 4.2.1.3.1.4. of this annex. It is recommended that this performance be achieved by the use of a sharp-edged, open-ended probe facing directly into the direction of flow plus a pre-classifier (cyclone impactor, etc.). An appropriate sample probe, such as that indicated in Figure A5/11, may alternatively be used provided it achieves the pre-classification performance specified in paragraph 4.2.1.3.1.4. of this annex.

4.2.1.3.1.2. The sample probe shall be installed at least 10 tunnel diameters downstream of the exhaust gas inlet to the tunnel and have an internal diameter of at least 8 mm.

If more than one simultaneous sample is drawn from a single sample probe, the flow drawn from that probe shall be split into identical sub-flows to avoid sampling artefacts.

If multiple probes are used, each probe shall be sharp-edged, open-ended and facing directly into the direction of flow. Probes shall be equally spaced around the central longitudinal axis of the dilution tunnel, with a spacing between probes of at least 5 cm.

4.2.1.3.1.3. The distance from the sampling tip to the filter mount shall be at least five probe diameters, but shall not exceed 2,000 mm.

4.2.1.3.1.4. The pre-classifier (e.g. cyclone, impactor, etc.) shall be located upstream of the filter holder assembly. The pre-classifier 50 per cent cut point particle diameter shall be between 2.5 μm and 10 μm at the volumetric flow rate selected for sampling PM. The pre-classifier shall allow at least 99 per cent of the mass concentration of 1 μm particles entering the pre-classifier to pass through the exit of the pre-classifier at the volumetric flow rate selected for sampling PM.

4.2.1.3.2. Particle transfer tube (PTT)

Any bends in the PTT shall be smooth and have the largest possible radii.

4.2.1.3.3. Secondary dilution

4.2.1.3.3.1. As an option, the sample extracted from the CVS for the purpose of PM measurement may be diluted at a second stage, subject to the following requirements:

4.2.1.3.3.1.1. Secondary dilution air shall be filtered through a medium capable of reducing particles in the most penetrating particle size of the filter material by ≥ 99.95 per cent, or through a HEPA filter of at least Class H13 of EN 1822:2019. The dilution air may optionally be charcoal-scrubbed before being passed to the HEPA filter. It is recommended that an additional coarse particle filter be situated before the HEPA filter and after the charcoal scrubber, if used.

4.2.1.3.3.1.2. The secondary dilution air should be injected into the PTT as close to the outlet of the diluted exhaust from the dilution tunnel as possible.

4.2.1.3.3.1.3. The residence time from the point of secondary diluted air injection to the filter face shall be at least 0.25 seconds, but no longer than 5 seconds.

4.2.1.3.3.1.4. If the double diluted sample is returned to the CVS, the location of the sample return shall be selected so that it does not interfere with the extraction of other samples from the CVS.

4.2.1.3.4. Sample pump and flow meter

4.2.1.3.4.1. The sample gas flow measurement unit shall consist of pumps, gas flow regulators and flow measuring units.

4.2.1.3.4.2. The temperature of the gas flow in the flow meter may not fluctuate by more than ±3 °C except:

(a) When the sampling flow meter has real time monitoring and flow control operating at a frequency of 1 Hz or faster;

(b) During regeneration tests on vehicles equipped with periodically regenerating after-treatment devices.

Should the volume of flow change unacceptably as a result of excessive filter loading, the test shall be invalidated. When it is repeated, the flow rate shall be decreased.

4.2.1.3.5. Filter and filter holder

4.2.1.3.5.1. A valve shall be located downstream of the filter in the direction of flow. The valve shall open and close within 1 second of the start and end of test.

4.2.1.3.5.2. For a given test, the gas filter face velocity shall be set to an initial value within the range 20 cm/s to 105 cm/s and shall be set at the start of the test so that 105 cm/s will not be exceeded when the dilution system is being operated with sampling flow proportional to CVS flow rate.

4.2.1.3.5.3. Fluorocarbon coated glass fibre filters or fluorocarbon membrane filters shall be used.

All filter types shall have a 0.3 μm DOP (di-octylphthalate) or PAO (poly-alpha-olefin) CS 68649-12-7 or CS 68037-01-4 collection efficiency of at least 99 per cent at a gas filter face velocity of 5.33 cm/s measured according to one of the following standards:

(a) U.S.A. Department of Defense Test Method Standard, MIL-STD-282 method 102.8: DOP-Smoke Penetration of Aerosol-Filter Element;

(b) U.S.A. Department of Defense Test Method Standard, MIL-STD-282 method 502.1.1: DOP-Smoke Penetration of Gas-Mask Canisters;

(c) Institute of Environmental Sciences and Technology, IEST-RP-CC021: Testing HEPA and ULPA Filter Media.

4.2.1.3.5.4. The filter holder assembly shall be of a design that provides an even flow distribution across the filter stain area. The filter shall be round and have a stain area of at least 1,075 mm2.

4.2.2. Weighing chamber (or room) and analytical balance specifications

4.2.2.1. Weighing chamber (or room) conditions

(a) The temperature of the weighing chamber (or room) in which the particulate sampling filters are conditioned and weighed shall be maintained to within 22 °C ±2 °C (22 °C ±1 °C if possible) during all filter conditioning and weighing;

(b) Humidity shall be maintained at a dew point of less than 10.5 °C and a relative humidity of 45 per cent ±8 per cent;

(c) Limited deviations from weighing chamber (or room) temperature and humidity specifications shall be permitted provided their total duration does not exceed 30 minutes in any one filter conditioning period;

(d) The levels of ambient contaminants in the weighing chamber (or room) environment that would settle on the particulate sampling filters during their stabilisation shall be minimised;

(e) During the weighing operation no deviations from the specified conditions are permitted.

4.2.2.2. Linear response of an analytical balance

The analytical balance used to determine the filter weight shall meet the linearity verification criteria of Table A5/1 applying a linear regression. This implies a precision of at least ±2 µg and a resolution of at least 1 µg (1 digit = 1 µg). At least 4 equally-spaced reference weights shall be tested. The zero value shall be within ±1 µg.

Table A5/1

**Analytical balance verification criteria**

| *Measurement system* | *Intercept a0* | *Slope a1* | *Standard error of estimate ( SEE)* | *Coefficient of determination r2* |
| --- | --- | --- | --- | --- |
| Particulate balance | ≤ 0.1 mg | 0.99 – 1.01 | ≤ 1 per cent max | ≥ 0.998 |

4.2.2.3. Elimination of static electricity effects

**The effects of static electricity shall be nullified. This may be achieved by grounding the balance through placement upon an antistatic mat and neutralisation of the particulate sampling filters prior to weighing using a polonium neutraliser or a device of similar effect. Alternatively, nullification of static effects may be achieved through equalization of the static charge.**

4.2.2.4. Buoyancy correction

The sample and reference filter weights shall be corrected for their buoyancy in air. The **buoyancy correction is a function of sampling filter density, air density and the density of the balance calibration** weight, and does not account for the buoyancy of the particulate matter itself.

If the density of the filter material is not known, the following densities shall be used:

(a) PTFE coated glass fibre filter: 2,300 kg/m3;

(b) PTFE membrane filter: 2,144 kg/m3;

(c) PTFE membrane filter with polymethylpentene support ring: 920 kg/m3.

For stainless steel calibration weights, a density of 8,000 kg/m³ shall be used. If the material of the calibration weight is different, its density shall be known and be used. International Recommendation OIML R 111-1 Edition 2004(E) (or equivalent) from International Organization of Legal Metrology on calibration weights should be followed.

The following equation shall be used:

where:

is the corrected particulate sample mass, mg;

is the uncorrected particulate sample mass, mg;

is the density of the air, kg/m3;

is the density of balance calibration weight, kg/m3;

is the density of the particulate sampling filter, kg/m3.

The density of the air shall be calculated using the following equation:

is the total atmospheric pressure, kPa;

is the air temperature in the balance environment, Kelvin (K);

is the molar mass of air in a balanced environment, 28.836 g mol-1;

R is the molar gas constant, 8.3144 J mol-1 K-1.

4.3. PN measurement equipment (if PN measurement is required)

4.3.1. Specification

4.3.1.1. System overview

4.3.1.1.1. The particle sampling system shall consist of a probe or sampling point extracting a sample from a homogenously mixed flow in a dilution system, a volatile particle remover (VPR) upstream of a particle number counter (PNC) and suitable transfer tubing. See Figure A5/14.

4.3.1.1.2. It is recommended that a particle size pre-classifier (PCF) (e.g. cyclone, impactor, etc.) be located prior to the inlet of the VPR. The PCF 50 per cent cut point particle diameter shall be between 2.5 µm and 10 µm at the volumetric flow rate selected for particle sampling. The PCF shall allow at least 99 per cent of the mass concentration of 1 µm particles entering the PCF to pass through the exit of the PCF at the volumetric flow rate selected for particle sampling.

A sample probe acting as an appropriate size-classification device, such as that shown in Figure A5/11, is an acceptable alternative to the use of a PCF.

4.3.1.2. General requirements

4.3.1.2.1. The particle sampling point shall be located within a dilution system. In the case that a double dilution system is used, the particle sampling point shall be located within the primary dilution system.

4.3.1.2.1.1. The sampling probe tip or PSP, and the PTT, together comprise the particle transfer system (PTS). The PTS conducts the sample from the dilution tunnel to the entrance of the VPR. The PTS shall meet the following conditions:

(a) The sampling probe shall be installed at least 10 tunnel diameters downstream of the exhaust gas inlet, facing upstream into the tunnel gas flow with its axis at the tip parallel to that of the dilution tunnel;

(b) The sampling probe shall be upstream of any conditioning device (e.g. heat exchanger);

(c) The sampling probe shall be positioned within the dilution tunnel so that the sample is taken from a homogeneous diluent/exhaust mixture.

4.3.1.2.1.2. Sample gas drawn through the PTS shall meet the following conditions:

(a) In the case that a full flow exhaust dilution system, is used it shall have a flow Reynolds number Re lower than 1,700;

(b) In the case that a double dilution system is used, it shall have a flow Reynolds number Re lower than 1,700 in the PTT i.e. downstream of the sampling probe or point;

(c) Shall have a residence time ≤ 3 seconds.

4.3.1.2.1.3. Any other sampling configuration for the PTS for which equivalent solid particle penetration at 30 nm can be demonstrated shall be considered acceptable.

4.3.1.2.1.4. The outlet tube (OT), conducting the diluted sample from the VPR to the inlet of the PNC, shall have the following properties:

(a) An internal diameter ≥ 4mm;

(b) A sample gas flow residence time of ≤ 0.8 seconds.

4.3.1.2.1.5. Any other sampling configuration for the OT for which equivalent solid particle penetration at 30 nm can be demonstrated shall be considered acceptable.

4.3.1.2.2. The VPR shall include devices for sample dilution and for volatile particle removal.

4.3.1.2.3. All parts of the dilution system and the sampling system from the exhaust pipe up to the PNC, which are in contact with raw and diluted exhaust gas, shall be made of electrically conductive materials , shall be electrically grounded to prevent electrostatic effects and shall be designed to minimize deposition of the particles.

4.3.1.2.4. The particle sampling system shall incorporate good aerosol sampling practice that includes the avoidance of sharp bends and abrupt changes in cross-section, the use of smooth internal surfaces and the minimization of the length of the sampling line. Gradual changes in the cross-section are permitted.

4.3.1.3. Specific requirements

4.3.1.3.1. The particle sample shall not pass through a pump before passing through the PNC.

4.3.1.3.2. A sample pre-classifier is recommended.

4.3.1.3.3. The VPR shall:

1. Be capable of diluting the sample in one or more stages to achieve a particle number concentration below the upper threshold of the single particle count mode of the PNC;
2. Have a gas temperature at the inlet to the PNC below the maximum allowed inlet temperature specified by the PNC manufacturer;
3. Include an initial heated dilution stage that outputs a sample at a temperature of ≥ 150 °C and ≤ 350 °C ±10 °C, and dilutes by a factor of at least 10;
4. Control heated stages to constant nominal operating temperatures, within the range ≥ 150 °C and ≤ 400 °C ±10 °C;
5. Provide an indication of whether or not heated stages are at their correct operating temperatures;
6. Achieve a solid particle penetration efficiency of at least 70 per cent for particles of 100 nm electrical mobility diameter;
7. Achieve a particle concentration reduction factor for particles of 30 nm and 50 nm electrical mobility diameters that is no more than 30 per cent and 20 per cent respectively higher, and no more than 5 per cent lower than that for particles of 100 nm electrical mobility diameter for the VPR as a whole;

The particle concentration reduction factor at each particle size shall be calculated using the following equation:

where:

is the upstream particle number concentration for particles of diameter ;

is the downstream particle number concentration for particles of diameter ;

is the particle electrical mobility diameter (30, 50 or 100 nm).

and shall be corrected to the same conditions.

The arithmetic average particle concentration reduction factor at a given dilution setting shall be calculated using the following equation:

It is recommended that the VPR is calibrated and validated as a complete unit;

1. Be designed according to good engineering practice to ensure particle concentration reduction factors are stable across a test;
2. Achieve more than 99.0 per cent vaporization of 30 nm tetracontane (CH3(CH2)38CH3) particles, with an inlet concentration of ≥ 10,000 per cm³, by means of heating and reduction of partial pressures of the tetracontane.

4.3.1.3.3.1. The solid particle penetration at a particle size, , shall be calculated using the following equation:

Where

is the upstream particle number concentration for particles of diameter ;

is the downstream particle number concentration for particles of diameter ;

is the particle electrical mobility diameter

DF is the dilution factor between measurement positions of and determined either with trace gases, or flow measurements.

4.3.1.3.4. The PNC shall:

1. Operate under full flow operating conditions;
2. Have a counting accuracy of ±10 per cent across the range 1 per cm³ to the upper threshold of the single particle count mode of the PNC against a suitable traceable standard. At concentrations below 100 per cm³, measurements averaged over extended sampling periods may be required to demonstrate the accuracy of the PNC with a high degree of statistical confidence;
3. Have a resolution of at least 0.1 particles per cm³ at concentrations below 100 per cm³;
4. Operate under single counting mode only and have a linear response to particle number concentrations within the instrument’s specified measurement range;
5. Have a data reporting frequency equal to or greater than a frequency of 0.5 Hz;
6. Have a t90 response time over the measured concentration range of less than 5 seconds;
7. Introduce a correction with a calibration factor as determined in paragraph 5.7.1.3. of this annex;
8. Have counting efficiencies at the different particle sizes as specified in Table A5/2.
9. The PNC calibration factor from the linearity calibration against a traceable reference shall be applied to determine PNC counting efficiency. The counting efficiency shall be reported including the calibration factor from linearity calibration against a traceable reference.
10. If the PNC applies some other working liquid besides n-butyl alcohol or isopropyl alcohol, the counting efficiency of the PNC shall be demonstrated with 4cSt polyalphaolefin and soot-like particles.

Table A5/2

**PNC counting efficiency**

| *Nominal particle electrical mobility diameter (nm)* | *PNC counting efficiency (per cent)* |
| --- | --- |
| 23 | 50 ±12 |
| 41 | > 90 |

4.3.1.3.5. If the PNC makes use of a working liquid, it shall be replaced at the frequency specified by the instrument manufacturer.

4.3.1.3.6. Where not held at a known constant level at the point at which PNC flow rate is controlled, the pressure and/or temperature at the PNC inlet shall be measured for the purposes of correcting particle number concentration measurements to standard conditions. The standard conditions are 101.325 kPa pressure and 0 °C temperature.

4.3.1.3.7. The sum of the residence time of the PTS, VPR and OT plus the t90 response time of the PNC shall be no greater than 20 seconds.

4.3.1.4. Recommended system description

The following paragraph contains the recommended practice for measurement of PN. However, systems meeting the performance specifications in paragraphs 4.3.1.2. and 4.3.1.3. of this annex are acceptable. See Figure A5/14.

Figure A5/14

**A recommended particle sampling system**



OT

The evaporation tube, ET, may be catalytically active with a wall temperature of 350 °C (±10 °C).

5. Calibration intervals and procedures

5.1. Calibration intervals

All instruments in Table A5/3 shall be calibrated at/after major maintenance intervals.

Table A5/3

**Instrument calibration intervals**

|  |  |  |
| --- | --- | --- |
| *Instrument checks* | *Interval* | *Criterion* |
| Gas analyser linearization (calibration) | Every 6 months | ±2 per cent of reading |
| Mid-span | Every 6 months | ±2 per cent |
| CO NDIR:  CO2/H2O interference | Monthly | -1 to 3 ppm |
| NOx converter check | Monthly | > 95 per cent |
| CH4 cutter check | Yearly | 98 per cent of ethane |
| FID CH4 response | Yearly | See paragraph 5.4.3. of this annex. |
| FID air/fuel flow | At major maintenance | According to the instrument manufacturer. |
| NO/NO2 NDUV:  H2O, HC interference | At major maintenance | According to the instrument manufacturer. |
| Laser infrared spectrometers (modulated high resolution narrow band infrared analysers): interference check | Yearly | According to the instrument manufacturer. |
| QCL | Yearly | According to the instrument manufacturer. |
| GC methods | See paragraph 7.2. of this annex. | See paragraph 7.2. of this annex. |
| LC methods | Yearly | According to the instrument manufacturer. |
| Photoacoustics | Yearly | According to the instrument manufacturer. |
| FTIR: linearity verification | Within 370 days before testing | See paragraph 7.1. of this annex. |
| Microgram balance linearity | Yearly | See paragraph 4.2.2.2. of this annex. |
| PNC (particle number counter) (if applicable) | See paragraph 5.7.1.1. of this annex | See paragraph 5.7.1.3. of this annex. |
| VPR (volatile particle remover) | See paragraph 5.7.2.1. of this annex. | See paragraph 5.7.2. of this annex. |

Table A5/4

**Constant volume sampler (CVS) calibration intervals**

| *CVS* | *Interval* | *Criterion* |
| --- | --- | --- |
| CVS flow | After overhaul | ±2 per cent |
| Temperature sensor | Yearly | ±1 °C |
| Pressure sensor | Yearly | ±0.4 kPa |
| Injection check | Monthly | ±2 per cent |

Table A5/5

**Environmental data calibration intervals**

| *Climate* | *Interval* | *Criterion* |
| --- | --- | --- |
| Temperature | Yearly | ±1 °C |
| Moisture dew | Yearly | ±5 per cent RH |
| Ambient pressure | Yearly | ±0.4 kPa |
| Cooling fan | After overhaul | According to paragraph 1.1.1. of this annex. |

5.2. Analyser calibration procedures

5.2.1. Each analyser shall be calibrated as specified by the instrument manufacturer or at least as often as specified in Table A5/3.

5.2.2. Each normally used operating range shall be linearized by the following procedure:

5.2.2.1. The analyser linearization curve shall be established by at least five calibration points spaced as uniformly as possible. The nominal concentration of the calibration gas of the highest concentration shall be not less than 80 per cent of the full scale.

5.2.2.2. The calibration gas concentration required may be obtained by means of a gas divider, diluting with purified N2 or with purified synthetic air.

5.2.2.3. The linearization curve shall be calculated by the least squares method. If the resulting polynomial degree is greater than 3, the number of calibration points shall be at least equal to this polynomial degree plus 2.

5.2.2.4. The linearization curve shall not differ by more than ±2 per cent from the nominal value of each calibration gas.

5.2.2.5. From the trace of the linearization curve and the linearization points it is possible to verify that the calibration has been carried out correctly. The different characteristic parameters of the analyser shall be indicated, particularly:

(a) Analyser and gas component;

(b) Range;

(c) Date of linearisation.

5.2.2.6. If the responsible authority is satisfied that alternative technologies (e.g. computer, electronically controlled range switch, etc.) give equivalent accuracy, these alternatives may be used.

5.3. Analyser zero and calibration verification procedure

5.3.1. Each normally used operating range shall be checked prior to each analysis in accordance with paragraphs 5.3.1.1. and 5.3.1.2. of this annex

5.3.1.1. The calibration shall be checked by use of a zero gas and by use of a calibration gas according to paragraph 2.14.2.3. of Annex B6.

5.3.1.2. After testing, zero gas and the same calibration gas shall be used for re-checking according to paragraph 2.14.2.4. of Annex B6.

5.4. FID hydrocarbon response check procedure

5.4.1. Detector response optimization

The FID shall be adjusted as specified by the instrument manufacturer. Propane in air shall be used on the most common operating range.

5.4.2. Calibration of the HC analyser

5.4.2.1. The analyser shall be calibrated using propane in air and purified synthetic air.

5.4.2.2. A calibration curve as described in paragraph 5.2.2. of this annex shall be established.

5.4.3. Response factors of different hydrocarbons and recommended limits

5.4.3.1. The response factor, Rf, for a particular hydrocarbon compound is the ratio of the FID C1 reading to the gas cylinder concentration, expressed as ppm C1.

The concentration of the test gas shall be at a level to give a response of approximately 80 per cent of full-scale deflection for the operating range. The concentration shall be known to an accuracy of ±2 per cent in reference to a gravimetric standard expressed in volume. In addition, the gas cylinder shall be preconditioned for 24 hours at a temperature between 20 and 30 °C.

5.4.3.2. The methane factor RfCH4 shall be measured and determined when introducing an analyser into service, and yearly thereafter or after major maintenance intervals, whichever comes first.

The propylene response factor RfC3H6 and the toluene response factor RfC7H8 shall be measured when introducing an analyser into service. It is recommended that they be measured at or after major maintenance which might possibly affect the response factors.

The test gases to be used and the recommended response factors are:

Methane and purified air:

or 1.00 < Rf < 1.05 for NG/biomethane fuelled vehicles

Propylene and purified air:

Toluene and purified air:

The factors are relative to an of 1.00 for propane and purified air.

5.5. NOx converter efficiency test procedure

5.5.1. Using the test set up as shown in Figure A5/15 and the procedure described below, the efficiency of converters for the conversion of NO2 into NO shall be tested by means of an ozonator as follows:

5.5.1.1. The analyser shall be calibrated in the most common operating range following the manufacturer's specifications using zero and calibration gas (the NO content of which shall amount to approximately 80 per cent of the operating range and the NO2 concentration of the gas mixture shall be less than 5 per cent of the NO concentration). The NOx analyser shall be in the NO mode so that the calibration gas does not pass through the converter. The indicated concentration shall be recorded.

5.5.1.2. Via a T-fitting, oxygen or synthetic air shall be added continuously to the calibration gas flow until the concentration indicated is approximately 10 per cent less than the indicated calibration concentration given in paragraph 5.5.1.1. of this annex. The indicated concentration (c) shall be recorded. The ozonator shall be kept deactivated throughout this process.


5.5.1.3. The ozonator shall now be activated to generate enough ozone to bring the NO concentration down to 20 per cent (minimum 10 per cent) of the calibration concentration given in paragraph 5.5.1.1. of this annex. The indicated concentration (d) shall be recorded.

5.5.1.4. The NOx analyser shall be subsequently switched to the NOx mode, whereby the gas mixture (consisting of NO, NO2, O2 and N2) now passes through the converter. The indicated concentration (a) shall be recorded.

5.5.1.5. The ozonator shall now be deactivated. The mixture of gases described in paragraph 5.5.1.2. of this annex shall pass through the converter into the detector. The indicated concentration (b) shall be recorded.

Figure A5/15

**NOx converter efficiency test configuration**



5.5.1.6. With the ozonator deactivated, the flow of oxygen or synthetic air shall be shut off. The NO2 reading of the analyser shall then be no more than 5 per cent above the figure given in paragraph 5.5.1.1. of this annex.

5.5.1.7. The per cent efficiency of the NOx converter shall be calculated using the concentrations a, b, c and d determined in paragraphs 5.5.1.2. to 5.5.1.5. inclusive of this annex using the following equation:

The efficiency of the converter shall not be less than 95 per cent. The efficiency of the converter shall be tested in the frequency defined in Table A5/3.

5.6. Calibration of the microgram balance

The calibration of the microgram balance used for particulate sampling filter weighing shall be traceable to a national or international standard. The balance shall comply with the linearity requirements given in paragraph 4.2.2.2. of this annex. The linearity verification shall be performed at least every 12 months or whenever a system repair or change is made that could influence the calibration.

5.7. Calibration and validation of the particle sampling system (if PN measurement is required)

Examples of calibration/validation methods are available at: <http://www.unece.org/trans/main/wp29/wp29wgs/wp29grpe/pmpFCP.html>

5.7.1. Calibration of the PNC

5.7.1.1. The responsible authority shall ensure the existence of a calibration certificate for the PNC demonstrating compliance with a traceable standard within a 13-month period prior to the emissions test. Between calibrations either the counting efficiency of the PNC shall be monitored for deterioration or the PNC wick shall be routinely changed every 6 months if recommended by the instrument manufacturer. See Figures A5/16 and A5/17. PNC counting efficiency may be monitored against a reference PNC or against at least two other measurement PNCs. If the PNC reports particle number concentrations within ±10 per cent of the arithmetic average of the concentrations from the reference PNC, or a group of two or more PNCs, the PNC shall subsequently be considered stable, otherwise maintenance of the PNC is required. Where the PNC is monitored against two or more other measurement PNCs, it is permitted to use a reference vehicle running sequentially in different test cells each with its own PNC.

# Figure A5/16

# **Nominal PNC annual sequence**





Figure A5/17

**Extended PNC annual sequence (in the case that a full PNC calibration is delayed)**



5.7.1.2. The PNC shall also be recalibrated and a new calibration certificate issued following any major maintenance.

5.7.1.3. Calibration shall be undertaken according to ISO 27891:2015 and shall be traceable to a national or international standard by comparing the response of the PNC under calibration with that of:

(a) A calibrated aerosol electrometer when simultaneously sampling electrostatically classified calibration particles; or

(b) A second full flow PNC with counting efficiency above 90 per cent for 23 nm equivalent electrical mobility diameter particles that has been calibrated by the method described above. The second PNC counting efficiency shall be taken into account in the calibration.

5.7.1.3.1. For the requirements of paragraphs 5.7.1.3.(a) and 5.7.1.3.(b), calibration shall be undertaken using at least six standard concentrations across the PNC’s measurement range. These standard concentrations shall be as uniformly spaced as possible between the standard concentration of 2.000 particles per cm³ or below and the maximum of the PNC’s range in single particle count mode.

5.7.1.3.2. For the requirements of paragraphs 5.7.1.3.(a) and 5.7.1.3.(b), the selected points shall include a nominal zero concentration point produced by attaching HEPA filters of at least Class H13 of EN 1822:2019, or equivalent performance, to the inlet of each instrument. The gradient from a linear least squares regression of the two data sets shall be calculated and recorded. A calibration factor equal to the reciprocal of the gradient shall be applied to the PNC under calibration. Linearity of response is calculated as the square of the Pearson product moment correlation coefficient (r) of the two data sets and shall be equal to or greater than 0.97. In calculating both the gradient and r2, the linear regression shall be forced through the origin (zero concentration on both instruments). The calibration factor shall be between 0.9 and 1.1. Each concentration measured with the PNC under calibration, shall be within ±5 per cent of the measured reference concentration multiplied with the gradient, with the exception of the zero point.

5.7.1.4. Calibration shall also include a check, according to the requirements of paragraph 4.3.1.3.4.(h) of this annex, on the PNC’s counting efficiency with particles of 23 nm electrical mobility diameter. A check of the counting efficiency with 41 nm particles is not required during periodical calibration.

5.7.2. Calibration/validation of the VPR

5.7.2.1. Calibration of the VPR’s particle concentration reduction factors across its full range of dilution settings, at the instrument’s fixed nominal operating temperatures, shall be required when the unit is new and following any major maintenance. The periodic validation requirement for the VPR’s particle concentration reduction factor is limited to a check at a single setting, typical of that used for measurement on particulate filter-equipped vehicles. The responsible authority shall ensure the existence of a calibration or validation certificate for the VPR within a 6-month period prior to the emissions test. If the VPR incorporates temperature monitoring alarms, a 13-month validation interval is permitted.

It is recommended that the VPR is calibrated and validated as a complete unit.

The VPR shall be characterised for particle concentration reduction factor with solid particles of 30, 50 and 100 nm electrical mobility diameter. Particle concentration reduction factors for particles of 30 nm and 50 nm electrical mobility diameters shall be no more than 30 per cent and 20 per cent higher respectively, and no more than 5 per cent lower than that for particles of 100 nm electrical mobility diameter. For the purposes of validation, the arithmetic average of the particle concentration reduction factor calculated for particles of 30 nm, 50 nm and 100 nm electrical mobility diameters shall be within ±10 per cent of the arithmetic average particle concentration reduction factor determined during the latest complete calibration of the VPR.

5.7.2.2. The test aerosol for these measurements shall be solid particles of 30, 50 and 100 nm electrical mobility diameter and a minimum concentration of 5,000 particles per cm³ at the VPR inlet. As an option, a polydisperse aerosol with an electrical mobility median diameter of 50 nm may be used for validation. The test aerosol shall be thermally stable at the VPR operating temperatures. Particle number concentrations shall be measured upstream and downstream of the components.

The particle concentration reduction factor for each monodisperse particle size, , shall be calculated using the following equation:

where:

is the upstream particle number concentration for particles of diameter ;

is the downstream particle number concentration for particles of diameter ;

is the particle electrical mobility diameter (30, 50 or 100 nm).

and shall be corrected to the same conditions.

The arithmetic average particle concentration reduction factor at a given dilution setting shall be calculated using the following equation:

Where a polydisperse 50 nm aerosol is used for validation, the arithmetic average particle concentration reduction factor at the dilution setting used for validation shall be calculated using the following equation:

where:

is the upstream particle number concentration;

is the downstream particle number concentration.

5.7.2.3. The VPR shall demonstrate greater than 99.0 per cent removal of tetracontane (CH3(CH2)38CH3) particles of at least 30 nm electrical mobility diameter with an inlet concentration ≥ 10,000 per cm³ when operated at its minimum dilution setting and manufacturer's recommended operating temperature.

5.7.2.4. The instrument manufacturer shall provide the maintenance or replacement interval that ensures that the removal efficiency of the VPR does not drop below the technical requirements. If such information is not provided, the volatile removal efficiency shall be checked yearly for each instrument.

5.7.2.5. The instrument manufacturer shall prove the solid particle penetration by testing one unit for each PN-system model. A PN-system model here covers all PN-systems with the same hardware, i.e. same geometry, conduit materials, flows and temperature profiles in the aerosol path. at a particle size, , shall be calculated using the equation specified in paragraph 4.3.1.3.3.1.

5.7.3. PN measurement system check procedures

On a monthly basis, the flow into the PNC shall have a measured value within 5 per cent of the PNC nominal flow rate when checked with a calibrated flow meter. Here the term ‘nominal flow rate’ refers to the flow rate stated in the last calibration for the PNC by the instrument manufacturer.

5.8. Accuracy of the mixing device

In the case that a gas divider is used to perform the calibrations as defined in paragraph 5.2. of this annex, the accuracy of the mixing device shall be such that the concentrations of the diluted calibration gases may be determined to within ±2 per cent. A calibration curve shall be verified by a mid-span check as described in paragraph 5.3. of this annex. A calibration gas with a concentration below 50 per cent of the analyser range shall be within 2 per cent of its certified concentration.

6. Reference gases

6.1. Pure gases

6.1.1. All values in ppm mean volume-ppm (vpm) which is considered equal to mol-ppm

6.1.2. The following pure gases shall be available, if necessary, for calibration and operation:

6.1.2.1. Nitrogen:

Purity: ≤1 ppm C1, ≤1 ppm CO, ≤400 ppm CO2, ≤0.1 ppm NO, ≤0.1 ppm N2O, ≤0.1 ppm NH3.

6.1.2.2. Synthetic air:

Purity: ≤1 ppm C1, ≤1 ppm CO, ≤400 ppm CO2, ≤0.1 ppm NO, ≤0.1 ppm NO2; oxygen content between 18 and 21 per cent volume.

6.1.2.3. Oxygen:

Purity: > 99.5 per cent vol. O2.

6.1.2.4. Hydrogen (and mixture containing helium or nitrogen):

Purity: ≤1 ppm C1, ≤400 ppm CO2; hydrogen content between 39 and 41 per cent volume.

6.1.2.5. Carbon monoxide:

Minimum purity 99.5 per cent.

6.1.2.6. Propane:

Minimum purity 99.5 per cent.

6.2. Calibration gases

The true concentration of a calibration gas shall be within ±1 per cent of the stated value or as given below, and shall be traceable to national or international standards.

Mixtures of gases having the following compositions shall be available with bulk gas specifications according to paragraphs 6.1.2.1. or 6.1.2.2. of this annex:

(a) C3H8 in synthetic air (see paragraph 6.1.2.2. of this annex);

(b) CO in nitrogen;

(c) CO2 in nitrogen;

(d) CH4 in synthetic air;

(e) NO in nitrogen (the amount of NO2 contained in this calibration gas shall not exceed 5 per cent of the NO content).

Annex B6

Type 1 test procedures and test conditions

1. Description of tests

1.1. The Type 1 test is used to verify the emissions of gaseous compounds, particulate matter, particle number (if PN measurement is required), CO2 emission, fuel consumption, electric energy consumption and electric ranges over the applicable WLTP test cycle and OBFCM accuracy (where applicable).

1.1.1. The tests shall be carried out according to the method described in paragraph 2. of this annex or paragraph 3. of Annex B8 for pure electric, hybrid electric and compressed hydrogen fuel cell hybrid vehicles. Exhaust gases, particulate matter and particle number (if PN measurement is required) shall be sampled and analysed by the prescribed methods.

1.1.2. When the reference fuel to be used is LPG or NG/biomethane, the following provisions shall apply additionally.

1.1.2.1. Exhaust emissions approval of a parent vehicle

1.1.2.1.1. The parent vehicle should demonstrate its capability to adapt to any fuel composition that may occur across the market. In the case of LPG there are variations in C3/C4 composition. In the case of NG/biomethane there are generally two types of fuel, high calorific fuel (H-gas) and low calorific fuel (Lgas), but with a significant spread within both ranges; they differ significantly in Wobbe index. These variations are reflected in the reference fuels.

1.1.2.1.2. In the case of vehicles fuelled by LPG, NG/biomethane, the parent vehicle(s) shall be tested in the Type 1 test on the two extreme reference fuels of Annex B3. In the case of NG/biomethane, if the transition from one fuel to another is in practice aided through the use of a switch, this switch shall not be used during type approval. In such a case on the manufacturer's request and with the agreement of the approval authority the pre-conditioning cycle referred in paragraph 2.6. of this annex may be extended.

1.1.2.1.3. The vehicle is considered to conform if, under the tests and reference fuels mentioned in paragraph 1.1.2.1.2. of this annex, the vehicle complies with the emission limits.

1.1.2.1.4. In the case of vehicles fuelled by LPG or NG/biomethane, the ratio of emission results "r" shall be determined for each pollutant as follows:

|  |  |  |
| --- | --- | --- |
| *Type(s) of fuel* | *Reference fuels* | *Calculation of "r"* |
| LPG and petrol or LPG only | Fuel A |  |
| Fuel B |
| NG/biomethane and petrol or NG/biomethane only | Fuel G20 |  |
| Fuel G25 |

1.1.2.2. Exhaust emissions approval of a member of the family:

For the type approval of a mono fuel gas vehicle and bi fuel gas vehicles operating in gas mode, fuelled by LPG or NG/Biomethane, as a member of the family, a Type 1 test shall be performed with one gas reference fuel. This reference fuel may be either of the gas reference fuels. The vehicle is considered to comply if the following requirements are met:

1.1.2.2.1. The vehicle complies with the definition of a family member as defined in paragraph 6.3.6.3. of this Regulation;

1.1.2.2.2. If the test fuel is reference fuel A for LPG or G20 for NG/biomethane, the emission result shall be multiplied by the relevant factor "r" calculated in paragraph 1.1.2.1.4. of this annex if r > 1; if r < 1, no correction is needed;

1.1.2.2.3. If the test fuel is reference fuel B for LPG or G25 for NG/biomethane, the emission result shall be divided by the relevant factor "r" calculated in paragraph 1.1.2.1.4. of this annex if r < 1; if r > 1, no correction is needed;

1.1.2.2.4. On the manufacturer's request, the Type 1 test may be performed on both reference fuels, so that no correction is needed;

1.1.2.2.5. The vehicle shall comply with the emission limits valid for the relevant category for both measured and calculated emissions;

1.1.2.2.6. If repeated tests are made on the same engine the results on reference fuel G20, or A, and those on reference fuel G25, or B, shall first be averaged; the "r" factor shall then be calculated from these averaged results;

1.1.2.2.7. Without prejudice to paragraph 2.6.4.1.2. of this annex, during the Type 1 test it is permissible to use petrol only or simultaneously with gas when operating in gas mode provided that the energy consumption of gas is higher than 80 per cent of the total amount of energy consumed during the test. This percentage shall be calculated in accordance with the method set out in Appendix 3 to this annex.

1.2. The number of tests shall be determined according to the flowchart in Figure A6/1. The limit value is the maximum allowed value for the respective criteria emission as specified in Table 1 of this Regulation.

1.2.1. The flowchart in Figure A6/1 shall be applicable only to the whole applicable WLTP test cycle and not to single phases.

1.2.2. The test results shall be the values after the applicable adjustments specified in the post-processing tables in Annex B7 and Annex B8 are applied.

1.2.3. Determination of total cycle values

1.2.3.1. If during any of the tests a criteria emissions limit is exceeded, the vehicle shall be rejected.

1.2.3.2. Depending on the vehicle type, the manufacturer shall declare as applicable the total cycle values of the CO2 emission, the electric energy consumption, fuel consumption, fuel efficiency, as well as PER, EAER and AER according to Table A6/1.

1.2.3.3. The declared value of the equivalent all electric rangefor OVC-HEVs shall not be determined according to Figure A6/1. The declared value shall be taken as the type approval value if it is less than the calculated EAER value according to paragraph 4.4.4.1. If that is not the case, the calculated EAER shall be taken as the type approval value.

For 4 phase WLTP test

The declared value of the electric energy consumption for OVC-HEVs under charge-depleting operating condition shall not be determined according to Figure A6/1. It shall be taken as the type approval value if the declared CO2 value is accepted as the approval value. If that is not the case, the measured value of electric energy consumption shall be taken as the type approval value. Evidence of a correlation between declared CO2 emission and electric energy consumption shall be submitted to the responsible authority in advance, if applicable.

For 3 phase WLTP test

The declared value of the fuel efficiency for OVC-HEVs under charge-depleting operating condition shall not be determined according to Figure A6/1. It shall be taken as the type approval value if the declared electric energy consumption value is accepted as the approval value. If that is not the case, the measured value of fuel efficiency shall be taken as the type approval value. Evidence of a correlation between declared fuel efficiency and electric energy consumption shall be submitted to the responsible authority in advance, if applicable.

1.2.3.4. If after the first test all criteria in row 1 of the applicable Table A6/2 are fulfilled, all values declared by the manufacturer shall be accepted as the type approval value. If any one of the criteria in row 1 of the applicable Table A6/2 is not fulfilled, a second test shall be performed with the same vehicle.

1.2.3.5. After the second test, the arithmetic average results of the two tests shall be calculated. If all criteria in row 2 of the applicable Table A6/2 are fulfilled by these arithmetic average results, all values declared by the manufacturer shall be accepted as the type approval value. If any one of the criteria in row 2 of the applicable Table A6/2 is not fulfilled, a third test shall be performed with the same vehicle.

1.2.3.6. After the third test, the arithmetic average results of the three tests shall be calculated. For all parameters which fulfil the corresponding criterion in row 3 of the applicable Table A6/2, the declared value shall be taken as the type approval value. For any parameter which does not fulfil the corresponding criterion in row 3 of the applicable Table A6/2, the arithmetic average result shall be taken as the type approval value.

1.2.3.7. In the case that any one of the criterion of the applicable Table A6/2 is not fulfilled after the first or second test, at the request of the manufacturer and with the approval of the responsible authority, the values may be re-declared as higher values for emissions or consumption, or as lower values for electric ranges, in order to reduce the required number of tests for type approval.

1.2.3.8. Determination of the acceptance values

1.2.3.8.1. For 4 phase WLTP test only

Additional to the requirement of paragraph 1.2.3.8.2., the following acceptance values for dCO21, dCO22 and dCO23 shall be used in relation to the criteria for the number of tests in Table A6/2:

For the CO2 emissions from the 4 phases of a WLTP test;

dCO21 = 0.990

dCO22 = 0.995

dCO23 = 1.000

1.2.3.8.2. For 4 phase WLTP test only:

If the charge-depleting Type 1 test for OVC-HEVs consists of two or more applicable WLTP test cycles and the dCO2x value is below 1.0, the dCO2x value shall be replaced by 1.0.

1.2.3.9. In the case that a test result or an average of test results was taken and confirmed as the type approval value, this result shall be referred to as the “declared value” for further calculations.

Table A6/1

**Applicable rules for a manufacturer’s declared values (total cycle values)(a) (as applicable)**

| *Powertrain* | | *For 4 phase WLTP test*  *MCO2 (b)*  *(g/km)* | *For 4 phase WLTP test*  *FC*  *(kg/100 km)* | *For 3 phase WLTP*  *FE (km/l or km/kg)* | *Electric energy consumption(c)*  *(Wh/km)* | *All electric range / Equivalent all-electric range/ Pure Electric Range (c)*  *(km)* |
| --- | --- | --- | --- | --- | --- | --- |
| Vehicles tested according to Annex B6 (pure ICE) | | MCO2  Paragraph 3. of Annex B7. | - | FE  Paragraph 1.4. of Annex B7. | - | - |
| NOVC-FCHV | | - | FCCS  Paragraph 4.2.1.2.1. of Annex B8. | FECS  Paragraph 4.2.1.2.1. of Annex B8. | - | - |
| NOVC-HEV | | MCO2,CS  Paragraph 4.1.1. of Annex B8. | - | FECS  Paragraph 4.1.1.1. of Annex B8. | - | - |
| OVC-HEV | CD | MCO2,CD  Paragraph 4.1.2. of Annex B8. | - | FECD  Paragraph 4.6.1. of Annex B8. | For 4 phase WLTP test: ECAC,CD  Paragraph 4.3.1. of Annex B8. | AER  Paragraph 4.4.1.1. of Annex B8. |
| CS | MCO2,CS  Paragraph 4.1.1. of Annex B8. | - | FECS  Paragraph 4.1.1.1. of Annex B8. | - | - |
| CD/CS | - | - | - | For 3 phase WLTP: EC  Paragraph 4.6.2. of Annex B8 | EAER(d)  Paragraph 4.4.4.1. of Annex B8 |
| PEV | | - | - | - | ECWLTC(d)  Paragraph 4.3.4.2. of Annex B8. | PERWLTC(d)  Paragraph 4.4.2. of Annex B8. |

(a) The declared value shall be the value to which the necessary corrections, as applicable, are applied

(b) Rounding to 2 places of decimal according to paragraph 6.1.8. of this Regulation

(c) Rounding to one place of decimal according to paragraph 6.1.8. of this Regulation

(d) The declared value shall be provided for the 3 phase WLTP and 4 phase WLTP (as applicable)

Figure A6/1

**Flowchart for the number of Type 1 tests**

First test

Any of criteria emissions > Limit

Yes

All criteria in Table A6/2 within the “first test” row are fulfilled.

No

Yes

Second test

Any of criteria emissions > Limit

Yes

No

Yes

Third test

Any of criteria emissions > Limit

Yes

Rejected

No

Declared value or mean of three accepted, depending on judgment result of each value

All declared values and emissions accepted

No

No

All criteria in Table A6/2 within the “second test” row are fulfilled.

Table A6/2

**Criteria for number of tests**

For pure ICE vehicles, NOVC-HEVs and OVC-HEVs charge-sustaining Type 1 tests.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | *Test* | *Judgement parameter* | *Criteria emission* | *For 4 phase WLTP test*: *MCO2* | For 3 phase WLTP *FE* |
| Row 1 | First test | First test results | ≤ Regulation limit × 0.9 | ≤ Declared value × dCO21(b) | ≥ Declared value × 1.0 |
| Row 2 | Second test | Arithmetic average of the first and second test results | ≤ Regulation limit × 1.0(a) | ≤ Declared value × dCO22(b) | ≥ Declared value × 1.0 |
| Row 3 | Third test | Arithmetic average of three test results | ≤ Regulation limit × 1.0(a) | ≤ Declared value × dCO23(b) | ≥ Declared value × 1.0 |

(a) Each test result shall fulfil the regulation limit.

(b) dCO21, dCO22, and dCO23 shall be determined according to paragraph 1.2.3.8. of this annex

For OVC-HEVs charge-depleting Type 1 tests.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | *Test* | *Judgement parameter* | *Criteria emissions* | *For 4 phase WLTP test: MCO2,CD* | *For 3 phase WLTP test: EC* | *For 4 phase WLTP test: AER* |
| Row 1 | First test | First test results | ≤ Regulation limit × 0.9(a) | ≤ Declared value × dCO21(c) | ≤ Declared value ×1.0 | ≥ Declared value × 1.0 |
| Row 2 | Second test | Arithmetic average of the first and second test results | ≤ Regulation limit × 1.0(b) | ≤ Declared value × dCO22(c) | ≤ Declared value ×1.0 | ≥ Declared value × 1.0 |
| Row 3 | Third test | Arithmetic average of three test results | ≤ Regulation limit × 1.0(b) | ≤ Declared value × dCO23(c) | ≤ Declared value ×1.0 | ≥ Declared value × 1.0 |

(a) "0.9" shall be replaced by “1.0” for a charge-depleting Type 1 test for OVC-HEVs, only if the charge-depleting test contains two or more applicable WLTC cycles.

(b) Each test result shall fulfil the regulation limit.

(c) dCO21, dCO22 and dCO23 shall be determined according to paragraph 1.2.3.8. of this annex.

For PEVs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | *Test* | *Judgement parameter* | *Electric energy consumption* | *PER* |
| Row 1 | First test | First test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |
| Row 2 | Second test | Arithmetic average of the first and second test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |
| Row 3 | Third test | Arithmetic average of three test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |

For NOVC-FCHVs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | *Test* | *Judgement parameter* | For 4 phase WLTP test: *FCCS* (upper value) | For 3 phase WLTP -: *FECS* (lower value) |
| Row 1 | First test | First test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |
| Row 2 | Second test | Arithmetic average of the first and second test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |
| Row 3 | Third test | Arithmetic average of three test results | ≤ Declared value × 1.0 | ≥ Declared value × 1.0 |

1.2.4. Determination of phase-specific values

1.2.4.1. Phase-specific value for CO2

1.2.4.1.1. After the total cycle declared value of the CO2 emission is accepted, the arithmetic average of the phase-specific values of the test results in g/km shall be multiplied by the adjustment factor CO2\_AF to compensate for the difference between the declared value and the test results. This corrected value shall be the type approval value for CO2.

where:

where:

is the arithmetic average CO2 emission result for the L phase test result(s), g/km;

is the arithmetic average CO2 emission result for the M phase test result(s), g/km;

is the arithmetic average CO2 emission result for the H phase test result(s), g/km;

is the arithmetic average CO2 emission result for the exH phase test result(s), g/km;

DL is theoretical distance of phase L, km;

DM is theoretical distance of phase M, km;

DH is theoretical distance of phase H, km;

DexH is theoretical distance of phase exH, km.

1.2.4.1.2. If the total cycle declared value of the CO2 emission is not accepted, the type approval phase-specific CO2 emission value shall be calculated by taking the arithmetic average of the all test results for the respective phase.

1.2.4.2. Phase-specific values for fuel consumption

The fuel consumption value shall be calculated by the phase-specific CO2 emission using the equations in paragraph 1.2.4.1. of this annex and the arithmetic average of the emissions.

2. Type 1 test

2.1. Overview

2.1.1. The Type 1 test shall consist of prescribed sequences of dynamometer preparation, fuelling, soaking, and operating conditions.

2.1.2. The Type 1 test shall consist of vehicle operation on a chassis dynamometer on the applicable WLTC for the interpolation family. A proportional part of the diluted exhaust emissions shall be collected continuously for subsequent analysis using a constant volume sampler. The applicable WLTC for each part of the procedure shall be taken from the following table:

| *Vehicle type* | | *Driven WLTC for preconditioning* | *Driven WLTC for Type 1 test* | *Calculation of final results* |
| --- | --- | --- | --- | --- |
| Pure ICE | | 4 phases | 4 phases | 3 phases and 4 phases |
| NOVC-HEV | | 4 phases | 4 phases | 3 phases and 4 phases |
| OVC-HEV | CD | Same as Type 1 test | 3 phases and 4 phases (separate tests) | Same as Type 1 test and city cycle during 4 phase test |
| CS | 4 phases | 4 phases | 3 phases and 4 phases |
| NOVC-FCHV | | 4 phases | 4 phases | 3 phases and 4 phases |
| PEV | | According to manufacturer’s recommendation | 4 phases\* | 3 phases, 4 phases and city cycle |

\* Dynamic segment of shortened Type 1 test consists of 4 phases followed by city cycle

2.1.3. Background concentrations shall be measured for all compounds for which dilute mass emissions measurements are conducted. For exhaust emissions testing, this requires sampling and analysis of the dilution air.

2.1.3.1. Background particulate measurement

2.1.3.1.1. Where the manufacturer requests subtraction of either dilution air or dilution tunnel background particulate mass from emissions measurements, these background levels shall be determined according to the procedures listed in paragraphs 2.1.3.1.1.1. to 2.1.3.1.1.3. inclusive of this annex.

2.1.3.1.1.1. The maximum permissible background correction shall be a mass on the filter equivalent to 1 mg/km at the flow rate of the test.

2.1.3.1.1.2. If the background exceeds this level, the default figure of 1 mg/km shall be subtracted.

2.1.3.1.1.3. Where subtraction of the background contribution gives a negative result, the background level shall be considered to be zero.

2.1.3.1.2. Dilution air background particulate mass level shall be determined by passing filtered dilution air through the particulate background filter. This shall be drawn from a point immediately downstream of the dilution air filters. Background levels in g/m3 shall be determined as a rolling arithmetic average of at least 14 measurements with at least one measurement per week.

2.1.3.1.3. Dilution tunnel background particulate mass level shall be determined by passing filtered dilution air through the particulate background filter. This shall be drawn from the same point as the particulate matter sample. Where secondary dilution is used for the test, the secondary dilution system shall be active for the purposes of background measurement. One measurement may be performed on the day of test, either prior to or after the test.

2.1.3.2. Background particle number determination (if PN measurement is required)

2.1.3.2.1. Where a manufacturer requests a background correction, these background levels shall be determined as follows:

2.1.3.2.1.1. The background value may be either calculated or measured. The maximum permissible background correction shall be related to the maximum allowable leak rate of the particle number measurement system (0.5 particles per cm³) scaled from the particle concentration reduction factor, PCRF, and the CVS flow rate used in the actual test;

2.1.3.2.1.2. Either the responsible authority or the manufacturer may request that actual background measurements are used instead of calculated ones.

2.1.3.2.1.3. Where subtraction of the background contribution gives a negative result, the PN result shall be considered to be zero.

2.1.3.2.2. The dilution air background particle number level shall be determined by sampling filtered dilution air. This shall be drawn from a point immediately downstream of the dilution air filters into the PN measurement system. Background levels in particles per cm³ shall be determined as a rolling arithmetic average of least 14 measurements with at least one measurement per week.

2.1.3.2.3. The dilution tunnel background particle number level shall be determined by sampling filtered dilution air. This shall be drawn from the same point as the PN sample. Where secondary dilution is used for the test the secondary dilution system shall be active for the purposes of background measurement. One measurement may be performed on the day of test, either prior to or after the test using the actual PCRF and the CVS flow rate utilised during the test.

2.2. General test cell equipment

2.2.1. Parameters to be measured

2.2.1.1. The following temperatures shall be measured with an accuracy of ±1.5 °C:

(a) Test cell ambient air;

(b) Dilution and sampling system temperatures as required for emissions measurement systems defined in Annex B5.

2.2.1.2. Atmospheric pressure shall be measurable with a precision of ±0.1 kPa.

2.2.1.3. Specific humidity H shall be measurable with a precision of ±1 g H2O/kg dry air.

2.2.2. Test cell and soak area

2.2.2.1. Test cell

2.2.2.1.1. The test cell shall have a temperature set point of 23 °C. The tolerance of the actual value shall be within ±5 °C. The air temperature and humidity shall be measured at the test cell's cooling fan outlet at a minimum frequency of 0.1 Hz. For the temperature at the start of the test, see paragraph 2.8.1. of this annex.

2.2.2.1.2. The specific humidity H of either the air in the test cell or the intake air of the engine shall be such that:

(g H2O/kg dry air)

2.2.2.1.3. Humidity shall be measured continuously at a minimum frequency of 0.1 Hz.

2.2.2.2. Soak area

The soak area shall have a temperature set point of 23 °C and the tolerance of the actual value shall be within ±3 °C on a 5-minute running arithmetic average and shall not show a systematic deviation from the set point. The temperature shall be measured continuously at a minimum frequency of 0.033 Hz (every 30 s).

2.3. Test vehicle

2.3.1. General

The test vehicle shall conform in all its components with the production series, or, if the vehicle is different from the production series (e.g. for worst case testing), a full description shall be recorded. In selecting the test vehicle, the manufacturer and the responsible authority shall agree which vehicle model is representative for the interpolation family.

In the case that vehicles within an interpolation family are equipped with different emission control systems that could have an effect on the emission behaviour, the manufacturer shall either demonstrate to the responsible authority that the test vehicle(s) selected and its (their) results from the Type 1 test are representative for the interpolation family, or demonstrate the fulfilment of the criteria emission within the interpolation family by testing one or more individual vehicles that differ in their emission control systems.

For the measurement of emissions, the road load as determined with test vehicle H shall be applied. In the case of a road load matrix family, for the measurement of emissions, the road load as calculated for vehicle HM according to paragraph 5.1. of Annex B4 shall be applied.

If at the request of the manufacturer the interpolation method is used (see paragraph 3.2.3.2. of Annex B7), an additional measurement of emissions shall be performed with the road load as determined with test vehicle L. Tests on vehicles H and L should be performed with the same test vehicle and shall be tested with the shortest n/v ratio (with a tolerance of ±1.5 per cent) within the interpolation family. In the case of a road load matrix family, an additional measurement of emissions shall be performed with the road load as calculated for vehicle LM according to paragraph 5.1. of Annex B4.

Road load coefficients and the test mass of test vehicle L and H may be taken from different road load matrix families. They may also be taken from different road load families as long as the difference between these road load families has been demonstrated to and accepted by the responsible authority, and results from either applying paragraph 6.8. of Annex B4 or tyres taken from different tyre categories, while the requirements in paragraph 2.3.2. of this annex are maintained.

2.3.2. CO2 interpolation range


2.3.2.1. The interpolation method shall only be used if the difference in CO2 over the applicable cycle resulting from the table below between test vehicles L and H is between a minimum of 5 g/km and a maximum defined in paragraph 2.3.2.2. of this annex.

2.3.2.2. The maximum difference in CO2 emissions allowed over the applicable cycle resulting from the table below between test vehicles L and H shall be 20 per cent plus 5 g/km of the CO2 emissions from vehicle H, but at least 15 g/km and not exceeding 30 g/km. See Figure A6/2.

|  |  |
| --- | --- |
| For 4-phase WLTP test | For 3-phase WLTP test |
| step 9 of Table A7/1 of Annex B7 | step 6 of Table A7/1 of Annex B7 |

Figure A6/2

**Interpolation range for pure ICE vehicles**




This restriction does not apply in relation to the application of a road load matrix family or when the calculation of the road load of vehicles L and H is based on the default road load.

2.3.2.2.1. The allowed interpolation range defined in paragraph 2.3.2.2. of this annex may be increased by 10 g/km CO2 (see Figure A6/3) if a vehicle M is tested within that family and the conditions according to paragraph 2.3.2.4. of this annex are fulfilled. This increase is allowed only once within an interpolation family.

Figure A6/3

**Interpolation range for pure ICE vehicles with vehicle M**



2.3.2.3. At the request of the manufacturer and with approval of the responsible authority, the application of the interpolation method on individual vehicle values within a family may be extended if the maximum extrapolation of an individual vehicle (Step 10 in Table A7/1 of Annex B7) is not more than 3 g/km above the CO2 emission of vehicle H (Step 9 in Table A7/1 of Annex B7) and/or is not more than 3 g/km below the CO2 emission of vehicle L (Step 9 in Table A7/1 of Annex B7). This extrapolation is valid only within the absolute boundaries of the interpolation range specified in paragraph 2.3.2.2.

It is not necessary to check the above 3 g/km criteria for results after 3 phases.

For the application of a road load matrix family, or when the calculation of the road load of vehicles L and H is based on the default road load, extrapolation is not permitted.


2.3.2.4. Vehicle M

Vehicle M is a vehicle within the interpolation family between the vehicles L and H with a cycle energy demand which is preferably closest to the average of vehicles L and H.

The limits of the selection of vehicle M (see Figure A6/4) are such that neither the difference in CO2 emission values between vehicles H and M nor the difference in CO2 emission values between vehicles M and L is greater than the allowed CO2 range in accordance with paragraph 2.3.2.2. of this annex. The defined road load coefficients and the defined test mass shall be recorded.

Figure A6/4

**Limits for the selection of vehicle M**



For 4-phase WLTP

The linearity of the corrected measured and averaged CO2 emission for vehicle M, MCO2,c,6,M according to step 6 of Table A7/1 of Annex B7, shall be verified against the linearly interpolated CO2 emission between vehicles L and H over the applicable cycle by using the corrected measured and averaged CO2 emission MCO2,c,6,H of vehicle H and MCO2,c,6,L of vehicle L, according to step 6 of Table A7/1 of Annex B7, for the linear CO2 emission interpolation.

For 3-phase WLTP


An additional averaging of tests using the CO2-output of step 4a is necessary (not described in Table A7/1). The linearity of the corrected measured and averaged CO2 emission for vehicle M, MCO2,c,4a,M according to step 4a of Table A7/1 of Annex B7, shall be verified against the linearly interpolated CO2 emission between vehicles L and H over the applicable cycle by using the corrected measured and averaged CO2 emission MCO2,c,4a,H values of vehicle H and MCO2,c,4a,L of vehicle L, according to step 4a of Table A7/1 of Annex B7, for the linear CO2 emission interpolation.

For 3-phase and 4-phase WLTP

The linearity criterion for vehicle M (see Figure A6/5) shall be considered fulfilled, if the CO2 emission of the vehicle M over the applicable WLTC minus the CO2 emission derived by interpolation is less than 2 g/km or 3 per cent of the interpolated value, whichever value is lower, but at least 1 g/km.

Figure A6/5

**Linearity criterion for vehicle M**



If the linearity criterion is fulfilled, the CO2 values of individual vehicles shall be interpolated between vehicles L and H.

If the linearity criterion is not fulfilled, the interpolation family shall be split into two sub-families for vehicles with a cycle energy demand between vehicles L and M, and vehicles with a cycle energy demand between vehicles M and H. In such a case, the final CO2 emissions of vehicle M shall be determined in accordance with the same process as for vehicles L or H. See step 9 in Table A7/1 of Annex B7.

For vehicles with a cycle energy demand between that of vehicles L and M, each parameter of vehicle H necessary for the application of the interpolation method on individual values shall be substituted by the corresponding parameter of vehicle M.

For vehicles with a cycle energy demand between that of vehicles M and H, each parameter of vehicle L necessary for the application of the interpolation method on individual values shall be substituted by the corresponding parameter of vehicle M.

2.3.3. Run-in

The vehicle shall be presented in good technical condition. It shall have been run-in and driven between 3,000 and 15,000 km before the test. The engine, transmission and vehicle shall be run-in in accordance with the manufacturer’s recommendations.

2.4. Settings

2.4.1. Dynamometer settings and verification shall be performed according to Annex B4.

2.4.2. Dynamometer operation

2.4.2.1. Auxiliary devices shall be switched off or deactivated during dynamometer operation unless their operation is required by legislation (e.g. daylight running lamps).

2.4.2.1.1. If the vehicle is equipped with a coasting functionality, this functionality shall be deactivated either by a switch or by the vehicle’s dynamometer operation mode during chassis dynamometer testing, except for tests where the coasting functionality is explicitly required by the test procedure.

2.4.2.1.2. For tests performed after [xx-xx-20xx[[18]](#footnote-19)], the rear position lamps shall be set to the operating condition which is applied at ambient lighting conditions exceeding 7,000 lux (e.g. by the vehicle's dynamometer operation mode).

2.4.2.2. The vehicle’s dynamometer operation mode, if any, shall be activated by using the manufacturer's instruction (e.g. using vehicle steering wheel buttons in a special sequence, using the manufacturer’s workshop tester, removing a fuse).

The manufacturer shall provide the responsible authority a list of the deactivated devices and/or functionalities and justification for the deactivation. The dynamometer operation mode shall be approved by the responsible authority and the use of a dynamometer operation mode shall be recorded.

2.4.2.3. The vehicle’s dynamometer operation mode shall not activate, modulate, delay or deactivate the operation of any part (with the exclusion of the coasting functionality) that affects the emissions and fuel consumption under the test conditions. Any device that affects the operation on a chassis dynamometer shall be set to ensure a proper operation.

2.4.2.4. Allocation of dynamometer type to test vehicle

2.4.2.4.1. If the test vehicle has two powered axles, and under WLTP conditions it is partially or permanently operated with two axles being powered or recuperating energy over the applicable cycle the vehicle shall be tested on a dynamometer in 4WD operation which fulfils the specifications in paragraphs 2.2. and 2.3. of Annex B5.

2.4.2.4.2. If the test vehicle is tested with only one powered axle, the test vehicle shall be tested on a dynamometer in 2WD operation which fulfils the specifications in paragraph 2.2. of Annex B5.

At the request of the manufacturer and with the approval of the approval authority a vehicle with one powered axle may be tested on a 4WD dynamometer in 4WD operation mode.

2.4.2.4.3. If the test vehicle is operated with two axles being powered in dedicated driver-selectable modes which are not intended for normal daily operation but only for special limited purposes, such as ‘mountain mode’ or ‘maintenance mode’, or when the mode with two powered axles is only activated in an off-road situation, the vehicle shall be tested on a dynamometer in 2WD operation which fulfils the specifications in paragraph 2.2. of Annex B5.

At the request of the manufacturer and with the approval of the approval authority, the vehicle may be tested on a 4WD dynamometer in 4WD operation mode.

2.4.2.4.4. If the test vehicle is tested on a 4WD dynamometer in 2WD operation the wheels on the non-powered axle may rotate during the test, provided that the vehicle dynamometer operation mode and vehicle coastdown mode support this way of operation.

Figure A6/5a

**Possible test configurations on 2WD and 4WD dynamometers**



2.4.2.5. Demonstration of equivalency between a dynamometer in 2WD operation and a dynamometer in 4WD operation

2.4.2.5.1. At the request of the manufacturer and with the approval of the approval authority, the vehicle which has to be tested on a dynamometer in 4WD operation may alternatively be tested on a dynamometer in 2WD operation if the following conditions are met:

(a) the test vehicle is converted to have only one powered axle;

(b) the manufacturer demonstrates to the approval authority that the CO2, fuel consumption and/or electrical energy consumption of the converted vehicle is the same or higher as for the non-converted vehicle being tested on a dynamometer in 4WD operation;

(c) a safe operation is ensured for the test (e.g. by removing a fuse or dismounting a drive shaft) and an instruction is provided together with the dynamometer operation mode;

(d) the conversion is only applied to the vehicle tested at the chassis dynamometer, the road load determination procedure shall be applied to the unconverted test vehicle.

2.4.2.5.2. This demonstration of equivalency shall apply to all vehicles in the same road load family. At the request of the manufacturer, and with approval of the approval authority, this demonstration of equivalency may be extended to other road load families upon evidence that a vehicle from the worst-case road load family was selected as the test vehicle.

2.4.2.6. Information on whether the vehicle was tested on a 2WD dynamometer or a 4WD dynamometer and whether it was tested on a dynamometer in 2WD operation or 4WD operation shall be included in all relevant test reports. In the case that the vehicle was tested on a 4WD dynamometer, with that dynamometer in 2WD operation, this information shall also indicate whether or not the wheels on the non-powered wheels were rotating.

2.4.3. The vehicle’s exhaust system shall not exhibit any leak likely to reduce the quantity of gas collected. If applicable, openings in the exhaust system designed to remove condensate shall be sealed prior to the test.

Openings in the exhaust system designed to remove condensate shall fulfil the following requirements:

(a) The openings shall be located downstream of the last component reducing tailpipe emissions (e.g. catalytic converter, particulate trap) of the exhaust after-treatment system.

(b) The openings shall be documented within the WLTP Test Report in accordance with Appendix 1 to Annex A1.

2.4.4. The settings of the powertrain and vehicle controls shall be those prescribed by the manufacturer for series production.

2.4.5. Tyres shall be of a type specified as original equipment by the vehicle manufacturer. Tyre pressure may be increased by up to 50 per cent above the pressure specified in paragraph 4.2.2.3. of Annex B4. The same tyre pressure shall be used for the setting of the dynamometer and for all subsequent testing. The tyre pressure used shall be recorded.

2.4.6. Reference fuel

The appropriate reference fuel as specified in Annex B3 shall be used for testing.

2.4.7. Test vehicle preparation

2.4.7.1. The vehicle shall be approximately horizontal during the test so as to avoid any abnormal distribution of the fuel.

2.4.7.2. If necessary, the manufacturer shall provide additional fittings and adapters, as required to accommodate a fuel drain at the lowest point possible in the tank(s) as installed on the vehicle, and to provide for exhaust sample collection.

2.4.7.3. For PM sampling during a test when the regenerating device is in a stabilized loading condition (i.e. the vehicle is not undergoing a regeneration), it is recommended that the vehicle has completed more than 1/3 of the mileage between scheduled regenerations or that the periodically regenerating device has undergone equivalent loading off the vehicle.

2.5. Preliminary testing cycles

Preliminary testing cycles may be carried out if requested by the manufacturer to follow the speed trace within the prescribed limits.

2.6. Test vehicle preconditioning

2.6.1. Vehicle preparation

2.6.1.1. Fuel tank filling

The fuel tank(s) shall be filled with the specified test fuel. If the existing fuel in the fuel tank(s) does not meet the specifications contained in paragraph 2.4.6. of this annex, the existing fuel shall be drained prior to the fuel fill. The evaporative emission control system shall neither be abnormally purged nor abnormally loaded.

2.6.1.2. REESSs charging

Before the preconditioning test cycle, the REESSs shall be fully charged. At the request of the manufacturer, charging may be omitted before preconditioning. The REESSs shall not be charged again before official testing.

2.6.1.3. Tyre pressures

The tyre pressure of the driving wheels shall be set in accordance with paragraph 2.4.5. of this annex.

2.6.1.4. Gaseous fuel vehicles

Between the tests on the first gaseous reference fuel and the second gaseous reference fuel, for vehicles with positive ignition engines fuelled with LPG or NG/biomethane or so equipped that they can be fuelled with either petrol or LPG or NG/biomethane, the vehicle shall be preconditioned again before the test on the second reference fuel.

2.6.2. Test cell

2.6.2.1. Temperature

During preconditioning, the test cell temperature shall be the same as defined for the Type 1 test (paragraph 2.2.2.1.1. of this annex).

2.6.2.2. Background measurement

In a test facility in which there may be possible contamination of a low particulate emitting vehicle test with residue from a previous test on a high particulate emitting vehicle, it is recommended, for the purpose of sampling equipment preconditioning, that a 120 km/h steady state drive cycle of 20 minutes duration be driven by a low particulate emitting vehicle. Longer and/or higher speed running is permissible for sampling equipment preconditioning if required. Dilution tunnel background measurements, if applicable, shall be taken after the tunnel preconditioning, and prior to any subsequent vehicle testing.

2.6.3. Procedure

2.6.3.1. The test vehicle shall be placed, either by being driven or pushed, on a dynamometer and operated through the applicable WLTCs. The vehicle need not be cold, and may be used to set the dynamometer load.

2.6.3.2. The dynamometer load shall be set according to paragraphs 7. and 8. of Annex B4. In the case that a dynamometer in 2WD operation is used for testing, the road load setting shall be carried out on a dynamometer in 2WD operation, and in the case that a dynamometer in 4WD operation is used for testing the road load setting shall be carried out on a dynamometer in 4WD operation.

2.6.4. Operating the vehicle

2.6.4.1. The powertrain start procedure shall be initiated by means of the devices provided for this purpose according to the manufacturer's instructions.

A non-vehicle initiated switching of mode of operation during the test shall not be permitted unless otherwise specified.

2.6.4.1.1. If the initiation of the powertrain start procedure is not successful, e.g. the engine does not start as anticipated or the vehicle displays a start error, the test is void, preconditioning tests shall be repeated and a new test shall be driven.

2.6.4.1.2. In the cases where LPG or NG/biomethane is used as a fuel, it is permissible that the engine is started on petrol and switched automatically to LPG or NG/biomethane after a predetermined period of time that cannot be changed by the driver. This period of time shall not exceed 60 seconds.

It is also permissible to use petrol only or simultaneously with gas when operating in gas mode provided that the energy consumption of gas is higher than 80 per cent of the total amount of energy consumed during the Type 1 test. This percentage shall be calculated in accordance with the method set out in Appendix 3 to this annex.

2.6.4.2. The cycle starts on initiation of the powertrain start procedure.

2.6.4.3. For preconditioning, the applicable WLTC shall be driven.

At the request of the manufacturer or the responsible authority, additional WLTCs may be performed in order to bring the vehicle and its control systems to a stabilized condition.

The extent of such additional preconditioning shall be included in all relevant test reports.

2.6.4.4. Accelerations

The vehicle shall be operated with the necessary accelerator control movement to accurately follow the speed trace.

The vehicle shall be operated smoothly following representative shift speeds and procedures.

For manual transmissions, the accelerator control shall be released during each shift and the shift shall be accomplished in minimum time.

If the vehicle cannot follow the speed trace, it shall be operated at maximum available power until the vehicle speed reaches the respective target speed again.

2.6.4.5. Deceleration

During decelerations, the driver shall deactivate the accelerator control but shall not manually disengage the clutch until the point specified in paragraphs 3.3. or 4.(f) of Annex B2.

If the vehicle decelerates faster than prescribed by the speed trace, the accelerator control shall be operated such that the vehicle accurately follows the speed trace.

If the vehicle decelerates too slowly to follow the intended deceleration, the brakes shall be applied such that it is possible to accurately follow the speed trace.

2.6.4.6. Brake application

During stationary/idling vehicle phases, the brakes shall be applied with appropriate force to prevent the drive wheels from turning.

2.6.5. Use of the transmission

2.6.5.1. Manual shift transmissions

2.6.5.1.1. The gear shift prescriptions specified in Annex B2 shall be followed. Vehicles tested according to Annex B8 shall be driven according to paragraph 1.5. of that annex.

2.6.5.1.2. The gear change shall be started and completed within ±1.0 second of the prescribed gear shift point.

2.6.5.1.3. The clutch shall be depressed within ±1.0 second of the prescribed clutch operating point.

2.6.5.2. Automatic shift transmissions

2.6.5.2.1. After initial engagement, the selector shall not be operated at any time during the test. Initial engagement shall be done 1 second before beginning the first acceleration.

2.6.5.2.2. Vehicles with an automatic transmission with a manual mode shall not be tested in manual mode.

2.6.6. Driver-selectable modes

2.6.6.1. Vehicles equipped with a predominant mode shall be tested in that mode. At the request of the manufacturer, the vehicle may alternatively be tested with the driver-selectable mode in the worst-case position for CO2 emissions.

The manufacturer shall provide evidence to the responsible authority of the existence of a mode that fulfils the requirements of paragraph 3.5.9. of this Regulation. With the agreement of the responsible authority, the predominant mode may be used as the only mode for the determination of criteria emissions, CO2 emissions, and fuel consumption.

2.6.6.2. If the vehicle has no predominant mode because it has two or more configurable start modes, the worst case mode for CO2 emissions and fuel consumption within those configurable start modes shall be tested and may be used as the only mode for the determination of criteria emissions, CO2 emissions and fuel consumption.

2.6.6.3. If the vehicle has no predominant mode or the requested predominant mode is not agreed by the responsible authority as being a predominant mode, or there are not two or more configurable start modes, the vehicle shall be tested for criteria emissions, CO2 emissions, and fuel consumption in the best case mode and worst case mode. Best and worst case modes shall be identified by the evidence provided on the CO2 emissions and fuel consumption in all modes. CO2 emissions and fuel consumption shall be the arithmetic average of the test results in both modes. Test results for both modes shall be recorded.

At the request of the manufacturer, the vehicle may alternatively be tested with the driver-selectable mode in the worst case position for CO2 emissions.

2.6.6.4. On the basis of technical evidence provided by the manufacturer and with the agreement of the responsible authority, the dedicated driver-selectable modes for very special limited purposes shall not be considered (e.g. maintenance mode, crawler mode). All remaining modes used for forward driving shall be considered and the criteria emissions limits shall be fulfilled in all these modes.

2.6.6.5. Paragraphs 2.6.6.1. to 2.6.6.4. inclusive of this annex shall apply to all vehicle systems with driver-selectable modes, including those not solely specific to the transmission.

2.6.7. Voiding of the Type 1 test and completion of the cycle

If the engine stops unexpectedly, the preconditioning or Type 1 test shall be declared void.

After completion of the cycle, the engine shall be switched off. The vehicle shall not be restarted until the beginning of the test for which the vehicle has been preconditioned.

2.6.8. Data required, quality control

2.6.8.1. Speed measurement

During the preconditioning, speed shall be measured against time or collected by the data acquisition system at a frequency of not less than 1 Hz so that the actual driven speed can be assessed.

2.6.8.2. Distance travelled

The distance actually driven by the vehicle shall be recorded for each WLTC phase.

2.6.8.3. Speed trace tolerances

Vehicles that cannot attain the acceleration and maximum speed values required in the applicable WLTC shall be operated with the accelerator control fully activated until they once again reach the required speed trace. Speed trace violations under these circumstances shall not void a test. Deviations from the driving cycle shall be recorded.

2.6.8.3.1. Unless otherwise stated in the specific sections, the following tolerances shall be permitted between the actual vehicle speed and the prescribed speed of the applicable test cycles based on the driving events:

2.6.8.3.1.1. Tolerance (1)

(a) Upper limit: 2.0 km/h higher than the highest point of the trace within ±5.0 second of the given point in time;

(b) Lower limit: 2.0 km/h lower than the lowest point of the trace within ±5.0 second of the given time.

2.6.8.3.1.2. Tolerance (2)

Speed tolerances greater than those prescribed shall be accepted provided the tolerances are never exceeded for more than 1 second on any one occasion. There shall be no more than ten such deviations per test cycle

(a) Upper limit: 2.0 km/h higher than the highest point of the trace within ±1.0 second of the given point in time;

(b) Lower limit: 2.0 km/h lower than the lowest point of the trace within ±1.0 second of the given time.

2.6.8.3.1.3. Tolerance (3)

|  |  |
| --- | --- |
| IWR | in the range of – 2.0 to + 4.0 per cent |
| RMSSE | less than 0.8 km/h |

2.6.8.3.1.4. Tolerance (4)

|  |  |
| --- | --- |
| IWR | in the range of – 2.0 to + 4.0 per cent |
| RMSSE | manufacturer declared criteria but shall not be greater than 1.3 km/h |

2.6.8.3.1.5. IWR and RMSSE drive trace indices shall be calculated in accordance with the requirements of paragraph 7. of Annex B7.

2.6.8.3.2. The vehicle operation events and tolerances to be permitted for these events are as follows:


|  |  |  |  |
| --- | --- | --- | --- |
| Vehicle operation | Warm-up cycle for dynamometer setting | Pre-conditioning | Performance parameter measurement test after preconditioning |
| Annex B6 and B8;  Type 1 Tests | Tolerance (1) | Tolerance (2) | Tolerance (2)\* and  Tolerance (3) |
| Annex C3:  Type 4 Test | Tolerance (1) | Tolerance (2) | Tolerance (2)\* |
| Annex C5 Appendix1;  OBD Demonstration Tests | Tolerance (1) | Tolerance (2) | Tolerance (2)\* |
| COP Tests | Tolerance (1) | Tolerance (2) | Tolerance (2)\* and  Tolerance (4) |
| Derive run-in factor for COP | Tolerance (1) | Tolerance (2) | Tolerance (2)\* and  Tolerance (3) |

\* the tolerance shall not be shown to the driver

If the speed trace is outside the respective validity range for any of the tests, those individual tests shall be considered invalid.

Figure A6/6

**Speed trace tolerances**



2.6.8.4. Alternator (DC/DC converter) current measurement

During the Type 1 test, the alternator current shall be measured following the procedure and requirements set out in paragraph 2. of Appendix 2 to Annex B6. In the case of OVC-HEVs and NOVC-HEVs the DC/DC converter current shall be measured following the procedure and requirements set out in paragraph 2. of Appendix 3 to Annex B8. The measured data (1 Hz integrated frequency) for each test performed shall be made available by the approval authority if requested by a regional authority.

2.6.8.5. OBFCM data recording and storing

During the Type 1 test, the following parameters referred in Appendix 5 of this Regulation shall be recorded and saved (1 Hz sampling frequency) by the testing lab and shall be made available by the approval authority if requested by a regional authority:

(a) Engine fuel rate (grams/second);

(b) Engine fuel rate (litres/hour);

(c) Vehicle fuel rate (grams/second).

2.7. Soaking

2.7.1. After preconditioning and before testing, the test vehicle shall be kept in an area with ambient conditions as specified in paragraph 2.2.2.2. of this annex.

2.7.2. The vehicle shall be soaked for a minimum of 6 hours and a maximum of 36 hours with the engine compartment cover opened or closed. If not excluded by specific provisions for a particular vehicle, cooling may be accomplished by forced cooling down to the set point temperature. If cooling is accelerated by fans, the fans shall be placed so that the maximum cooling of the drive train, engine and exhaust after-treatment system is achieved in a homogeneous manner.

2.8. Emission and fuel consumption test (Type 1 test)

2.8.1. The test cell temperature at the start of the test shall be within ±3 °C of the set point of 23 °C. The engine oil temperature and coolant temperature, if any, shall be within ±2 °C of the set point of 23 °C.

2.8.2. The test vehicle shall be pushed onto a dynamometer.

2.8.2.1. The drive wheels of the vehicle shall be placed on the dynamometer without starting the engine.

2.8.2.2. The drive-wheel tyre pressures shall be set in accordance with the provisions of paragraph 2.4.5. of this annex.

2.8.2.3. The engine compartment cover shall be closed.

2.8.2.4. An exhaust connecting tube shall be attached to the vehicle tailpipe(s) immediately before starting the engine.

2.8.2.5. The tested vehicle shall be placed on the chassis dynamometer according to paragraphs 7.3.3. to 7.3.3.1.4. of Annex B4.

2.8.3. Starting of the powertrain and driving

2.8.3.1. The powertrain start procedure shall be initiated by means of the devices provided for this purpose according to the manufacturer's instructions.

2.8.3.2. The vehicle shall be driven as described in paragraphs 2.6.4. to 2.6.8. inclusive of this annex over the applicable WLTC, as described in Annex B1.

2.8.4. RCB data shall be measured for each phase of the WLTC as defined in Appendix 2 to this annex.

2.8.5. Actual vehicle speed shall be sampled with a measurement frequency of 10 Hz and the drive trace indices described in paragraph 7. of Annex B7 shall be calculated and reported.

2.9. Gaseous sampling

Gaseous samples shall be collected in bags and the compounds analysed at the end of the test or a test phase, or the compounds may be analysed continuously and integrated over the cycle.

2.9.1. The following steps shall be taken prior to each test:

2.9.1.1. The purged, evacuated sample bags shall be connected to the dilute exhaust and dilution air sample collection systems.

2.9.1.2. Measuring instruments shall be started according to the instrument manufacturer's instructions.

2.9.1.3. The CVS heat exchanger (if installed) shall be pre-heated or pre-cooled to within its operating test temperature tolerance as specified in paragraph 3.3.5.1. of Annex B5.

2.9.1.4. Components such as sample lines, filters, chillers and pumps shall be heated or cooled as required until stabilised operating temperatures are reached.

2.9.1.5. CVS flow rates shall be set according to paragraph 3.3.4. of Annex B5, and sample flow rates shall be set to the appropriate levels.

2.9.1.6. Any electronic integrating device shall be zeroed and may be re-zeroed before the start of any cycle phase.

2.9.1.7. For all continuous gas analysers, the appropriate ranges shall be selected. These may be switched during a test only if switching is performed by changing the calibration over which the digital resolution of the instrument is applied. The gains of an analyser’s analogue operational amplifiers may not be switched during a test.

2.9.1.8. All continuous gas analysers shall be zeroed and calibrated using gases fulfilling the requirements of paragraph 6. of Annex B5.

2.10. Sampling for PM determination

2.10.1. The steps described in paragraphs 2.10.1.1. to 2.10.1.2.2. inclusive of this annex shall be taken prior to each test.

2.10.1.1. Filter selection

A single particulate sample filter without back-up shall be employed for the complete applicable WLTC. In order to accommodate regional cycle variations, a single filter may be employed for the first three phases and a separate filter for the fourth phase.

2.10.1.2. Filter preparation

2.10.1.2.1. At least 1 hour before the test, the filter shall be placed in a petri dish protecting against dust contamination and allowing air exchange, and placed in a weighing chamber (or room) for stabilization.

At the end of the stabilization period, the filter shall be weighed and its weight shall be recorded. The filter shall subsequently be stored in a closed petri dish or sealed filter holder until needed for testing. The filter shall be used within 8 hours of its removal from the weighing chamber (or room).

The filter shall be returned to the stabilization room within 1 hour after the test and shall be conditioned for at least 1 hour before weighing.

2.10.1.2.2. The particulate sample filter shall be carefully installed into the filter holder. The filter shall be handled only with forceps or tongs. Rough or abrasive filter handling will result in erroneous weight determination. The filter holder assembly shall be placed in a sample line through which there is no flow.

2.10.1.2.3. It is recommended that the microbalance be checked at the start of each weighing session, within 24 hours of the sample weighing, by weighing one reference item of approximately 100 mg. This item shall be weighed three times and the arithmetic average result recorded. If the arithmetic average result of the weighings is ±5 μg of the result from the previous weighing session, the weighing session and balance are considered valid.

2.11. PN sampling (if PN measurement is required)

2.11.1. The steps described in paragraphs 2.11.1.1. to 2.11.1.2. inclusive of this annex shall be taken prior to each test:

2.11.1.1. The particle specific dilution system and measurement equipment shall be started and made ready for sampling;

2.11.1.2. The correct function of the PNC and VPR elements of the particle sampling system shall be confirmed according to the procedures listed in paragraphs 2.11.1.2.1. to 2.11.1.2.4. inclusive of this annex.

2.11.1.2.1. A leak check, using a filter of appropriate performance attached to the inlet of the entire PN measurement system, VPR and PNC, shall report a measured concentration of less than 0.5 particles per cm³.

2.11.1.2.2. Each day, a zero check on the PNC, using a filter of appropriate performance at the PNC inlet, shall report a concentration of ≤ 0.2 particles per cm³. Upon removal of the filter, the PNC shall show an increase in measured concentration and a return to ≤ 0.2 particles per cm³ on replacement of the filter. The PNC shall not report any error.

2.11.1.2.3. It shall be confirmed that the measurement system indicates that the evaporation tube, where featured in the system, has reached its correct operating temperature.

2.11.1.2.4. It shall be confirmed that the measurement system indicates that the diluter PND1 has reached its correct operating temperature.

2.12. Sampling during the test

2.12.1. The dilution system, sample pumps and data collection system shall be started.

2.12.2. The PM and, if PN measurement is required, PN sampling systems shall be started.

2.12.3. Particle number, if PN measurement is required, shall be measured continuously. The arithmetic average concentration shall be determined by integrating the analyser signals over each phase.

2.12.4. Sampling shall begin before or at the initiation of the powertrain start procedure and end on conclusion of the cycle.

2.12.5. Sample switching

2.12.5.1. Gaseous emissions

Sampling from the diluted exhaust and dilution air shall be switched from one pair of sample bags to subsequent bag pairs, if necessary, at the end of each phase of the applicable WLTC to be driven.

2.12.5.2. Particulate

The requirements of paragraph 2.10.1.1. of this annex shall apply.

2.12.6. Dynamometer distance shall be recorded for each phase.

2.13. Ending the test

2.13.1. The engine shall be turned off immediately after the end of the last part of the test.

2.13.2. The constant volume sampler, CVS, or other suction device shall be turned off, or the exhaust tube from the tailpipe or tailpipes of the vehicle shall be disconnected.

2.13.3. The vehicle may be removed from the dynamometer.

2.14. Post-test procedures

2.14.1. Gas analyser check

Zero and calibration gas reading of the analysers used for continuous diluted measurement shall be checked. The test shall be considered acceptable if the difference between the pre-test and post-test results is less than 2 per cent of the calibration gas value.

2.14.2. Bag analysis

2.14.2.1. Exhaust gases and dilution air contained in the bags shall be analysed as soon as possible. Exhaust gases shall, in any event, be analysed not later than 30 minutes after the end of the cycle phase.

The gas reactivity time for compounds in the bag shall be taken into consideration.

2.14.2.2. As soon as practical prior to analysis, the analyser range to be used for each compound shall be set to zero with the appropriate zero gas.

2.14.2.3. The calibration curves of the analysers shall be set by means of calibration gases of nominal concentrations of 70 to 100 per cent of the range.

2.14.2.4. The zero settings of the analysers shall be subsequently rechecked: if any reading differs by more than 2 per cent of the range from that set in paragraph 2.14.2.2. of this annex, the procedure shall be repeated for that analyser.

2.14.2.5. The samples shall be subsequently analysed.

2.14.2.6. After the analysis, zero and calibration points shall be rechecked using the same gases. The test shall be considered acceptable if the difference is less than 2 per cent of the calibration gas value.

2.14.2.7. The flow rates and pressures of the various gases through analysers shall be the same as those used during calibration of the analysers.

2.14.2.8. The content of each of the compounds measured shall be recorded after stabilization of the measuring device.

2.14.2.9. The mass and number of all emissions, where applicable, shall be calculated according to Annex B7.

2.14.2.10. Calibrations and checks shall be performed either:

(a) Before and after each bag pair analysis; or

(b) Before and after the complete test.

In case (b), calibrations and checks shall be performed on all analysers for all ranges used during the test.

In both cases, (a) and (b), the same analyser range shall be used for the corresponding ambient air and exhaust bags.

2.14.3. Particulate sample filter weighing

2.14.3.1. The particulate sample filter shall be returned to the weighing chamber (or room) no later than 1 hour after completion of the test. It shall be conditioned in a petri dish, which is protected against dust contamination and allows air exchange, for at least 1 hour, and weighed. The gross weight of the filter shall be recorded.

2.14.3.2. At least two unused reference filters shall be weighed within 8 hours of, but preferably at the same time as, the sample filter weighings. Reference filters shall be of the same size and material as the sample filter.

2.14.3.3. If the specific weight of any reference filter changes by more than ±5 μg between sample filter weighings, the sample filter and reference filters shall be reconditioned in the weighing chamber (or room) and reweighed.

2.14.3.4. The comparison of reference filter weighings shall be made between the specific weights and the rolling arithmetic average of that reference filter's specific weights. The rolling arithmetic average shall be calculated from the specific weights collected in the period after the reference filters were placed in the weighing chamber (or room). The averaging period shall be at least one day but not more than 15 days.

2.14.3.5. Multiple reconditionings and reweighings of the sample and reference filters are permitted until a period of 80 hours has elapsed following the measurement of gases from the emissions test. If, prior to or at the 80-hour point, more than half the number of reference filters meet the ±5 μg criterion, the sample filter weighing may be considered valid. If, at the 80-hour point, two reference filters are employed and one filter fails the ±5 μg criterion, the sample filter weighing may be considered valid under the condition that the sum of the absolute differences between specific and rolling means from the two reference filters shall be less than or equal to 10 μg.

2.14.3.6. In the case that less than half of the reference filters meet the ±5 μg criterion, the sample filter shall be discarded, and the emissions test repeated. All reference filters shall be discarded and replaced within 48 hours. In all other cases, reference filters shall be replaced at least every 30 days and in such a manner that no sample filter is weighed without comparison to a reference filter that has been present in the weighing chamber (or room) for at least one day.

2.14.3.7. If the weighing chamber (or room) stability criteria outlined in paragraph 4.2.2.1. of Annex B5 are not met, but the reference filter weighings meet the above criteria, the vehicle manufacturer has the option of accepting the sample filter weights or voiding the tests, repairing the weighing chamber (or room) control system and re-running the test.

Annex B6 - Appendix 1

Emissions test procedure for all vehicles equipped with periodically regenerating systems

1. General

1.1. This appendix defines the specific provisions regarding testing a vehicle equipped with periodically regenerating systems as defined in paragraph 3.8.1. of this Regulation.

1.2. During cycles where regeneration occurs, emission standards need not apply. If a periodic regeneration occurs at least once per Type 1 test and has already occurred at least once during vehicle preparation or the distance between two successive periodic regenerations is more than 4,000 km of driving repeated Type 1 tests, it does not require a special test procedure. In this case, this appendix does not apply and a Ki factor of 1.0 shall be used.

1.3. The provisions of this appendix shall not apply to PN emissions.

1.4. At the request of the manufacturer, and with approval of the responsible authority, the test procedure specific to periodically regenerating systems need not apply to a regenerative device if the manufacturer provides data demonstrating that, during cycles where regeneration occurs, emissions remain below the emissions limits specified in paragraph 6.3.10. of this Regulation for the relevant vehicle category. In this case, a fixed Ki value of 1.05 shall be used for CO2 and fuel consumption.

2. Test procedure

The test vehicle shall be capable of inhibiting or permitting the regeneration process provided that this operation has no effect on original engine calibrations. Prevention of regeneration is only permitted during loading of the regeneration system and during the preconditioning cycles. It is not permitted during the measurement of emissions during the regeneration phase. The emission test shall be carried out with the unchanged, original equipment manufacturer's (OEM) control unit. At the request of the manufacturer and with agreement of the responsible authority, an "engineering control unit" which has no effect on original engine calibrations may be used during Ki determination.

2.1. Exhaust emissions measurement between two WLTCs with regeneration events

2.1.1. The arithmetic average emissions between regeneration events and during loading of the regenerative device shall be determined from the arithmetic mean of several approximately equidistant (if more than two) Type 1 tests. As an alternative, the manufacturer may provide data to show that the emissions remain constant (±15 per cent) on WLTCs between regeneration events. In this case, the emissions measured during the Type 1 test may be used. In any other case, emissions measurements for at least two Type 1 cycles shall be completed: one immediately after regeneration (before new loading) and one as close as possible prior to a regeneration phase. All emissions measurements shall be carried out according to this annex and all calculations shall be carried out according to paragraph 3. of this appendix.

2.1.2. The loading process and determination shall be made during the Type 1 driving cycle on a chassis dynamometer or on an engine test bench using an equivalent test cycle. These cycles may be run continuously (i.e. without the need to switch the engine off between cycles). After any number of completed cycles, the vehicle may be removed from the chassis dynamometer and the test continued at a later time.

For Class 2 and Class 3 vehicles, at the request of the manufacturer and with the agreement of the responsible authority the Ki can be determined either with or without the Extra High phase.

Upon request of the manufacturer and with approval of the responsible authority, a manufacturer may develop an alternative procedure and demonstrate its equivalency, including filter temperature, loading quantity and distance driven. This may be done on an engine bench or on a chassis dynamometer.

2.1.3. The number of cycles D between two WLTCs where regeneration events occur, the number of cycles over which emission measurements are made n and the mass emissions measurement for each compound i over each cycle j shall be recorded.

2.2. Measurement of emissions during regeneration events

2.2.1. Preparation of the vehicle, if required, for the emissions test during a regeneration phase, may be completed using the preconditioning cycles in paragraph 2.6. of this annex or equivalent engine test bench cycles, depending on the loading procedure chosen in paragraph 2.1.2. of this appendix.

2.2.2. The test and vehicle conditions for the Type 1 test described in this Regulation apply before the first valid emission test is carried out.

2.2.3. Regeneration shall not occur during the preparation of the vehicle. This may be ensured by one of the following methods:

(a) A "dummy" regenerating system or partial system may be fitted for the preconditioning cycles;

(b) Any other method agreed between the manufacturer and the responsible authority.

2.2.4. A cold start exhaust emissions test including a regeneration process shall be performed according to the applicable WLTC.

2.2.5. If the regeneration process requires more than one WLTC, each WLTC shall be completed. Use of a single particulate sample filter for multiple cycles required to complete regeneration is permissible.

If more than one WLTC is required, subsequent WLTC(s) shall be driven immediately, without switching the engine off, until complete regeneration has been achieved. In the case that the number of gaseous emission bags required for the multiple cycles would exceed the number of bags available, the time necessary to set up a new test shall be as short as possible. The engine shall not be switched off during this period.

2.2.6. The emission values during regeneration for each compound i shall be calculated according to paragraph 3. of this appendix. The number of applicable test cycles  measured for complete regeneration shall be recorded.

3. Calculations

3.1. Calculation of the exhaust and CO2 emissions, and fuel consumption of a single regenerative system

where for each compound i considered:

is the mass emissions of compound i over test cycle j without regeneration, g/km;

is the mass emissions of compound i over test cycle j during regeneration, g/km (if , the first WLTC test shall be run cold and subsequent cycles hot);

is the mean mass emissions of compound i without regeneration, g/km;

is the mean mass emissions of compound i during regeneration, g/km;

is the mean mass emissions of compound i, g/km;

is the number of test cycles, between cycles where regenerative events occur, during which emissions measurements on Type 1 WLTCs are made, and shall be ≥ 1;

is the number of complete applicable test cycles required for regeneration;

is the number of complete applicable test cycles between two cycles where regeneration events occur.

The calculation of is shown graphically in Figure A6.App1/1.

# Figure A6.App1/1

# Parameters measured during emissions test during and between cycles where regeneration occurs (schematic example, the emissions during D may increase or decrease)



3.1.1. Calculation of the regeneration factor for each compound i considered

The manufacturer may elect to determine for each compound independently either additive offsets or multiplicative factors.

factor:

offset:

, and results, and the manufacturer’s choice of type of factor shall be recorded. The Ki result shall be included in all relevant test reports. Msi, Mpi and Ki results shall be included in all relevant test sheets.

may be determined following the completion of a single regeneration sequence comprising measurements before, during and after regeneration events as shown in Figure A6.App1/1.

3.2. Calculation of exhaust and CO2 emissions, and fuel consumption of multiple periodically regenerating systems

The following shall be calculated for one Type 1 operation cycle for criteria emissions and for CO2 emissions. The CO2 emissions used for that calculation shall be from the result of step 3 described in Table A7/1 of Annex B7 and Table A8/5 of Annex B8.

for

factor:

offset:

where:

is the mean mass emissions of all events k of compound i without regeneration, g/km;

is the mean mass emissions of all events k of compound i during regeneration, g/km;

is the mean mass emission of all events k of compound i, g/km;

is the mean mass emissions of event k of compound i without regeneration, g/km;

is the mean mass emissions of event k of compound i during regeneration, g/km;

is the mass emissions of event k of compound i in g/km without regeneration measured at point j where , g/km;

is the mass emissions of event k of compound i during regeneration (when , the first Type 1 test is run cold, and subsequent cycles are hot) measured at test cycle j where , g/km;

is the number of complete test cycles of event k, between two cycles where regenerative phases occur, during which emissions measurements (Type 1 WLTCs or equivalent engine test bench cycles) are made, and shall be ≥ 1;

is the number of complete applicable test cycles of event k required for complete regeneration;


is the number of complete applicable test cycles of event k between two cycles where regenerative phases occur;

is the number of complete regeneration events.

The calculation of is shown graphically in Figure A6.App1/2.

# Figure A6.App1/2

# **Parameters measured during emissions test during and between cycles where regeneration occurs (schematic example)**



The calculation of for multiple periodically regenerating systems is only possible after a certain number of regeneration events for each system.

After performing the complete procedure (A to B, see Figure A6.App1/2), the original starting condition A should be reached again.

3.3. Ki factors and Ki offsets shall be rounded to four places of decimal. For Ki offsets, the rounding shall be based on the physical unit of the emission standard value.

Annex B6 - Appendix 2

Test procedure for rechargeable electric energy storage system monitoring

1. General

In the case that NOVC-HEVs, OVC-HEVs and NOVC-FCHVs are tested, Appendices 2 and 3 to Annex B8 shall apply.

This appendix defines the specific provisions regarding the correction of test results for CO2 emission as a function of the energy balance for all REESSs.

The corrected values for CO2 emission shall correspond to a zero energy balance (), and shall be calculated using a correction coefficient determined as defined below.

2. Measurement equipment and instrumentation

2.1. Current measurement

REESS depletion shall be defined as negative current.

2.1.1. The REESS current(s) shall be measured during the tests using a clamp-on or closed type current transducer. The current measurement system shall fulfil the requirements specified in Table A8/1. The current transducer(s) shall be capable of handling the peak currents at engine starts and temperature conditions at the point of measurement.

In order to have an accurate measurement, zero adjustment and degaussing shall be performed before the test according to the instrument manufacturer's instructions.

2.1.2. Current transducers shall be fitted to any of the REESS on one of the cables connected directly to the REESS and shall include the total REESS current.

In case of shielded wires, appropriate methods shall be applied in accordance with the responsible authority.

In order to easily measure REESS current using external measuring equipment, manufacturers should preferably integrate appropriate, safe and accessible connection points in the vehicle. If this is not feasible, the manufacturer shall support the responsible authority by providing the means to connect a current transducer to the REESS cables in the manner described above.

2.1.3. The measured current shall be integrated over time at a minimum frequency of 20 Hz, yielding the measured value of Q, expressed in ampere-hours Ah. The integration may be done in the current measurement system.

2.2. Vehicle on-board data

2.2.1. Alternatively, the REESS current shall be determined using vehicle-based data. In order to use this measurement method, the following information shall be accessible from the test vehicle:

(a) Integrated charging balance value since last ignition run in Ah;

(b) Integrated on-board data charging balance value calculated at a minimum sample frequency of 5 Hz;

(c) The charging balance value via an OBD connector as described in SAE J1962.

2.2.2. The accuracy of the vehicle on-board REESS charging and discharging data shall be demonstrated by the manufacturer to the responsible authority.

The manufacturer may create a REESS monitoring vehicle family to prove that the vehicle on-board REESS charging and discharging data are correct. The accuracy of the data shall be demonstrated on a representative vehicle.

The following family criteria shall be valid:

(a) Identical combustion processes (i.e. positive ignition, compression ignition, two-stroke, four-stroke);

(b) Identical charge and/or recuperation strategy (software REESS data module);

(c) On-board data availability;

(d) Identical charging balance measured by REESS data module;

(e) Identical on-board charging balance simulation.

2.2.3. All REESS having no influence on CO2 emissions shall be excluded from monitoring.

3. REESS energy change-based correction procedure

3.1. Measurement of the REESS current shall start at the same time as the test starts and shall end immediately after the vehicle has driven the complete driving cycle.

3.2. The electricity balance Q measured in the electric power supply system shall be used as a measure of the difference in the REESS energy content at the end of the cycle compared to the beginning of the cycle. The electricity balance shall be determined for the total driven WLTC.

3.3. Separate values of shall be logged over the driven cycle phases.

3.4. Correction of CO2 emission over the whole cycle

3.4.1. (Reserved)

3.4.2. The correction shall be applied if is negative (corresponding to REESS discharging)

At the request of the manufacturer, the correction may be omitted and uncorrected values may be used if:

(a) is positive (corresponding to REESS charging);

(b) the manufacturer can prove to the responsible authority by measurement that there is no relation between and mass emission and between and fuel consumption.

Table A6.App2/1

**Energy content of fuel (as applicable)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Fuel | Petrol (E10H) | Ethanol (E85) | Diesel (B5H) | LPG | CNG |
| Heat value | 8.64 kWh/l | 6.41 kWh/l | 9.80 kWh/l | 12.86 x ρ kWh/l | 11.39 kWh/m³ |

ρ = test fuel density at 15°C (kg/l)

4. Applying the correction function

4.1. To apply the correction function, the electric energy change of a period j of all REESSs shall be calculated from the measured current and the nominal voltage:

where:

is the electric energy change of REESS i during the considered period j, Wh;

and:

where:

is the nominal REESS voltage determined according to IEC 60050-482, V;

is the electric current of REESS i during the considered period j, determined according to paragraph 2. of this appendix, A;

is the time at the beginning of the considered period j, s;

is the time at the end of the considered period j, s.

i is the index number of the considered REESS;

n is the total amount of REESS;

j is the index number for the considered period, where a period shall be any applicable cycle phase, combination of cycle phases and the applicable total cycle;

is the conversion factor from Ws to Wh.

4.2. For correction of CO2 emission, g/km, combustion process-specific Willans factors from Table A6.App2/3 shall be used.

4.3. The correction shall be performed and applied for the total cycle and for each of its cycle phases separately, and shall be recorded.

4.4. For this specific calculation, a fixed electric power supply system alternator efficiency shall be used:

4.5. The resulting CO2 emission difference for the considered period j due to load behaviour of the alternator for charging a REESS shall be calculated using the following equation:

where:

is the resulting mass emission difference of period j, g/km;

is the REESS energy change of the considered period j calculated according to paragraph 4.1. of this appendix, Wh;

is the driven distance of the considered period j, km;

j is the index number for the considered period, where a period shall be any applicable cycle phase, combination of cycle phases and the applicable total cycle;

0.0036 is the conversion factor from Wh to MJ;

is the efficiency of the alternator according to paragraph 4.4. of this appendix;

is the combustion process-specific Willans factor as defined in Table A6.App2/3, gCO2/MJ;

4.5.1. The CO2 values of each phase and the total cycle shall be corrected as follows:

MCO2,p,3 = (MCO2,p,1 - ΔMCO2,j)

MCO2,c,3 = (MCO2,c,2 - ΔMCO2,j)

where:

ΔMCO2,j is the result from paragraph 4.5. of this appendix for a period j, g/km.

4.6. For the correction of CO2 emission, g/km, the Willans factors in Table A6.App2/3 shall be used.

Table A6.App2/3

**Willans factors (as applicable)**

|  | | | *Naturally aspirated* | *Pressure-charged* |
| --- | --- | --- | --- | --- |
| Positive ignition | Petrol (E10H) | l/MJ | 0.0756 | 0.0803 |
| gCO2/MJ | 174 | 184 |
| CNG (G20) | m³/MJ | 0.0719 | 0.0764 |
|  | gCO2/MJ | 129 | 137 |
| LPG | l/MJ | 0.0950 | 0.101 |
| gCO2/MJ | 155 | 164 |
| E85 | l/MJ | 0.102 | 0.108 |
| gCO2/MJ | 169 | 179 |
| Compression ignition | Diesel (B5H) | l/MJ | 0.0611 | 0.0611 |
| gCO2/MJ | 161 | 161 |

Annex B6 - Appendix 3

Calculation of gas energy ratio for gaseous fuels (LPG and NG/biomethane)

1. Measurement of the mass of gaseous fuel consumed during the Type 1 test cycle

Measurement of the mass of gas consumed during the cycle shall be done by a fuel weighing system capable of measuring the weight of the storage container during the test in accordance with the following:

(a) An accuracy of ±2 per cent of the difference between the readings at the beginning and at the end of the test or better.

(b) Precautions shall be taken to avoid measurement errors.

Such precautions shall at least include the careful installation of the device according to the instrument manufacturer's recommendations and to good engineering practice.

(c) Other measurement methods are permitted if an equivalent accuracy can be demonstrated.

2. Calculation of the gas energy ratio

The fuel consumption value shall be calculated from the emissions of hydrocarbons, carbon monoxide, and carbon dioxide determined from the measurement results assuming that only the gaseous fuel is burned during the test.

The gas ratio of the energy consumed in the cycle shall be determined using the following equation:

where:

Ggasis the gas energy ratio, per cent;

Mgasis the mass of the gaseous fuel consumed during the cycle, kg;

FCnorm is the fuel consumption (l/100km for LPG, m3/100 km for NG/biomethane) calculated in accordance with paragraphs 6.6. and 6.7. of Annex B7;

dist is the distance recorded during the cycle, km;

ρ is the gas density:

ρ = 0.654 kg/m3 for NG/Biomethane**;**

ρ = 0.538 kg/litre for LPG;

cf is the correction factor, assuming the following values:

cf = 1 in the case of LPG or G20 reference fuel;

cf = 0.78 in the case of G25 reference fuel.

**Annex B6a**

Ambient Temperature Correction Test for the determination of CO2 emissions under representative regional temperature conditions

This annex is only applicable for the CO2 emissions from the 4 phases of a WLTP test;

1. Introduction

This annex describes the supplemental Ambient Temperature Correction Test (ATCT) procedure to determine the CO2 emissions under representative regional temperature conditions.

1.1. The CO2 emissions of ICE vehicles, NOVC-HEVs and the charge sustaining value of OVC-HEVs shall be corrected in accordance with the requirements of this annex. No correction is required for the CO2 value of the charge depleting test. No correction is required for an Electric Range.

1.2. In order to ensure statistical representativity, at the request of the manufacturer, all tests from which results are used in the calculations described in this Annex B6a can be repeated up to a maximum of 3 times and the arithmetic average of results used in the context of this Annex B6a. Where the tests have been performed only for the purpose of determining the FCF and without prejudice to paragraph 3.7.3. of this Annex B6a, the results of the additional tests shall not be taken into account for any other purposes.

2. Ambient Temperature Correction Test (ATCT) Family

2.1. Only vehicles which are identical with respect to all the following characteristics are permitted to be part of the same ATCT Family:

(a) Powertrain architecture (i.e. internal combustion, hybrid, fuel cell, or electric);

(b) Combustion process (i.e. two stroke or four stroke);

(c) Number and arrangement of cylinders;

(d) Method of engine combustion (i.e. indirect or direct injection);

(e) Type of cooling system (i.e. air, water, or oil);

(f) Method of aspiration (i.e. naturally aspirated, or charged);

(g) Fuel for which the engine is designed (i.e. petrol, diesel, NG, LPG, etc.);

(h) Catalytic converter (i.e. three-way catalyst, lean NOx trap, SCR, lean NOx catalyst or other(s));

(i) Whether or not a particulate trap is installed; and

(j) Exhaust gas recirculation (with or without, cooled or non-cooled).

In addition the vehicles shall be similar with respect to the following characteristics:

(k) The vehicles shall have a variation in engine cylinder capacity of no more than 30 per cent of the vehicle with the lowest capacity; and

(l) Engine compartment insulation shall be of a similar type regarding material, amount and location of the insulation. Manufacturers shall provide evidence (e.g. by CAD drawings) to the approval authority that for all vehicles in the family, the volume and weight of the insulation material which will be installed is greater than 90 per cent of that of the ATCT measured reference vehicle.

Difference in insulation material and location may also be accepted to be part of a single ATCT family under the condition that the test vehicle can be demonstrated as being the worst case with regards to engine compartment insulation.

If the manufacturer can demonstrate to the Type Approval Authority that it is ensured that the worst case concept is maintained (e.g. tested vehicle has no insulation), or if the ATCT is composed of a single Interpolation Family, the requirements to document the insulation materials may be waived.

2.1.1. If active heat storage devices are installed, only vehicles that meet the following requirements shall be considered to be part of the same ATCT Family:

(a) The heat capacity, defined by the enthalpy stored in the system, is within a range of 0 to 10 per cent above the enthalpy of the test vehicle; and

(b) The OEM can provide evidence to the technical service that the time for heat release at engine start within a family is within a range of 0 to 10 per cent below the time for the heat release of the test vehicle.

2.1.2. Only vehicles that meet the criteria set out in paragraph 3.9.4. of this Annex B6a shall be considered to be part of the same ATCT Family.

3. ATCT Procedure

The Type 1 test specified in Annex B6 shall be carried out with the exception of the requirements specified in paragraphs 3.1. to 3.9. of this Annex B6a. That also requires a new calculation and application of gearshift points in accordance with Annex B2 taking into account the different road load as specified in paragraph 3.4. of this Annex B6a.

3.1. Ambient conditions for ATCT

3.1.1. The temperature (Treg) at which the vehicle should be soaked and tested for the ATCT shall be 14 °C.

3.1.2. The minimum soaking time (tsoak\_ATCT) for the ATCT shall be 9 hours.

3.2. Test cell and soak area

3.2.1. Test cell

3.2.1.1. The test cell shall have a temperature set point equal to Treg. The actual temperature value shall be within ± 3 °C at the start of the test and within ± 5 °C during the test.

3.2.1.2. The specific humidity (H) of either the air in the test cell or the intake air of the engine shall be such that:

3.0 ≤ H ≤ 8.1  (g H2O/kg dry air)

3.2.1.3. The air temperature and humidity shall be measured at the cooling fan outlet at a rate of 0.1 Hz.

3.2.2. Soak area

3.2.2.1. The soak area shall have a temperature set point equal to Treg and the actual temperature value shall be within ± 3 °C on a 5 minute running arithmetic average and shall not show a systematic deviation from the set point. The temperature shall be measured continuously at a minimum frequency of 0.033 Hz.

3.2.2.2. The location of the temperature sensor for the soak area shall be representative to measure the ambient temperature around the vehicle and shall be checked by the technical service.

The sensor shall be at least 10 cm away from the wall of the soak area and shall be shielded from direct air flow.

The air-flow conditions within the soak room in the vicinity of the vehicle shall represent a natural convection flow representative for the dimension of the room (no forced convection).

3.3. Test vehicle

3.3.1. The vehicle to be tested shall be representative of the family for which the ATCT data are determined (as described in paragraph 2.1. of this Annex B6a).

3.3.2. From the ATCT Family, the Interpolation Family with the lowest engine capacity shall be selected (see paragraph 2 of this Annex B6a), and the test vehicle shall be in the ‘vehicle H’ configuration of this family.

3.3.3. Where applicable, the vehicle with the lowest enthalpy of the active heat storage device and the slowest heat release for the active heat storage device from the ATCT Family shall be selected.

3.3.4. The test vehicle shall meet the requirements detailed in paragraph 2.3. of Annex B6 and paragraph 2.1. of this Annex B6a.

3.4. Settings

3.4.1. Road load and dynamometer settings shall be as specified in Annex B4, including the requirement for the room temperature to be at 23 oC.

To take account of the difference in air density at 14 oC when compared to the air density at 20 oC, the chassis dynamometer shall be set as specified in paragraphs 7. and 8. of Annex B4 with the exception that f2\_TReg from the following equationshall be used as the target coefficient Ct.

f2\_TReg = f2 \* (Tref + 273)/(Treg + 273)

where:

f2 is the second order road load coefficient, at reference conditions, N/(km/h)2;

Tref is the road load reference temperature as specified in paragraph 3.2.10. of this Regulation, C;

Treg is the regional temperature, as defined in paragraph 3.1.1. of this Annex B6a, C.

In the case that a valid chassis dynamometer setting of the 23 °C test is available, the second order chassis dynamometer coefficient of Cd shall be adapted in accordance with the following equation:

Cd\_Treg = Cd + (f2\_TReg – f2)

3.4.2. The ATCT test and its road load setting shall be performed on a 2WD dynamometer in the case that the corresponding Type 1 test was done on a 2WD dynamometer; and it shall be performed on a 4WD dynamometer in the case that the corresponding Type 1 test was done on a 4WD dynamometer.

3.5. Preconditioning

At the request of the manufacturer preconditioning may be undertaken at Treg.

The engine temperature shall be within ± 2 °C of the set point of 23 °C or Treg, whichever temperature is chosen for the preconditioning.

3.5.1. Pure ICE vehicles shall be preconditioned as described in paragraph 2.6. of Annex B6.

3.5.2. NOVC-HEVs shall be preconditioned as described in paragraph 3.3.1.1. of Annex B8.

3.5.3. OVC-HEVs shall be preconditioned as described in paragraph 2.1.1. or 2.1.2. of Appendix 4 to Annex B8.

3.6. Soak procedure

3.6.1. After preconditioning and before testing, vehicles shall be kept in a soak area with the ambient conditions described in paragraph 3.2.2. of this Annex B6a.

3.6.2. From the end of the preconditioning until the soaking at *Treg*, the vehicle shall not be exposed to a different temperature than *Treg* for longer than 10 minutes.

3.6.3. The vehicle shall then be kept in the soak area such that the time from the end of the preconditioning test to the beginning of the ATCT test is equal to tsoak\_ATCT with a tolerance of an additional 15 minutes. At the request of the manufacturer, and upon approval of the approval authority, tsoak\_ATCT can be extended by up to 120 minutes. In this case, the extended time shall be used for the cool down specified in paragraph 3.9. of this Annex B6a.

3.6.4. The soak shall be performed without using a cooling fan and with all body parts positioned as intended under normal parking operation. The time between the end of the preconditioning and the start of the ATCT test shall be recorded.

3.6.5. The transfer from the soak area to the test cell shall be undertaken as quickly as possible. The vehicle shall not be exposed to a temperature different from Treg for longer than 10 minutes.

3.7. ATCT Test

3.7.1. The test cycle shall be the applicable WLTC specified in Annex B1 for that class of vehicle.

3.7.2. The procedures for undertaking the emissions test as specified in Annex B6 for pure ICE vehicles and in Annex B8 for NOVC-HEVs and for the charge-sustaining Type 1 test of OVC-HEVs shall be followed, with the exception that the ambient conditions for the test cell shall be those as described in paragraph 3.2.1. of this Annex B6a.

3.7.3. In particular, the tailpipe emissions defined by Table A7/1 Step no.2 for pure ICE vehicles and Table A8/5 Step no.2 for HEVs at an ATCT test shall not exceed the emission limits applicable to the vehicle tested defined in paragraph 6.3.10. of this Regulation.

3.8. Calculation and Documentation

3.8.1. The family correction factor, *FCF*, shall be calculated as follows:

*FCF = MCO2,Treg / MCO2,23°*

where

*MCO2,23°* is the CO2 emission of the average of all applicable Type 1 tests at 23 °C of vehicle H, after Step 3 of Table A7/1 of Annex B7 for pure ICE vehicles and after Step 3 of Table A8/5 of Annex B8 for OVC-HEVs and NOVC-HEVs, but without any further corrections, g/km;

*MCO2,Treg* is the CO2 emission over the complete WLTC cycle of the test at regional temperature after Step 3 of Table A7/1 of Annex B7 for pure ICE vehicles and after Step 3 of Table A8/5 of Annex B8 for OVC-HEVs and NOVC-HEVs but without any further corrections, g/km. For OVC-HEVs and NOVC-HEVs, the KCO2 factor as defined in Appendix 2 to Annex B8 shall be used.

Both MCO2,23° and MCO2,Treg shall be measured on the same test vehicle.

The *FCF* shall be included in all relevant test reports.

The *FCF* shall be rounded to 4 points of decimal.

3.8.2. The CO2 values for each pure ICE vehicle within the ATCT Family (as defined in paragraph 2.3. of this Annex B6a) shall be calculated using the following equations:

*MCO2,c,5 = MCO2,c,4 × FCF*

*MCO2,p,5 = MCO2,p,4 × FCF*

where

*MCO2,c,4* and *MCO2,p,4* are the CO2 emissions over the complete WLTC, c, and the cycle phases, p, resulting from the previous calculation step, g/km;

*MCO2,c,5* and *MCO2,p,5* are the CO2 emissions over the complete WLTC, c, and the cycle phases, p, including the ATCT correction, and shall be used for any further corrections or any further calculations, g/km;

3.8.3. The CO2 values for each OVC-HEV and NOVC-HEV within the ATCT Family (as defined in paragraph 2.3. of this Annex B6a) shall be calculated using the following equations:

*MCO2,CS,c,5 = MCO2,CS,c,4 × FCF*

*MCO2,CS,p,5 = MCO2,CS,p,4 × FCF*

where

*MCO2,CS,c,4* and *MCO2,CS,p,4* are the CO2 emissions over the complete WLTC, c, and the cycle phases, p, resulting from the previous calculation step, g/km;

*MCO2,CS,c,5* and *MCO2,CS,p,5* are the CO2 emissions over the complete WLTC, c, and the cycle phases, p, including the ATCT correction, and shall be used for any further corrections or any further calculations, g/km.

3.8.4. If a *FCF* is less than one, it is deemed to be equal to one, in the case of the worstcase approach, in accordance with paragraph 4.1 of this Annex B6a.

3.9. Provision for cool down

3.9.1. For the test vehicle serving as a reference vehicle for the ATCT Family and all vehicles H of the interpolation families within the ATCT Family, the end temperature of the engine coolant shall be measured after soaking at 23 °C for the duration of tsoak\_ATCT, with a tolerance of an additional 15 minutes, having beforehand driven the respective Type 1 test at 23 °C. The duration is measured from the end of that respective Type 1 test.

3.9.1.1. In the case that tsoak\_ATCT was extended inthe respective ATCT test, the same soaking time shall be used, with a tolerance of an additional 15 minutes.

3.9.2. The cool down procedure shall be undertaken as soon as possible after the end of the Type 1 test, with a maximum delay of 20 minutes. The measured soaking time is the time between the measurement of the end temperature and the end of the Type 1 test at 23 °C, and shall be included in all relevant test sheets.

3.9.3. The average temperature of the soak area of the last 3 hours shall be subtracted from the measured temperature of the engine coolant at the end of the soaking time specified in paragraph 3.9.1. This is referred to as ∆T\_ATCT, rounded to the nearest whole number.

3.9.4. If ∆T\_ATCT is higher or equal than -2 °C from the test vehicle ∆T\_ATCT, this Interpolation Family shall be considered to be a member of the same ATCT Family.

3.9.5. For all vehicles within an ATCT Family the coolant shall be measured at the same location in the cooling system. That location shall be as close as possible to the engine so that the coolant temperature is as representative as possible to the engine temperature.

3.9.6. The measurement of the temperature of the soak areas shall be as specified in paragraph 3.2.2.2. of this Annex B6a.

4. Alternatives in the measurement process

4.1. Worst case approach vehicle cool down or with regards to vehicle insulation

On request by the manufacturer and with approval by the approval authority, the Type 1 test procedure for cool down may be applied instead of provisions of paragraph 3.6 of this Annex B6a. For that purpose:

(a) The provisions of paragraph 2.7.2. of Annex B6 shall apply with the additional requirement of a minimum soak time of 9 hours.

(b) The engine temperature shall be within ± 2 °C of the set point Treg before the start of the ATCT test. That temperature shall be included in all relevant test sheets. In this case, the provision for cool down described in paragraph 3.9. of this Annex B6a and the criteria on engine compartment insulationcan be skipped for all vehicles in the family.

This alternative is not allowed if the vehicle is equipped with an active heat storage device.

The application of that approach shall be included in all relevant test reports.

The requirements to document the insulation materials may be waived.

4.2. ATCT family composed of a single Interpolation family

In the case, that the ATCT family consists of only one interpolation family, the provision for cool down described in paragraph 3.9. of this Annex B6a can be skipped. This shall be included in all relevant test reports.

4.3. Alternative engine temperature measurement

In the case that measuring the coolant temperature is not feasible, on request of the manufacturer and with approval of the approval authority, instead of using the coolant temperature for the provision for cool down described in paragraph 3.9. of this Annex B6a, the engine oil temperature may be used. In that case, for all vehicles within the family the engine oil temperature shall be used.

The application of that procedure shall be included in all relevant test reports.

Annex B7

Calculations

1. General requirements

1.1. Unless explicitly stated otherwise in Annex B8, all requirements and procedures specified in this annex shall apply for NOVC-HEVs, OVC-HEVs, NOVC-FCHVs and PEVs.

1.2. The calculation steps described in paragraph 1.4. of this annex shall be used for pure ICE vehicles only.

1.3. Rounding of test results

1.3.1. Intermediate steps in the calculations shall not be rounded unless intermediate rounding is required.

1.3.2. The final criteria emission results shall be rounded according to paragraph 6.1.8. of this Regulation in one step to the number of places to the right of the decimal point indicated by the applicable emission standard plus one additional significant figure.

1.3.3. The NOx correction factor shall be reported rounded according to paragraph 6.1.8. of this Regulation to two places of decimal.

1.3.4. The dilution factor shall be reported rounded according to paragraph 6.1.8. of this Regulation to two places of decimal.

1.3.5. For information not related to standards, good engineering judgement shall be used.

1.4. Stepwise procedure for calculating the final test results for vehicles using combustion engines

The results shall be calculated in the order described in Table A7/1. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

For the purpose of this table, the following nomenclature within the equations and results is used:

c complete applicable cycle (to be calculated both for results after 3-phases and for results after 4-phases);

p every applicable cycle phase;

i every applicable criteria emission component, without CO2;

CO2 CO2 emission.

Table A7/1

**Procedure for calculating final test results (FE applicable for the 3-phase WLTP only)**

Table A7/1 shall be performed separately for results after 4 phases and for results after 3 phases.

| *Step No.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Annex B6 | Raw test results | Mass emissions  Paragraphs 3. to 3.2.2. inclusive of this annex. | Mi,p,1, g/km;  MCO2,p,1, g/km. |
| 2 | Output step 1 | Mi,p,1, g/km;  MCO2,p,1, g/km. | Calculation of combined cycle values:  where:  Mi/CO2,c,2 are the emission results over the total cycle;  dp are the driven distances of the cycle phases, p. | Mi,c,2, g/km;  MCO2,c,2, g/km. |
| 3 | Output step 1  Output step 2 | MCO2,p,1, g/km;  MCO2,c,2, g/km. | RCB correction  Appendix 2 to Annex B6. | MCO2,p,3, g/km;  MCO2,c,3, g/km. |
| 4a | Output step 2  Output step 3 | Mi,c,2, g/km;  MCO2,c,3, g/km. | Emissions test procedure for all vehicles equipped with periodically regenerating systems, Ki.  Annex B6, Appendix 1.  Mi,c,4a = Ki × Mi,c,2  or  Mi,c,4a = Ki + Mi,c,2  and  MCO2,c,4a = KCO2 × MCO2,c,3  or  MCO2,c,4a = KCO2 + MCO2,c,3  Additive offset or multiplicative factor to be used according to Ki determination.  If Ki is not applicable:  Mi,c,4a = Mi,c,2  MCO2,c,4a = MCO2,c,3 | Mi,c,4a, g/km;  MCO2,c,4a, g/km. |
| 4b | Output step 3  Output step 4a | MCO2,p,3, g/km;  MCO2,c,3, g/km;  MCO2,c,4a, g/km. | If Ki is applicable, align CO2 phase values to the combined cycle value:  for every cycle phase p;  where:  If Ki is not applicable:  MCO2,p,4 = MCO2,p,3 | MCO2,p,4, g/km. |
| 4c | Output step 4a | Mi,c,4a, g/km;  MCO2,c,4a, g/km. | Mi,c,4c = Mi,c,4a  MCO2,c,4c = MCO2,c,4a | Mi,c,4c;  MCO2,c,4c |
| Calculate fuel efficiency (FEc,4c\_temp)　according to paragraph 6. of Annex B7.  FEc,4c = FEc,4c\_temp | FEc,4c, km/l; |
| 5  Result of a single test. | Output step 4b and 4c | MCO2,c,4c, g/km;  MCO2,p,4, g/km. | For results after 4 phases:  ATCT correction of MCO2,c,4c and MCO2,p,4 in accordance with paragraph 3.8.2. of Annex B6a.  For results after 3 phases:  MCO2,c,5 = MCO2,c,4c  MCO2,p,5 = MCO2,p,4 | MCO2,c,5, g/km;  MCO2,p,5, g/km. |
| Mi,c,4c, g/km;  FEc,4c, km/l; | Apply deterioration factors calculated in accordance with Annex C4 to the criteria emissions values.  FEc,5=FEc,4c | Mi,c,5, g/km;  FEc,5, km/l; |
| 6 | For results after 4 phases  Output step 5 | For every test:  Mi,c,5, g/km;  MCO2,c,5, g/km;  MCO2,p,5, g/km. | Averaging of tests and declared value.  Paragraphs 1.2. to 1.2.3. inclusive of Annex B6. | Mi,c,6, g/km;  MCO2,c,6, g/km;  MCO2,p,6, g/km.  MCO2,c,declared, g/km. |
| For results after 3 phases  Output step 5 | FEc,5, km/l;  Mi,c,5, g/km | Averaging of tests and declared value.  Paragraphs 1.2. to 1.2.3. inclusive of Annex B6.  Mi,c,5 = Mi,c,6  The conversion from FEc,declared to MCO2,c,declared shall be performed for the applicable cycle according to paragraph 6. of Annex B7. For that purpose, the criteria emission over the applicable cycle shall be used. | FEc,declared, km/l  FEc,6, km/l  Mi,c,6  MCO2,c,declared, g/km. |
| 7 | For results after 4 phases:  Output step 6 | MCO2,c,6, g/km;  MCO2,p,6, g/km.  MCO2,c,declared, g/km. | Alignment of phase values according to  paragraph 1.2.4. of Annex B6.  and:  MCO2,c,7 = MCO2,c,declared | MCO2,c,7, g/km;  MCO2,p,7, g/km. |
| For results after 3 phases:  Output step 5  Output step 6 | MCO2,c,5, g/km;  MCO2,p,5, g/km;  MCO2,c,declared, g/km. | Alignment of phase values according to paragraph 1.2.4. of Annex B6. | MCO2,p,7, g/km. |
| 8  Result of a Type 1 test for a test vehicle. | For results after 4 phases :  Output steps 6  Output steps 7 | Mi,c,6, g/km;  MCO2,c,7, g/km;  MCO2,p,7, g/km. | Calculation of fuel consumption according to Paragraph 6 of this annex.  The calculation of fuel consumption shall be performed for the applicable cycle and its phases separately. For that purpose:  (a) the applicable phase or cycle CO2 values shall be used;  (b) the criteria emission over the complete cycle shall be used.  and:  Mi,c,8 = Mi,c,6  MCO2,c,8 = MCO2,c,7  MCO2,p,8 = MCO2,p,7 | FCc,8, l/100 km;  FCp,8, l/100 km;  Mi,c,8, g/km;  MCO2,c,8, g/km;  MCO2,p,8, g/km. |
|  | For results after 3 phases :  Output steps 6  Output steps 7 | Mi,c,6, g/km;  FEc,6, km/l  MCO2,p,7, g/km. | Calculation of fuel consumption and conversion to fuel efficiency for phase value only according to paragraph 6 of this annex.  The calculation of fuel consumption shall be performed for the phases separately. For that purpose:  (a) the applicable phase CO2 values shall be used;  (b) the criteria emission over the complete cycle shall be used.  and:  Mi,c,8 = Mi,c,6  FEc,8 = FEc,6 | FCp,8, l/100 km;  FEp,8, km/l;  Mi,c,8, g/km;  FEc,8, km/l. |
| 9  For results after 4 phases  Final criteria emission result | Output step 8 | For each of the test vehicles H and L:  Mi,c,8, g/km;  MCO2,c,8, g/km;  MCO2,p,8, g/km;  FCc,8, l/100 km;  FCp,8, l/100 km;  FEc,8, km/l.  FEp,8, km/l | For results after 4 phases;  If in addition to a test vehicle H a test vehicle M and/ or vehicle L was also tested, the resulting criteria emission value shall be the highest of the two or, in case vehicle M does not meet the linearity criterion three values and referred to as Mi,c.  In the case of the combined THC + NOx emissions, the highest value of the sum referring to either the vehicle H or vehicle L or, if applicable, vehicle M is to be taken as the type approval value.  Otherwise, if no vehicle L was tested,  Mi,c = Mi,c,8  For CO2, FE and FC, the values derived in step 8 shall be used, and CO2 values shall be rounded according to paragraph 6.1.8. of this Regulation to two places of decimal, and FE and FC values shall be rounded according to paragraph 6.1.8. of this Regulation to three places of decimal. | Mi,c, g/km;  MCO2,c,H, g/km;  MCO2,p,H, g/km;  FCc,H, l/100 km;  FCp,H, l/100 km;  FEc,H, km/l;  FEp,H, km/l;  and if a vehicle L was tested:  MCO2,c,L, g/km;  MCO2,p,L, g/km;  FCc,L, l/100 km;  FCp,L, l/100 km;  FEc,L, km/l;  FEp,L, km/l. |
| 10  Result of an individual vehicle.  Final CO2, FE and FC result. | Output step 9 | MCO2,c,H, g/km;  MCO2,p,H, g/km;  FCc,H, l/100 km;  FCp,H, l/100 km;  FEc,H, km/l;  FEp,H, km/l;  and if a vehicle L was tested:  MCO2,c,L, g/km;  MCO2,p,L, g/km;  FCc,L, l/100 km;  FCp,L, l/100 km.  FEc,L, km/l;  FEp,L, km/l. | Fuel consumption, fuel efficiency and CO2 calculations for individual vehicles in an interpolation family.  Paragraph 3.2.3. of this annex.  Fuel consumption, fuel efficiency and CO2 calculations for individual vehicles in a road load matrix family  Paragraph 3.2.4. of this annex.  CO2 emissions shall be expressed in grams per kilometre (g/km) rounded to the nearest whole number;  FC values shall be rounded according to paragraph 6.1.8. of this Regulation to one place of decimal, expressed in (l/100 km) ;  FE values shall be rounded according to paragraph 6.1.8. of this Regulation to one place of decimal, expressed in (km/l). | MCO2,c,ind g/km;  MCO2,p,ind, g/km;  FCc,ind l/100 km;  FCp,ind, l/100 km  FEc,ind, km/l.  FEp,ind, km/l |

2. Determination of diluted exhaust gas volume

2.1. Volume calculation for a variable dilution device capable of operating at a constant or variable flow rate

The volumetric flow shall be measured continuously. The total volume shall be measured for the duration of the test.

2.2. Volume calculation for a variable dilution device using a positive displacement pump

2.2.1. The volume shall be calculated using the following equation:

where:

is the volume of the diluted gas, in litres per test (prior to correction);

is the volume of gas delivered by the positive displacement pump in testing conditions, litres per pump revolution;

is the number of revolutions per test.

2.2.1.1. Correcting the volume to standard conditions

The diluted exhaust gas volume, V, shall be corrected to standard conditions according to the following equation:

where:

is the test room barometric pressure, kPa;

is the vacuum at the inlet of the positive displacement pump relative to the ambient barometric pressure, kPa;

is the arithmetic average temperature of the diluted exhaust gas entering the positive displacement pump during the test, Kelvin (K).

3. Mass emissions

3.1. General requirements (as applicable)

3.1.1. Assuming no compressibility effects, all gases involved in the engine's intake, combustion and exhaust processes may be considered to be ideal according to Avogadro’s hypothesis.

3.1.2. The mass of gaseous compounds emitted by the vehicle during the test shall be determined by the product of the volumetric concentration of the gas in question and the volume of the diluted exhaust gas with due regard for the following densities under the reference conditions of 273.15 K (0 °C) and 101.325 kPa:

Carbon monoxide (CO)  g/l

Carbon dioxide (CO2)  g/l

Hydrocarbons:

for petrol (E10H) (C1H1.93 O0.033)  g/l

for diesel (B5H) (C1H1.86O0.005)  g/l

for LPG (C1H2.525)  g/l

for NG/biomethane (CH4)  g/l

for ethanol (E85) (C1H2.74O0.385)  g/l

Nitrogen oxides (NOx)  g/1

The density for NMHC mass calculations shall be equal to that of total hydrocarbons at 273.15 K (0 °C) and 101.325 kPa, and is fuel-dependent. The density for propane mass calculations (see paragraph 3.5. of Annex B5) is 1.967 g/l at standard conditions.

If a fuel type is not listed in this paragraph, the density of that fuel shall be calculated using the equation given in paragraph 3.1.3. of this annex.

3.1.3. The general equation for the calculation of total hydrocarbon density for each reference fuel with a mean composition of CXHYOZ is as follows:

where:

ρTHC is the density of total hydrocarbons and non-methane hydrocarbons, g/l;

MWC is the molar mass of carbon (12.011 g/mol);

MWH is the molar mass of hydrogen (1.008 g/mol);

MWO is the molar mass of oxygen (15.999 g/mol);

VM is the molar volume of an ideal gas at 273.15 K (0° C) and 101.325 kPa (22.413 l/mol);

H/C is the hydrogen to carbon ratio for a specific fuel CXHYOZ;

O/C is the oxygen to carbon ratio for a specific fuel CXHYOZ.

3.2. Mass emissions calculation

3.2.1. Mass emissions of gaseous compounds per cycle phase shall be calculated using the following equations:

where:

is the mass emission of compound i per test or phase, g/km;

is the volume of the diluted exhaust gas per test or phase expressed in litres per test/phase and corrected to standard conditions (273.15 K

(0 °C) and 101.325 kPa);

is the density of compound i in grams per litre at standard temperature and pressure (273.15 K (0 °C) and 101.325 kPa);

is a humidity correction factor applicable only to the mass emissions of oxides of nitrogen, NO2 and NOx, per test or phase;

is the concentration of compound i per test or phase in the diluted exhaust gas expressed in ppm and corrected by the amount of compound i contained in the dilution air;

is the distance driven over the applicable WLTC, km;

n is the number of phases of the applicable WLTC.

3.2.1.1. The concentration of a gaseous compound in the diluted exhaust gas shall be corrected by the amount of the gaseous compound in the dilution air using the following equation:

where:

is the concentration of gaseous compound i in the diluted exhaust gas corrected by the amount of gaseous compound i contained in the dilution air, ppm;

is the measured concentration of gaseous compound i in the diluted exhaust gas, ppm;

is the concentration of gaseous compound i in the dilution air, ppm;

is the dilution factor.

3.2.1.1.1. The dilution factor shall be calculated using the equation for the concerned fuel (as applicable):

for petrol (E10H)

for diesel (B5H)

for LPG

for NG/biomethane

for ethanol (E85)

for hydrogen

With respect to the equation for hydrogen:

CH2O is the concentration of H2O in the diluted exhaust gas contained in the sample bag, per cent volume;

CH2O-DA is the concentration of H2O in the dilution air, per cent volume;

CH2 is the concentration of H2 in the diluted exhaust gas contained in the sample bag, ppm.

If a fuel type is not listed in this paragraph, the DF for that fuel shall be calculated using the equations in paragraph 3.2.1.1.2. of this annex.

If the manufacturer uses a DF that covers several phases, it shall calculate a DF using the mean concentration of gaseous compounds for the phases concerned.

The mean concentration of a gaseous compound shall be calculated using the following equation:

where:

is mean concentration of a gaseous compound;

is the concentration of each phase;

is the Vmix of the corresponding phase;

n is the number of phases.

3.2.1.1.2. The general equation for calculating the dilution factor DF for each reference fuel with an arithmetic average composition of CxHyOz is as follows:

where:

is the concentration of CO2 in the diluted exhaust gas contained in the sample bag, per cent volume;

is the concentration of HC in the diluted exhaust gas contained in the sample bag, ppm carbon equivalent;

is the concentration of CO in the diluted exhaust gas contained in the sample bag, ppm.

3.2.1.1.3. Methane measurement

3.2.1.1.3.1. For methane measurement using a GC-FID, NMHC shall be calculated using the following equation:

where:

is the corrected concentration of NMHC in the diluted exhaust gas, ppm carbon equivalent;

is the concentration of THC in the diluted exhaust gas, ppm carbon equivalent and corrected by the amount of THC contained in the dilution air;

is the concentration of in the diluted exhaust gas, ppm carbon equivalent and corrected by the amount of contained in the dilution air;

is the FID response factor to methane determined and specified in paragraph 5.4.3.2. of Annex B5.

3.2.1.1.3.2. For methane measurement using an NMC-FID, the calculation of NMHC depends on the calibration gas/method used for the zero/calibration adjustment.

The FID used for the THC measurement (without NMC) shall be calibrated with propane/air in the normal manner.

For the calibration of the FID in series with an NMC, the following methods are permitted:

(a) The calibration gas consisting of propane/air bypasses the NMC;

(b) The calibration gas consisting of methane/air passes through the NMC.

It is highly recommended to calibrate the methane FID with methane/air through the NMC.

In case (a), the concentration of CH4 and NMHC shall be calculated using the following equations:

If RfCH4 < 1.05, it may be omitted from the equation above for CCH4.

In case (b), the concentration of CH4 and NMHC shall be calculated using the following equations:

where:

is the HC concentration with sample gas flowing through the NMC, ppm C;

is the HC concentration with sample gas bypassing the NMC, ppm C;

RfCH4 is the methane response factor as determined per paragraph 5.4.3.2. of Annex B5;

is the methane efficiency as determined per paragraph 3.2.1.1.3.3.1. of this annex;

is the ethane efficiency as determined per paragraph 3.2.1.1.3.3.2. of this annex.

If < 1.05, it may be omitted in the equations for case (b) above for CCH4 and CNMHC.

3.2.1.1.3.3. Conversion efficiencies of the non-methane cutter, NMC

The NMC is used for the removal of the non-methane hydrocarbons from the sample gas by oxidizing all hydrocarbons except methane. Ideally, the conversion for methane is 0 per cent, and for the other hydrocarbons represented by ethane is 100 per cent. For the accurate measurement of NMHC, the two efficiencies shall be determined and used for the calculation of the NMHC emission.

3.2.1.1.3.3.1. Methane conversion efficiency, EM

The methane/air calibration gas shall be flowed to the FID through the NMC and bypassing the NMC and the two concentrations recorded. The efficiency shall be determined using the following equation:

where:

is the HC concentration with CH4 flowing through the NMC, ppm C;

is the HC concentration with CH4 bypassing the NMC, ppm C.

3.2.1.1.3.3.2. Ethane conversion efficiency, EE

The ethane/air calibration gas shall be flowed to the FID through the NMC and bypassing the NMC and the two concentrations recorded. The efficiency shall be determined using the following equation:

where:

is the HC concentration with C2H6 flowing through the NMC, ppm C;

is the HC concentration with C2H6 bypassing the NMC, ppm C.

If the ethane conversion efficiency of the NMC is 0.98 or above, EE shall be set to 1 for any subsequent calculation.

3.2.1.1.3.4. If the methane FID is calibrated through the cutter, EM shall be 0.

The equation to calculate CCH4 in paragraph 3.2.1.1.3.2. (case (b)) in this annex becomes:

The equation to calculate CNMHC in paragraph 3.2.1.1.3.2. (case (b)) in this annex becomes:

The density used for NMHC mass calculations shall be equal to that of total hydrocarbons at 273.15 K (0 °C) and 101.325 kPa and is fuel-dependent.

3.2.1.1.4. Flow-weighted arithmetic average concentration calculation

The following calculation method shall be applied for CVS systems that are not equipped with a heat exchanger or for CVS systems with a heat exchanger that does not comply with paragraph 3.3.5.1. of Annex B5.

This flow weighted arithmetic average concentration calculation shall be used for all continuous diluted measurements including PN (if PN measurement is required). It may be optionally applied for CVS systems with a heat exchanger that complies with paragraph 3.3.5.1 of Annex B5.

where:

is the flow-weighted arithmetic average concentration;

is the CVS flow rate at time , m³/sec;

is the concentration at time , ppm;

sampling interval, s;

total CVS volume, m³;

is the test time, s.

3.2.1.2. Calculation of the NOx humidity correction factor

In order to correct the influence of humidity on the results of oxides of nitrogen, the following calculations apply:

where:

and:

is the specific humidity, grams of water vapour per kilogram dry air;

is the relative humidity of the ambient air, per cent;

is the saturation vapour pressure at ambient temperature, kPa;

is the atmospheric pressure in the room, kPa.

The KH factor shall be calculated for each phase of the test cycle.

The ambient temperature and relative humidity shall be defined as the arithmetic average of the continuously measured values during each phase.

3.2.2. Determination of the HC mass emissions from compression-ignition engines

3.2.2.1. To calculate HC mass emission for compression-ignition engines, the arithmetic average HC concentration shall be calculated using the following equation:

where:

is the integral of the recording of the heated FID over the test (t1 to t2);

is the concentration of HC measured in the diluted exhaust in ppm of and is substituted for in all relevant equations.

3.2.2.1.1. Dilution air concentration of HC shall be determined from the dilution air bags. Correction shall be carried out according to paragraph 3.2.1.1. of this annex.

3.2.3. Fuel consumption, fuel efficiency and CO2 calculations for individual vehicles in an interpolation family

3.2.3.1. Fuel consumption, fuel efficiency and CO2 emissions without using the interpolation method (i.e. using vehicle H only)

The CO2 value, as calculated in paragraphs 3.2.1. to 3.2.1.1.2. inclusive of this annex, and fuel efficiency/fuel consumption, as calculated according to paragraph 6. of this annex, shall be attributed to all individual vehicles in the interpolation family and the interpolation method shall not be applicable.

3.2.3.2. Fuel consumption and CO2 emissions using the interpolation method

The CO2 emissions and the fuel consumption for each individual vehicle in the interpolation family may be calculated according to paragraphs 3.2.3.2.1. to 3.2.3.2.5. inclusive of this annex.

3.2.3.2.1. Fuel consumption and CO2 emissions of test vehicles L and H

The mass of CO2 emissions, , and and its phases p, and , of test vehicles L and H, used for the following calculations, shall be taken from step 9 of Table A7/1.

Fuel consumption values are also taken from step 9 of Table A7/1 and are referred to as FCL,p and FCH,p.

3.2.3.2.2. Road load calculation for an individual vehicle

In the case that the interpolation family is derived from one or more road load families, the calculation of the individual road load shall only be performed within the road load family applicable to that individual vehicle.

3.2.3.2.2.1. Mass of an individual vehicle

The test masses of vehicles H and L shall be used as input for the interpolation method.

TMind, in kg, shall be the test mass of an individual vehicle according to paragraph 3.2.25. of this Regulation.

If the same test mass is used for test vehicles L and H, the value of shall be set to the mass of test vehicle H for the interpolation method.

3.2.3.2.2.2. Rolling resistance of an individual vehicle

3.2.3.2.2.2.1. The actual RRC values for the selected tyres on test vehicle L, RRL, and test vehicle H, RRH, shall be used as input for the interpolation method. See paragraph 4.2.2.1. of Annex B4.

If the tyres on the front and rear axles of vehicle L or H have different RRC values, the weighted mean of the rolling resistances shall be calculated using the equation in paragraph 3.2.3.2.2.2.3. of this annex.

3.2.3.2.2.2.2. For the tyres fitted to an individual vehicle, the value of the rolling resistance coefficient RRind shall be set to the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4.

In the case where individual vehicles can be supplied with a complete set of standard wheels and tyres and in addition a complete set of snow tyres (marked with 3 Peaked Mountain and Snowflake – 3PMS) with or without wheels, the additional wheels/tyres shall not be considered as optional equipment.

If the tyres on the front and rear axles belong to different energy efficiency classes, the weighted mean shall be used and calculated using the equation in paragraph 3.2.3.2.2.2.3. of this annex.

If the same tyres, or tyres with the same rolling resistance coefficient were fitted to test vehicles L and H, the value of for the interpolation method shall be set to .

3.2.3.2.2.2.3. Calculating the weighted mean of the rolling resistances

where:

represents vehicle L, H or an individual vehicle.

and RRH,FA are the actual RRCs of the front axle tyres on vehicles L and H respectively, kg/tonne;

is the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4 of the front axle tyres on the individual vehicle, kg/tonne;

RRL,RA, and RRH,RA are the actual RRCs of the rear axle tyres on vehicles L and H respectively, kg/tonne;

RRind,RA is the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4 of the rear axle tyres on the individual vehicle, kg/tonne;

is the proportion of the vehicle mass in running order on the front axle;

RRx shall not be rounded or categorised to tyre energy efficiency classes.

3.2.3.2.2.3. Aerodynamic drag of an individual vehicle

3.2.3.2.2.3.1. Determination of aerodynamic influence of optional equipment

The aerodynamic drag shall be measured for each of the aerodynamic drag-influencing items of optional equipment and body shapes in a wind tunnel fulfilling the requirements of paragraph 3.2. of Annex B4 verified by the responsible authority.

For the purpose of the interpolation method, the aerodynamic drag of optional equipment within one road load family shall be measured at the same wind speed, either vlow or vhigh, preferably vhigh, as defined in paragraph 6.4.3. of Annex B4. In the case that vlow or vhigh does not exist, (e.g. the road load of VL and/or VH are measured using the coastdown method), the aerodynamic force shall be measured at the same wind speed within the range ≥ 80 km/h and ≤ 150 km/h. For Class 1 vehicles, it shall be measured at the same wind speed of ≤ 150 km/h.

3.2.3.2.2.3.2. Alternative method for determination of aerodynamic influence of optional equipment

At the request of the manufacturer and with approval of the responsible authority, an alternative method (e.g. wind tunnel not fulfilling the criteria in Annex B4) may be used to determine Δ(CD×Af) if the following criteria are fulfilled:

(a) The alternative method shall fulfil an accuracy for Δ(CD×Af) of ±0.015 m².

(b) The alternative method shall only be used for types of aerodynamic-influencing optional equipment (e.g. wheels, cooling air control systems, spoilers etc.) for which equivalency has been demonstrated;

(c) Evidence of equivalency outlined in (a) and (b) shall be shown to the responsible authority in advance of the type approval for the road load family. For any alternative method, validation shall be based on wind tunnel measurements fulfilling the criteria of this Regulation;

(d) If the Δ(CD × Af) of a particular item of optional equipment is more than double the Δ(CD × Af) of the optional equipment for which the evidence was provided, aerodynamic drag shall not be determined by the alternative method; and

(e) Revalidation is necessary every four years in the case that a measurement method is used. In the case that a mathematical method is used, any change made to a simulation model or to the software likely to invalidate the validation report also requires revalidation.

3.2.3.2.2.3.2.1. The manufacturer shall declare the scope of applicable vehicles for the alternative method to the responsible authority and the declared scope shall be documented in relevant test reports when evidence of equivalency is shown to the responsible authority. The responsible authority may request the confirmation of equivalency for the alternative method by selecting the vehicle from the scope declared by the manufacturer after equivalency was demonstrated. The result shall fulfil an accuracy for Δ(CD×Af) of ±0.015 m². This procedure shall be based on wind tunnel measurements fulfilling the criteria of this Regulation. If this procedure is not satisfied, the approval of the alternative method is regarded as invalidated.

3.2.3.2.2.3.3. Application of aerodynamic influence on the individual vehicle

is the difference in the product of the aerodynamic drag coefficient multiplied by frontal area between an individual vehicle and test vehicle L due to options and body shapes on the vehicle that differ from those of test vehicle L, m2;

These differences in aerodynamic drag, Δ(CD×Af), shall be determined with an accuracy of ±0.015 m².

Δ(CD×Af)ind may be calculated according to the following equation maintaining the accuracy of ±0.015 m² also for the sum of items of optional equipment and body shapes:

where:

is the aerodynamic drag coefficient;

is the frontal area of the vehicle, m2;

is the number of items of optional equipment on the vehicle that are different between an individual vehicle and test vehicle L;

is the difference in the product of the aerodynamic drag coefficient multiplied by frontal area due to an individual feature, i, on the vehicle and is positive for an item of optional equipment that adds aerodynamic drag with respect to test vehicle L and vice versa, m2.

The sum of all Δ(CD×Af)i differences between test vehicles L and H shall correspond to Δ(CD×Af)LH.

3.2.3.2.2.3.4. Definition of complete aerodynamic delta between test vehicles L and H

The total difference of the aerodynamic drag coefficient multiplied by frontal area between test vehicles L and H shall be referred to as Δ(CD×Af)LH and shall be recorded, m².

3.2.3.2.2.3.5. Documentation of aerodynamic influences

The increase or decrease of the product of the aerodynamic drag coefficient multiplied by frontal area expressed as Δ(CD×Af) for all items of optional equipment and body shapes in the interpolation family that:

(a) have an influence on the aerodynamic drag of the vehicle; and

(b) are to be included in the interpolation,

shall be recorded, m².

3.2.3.2.2.3.6. Additional provisions for aerodynamic influences

The aerodynamic drag of vehicle H shall be applied to the whole interpolation family and Δ(CD×Af)LH shall be set to zero, if:

(a) the wind tunnel facility is not able to accurately determine Δ(CD×Af); or

(b) there are no drag-influencing items of optional equipment between the test vehicles H and L that are to be included in the interpolation method.

3.2.3.2.2.4. Calculation of road load coefficients for individual vehicles

The road load coefficients , and (as defined in Annex B4) for test vehicles H and L are referred to as , and ,and , and respectively. An adjusted road load curve for the test vehicle L is defined as follows:

Applying the least squares regression method in the range of the reference speed points, adjusted road load coefficients and shall be determined for with the linear coefficient set to . The road load coefficients , and for an individual vehicle in the interpolation family shall be calculated using the following equations:

or, if = 0, the equation for f0,ind below shall apply:

or, if , the equation for F2,ind below shall apply:

where:

In the case of a road load matrix family, the road load coefficients f0, f1 and f2 for an individual vehicle shall be calculated according to the equations in paragraph 5.1.1. of Annex B4.

3.2.3.2.3. Calculation of cycle energy demand

The cycle energy demand of the applicable WLTC Ek and the energy demand for all applicable cycle phases shall be calculated according to the procedure in paragraph 5. of this annex for the following sets k of road load coefficients and masses:

k=1:

(test vehicle L)

k=2:

(test vehicle H)

k=3:

(an individual vehicle in the interpolation family)

These three sets of road loads may be derived from different road load families.

3.2.3.2.4. For 4-phase WLTP test only

Calculation of the CO2 value for an individual vehicle within an interpolation family using the interpolation method

For each cycle phase p of the applicable cycle the mass of CO2 emissions g/km, for an individual vehicle shall be calculated using the following equation:

The mass of CO2 emissions, g/km, over the complete cycle for an individual vehicle shall be calculated using the following equation:

The terms E1,p, E2,p and E3,p and E1, E2 and E3 respectively shall be calculated as specified in paragraph 3.2.3.2.3. of this annex.

3.2.3.2.5. For 4-phase WLTP test

Calculation of the fuel consumption FC value for an individual vehicle within an interpolation family using the interpolation method

For each cycle phase p of the applicable cycle, the fuel consumption, l/100 km, for an individual vehicle shall be calculated using the following equation:

The fuel consumption, l/100 km, of the complete cycle for an individual vehicle shall be calculated using the following equation:

The terms E1,p, E2,p and E3,p, and E1, E2 and E3 respectively shall be calculated as specified in paragraph 3.2.3.2.3. of this annex.

For 3-phase WLTP

Calculation of the fuel efficiency FE value for an individual vehicle within an interpolation family using the interpolation method

For each cycle phase p of the applicable cycle, the fuel efficiency, km/l, for an individual vehicle shall be calculated using the following equation:

The fuel efficiency, in km/l, of the complete cycle for an individual vehicle shall be calculated using the following equation:

The terms E1,p, E2,p and E3,p, and E1, E2 and E3 respectively shall be calculated as specified in paragraph 3.2.3.2.3. of this annex.

3.2.3.2.6. For 4-phase WLTP test

The individual CO2 value determined in paragraph 3.2.3.2.4. of this annex may be increased by the original equipment manufacturer (OEM). In such cases:

(a) The CO2 phase values shall be increased by the ratio of the increased CO2 value divided by the calculated CO2 value;

(b) The fuel consumption values shall be increased by the ratio of the increased CO2 value divided by the calculated CO2 value.

This shall not compensate for technical elements that would effectively require a vehicle to be excluded from the interpolation family.

For 3-phase WLTP

The individual fuel efficiency value determined in paragraph 3.2.3.2.5. of this annex may be decreased by the original equipment manufacturer (OEM). In such cases:

(a) The fuel efficiency phase values shall be decreased by the ratio of the decreased fuel efficiencyvalue divided by the calculated fuel efficiency value.

This shall not compensate for technical elements that would effectively require a vehicle to be excluded from the interpolation family.

3.2.4. Fuel consumption, fuel efficiency and CO2 calculations for individual vehicles in a road load matrix family

The CO2 emissions and the fuel efficiency/fuel consumption for each individual vehicle in the road load matrix family shall be calculated according to the interpolation method described in paragraphs 3.2.3.2.3. to 3.2.3.2.5. inclusive of this annex. Where applicable, references to vehicle L and/or H shall be replaced by references to vehicle LM and/or HM respectively.

3.2.4.1. Determination of fuel consumption, fuel efficiency and CO2 emissions of vehicles LM and HM

The mass of CO2 emissions of vehicles LM and HM shall be determined according to the calculations in paragraph 3.2.1. of this annex for the individual cycle phases p of the applicable WLTC and are referred to as and respectively. Fuel consumption and fuel efficiency for individual cycle phases of the applicable WLTC shall be determined according to paragraph 6. of this annex and are referred to as FCLM,p, FCHM,p, FELM,p and FELM,p respectively.

3.2.4.1.1. Road load calculation for an individual vehicle

The road load force shall be calculated according to the procedure described in paragraph 5.1. of Annex B4.

3.2.4.1.1.1. Mass of an individual vehicle

The test masses of vehicles HM and LM selected according to paragraph 4.2.1.4. of Annex B4 shall be used as input.

TMind, in kg, shall be the test mass of the individual vehicle according to the definition of test mass in paragraph 3.2.25. of this Regulation.

If the same test mass is used for vehicles LM and HM, the value of TMind shall be set to the mass of vehicle HM for the road load matrix family method.

3.2.4.1.1.2. Rolling resistance of an individual vehicle

3.2.4.1.1.2.1. The RRC values for vehicle LM , RRLM, and vehicle HM, RRHM, selected under paragraph 4.2.1.4. of Annex B4, shall be used as input.

If the tyres on the front and rear axles of vehicle LM or HM have different rolling resistance values, the weighted mean of the rolling resistances shall be calculated using the equation in paragraph 3.2.4.1.1.2.3. of this annex.

3.2.4.1.1.2.2. For the tyres fitted to an individual vehicle, the value of the rolling resistance coefficient RRind shall be set to the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4.

In the case where individual vehicles can be supplied with a complete set of standard wheels and tyres and in addition a complete set of snow tyres (marked with 3 Peaked Mountain and Snowflake – 3PMS) with or without wheels, the additional wheels/tyres shall not be considered as optional equipment.

If the tyres on the front and the rear axles belong to different energy efficiency classes, the weighted mean shall be used and shall be calculated using the equation in paragraph 3.2.4.1.1.2.3. of this annex.

If the same rolling resistance is used for vehicles LM and HM, the value of shall be set to for the road load matrix family method.

3.2.4.1.1.2.3. Calculating the weighed mean of the rolling resistances

where:

represents vehicle L, H or an individual vehicle;

and RRHM,FA are the actual RRCs of the front axle tyres on vehicles L and H respectively, kg/tonne;

is the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4 of the front axle tyres on the individual vehicle, kg/tonne;

RRLM,RA, and RRHM,RA are the actual rolling resistance coefficients of the rear axle tyres on vehicles L and H respectively, kg/tonne;

RRind,RA is the RRC value of the applicable tyre energy efficiency class according to Table A4/2 of Annex B4 of the rear axle tyres on the individual vehicle, kg/tonne;

is the proportion of the vehicle mass in running order on the front axle.

RRx shall not be rounded or categorised to tyre energy efficiency classes.

3.2.4.1.1.3. Frontal area of an individual vehicle

The frontal area for vehicle LM, AfLM, and vehicle HM, AfHM, selected under paragraph 4.2.1.4. of Annex B4 shall be used as input.

Af,ind, in m2, shall be the frontal area of the individual vehicle.

If the same frontal area is used for vehicles LM and HM, the value of Af,ind shall be set to the frontal area of vehicle HM for the road load matrix family method.

3.2.5. Alternative interpolation calculation method

Upon request of the manufacturer and with approval of the responsible authority, a manufacturer may apply an alternative interpolation calculation procedure in the case that the interpolation method creates unrealistic phase-specific results or an unrealistic road load curve. Before such permission is granted, the manufacturer shall check and where possible correct:

(a) The reason for having small differences between the road load relevant characteristics between vehicle L and H in the case of unrealistic phase- specific results;

(b) The reason for having an unexpected difference between the f1,L and f1,H coefficients in the case of an unrealistic road load curve.

The request of the manufacturer to the responsible authority shall include evidence that such a correction is not possible, and that the resultant error is significant.

3.2.5.1. Alternative calculation to correct unrealistic phase-specific results

Alternatively to the procedures defined in paragraphs 3.2.3.2.4. and 3.2.3.2.5. of this annex, calculations of phase CO2, phase fuel efficiency and phase fuel consumption may be calculated according to the equations in paragraphs 3.2.5.1.1., 3.2.5.1.2. and 3.2.5.1.3. below.

3.2.5.1.1. Ratio determination for each phase of VL and VH

where:

are from step 9 in Table A7/1 in this annex.

3.2.5.1.2. Ratio determination for each phase for vehicle Vind

where:

is from step 10 in Table A7/1 in this annex and shall be rounded to the nearest whole number.

3.2.5.1.3. Phase per phase mass emission of vehicle Vind

3.2.5.2. Alternative calculation to correct an unrealistic road load curve

Alternatively to the procedure defined in paragraph 3.2.3.2.2.4. of this annex, road load coefficients may be calculated as follows:

Applying the least squares regression method in the range of the reference speed points, alternative adjusted road load coefficients f\*0,i and f\*2,i shall be determined for Fi(v) with the linear coefficient f\*1,i set to f1,A. f1,A is calculated as follows:

where:

E is the cycle energy demand as defined in paragraph 5. of this annex, Ws;

i is the subscript denoting vehicles L, H or ind;

HR is test vehicle H as described in paragraph 4.2.1.2.3.2. of Annex B4;

LR is test vehicle L as described in paragraph 4.2.1.2.3.2. of Annex B4.

3.3. PM

3.3.1. Calculation

PM shall be calculated using the following two equations:

where exhaust gases are vented outside tunnel;

and:

where exhaust gases are returned to the tunnel;

where:

is the volume of diluted exhaust gases (see paragraph 2. of this annex), under standard conditions;

is the volume of diluted exhaust gas flowing through the particulate sampling filter under standard conditions;

is the mass of particulate matter collected by one or more sample filters, mg;

is the distance driven corresponding to the test cycle, km.

3.3.1.1. Where correction for the background particulate mass from the dilution system has been used, this shall be determined in accordance with paragraph 2.1.3.1. of Annex B6. In this case, particulate mass (mg/km) shall be calculated using the following equations:

in the case that the exhaust gases are vented outside the tunnel;

and:

in the case that the exhaust gases are returned to the tunnel;

where:

is the volume of tunnel air flowing through the background particulate filter under standard conditions;

is the particulate mass from the dilution air, or the dilution tunnel background air, as determined by the one of the methods described in paragraph 2.1.3.1. of Annex B6;

is the dilution factor determined in paragraph 3.2.1.1.1. of this annex.

Where application of a background correction results in a negative result, it shall be considered to be zero mg/km.

3.3.2. Calculation of PM using the double dilution method

where:

is the volume of diluted exhaust gas flowing through the particulate sample filter under standard conditions;

is the volume of the double diluted exhaust gas passing through the particulate sampling filters under standard conditions;

is the volume of the secondary dilution air under standard conditions.

Where the secondary diluted sample gas for PM measurement is not returned to the tunnel, the CVS volume shall be calculated as in single dilution, i.e.:

where:

is the measured volume of diluted exhaust gas in the dilution system following extraction of the particulate sample under standard conditions.

4. Determination of PN (if PN measurement is required)

PN shall be calculated using the following equation:

where:

is the particle number emission, particles per kilometre;

is the volume of the diluted exhaust gas in litres per test (after primary dilution only in the case of double dilution) and corrected to standard conditions (273.15 K (0 °C) and 101.325 kPa);

is a calibration factor to correct the PNC measurements to the level of the reference instrument where this is not applied internally within the PNC. Where the calibration factor is applied internally within the PNC, the calibration factor shall be 1;

is the corrected particle number concentration from the diluted exhaust gas expressed as the arithmetic average number of particles per cubic centimetre from the emissions test including the full duration of the drive cycle. If the volumetric mean concentration results from the PNC are not measured at standard conditions (273.15 K (0 °C) and 101.325 kPa), the concentrations shall be corrected to those conditions ;

is either the dilution air or the dilution tunnel background particle number concentration, as permitted by the responsible authority, in particles per cubic centimetre, corrected for coincidence and to standard conditions (273.15 K (0 °C) and 101.325 kPa);

is the mean particle concentration reduction factor of the VPR at the dilution setting used for the test;

is the mean particle concentration reduction factor of the VPR at the dilution setting used for the background measurement;

is the distance driven corresponding to the applicable test cycle, km.

shall be calculated using the following equation:

where:

is a discrete measurement of particle number concentration in the diluted gas exhaust from the PNC; particles per cm³;

is the total number of discrete particle number concentration measurements made during the applicable test cycle and shall be calculated using the following equation:

where:

is the time duration of the applicable test cycle, s;

is the data logging frequency of the particle counter, Hz.

5. Calculation of cycle energy demand

Unless otherwise specified, the calculation shall be based on the target speed trace given in discrete time sample points.

The total energy demand E for the whole cycle or a specific cycle phase shall be calculated by summing over the corresponding cycle time between tstart +1 and tend according to the following equation:

where:

if

if

and:

tstart is the time at which the applicable test cycle or phase starts (see paragraph 3. of Annex B1), s;

tend is the time at which the applicable test cycle or phase ends (see paragraph 3. of Annex B1), s;

is the energy demand during time period (i-1) to (i), Ws;

is the driving force during time period (i-1) to (i), N;

is the distance travelled during time period (i-1) to (i), m.

where:

is the driving force during time period (i-1) to (i), N;

is the target velocity at time ti, km/h;

is the test mass, kg;

is the acceleration during time period (i-1) to (i), m/s²;

, , are the road load coefficients for the test vehicle under consideration (, or ) in N, N/km/h and in N/(km/h)² respectively.

where:

is the distance travelled in time period (i-1) to (i), m;

is the target velocity at time , km/h;

is time, s.

where:

is the acceleration during time period (i-1) to (i), m/s²;

is the target velocity at time , km/h;

is time, s.

6. Calculation of fuel consumption and fuel efficiency (as applicable)

6.1. The fuel characteristics required for the calculation of fuel consumption values shall be taken from Annex B3.

6.2. For 4-phase WLTP test

The fuel consumption values shall be calculated from the emissions of hydrocarbons, carbon monoxide, and carbon dioxide using the results of step 6 for criteria emissions and step 7 for CO2 of Table A7/1 in case of ICE or of Table A8/6 in case of NOVC-HEV and OVC-HEV.

For 3-phase WLTP

The fuel efficiency values shall be calculated from the emissions of hydrocarbons, carbon monoxide, and carbon dioxide using the results of the step as specified in the input column of the relevant table of this annex or Annex B8.

6.2.1. The general equation in paragraph 6.12. of this annex using H/C and O/C ratios shall be used for the calculation of fuel consumption.

6.2.2. For all equations in paragraph 6. of this annex:

FC is the fuel consumption of a specific fuel, l/100 km (or m³ per 100 km in the case of natural gas or kg/100 km in the case of hydrogen);

H/C is the hydrogen to carbon ratio of a specific fuel CXHYOZ;

O/C is the oxygen to carbon ratio of a specific fuel CXHYOZ;

MWC is the molar mass of carbon (12.011 g/mol);

MWH is the molar mass of hydrogen (1.008 g/mol);

MWO is the molar mass of oxygen (15.999 g/mol);

ρfuel is the test fuel density, kg/l. For gaseous fuels, fuel density at 15 °C;

HC are the emissions of hydrocarbon, g/km;

CO are the emissions of carbon monoxide, g/km;

CO2 are the emissions of carbon dioxide, g/km;

H2O are the emissions of water, g/km;

H2 are the emissions of hydrogen, g/km;

p1 is the gas pressure in the fuel tank before the applicable test cycle, Pa;

p2 is the gas pressure in the fuel tank after the applicable test cycle, Pa;

T1 is the gas temperature in the fuel tank before the applicable test cycle, K;

T2 is the gas temperature in the fuel tank after the applicable test cycle, K;

Z1 is the compressibility factor of the gaseous fuel at p1 and T1;

Z2 is the compressibility factor of the gaseous fuel at p2 and T2;

V is the interior volume of the gaseous fuel tank, m³;

d is the theoretical length of the applicable phase or cycle, km.

6.3. (Reserved)

6.4. (Reserved)

6.5. For a vehicle with a positive ignition engine fuelled with petrol (E10H)

6.6. For a vehicle with a positive ignition engine fuelled with LPG

6.6.1. If the composition of the fuel used for the test differs from the composition that is assumed for the calculation of the normalised consumption, on the manufacturer's request a correction factor cf may be applied, using the following equation:

The correction factor, , which may be applied, is determined using the following equation:

where:

is the actual H/C ratio of the fuel used.

6.7. For a vehicle with a positive ignition engine fuelled with NG/biomethane

6.8. (Reserved)

6.9. For a vehicle with a compression engine fuelled with diesel (B5H)

6.10. (Reserved)

6.11. For a vehicle with a positive ignition engine fuelled with ethanol (E85)

6.12. Fuel consumption for any test fuel may be calculated using the following equation:

6.13. Fuel consumption for a vehicle with a positive ignition engine fuelled by hydrogen:

For vehicles fuelled either with gaseous or liquid hydrogen, and with approval of the responsible authority, the manufacturer may choose to calculate fuel consumption using either the equation for FC below or a method using a standard protocol such as SAE J2572.

The compressibility factor, Z, shall be obtained from the following table:

Table A7/2

**Compressibility factor Z**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  | p(bar) |  |  |  |  |  |
|  |  | *5* | *100* | *200* | *300* | *400* | *500* | *600* | *700* | *800* | *900* |
|  | 33 | 0.859 | 1.051 | 1.885 | 2.648 | 3.365 | 4.051 | 4.712 | 5.352 | 5.973 | 6.576 |
|  | 53 | 0.965 | 0.922 | 1.416 | 1.891 | 2.338 | 2.765 | 3.174 | 3.570 | 3.954 | 4.329 |
|  | 73 | 0.989 | 0.991 | 1.278 | 1.604 | 1.923 | 2.229 | 2.525 | 2.810 | 3.088 | 3.358 |
|  | 93 | 0.997 | 1.042 | 1.233 | 1.470 | 1.711 | 1.947 | 2.177 | 2.400 | 2.617 | 2.829 |
|  | 113 | 1.000 | 1.066 | 1.213 | 1.395 | 1.586 | 1.776 | 1.963 | 2.146 | 2.324 | 2.498 |
|  | 133 | 1.002 | 1.076 | 1.199 | 1.347 | 1.504 | 1.662 | 1.819 | 1.973 | 2.124 | 2.271 |
|  | 153 | 1.003 | 1.079 | 1.187 | 1.312 | 1.445 | 1.580 | 1.715 | 1.848 | 1.979 | 2.107 |
|  | 173 | 1.003 | 1.079 | 1.176 | 1.285 | 1.401 | 1.518 | 1.636 | 1.753 | 1.868 | 1.981 |
| T(K) | 193 | 1.003 | 1.077 | 1.165 | 1.263 | 1.365 | 1.469 | 1.574 | 1.678 | 1.781 | 1.882 |
|  | 213 | 1.003 | 1.071 | 1.147 | 1.228 | 1.311 | 1.396 | 1.482 | 1.567 | 1.652 | 1.735 |
|  | 233 | 1.004 | 1.071 | 1.148 | 1.228 | 1.312 | 1.397 | 1.482 | 1.568 | 1.652 | 1.736 |
|  | 248 | 1.003 | 1.069 | 1.141 | 1.217 | 1.296 | 1.375 | 1.455 | 1.535 | 1.614 | 1.693 |
|  | 263 | 1.003 | 1.066 | 1.136 | 1.207 | 1.281 | 1.356 | 1.431 | 1.506 | 1.581 | 1.655 |
|  | 278 | 1.003 | 1.064 | 1.130 | 1.198 | 1.268 | 1.339 | 1.409 | 1.480 | 1.551 | 1.621 |
|  | 293 | 1.003 | 1.062 | 1.125 | 1.190 | 1.256 | 1.323 | 1.390 | 1.457 | 1.524 | 1.590 |
|  | 308 | 1.003 | 1.060 | 1.120 | 1.182 | 1.245 | 1.308 | 1.372 | 1.436 | 1.499 | 1.562 |
|  | 323 | 1.003 | 1.057 | 1.116 | 1.175 | 1.235 | 1.295 | 1.356 | 1.417 | 1.477 | 1.537 |
|  | 338 | 1.003 | 1.055 | 1.111 | 1.168 | 1.225 | 1.283 | 1.341 | 1.399 | 1.457 | 1.514 |
|  | 353 | 1.003 | 1.054 | 1.107 | 1.162 | 1.217 | 1.272 | 1.327 | 1.383 | 1.438 | 1.493 |

In the case that the required input values for p and T are not indicated in the table, the compressibility factor shall be obtained by linear interpolation between the compressibility factors indicated in the table, choosing the ones that are the closest to the value sought.

6.14. Calculation of fuel efficiency (FE)

This paragraph is applicable for the 3-phase WLTP only:

6.14.1. FE = 100/FC

where

FC is the fuel consumption of a specific fuel, l/100 km (or m³ per 100 km in the case of natural gas or kg/100 km in the case of hydrogen);

FE is fuel efficiency; km/l (or km/m³ in the case of natural gas, or km/ kg in the case of hydrogen).

7. Drive trace indices

7.1. General requirement

The prescribed speed between time points in Tables A1/1 to A1/12 shall be determined by linear interpolation at a frequency of 10 Hz.

In the case that the accelerator control is fully activated, the prescribed speed shall be used instead of the actual vehicle speed for drive trace index calculations during such periods of operation.

In the case of vehicles equipped with a manual transmission, it is allowed to exclude drive trace indices calculation during upward gear shift operation. From the moment of actual vehicle clutch operation until the actual vehicle speed has reached the prescribed speed in the higher gear shall be a maximum of 2 seconds. The type approval authority may request the manufacturer to demonstrate that it is not possible to meet the drive trace requirements without such exclusion, as a result of the design of the vehicle.

The on-board diagnostics (OBD) or electronic control unit (ECU) monitoring (data collection) system may be used in order to detect the position of the accelerator control. The collection of OBD and/or ECU data shall not influence the vehicle's emissions or performance.

7.2. Calculation of drive trace indices

The following indices shall be calculated according to SAE J2951(Revised JAN2014):

(a) IWR Inertial Work Rating, per cent;

(b) RMSSE Root Mean Squared Speed Error, km/h.

7.3. (Reserved)

7.4. Vehicle-specific application of drive trace indices

7.4.1. Pure ICE vehicles, NOVC-HEVs, NOVC-FCHVs

The drive trace indices IWR and RMSSE shall be calculated for the applicable test cycle and reported.

7.4.2. OVC-HEVs

7.4.2.1. Charge-sustaining Type 1 test (paragraph 3.2.5. of Annex B8)

The drive trace indices IWR and RMSSE shall be calculated for the applicable test cycle and reported.

7.4.2.2. Charge-depleting Type 1 test (paragraph 3.2.4.3. of Annex B8)

If the number of charge-depleting Type 1 test cycles is less than four, the drive trace indices IWR and RMSSE shall be calculated for each individual applicable test cycle of the charge-depleting Type 1 test and reported

If the number of charge-depleting Type 1 test cycles is greater than or equal to four, the drive trace indices IWR and RMSSE shall be calculated for each individual applicable test cycle of the charge-depleting Type 1 test and reported. In this case, the average IWR and the average RMSSE for the combination of any two cycles within the charge-depleting test shall be compared with the respective criteria specified in paragraph 2.6.8.3.1.3. of Annex B6, and the calculated IWR of any individual cycle within the charge-depleting test shall not be less than -3.0 nor greater than +5.0 per cent.

7.4.2.3. City cycle test (paragraph 3.2.4.3. of Annex B8 replacing WLTC with WLTCcity)


For the application of the drive trace index calculation, two consecutively driven city test cycles (L and M) shall be considered as one cycle.

For the city cycle during which the combustion engine starts to consume fuel, the drive indices IWR and RMSSE shall not be calculated individually. Instead, depending on the number of completed city cycles before the city cycle during which the combustion engine starts, the incomplete city cycle shall be combined with the previous city cycles as follows and shall be considered as one cycle in the context of the drive trace index calculations.

If the number of completed city cycles is even, the incomplete city cycle shall be combined with the previous two completed city cycles. See the example in Figure A7/1 below.

Figure A7/1


**Example with an even number of completed city test cycles before the city cycle where the combustion engine start**



If the number of completed city cycles is odd, the incomplete city cycle shall be combined with the previous three completed city cycles. See the example in Figure A7/2 below.

Figure A7/2

**Example with an odd number of completed city test cycles before the city cycle where the combustion engine start**

****

If the number of cycles derived according to Figure A7/1 or Figure A7/2 is less than four, the drive trace indices IWR and RMSSE shall be calculated for each individual cycle and reported.

If the number of cycles derived according to Figure A7/1 or Figure A7/2 is greater than or equal to four, the drive trace indices IWR and RMSSE shall be calculated for each individual cycle. In this case, the average IWR and the average RMSSE for the combination of any two cycles shall be compared with the respective criteria specified in paragraph 2.6.8.3.1.3. of Annex B6 and the IWR of any individual cycle shall not be less than -3.0 or greater than +5.0 per cent.

7.4.3. PEV

7.4.3.1. Consecutive cycle test

The consecutive cycle test procedure shall be performed according to paragraph 3.4.4.1. of Annex B8. The drive trace indices IWR and RMSSE shall be calculated for each individual test cycle of the consecutive cycle test procedure and reported. The test cycle during which the break-off criterion is reached, as specified in paragraph 3.4.4.1.3. of Annex B8, shall be combined with the preceding test cycle. The drive trace indices IWR and RMSSE shall be calculated considering this as one cycle.

7.4.3.2. Shortened Type 1 test

The drive trace indices IWR and RMSSE for the shortened Type 1 test procedure, as performed according to paragraph 3.4.4.2. of Annex B8, shall be calculated separately for each dynamic segment 1 and 2 and reported. The calculation of drive trace indices during the constant speed segments shall be omitted.

7.4.3.3. City cycle test procedure (paragraph 3.4.4.1. of Annex B8 replacing WLTC with WLTCcity)


For the application of the drive trace index calculation, two consecutively driven city test cycles shall be considered as one cycle.

For the city cycle during which the break-off criterion is reached as specified in paragraph 3.4.4.1.3. of Annex B8, the drive trace indices IWR and RMSSE shall not be calculated individually. Instead, depending on the number of completed city cycles before the city cycle when the break-off criterion is reached, the incomplete city cycle shall be combined with previous city cycles and shall be considered as one cycle in the context of the drive trace index calculations.

If the number of completed city cycles is even, the incomplete city cycle shall be combined with the previous two completed city cycles. See the example in Figure A7/3 below.

Figure A7/3


**Example with an even number of completed city test cycles before the city cycle with the break-off criterion**



If the number of completed city cycles is odd, the incomplete city cycle shall be combined with the previous three completed city cycles. See the example in Figure A7/4 below.

Figure A7/4

**Example with an odd number of completed city test cycles before the city cycle with the break-off criterion**

****

If the number of cycles derived according to Figure A7/3 or Figure A7/4 is less than four, the drive trace indices IWR and RMSSE shall be calculated for each of these cycles and reported.

If the number of cycles derived according to Figure A7/3 or Figure A7/4 is greater than or equal to four, the drive trace indices IWR and RMSSE shall be calculated for each of these cycles and reported. In this case, the average IWR and the average RMSSE for the combination of any two cycles shall be compared with the respective criteria as specified in paragraph 2.6.8.3.1. of Annex B6 and the IWR of any individual cycle shall not be less than -3.0 or greater than +5.0 per cent.

8. Calculating n/v ratios

n/v ratios shall be calculated using the following equation:

where:

n is engine speed, min-1;

v is the vehicle speed, km/h;

ri is the transmission ratio in gear i;

raxle is the axle transmission ratio.

Udyn is the dynamic rolling circumference of the tyres of the drive axle and is calculated using the following equation:

where:

H/W is the tyre’s aspect ratio, e.g. "45" for a 225/45 R17 tyre;

W is the tyre width, mm; e.g. "225" for a 225/45 R17 tyre;

R is the wheel diameter, inch; e.g. "17" for a 225/45 R17 tyre.

Udyn shall be rounded according to paragraph 6.1.8. of this Regulation to whole millimetres.

If Udyn is different for the front and the rear axles, the value of n/v for the mainly powered axle shall be applied on a dynamometer in both 2WD and 4WD operation mode.

Upon request, the responsible authority shall be provided with the necessary information for that selection.

Annex B8

Pure electric, hybrid electric and compressed hydrogen fuel cell hybrid vehicles

1. General requirements

In the case of testing NOVC-HEVs, OVC-HEVs and NOVC-FCHVs, Appendix 2 and Appendix 3 to this annex shall replace Appendix 2 to Annex B6.

Unless stated otherwise, all requirements in this annex shall apply to vehicles with and without driver-selectable modes. Unless explicitly stated otherwise in this annex, all of the requirements and procedures specified in Annex B6 and Annex B7 shall continue to apply for NOVC-HEVs, OVC-HEVs, NOVC-FCHVs and PEVs.

1.1. Units, accuracy and resolution of electric parameters

Units, accuracy and resolution of measurements shall be as shown in Table A8/1.

Table A8/1

**Parameters, units, accuracy and resolution of measurements**

| *Parameter* | *Units* | *Accuracy* | *Resolution* |
| --- | --- | --- | --- |
| Electrical energy (a) | Wh | ±1 per cent | 0.001 kWh(b) |
| Electrical current | A | ±0.3 per cent FSD or  ±1 per cent of reading (c,d) | 0.1 A |
| Electric voltage | V | ±0.3 per cent FSD or  ±1 per cent of reading (c) | 0.1 V |
| (a) Equipment: static meter for active energy.  (b) AC watt-hour meter, Class 1 according to IEC 62053-21 or equivalent.  (c) Whichever is greater.  (d) Current integration frequency 20 Hz or more. | | | |

Table A8/2

(Reserved)

1.2. Emission and fuel consumption testing

Parameters, units and accuracy of measurements shall be the same as those required for pure ICE vehicles.

1.3. Rounding of test results

1.3.1. Unless intermediate rounding is required, intermediate steps in the calculations shall not be rounded.

1.3.2. In the case of OVC-HEVs and NOVC-HEVs, the final criteria emission results shall be rounded according to paragraph 1.3.2. of Annex B7, the NOx correction factor KH shall be rounded according to paragraph 1.3.3. of Annex B7, and the dilution factor DF shall be rounded according to paragraph 1.3.4. of Annex B7.

1.3.3. For information not related to standards, good engineering judgement shall be used.

1.3.4. Rounding of range, CO2, energy consumption and fuel consumption results is described in the calculation tables of this annex.

1.4. Vehicle classification

All OVC-HEVs, NOVC-HEVs, PEVs and NOVC-FCHVs shall be classified as Class 3 vehicles. The applicable test cycle for the Type 1 test procedure shall be determined according to paragraph 1.4.2. of this annex based on the corresponding reference test cycle as described in paragraph 1.4.1. of this annex.

1.4.1. Reference test cycle

1.4.1.1. The Class 3 reference test cycles are specified in paragraph 3.3. of Annex B1.

1.4.1.2. For PEVs, the downscaling procedure, according to paragraphs 8.2.3. and 8.3. of Annex B1, may be applied on the test cycles according to paragraph 3.3. of Annex B1 by replacing the rated power with maximum net power according to UN Regulation No. 85. In such a case, the downscaled cycle is the reference test cycle.

1.4.2. Applicable test cycle

1.4.2.1. Applicable WLTP test cycle

The reference test cycle according to paragraph 1.4.1. of this annex shall be the applicable WLTP test cycle (WLTC) for the Type 1 test procedure.

In the case that paragraph 9. of Annex B1 is applied based on the reference test cycle as described in paragraph 1.4.1. of this annex, this modified test cycle shall be the applicable WLTP test cycle (WLTC) for the Type 1 test procedure.

1.4.2.2. Applicable WLTP city test cycle

The Class 3 WLTP city test cycle (WLTCcity) is specified in paragraph 3.5. of Annex B1.

1.5. OVC-HEVs, NOVC-HEVs,NOVC-FCHVs and PEVs with manual transmissions

The vehicles shall be driven according to the technical gear shift indicator, if available, or according to instructions incorporated in the manufacturer's handbook.

2. Run-in of test vehicle

The vehicle tested according to this annex shall be presented in good technical condition and shall be run-in in accordance with the manufacturer’s recommendations. In the case that the REESSs are operated above the normal operating temperature range, the operator shall follow the procedure recommended by the vehicle manufacturer in order to keep the temperature of the REESS in its normal operating range. The manufacturer shall provide evidence that the thermal management system of the REESS is neither disabled nor reduced.

2.1. OVC-HEVs and NOVC-HEVs shall have been run-in according to the requirements of paragraph 2.3.3. of Annex B6.

2.2. NOVC-FCHVs shall have been run-in at least 300 km with their fuel cell and REESS installed.

2.3. PEVs shall have been run-in at least 300 km or one full charge distance, whichever is longer.

2.4. All REESS having no influence on CO2 emissions or H2 consumption shall be excluded from monitoring.

3. Test procedure

3.1. General requirements

3.1.1. For all OVC-HEVs, NOVC-HEVs, PEVs and NOVC-FCHVs, the following shall apply where applicable:

3.1.1.1. Vehicles shall be tested according to the applicable test cycles described in paragraph 1.4.2. of this annex.

3.1.1.2. If the vehicle cannot follow the applicable test cycle within the speed trace tolerances according to paragraph 2.6.8.3.1.2. of Annex B6, the accelerator control shall, unless stated otherwise, be fully activated until the required speed trace is reached again.

3.1.1.3. The powertrain start procedure shall be initiated by means of the devices provided for this purpose according to the manufacturer's instructions.

3.1.1.4. For OVC-HEVs, NOVC-HEVs, NOVC-FCHVs and PEVs, exhaust emissions sampling and measurement of electric energy consumption shall begin for each applicable test cycle before or at the initiation of the vehicle start procedure and end at the conclusion of each applicable test cycle.

3.1.1.5. For OVC-HEVs and NOVC-HEVs, gaseous emission compounds and particle number, shall be analysed for each individual test phase. For phases where no combustion engine operates, it is permitted to omit the phase analysis and to set the emission results to zero.

3.1.1.6. For OVC-HEVs and NOVC-HEVs, without prejudice to paragraph 2.10.1.1. of Annex B6, particulate matter emission shall be analysed for each applicable test cycle. For cycles where no combustion engine operates, it is permitted to set the emission results to zero.

3.1.2. Forced cooling as described in paragraph 2.7.2. of Annex B6 is only permitted for the charge-sustaining Type 1 test for OVC-HEVs according to paragraph 3.2. of this annex and for testing NOVC-HEVs according to paragraph 3.3. of this annex.

3.1.3. The requirements of paragraphs 2.2.2.1.2. and 2.2.2.1.3. of Annex B6 are exempted when testing was conducted for PEVs according to paragraph 3.4. and for FCHVs according to paragraph 3.5.

3.2. OVC-HEVs

3.2.1. Vehicles shall be tested under charge-depleting operating condition (CD condition), and charge-sustaining operating condition (CS condition)

3.2.2. Vehicles may be tested according to four possible test sequences:

3.2.2.1. Option 1: charge-depleting Type 1 test with no subsequent charge-sustaining Type 1 test.

3.2.2.2. Option 2: charge-sustaining Type 1 test with no subsequent charge-depleting Type 1 test.

3.2.2.3. Option 3: charge-depleting Type 1 test with a subsequent charge-sustaining Type 1 test.

3.2.2.4. Option 4: charge-sustaining Type 1 test with a subsequent charge-depleting Type 1 test.

# Figure A8/1

# **Possible test sequences in the case of OVC-HEV testing**

3.2.3. The driver-selectable mode shall be set as described in the following test sequences (Option 1 to Option 4).

3.2.4. Charge-depleting Type 1 test with no subsequent charge-sustaining Type 1 test (Option 1)

# The test sequence according to Option 1, described in paragraphs 3.2.4.1. to 3.2.4.7. inclusive of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/1 in Appendix 1 to this annex.

3.2.4.1. Preconditioning

The vehicle shall be prepared according to the procedures in paragraph 2.2. of Appendix 4 to this annex.

3.2.4.2. Test conditions

3.2.4.2.1. The test shall be carried out with a fully charged REESS according to the charging requirements as described in paragraph 2.2.3. of Appendix 4 to this annex and with the vehicle operated in charge-depleting operating condition as defined in paragraph 3.3.5. of this Regulation.

3.2.4.2.2. Selection of a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the charge-depleting Type 1 test shall be selected according to paragraph 2. of Appendix 6 to this annex.

3.2.4.3. Charge-depleting Type 1 test procedure

3.2.4.3.1. The charge-depleting Type 1 test procedure shall consist of a number of consecutive cycles, each followed by a soak period of no more than 30 minutes until charge-sustaining operating condition is achieved.

3.2.4.3.2. During soaking between individual applicable test cycles, the powertrain shall be deactivated and the REESS shall not be recharged from an external electric energy source. The instrumentation for measuring the electric current of all REESSs and for determining the electric voltage of all REESSs according to Appendix 3 of this annex shall not be turned off between test cycle phases. In the case of ampere-hour meter measurement, the integration shall remain active throughout the entire test until the test is concluded.

Restarting after soak, the vehicle shall be operated in the driver-selectable mode according to paragraph 3.2.4.2.2. of this annex.

3.2.4.3.3. In deviation from paragraph 5.3.1. of Annex B5 and additional to paragraph 5.3.1.2. of Annex B5, analysers may be calibrated and zero- checked before and after the charge-depleting Type 1 test.

3.2.4.4. End of the charge-depleting Type 1 test

The end of the charge-depleting Type 1 test is considered to have been reached when the break-off criterion according to paragraph 3.2.4.5. of this annex is reached for the first time. The number of applicable WLTP test cycles up to and including the one where the break-off criterion was reached for the first time is set to n+1.

The applicable WLTP test cycle n is defined as the transition cycle.

The applicable WLTP test cycle n+1 is defined to be the confirmation cycle.

For vehicles without a charge-sustaining capability over the complete applicable WLTP test cycle, the end of the charge-depleting Type 1 test is reached by an indication on a standard on-board instrument panel to stop the vehicle, or when the vehicle deviates from the prescribed speed trace tolerance for 4 consecutive seconds or more. The accelerator control shall be deactivated and the vehicle shall be braked to standstill within 60 seconds.

3.2.4.5. Break-off criterion

3.2.4.5.1. Whether the break-off criterion has been reached for each driven applicable WLTP test cycle shall be evaluated.

3.2.4.5.2. The break-off criterion for the charge-depleting Type 1 test is reached when the relative electric energy change REECi, as calculated using the following equation, is less than 0.04.

where:

is the relative electric energy change of the applicable test cycle considered i of the charge-depleting Type 1 test;

is the change of electric energy of all REESSs for the considered charge-depleting Type 1 test cycle i calculated according to paragraph 4.3. of this annex, Wh;

is the cycle energy demand of the considered applicable WLTP test cycle calculated according to paragraph 5. of Annex B7, Ws;

i is the index number for the considered applicable WLTP test cycle;

is a conversion factor to Wh for the cycle energy demand.

3.2.4.6. REESS charging and measuring the recharged electric energy

3.2.4.6.1. The vehicle shall be connected to the mains within 120 minutes after the applicable WLTP test cycle n+1 in which the break-off criterion for the charge-depleting Type 1 test is reached for the first time.

The REESS is fully charged when the end-of-charge criterion, as defined in paragraph 2.2.3.2. of Appendix 4 to this annex, is reached.

3.2.4.6.2. The electric energy measurement equipment, placed between the vehicle charger and the mains, shall measure the recharged electric energy EAC delivered from the mains, as well as its duration. Electric energy measurement may be stopped when the end-of-charge criterion, as defined in paragraph 2.2.3.2. of Appendix 4 to this annex, is reached.

3.2.4.7. Each individual applicable WLTP test cycle within the charge-depleting Type 1 test shall fulfil the applicable criteria emission limits according to paragraph 1.2. of AnnexB6.

3.2.5. Charge-sustaining Type 1 test with no subsequent charge-depleting Type 1 test (Option 2)

# The test sequence according to Option 2, as described in paragraphs 3.2.5.1. to 3.2.5.3.3. inclusive of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/2 in Appendix 1 to this annex.

3.2.5.1. Preconditioning and soaking

The vehicle shall be prepared according to the procedures in paragraph 2.1. of Appendix 4 to this annex.

3.2.5.2. Test conditions

3.2.5.2.1. Tests shall be carried out with the vehicle operated in charge-sustaining operating condition as defined in paragraph 3.3.6. of this Regulation.

3.2.5.2.2. Selection of a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the charge-sustaining Type 1 test shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.2.5.3. Type 1 test procedure

3.2.5.3.1. Vehicles shall be tested according to the Type 1 test procedures described in Annex B6.

3.2.5.3.2. If required, the CO2 emission shall be corrected according to Appendix 2 to this annex.

3.2.5.3.3. The test according to paragraph 3.2.5.3.1. of this annex shall fulfil the applicable criteria emission limits according to paragraph 1.2. of Annex B6.

3.2.6. Charge-depleting Type 1 test with a subsequent charge-sustaining Type 1 test (Option 3)

# The test sequence according to Option 3, as described in paragraphs 3.2.6.1. to 3.2.6.3. inclusive of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/3 in Appendix 1 to this annex.

3.2.6.1. For the charge-depleting Type 1 test, the procedure described in paragraphs 3.2.4.1. to 3.2.4.5. inclusive as well as paragraph 3.2.4.7. of this annex shall be followed.

3.2.6.2. Subsequently, the procedure for the charge-sustaining Type 1 test described in paragraphs 3.2.5.1. to 3.2.5.3. inclusive of this annex shall be followed. Paragraphs 2.1.1. and 2.1.2. of Appendix 4 to this annex shall not apply.

3.2.6.3. REESS charging and measuring the recharged electric energy

3.2.6.3.1. The vehicle shall be connected to the mains within 120 minutes after the conclusion of the charge-sustaining Type 1 test.

The REESS is fully charged when the end-of-charge criterion as defined in paragraph 2.2.3.2. of Appendix 4 to this annex is reached.

3.2.6.3.2. The energy measurement equipment, placed between the vehicle charger and the mains, shall measure the recharged electric energy EAC delivered from the mains, as well as its duration. Electric energy measurement may be stopped when the end-of-charge criterion as defined in paragraph 2.2.3.2. of Appendix 4 to this annex is reached.

3.2.7. Charge-sustaining Type 1 test with a subsequent charge-depleting Type 1 test (Option 4)

# The test sequence according to Option 4, described in paragraphs 3.2.7.1. and 3.2.7.2. of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/4 of Appendix 1 to this annex.

3.2.7.1. For the charge-sustaining Type 1 test, the procedure described in paragraphs 3.2.5.1. to 3.2.5.3. inclusive of this annex, as well as paragraph 3.2.6.3.1. of this annex, shall be followed.

3.2.7.2. Subsequently, the procedure for the charge-depleting Type 1 test described in paragraphs 3.2.4.2. to 3.2.4.7. inclusive of this annex shall be followed.

3.3. NOVC-HEVs

The test sequence described in paragraphs 3.3.1. to 3.3.3. inclusive of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/5 of Appendix 1 to this annex.

3.3.1. Preconditioning and soaking

3.3.1.1. Vehicles shall be preconditioned according to paragraph 2.6. of Annex B6.

In addition to the requirements of paragraph 2.6. of Annex B6, the level of the state of charge of the traction REESS for the charge-sustaining test may be set according to the manufacturer’s recommendation before preconditioning in order to achieve a test under charge-sustaining operating condition.

3.3.1.2. Vehicles shall be soaked according to paragraph 2.7. of Annex B6.

3.3.2. Test conditions

3.3.2.1. Vehicles shall be tested under charge-sustaining operating condition as defined in paragraph 3.3.6. of this Regulation.

3.3.2.2. Selection of a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the charge-sustaining Type 1 test shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.3.3. Type 1 test procedure

3.3.3.1. Vehicles shall be tested according to the Type 1 test procedure described in Annex B6.

3.3.3.2. If required, the CO2 emission shall be corrected according to Appendix 2 to this annex.

3.3.3.3. The charge-sustaining Type 1 test shall fulfil the applicable criteria emission limits according to paragraph 1.2. of Annex B6.

3.4. PEVs

3.4.1. General requirements

The test procedure to determine the pure electric range and electric energy consumption shall be selected according to the estimated pure electric range (PER) of the test vehicle from Table A8/3. In the case that the interpolation method is applied, the applicable test procedure shall be selected according to the PER of vehicle H within the specific interpolation family.

Table A8/3

**Procedures to determine pure electric range and electric energy consumption (as applicable)**

|  |  |  |
| --- | --- | --- |
| *Applicable test cycle* | *The estimated PER is…* | *Applicable test procedure* |
| Test cycle according to paragraph 1.4.2.1. of this annex including the extra high phase. | …less than the length of 3 applicable WLTP test cycles. | Consecutive cycle Type 1 test procedure (according to paragraph 3.4.4.1. of this annex). |
| … equal to or greater than the length of 3 applicable WLTP test cycles. | Shortened Type 1 test procedure (according to paragraph 3.4.4.2. of this annex). |
| Test cycle according to paragraph 1.4.2.1. of this annex excluding the extra high phase. | …less than the length of 4 applicable WLTP test cycles. | Consecutive cycle Type 1 test procedure (according to paragraph 3.4.4.1. of this annex). |
| …equal to or greater than the length of 4 applicable WLTP test cycles. | Shortened Type 1 test procedure (according to paragraph 3.4.4.2. of this annex). |
| City cycle according to paragraph 1.4.2.2. of this annex. | …not available over the applicable WLTP test cycle. | Consecutive cycle Type 1 test procedure (according to paragraph 3.4.4.1. of this annex). |

The manufacturer shall give evidence to the responsible authority concerning the estimated pure electric range (PER) prior to the test. In the case that the interpolation method is applied, the applicable test procedure shall be determined based on the estimated PER of vehicle H of the interpolation family. The PER determined by the applied test procedure shall confirm that the correct test procedure was applied.

The test sequence for the consecutive cycle Type 1 test procedure, as described in paragraphs 3.4.2., 3.4.3. and 3.4.4.1. of this annex, as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/6 of Appendix 1 to this annex.

The test sequence for the shortened Type 1 test procedure, as described in paragraphs 3.4.2., 3.4.3. and 3.4.4.2. of this annex as well as the corresponding REESS state of charge profile, are shown in Figure A8.App1/7 in Appendix 1 to this annex.

3.4.2. Preconditioning

The vehicle shall be prepared according to the procedures in paragraph 3. of Appendix 4 to this annex.

3.4.3. Selection of a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the test shall be selected according to paragraph 4. of Appendix 6 to this annex.

3.4.4. PEV Type 1 test procedures

3.4.4.1. Consecutive cycle Type 1 test procedure

3.4.4.1.1. Speed trace and breaks

The test shall be performed by driving consecutive applicable test cycles until the break-off criterion according to paragraph 3.4.4.1.3. of this annex is reached.

Breaks for the driver and/or operator are permitted only between test cycles and with a maximum total break time of 10 minutes. During the break, the powertrain shall be switched off.

3.4.4.1.2. REESS current and voltage measurement

From the beginning of the test until the break-off criterion is reached, the electric current of all REESSs shall be measured according to Appendix 3 to this annex and the electric voltage shall be determined according to Appendix 3 to this annex.

3.4.4.1.3. Break-off criterion

The break-off criterion is reached when the vehicle exceeds the prescribed speed trace tolerance as specified in paragraph 2.6.8.3.1.2. of Annex B6 for 4 consecutive seconds or more. The accelerator control shall be deactivated. The vehicle shall be braked to standstill within 60 seconds.

3.4.4.2. Shortened Type 1 test procedure

3.4.4.2.1. Speed trace

The shortened Type 1 test procedure consists of two dynamic segments ( and ) combined with two constant speed segments ( and ) as shown in Figure A8/2.

Figure A8/2

**Shortened Type 1 test procedure speed trace**



3.4.4.2.1.1. Dynamic segments

Each dynamic segment and consists of an applicable WLTP test cycle according to paragraph 1.4.2.1. of this annex followed by an applicable WLTP city test cycle according to paragraph 1.4.2.2. of this annex.

3.4.4.2.1.2. Constant speed segment

The constant speeds during segments and shall be identical. If the interpolation method is applied, the same constant speed shall be applied within the interpolation family.

(a) Speed specification

The minimum speed of the constant speed segments shall be 100 km/h. If the extra high phase (Extra High3) is excluded (as applicable), the minimum speed of the constant speed segments shall be set to 80 km/h. At the request of manufacturer and with approval of the responsible authority, a higher constant speed in the constant speed segments may be selected.

The acceleration to the constant speed level shall be smooth and accomplished within 1 minute after completion of the dynamic segments and, in the case of a break according to Table A8/4, after initiating the powertrain start procedure.

The deceleration from the constant speed level shall be smooth and accomplished within 1 minute after completion of the constant speed segments.

If the maximum speed of the vehicle is lower than the required minimum speed for the constant speed segments according to the speed specification of this paragraph, the required speed in the constant speed segments shall be equal to the maximum speed of the vehicle.

(b) Distance determination of CSSE and CSSM

The length of the constant speed segment shall be determined based on the percentage of the usable REESS energy according to paragraph 4.4.2.1. of this annex. The remaining energy in the traction REESS after dynamic speed segment shall be equal to or less than 10 per cent of. The manufacturer shall provide evidence to the responsible authority after the test that this requirement is fulfilled.

The length of constant speed segment CSSM may be calculated using the following equation:

where:

dCSSM is the length of constant speed segment CSSM, km;

is the estimated pure electric range of the considered PEV, km;

is the length of dynamic speed segment 1, km;

is the length of dynamic speed segment 2, km;

is the length of constant speed segment , km.

3.4.4.2.1.3. Breaks

Breaks for the driver and/or operator are permitted only in the constant speed segments as prescribed in Table A8/4.

Table A8/4

**Breaks for the driver and/or test operator**

| *Distance driven in constant speed segment CSSM (km)* | *Maximum total break (min)* |
| --- | --- |
| Up to 100 | 10 |
| Up to 150 | 20 |
| Up to 200 | 30 |
| Up to 300 | 60 |
| More than 300 | Shall be based on the manufacturer’s recommendation |
| *Note:* During a break, the powertrain shall be switched off. | |

3.4.4.2.2. REESS current and voltage measurement

From the beginning of the test until the break-off criterion is reached, the electric current of all REESSs and the electric voltage of all REESSs shall be determined according to Appendix 3 to this annex.

3.4.4.2.3. Break-off criterion

The break-off criterion is reached when the vehicle exceeds the prescribed speed trace tolerance as specified in paragraph 2.6.8.3.1.2. of Annex B6 for 4 consecutive seconds or more in the second constant speed segment . The accelerator control shall be deactivated. The vehicle shall be braked to a standstill within 60 seconds.

3.4.4.3. REESS charging and measuring the recharged electric energy

3.4.4.3.1. After coming to a standstill according to paragraph 3.4.4.1.3. of this annex for the consecutive cycle Type 1 test procedure and in paragraph 3.4.4.2.3. of this annex for the shortened Type 1 test procedure, the vehicle shall be connected to the mains within 120 minutes.

The REESS is fully charged when the end-of-charge criterion, as defined in paragraph 2.2.3.2. of Appendix 4 to this annex, is reached.

3.4.4.3.2. The energy measurement equipment, placed between the vehicle charger and the mains, shall measure the recharged electric energy EAC delivered from the mains as well as its duration. Electric energy measurement may be stopped when the end-of-charge criterion, as defined in paragraph 2.2.3.2. of Appendix 4 to this annex, is reached.

3.5. NOVC-FCHVs

The test sequence, described in paragraphs 3.5.1. to 3.5.3. inclusive of this annex, as well as the corresponding REESS state of charge profile, is shown in Figure A8.App1/5 in Appendix 1 to this annex.

3.5.1. Preconditioning and soaking

Vehicles shall be conditioned and soaked according to paragraph 3.3.1. of this annex.

3.5.2. Test conditions

3.5.2.1. Vehicles shall be tested under charge-sustaining operating conditions as defined in paragraph 3.3.6. of this Regulation.

3.5.2.2. Selection of a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the charge-sustaining Type 1 test shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.5.3. Type 1 test procedure

3.5.3.1. Vehicles shall be tested according to the Type 1 test procedure described in Annex B6 and fuel consumption calculated according to Appendix 7 to this annex.

3.5.3.2. If required, fuel consumption shall be corrected according to Appendix 2 to this annex.

4. Calculations for hybrid electric, pure electric and compressed hydrogen fuel cell vehicles

For results after 4 phases and results after 3 phases, the calculations in this chapter need to be performed separately.

4.1. Calculations of gaseous emission compounds, particulate matter emission and particle number emission

4.1.1. Charge-sustaining mass emission of gaseous emission compounds, particulate matter emission and particle number emission for OVC-HEVs and NOVC-HEVs

The charge-sustaining particulate matter emission shall be calculated according to paragraph 3.3. of Annex B7.

The charge-sustaining particle number emission shall be calculated according to paragraph 4. of Annex B7.

4.1.1.1. Stepwise procedure for calculating the final test results of the charge-sustaining Type 1 test for NOVC-HEVs and OVC-HEVs

The results shall be calculated in the order described in Table A8/5. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

For the purpose of this table, the following nomenclature within the equations and results is used:

complete applicable test cycle (to be calculated both for results after 3-phases and for results after 4-phases);

every applicable cycle phase, for the purpose of EAERcity calculation (as applicable), p shall represent the city driving cycle;

applicable criteria emission component (except CO2);

CS charge-sustaining;

CO2 CO2 emission.

Table A8/5

**Calculation of final charge-sustaining gaseous emission and fuel efficiency values (FE applicable for results after 3 phases only)**

Table A8/5 shall be performed separately for results after 4 phases and for results after 3 phases.

| *Step No.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Annex B6 | Raw test results | Charge-sustaining mass emissions  Paragraphs 3. to 3.2.2. inclusive of Annex B7. | , g/km; , g/km. |
| 2 | Output step 1 | , g/km; , g/km. | Calculation of combined charge-sustaining cycle values:  where:  is the charge-sustaining mass emission result over the total cycle;  is the charge-sustaining CO2 emission result over the total cycle;  are the driven distances of the cycle phases p. | , g/km; , g/km. |
| 3 | Output step 1 | , g/km; | REESS electric energy change correction  Paragraphs 4.1.1.2. to 4.1.1.5. inclusive of this annex. | , g/km; , g/km. |
| Output step 2 | , g/km. |
| 4a | Output step 2 | , g/km; | Charge-sustaining mass emission correction for all vehicles equipped with periodically regenerating systems according to Annex B6, Appendix 1.  or and or  Additive offset or multiplicative factor to be used according to Ki determination.  If Ki is not applicable: | , g/km; , g/km. |
| Output step 3 | , g/km. |
| 4b | Output step 3 | , g/km; , g/km; | If Ki is applicable, align CO2 phase values to combined cycle value:  for every cycle phase p;  where:  If Ki is not applicable: | , g/km. |
| Output step 4a | , g/km. |
| 4c | Output step 4a | Mi,CS,c,4a, g/km;  MCO2,CS,c,4a, g/km. | Mi,CS,c,4c = Mi,CS,c,4a  MCO2,CS,c,4c = MCO2,CS,c,4a | Mi,CS,c,4c, g/km;  MCO2,CS,c,4c, g/km. |
| Calculate fuel efficiency (FECS,,4c\_temp) according to paragraph 6.14.1. of Annex B7.  FECS,c,4c = FECS,c,4c\_temp | FE CS,c,4c, km/l; |
| 5  Result of a single test. | Output step 4b and 4c | , g/km; , g/km; | For results after 4 phases:  ATCT correction of MCO2,CS,c,4c and MCO2,CS,p,4 in accordance with paragraph 3.8.3. of Annex B6a.  For results after 3 phases:  MCO2,CS,c,5 = MCO2,CS,c,4c  MCO2,CS,p,5 = MCO2,CS,p,4 | , g/km;, g/km. |
|  | , g/km;FECS,c,4c, km/l; | Apply deterioration factors calculated in accordance with Annex C4 to the criteria emissions values.  FE CS,c,5  = FE CS,c,4c | , g/km;  FE CS,c,5, km/l; |
| 6  results of a Type 1 test for a test vehicle. | For results after 4 phases Output step 5 | For every test: , g/km;, g/km;, g/km. | Averaging of tests and declared value according to paragraphs 1.2. to 1.2.3. inclusive of  Annex B6. | , g/km;, g/km;, g/km; , g/km. |
| For results after 3 phases  Output step 5 | FECS,c,5, km/l;  Mi,CS,c,5, g/km; MCO2,CS,c,5, g/km; MCO2,CS,p,5, g/km. | Averaging of tests and declared value according to paragraphs 1.2. to 1.2.3. inclusive of Annex B6.  The conversion from FECS,c,declared to MCO2,CS,c,declared shall be performed for the applicable cycle. For that purpose, the average criteria emission over the complete cycle shall be used. | FECS,c,declared, km/l; Mi,CS,c,6, g/km; MCO2,CS,c,6, g/km; MCO2,CS,p,6, g/km;  MCO2,CS,c,declared, g/km. |
| 7  results of a Type 1 test for a test vehicle. | Output step 6 | , g/km;, g/km; , g/km. | Alignment of phase values according to paragraph 1.2.4. of Annex B6,  and: | , g/km; , g/km. |
| 8  Final criteria emission result.  If the interpolation method is not applied, step No. 9 is not required and the output of this step is the final CO2 result. | Output step 6 | For each of the test vehicles H and L and, if applicable, vehicle M:  , g/km; | For results after 4 phases only  If in addition to a test vehicle H a test vehicle M and/or vehicle L was also tested, the resulting criteria emission value shall be the highest of the two or, in case vehicle M does not meet the linearity criterion three values and referred to as  In the case of the combined THC+NOx emissions, the highest value of the sum referring to either the vehicle H or vehicle L or, if applicable, vehicle M is to be taken as the type approval value.  Otherwise, if no vehicle L or if applicable vehicle M was tested,  For results after 3 phases and after 4 phases  In the case that the interpolation method is applied, intermediate rounding shall be applied according to paragraph 6.1.8. of this Regulation:  CO2 values derived in step 7 of this table shall be rounded to two places of decimal. Also, the output for CO2 is available for vehicle H and vehicle L and, if applicable, for vehicle M.  In the case that the interpolation method is not applied, final rounding shall be applied according to paragraph 6.1.8. of this Regulation:  CO2 values derived in step 7 of this table shall be rounded to the nearest whole number. | , g/km; , g/km; , g/km; |
| Output step 7 | For each of the test vehicles H and L and, if applicable, vehicle M: , g/km; , g/km. |
| For results after 4 phases only  9  Result of an individual vehicle.  Final CO2 result. | Output step 8 | , g/km; , g/km; | CO2 emission calculation according to paragraph 4.5.4.1. of this annex for individual vehicles in an interpolation family.  Final rounding of individual vehicle CO2 values shall be performed according to paragraph 6.1.8. of this Regulation.  CO2 values shall be rounded to the nearest whole number.  Output is available for each individual vehicle. | , g/km; , g/km. |

4.1.1.2. In the case that the correction according to paragraph 1.1.4. of Appendix 2 to this annex was not applied, the following charge-sustaining CO2 emission shall be used:

where:

is the charge-sustaining CO2 emission of the charge-sustaining Type 1 test according to Table A8/5, step No. 3, g/km;

is the non-balanced charge-sustaining CO2 emission of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to Table A8/5, step No. 2, g/km.

4.1.1.3. If the correction of the charge-sustaining CO2 emission is required according to paragraph 1.1.3. of Appendix 2 to this annex or in the case that the correction according to paragraph 1.1.4. of Appendix 2 to this annex was applied, the CO2 emission correction coefficient shall be determined according to paragraph 2. of Appendix 2 to this annex. The corrected charge-sustaining CO2 emission shall be determined using the following equation:

where:

is the charge-sustaining CO2 emission of the charge-sustaining Type 1 test according to Table A8/5, step No. 3, g/km;

is the non-balanced CO2 emission of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to Table A8/5, step No. 2, g/km;

is the electric energy consumption of the charge-sustaining Type 1 test according to paragraph 4.3. of this annex, Wh/km;

is the CO2 emission correction coefficient according to paragraph 2.3.2. of Appendix 2 to this annex, (g/km)/(Wh/km).

4.1.1.4. In the case that phase-specific CO2 emission correction coefficients have not been determined, the phase-specific CO2 emission shall be calculated using the following equation:

where:

is the charge-sustaining CO2 emission of phase p of the charge-sustaining Type 1 test according to Table A8/5, step No. 3, g/km;

is the non-balanced CO2 emission of phase p of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to Table A8/5, step No. 1, g/km;

is the electric energy consumption of phase p of the charge-sustaining Type 1 test according to paragraph 4.3. of this annex, Wh/km;

is the CO2 emission correction coefficient according to paragraph 2.3.2. of Appendix 2 to this annex, (g/km)/(Wh/km).

4.1.1.5. In the case that phase-specific CO2 emission correction coefficients have been determined, the phase-specific CO2 emission shall be calculated using the following equation:

where:

is the charge-sustaining CO2 emission of phase p of the charge-sustaining Type 1 test according to Table A8/5, step No. 3, g/km;

is the non-balanced CO2 emission of phase p of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to Table A8/5, step No. 1, g/km;

is the electric energy consumption of phase p of the charge-sustaining Type 1 test, determined according to paragraph 4.3. of this annex, Wh/km;

is the CO2 emission correction coefficient according to paragraph 2.3.2.2. of Appendix 2 to this annex, (g/km)/(Wh/km);

is the index of the individual phase within the applicable WLTP test cycle.

4.1.2. Charge-depleting CO2 emission for OVC-HEVs

For 4-phase WLTP test

The utility factor-weighted charge-depleting CO2 emission MCO2,CD shall be calculated using the following equation:

For 3-phase WLTP test

The charge-depleting CO2 emission MCO2,CD shall be calculated using the following equation:

where:

is the utility factor-weighted charge-depleting CO2 emission, g/km;

is the CO2 emission determined according to paragraph 3.2.1. of Annex B7 of phase j of the charge-depleting Type 1 test, g/km;

is the utility factor of phase j according to Appendix 5 to this annex;

is the index number of the considered phase;

is the number of phases driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied, k shall be the number of phases driven up to the end of the transition cycle of vehicle L,

If the transition cycle number driven by vehicle H, , and, if applicable, by an individual vehicle within the vehicle interpolation family, , is lower than the transition cycle number driven by vehicle L, , the confirmation cycle of vehicle H and, if applicable, an individual vehicle shall be included in the calculation. The CO2 emission of each phase of the confirmation cycle shall be subsequently corrected to an electric energy consumption of zero by using the CO2 correction coefficient according to Appendix 2 to this annex.

4.1.3. This paragraph is applicable for 4-phase WLTP test only:

Utility factor-weighted mass emissions of gaseous compounds, particulate matter emission and particle number emission for OVC-HEVs

4.1.3.1. The utility factor-weighted mass emission of gaseous compounds

4.1.3.1.1. For calculating the utility factor-weighted mass of gaseous compounds (except CO2 emission), the following equation shall be used

where:

is the utility factor-weighted mass emission compound i, g/km;

is the index of the considered gaseous emission compound (except CO2);

is the utility factor of phase j according to Appendix 5 to this annex;

is the mass emission of the gaseous emission compound i determined according to paragraph 3.2.1. of Annex B7 of phase j of the charge-depleting Type 1 test, g/km;

is the charge-sustaining mass emission of gaseous emission compound i for the charge-sustaining Type 1 test according to Table A8/5, step No. 6, g/km;

is the index number of the considered phase;

is the number of phases driven until the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

4.1.3.1.2. For calculating the utility-factor weighted CO2 emission the following equation shall be used:

where:

is the utility-factor weighted charge-depleting CO2 emission, g/km.

is the declared charge-depleting CO2 emission according to Table A8/8, step no. 14, g/km.

is the declared charge-sustaining CO2 emission according to Table A8/5, step no. 7, g/km.

j is the index number of the considered phase;

k is the number of phases driven until the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied for CO2, k shall be the number of phases driven up to the end of the transition cycle of vehicle L .

If the transition cycle number driven by vehicle H, , and, if applicable, by an individual vehicle within the vehicle interpolation family is lower than the transition cycle number driven by vehicle L, , the confirmation cycle of vehicle H and, if applicable, an individual vehicle shall be included in the calculation. The CO2 emission of each phase of the confirmation cycle shall then be corrected to an electric energy consumption of zero ) by using the CO2 correction coefficient according to Appendix 2 to this annex.

4.1.3.2. The utility factor-weighted particle number emission shall be calculated using the following equation:

where:

is the utility factor-weighted particle number emission, particles per kilometre;

is the utility factor of phase j according to Appendix 5 to this annex;

is the particle number emission during phase j determined according to paragraph 4. of Annex B7 for the charge-depleting Type 1 test, particles per kilometre;

is the particle number emission determined according to paragraph 4.1.1. of this annex for the charge-sustaining Type 1 test, particles per kilometre;

is the index number of the considered phase;

is the number of phases driven until the end of transition cycle n according to paragraph 3.2.4.4. of this annex.

4.1.3.3. The utility factor-weighted particulate matter emission shall be calculated using the following equation:

where:

is the utility factor-weighted particulate matter emission, mg/km;

is the utility factor of cycle c according to Appendix 5 to this annex;

is the charge-depleting particulate matter emission during cycle c determined according to paragraph 3.3. of Annex B7 for the charge-depleting Type 1 test, mg/km;

is the particulate matter emission of the charge-sustaining Type 1 test according to paragraph 4.1.1. of this annex, mg/km;

is the index number of the cycle considered;

is the number of applicable WLTP test cycles driven until the end of the transition cycle n according to paragraph 3.2.4.4. of this annex.

4.2. Calculation of fuel consumption and fuel efficiency

4.2.1. Charge-sustaining fuel consumption and fuel efficiency for OVC-HEVs, NOVC-HEVs and NOVC-FCHVs

4.2.1.1. The charge-sustaining fuel consumption and fuel efficiency for OVC-HEVs and NOVC-HEVs shall be calculated stepwise according to Table A8/6.

Table A8/6

**Calculation of final charge-sustaining fuel consumption and fuel efficiency for OVC-HEVs, NOVC-HEVs (FE applicable for results after 3 phases only)**

Table A8/6 shall be performed separately for results after 4 phases and for results after 3 phases.

| *Step No.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Output step 6,  Table A8/5 | , g/km;  , g/km; FECS,c,declared, km/l; | Calculation of fuel consumption FCCS,c according to paragraph 6. of Annex B7 based on MCO2,CS,C,7 and conversion to fuel efficiency FECS,p,1. for phase value  FECS,c,1, = FECS,c,declared,  The calculation of fuel consumption shall be performed separately for the applicable cycle and its phases.  For that purpose: (a) the applicable phase or cycle CO2 values shall be used; (b) the criteria emission over the complete cycle shall be used. | , l/100 km; FECS,c,1, km/l;   , l/100 km. km/l |
| Output step 7,  Table A8/5 | , g/km; , g/km. |
| 2  If the interpolation method is not applied, step No. 3 is not required and the output of this step is the final result. | Output step 1 | , l/100 km; , l/100 km;  FECS,c,1, km/l. , km/l | For FC and FE, the values derived in step No. 1 of this table shall be used.  In the case that the interpolation method is applied, intermediate rounding shall be applied according to paragraph 6.1.8. of this Regulation.  FC and FE values shall be rounded to three places of decimal.  Output is available for vehicle H and vehicle L and, if applicable, for vehicle M.  In the case that the interpolation method is not applied, final rounding shall be applied according to paragraph 6.1.8. of this Regulation.  FC and FE values shall be rounded to first place of decimal. | , l/100 km; , l/100 km;  FECS,c, km/l.  FECS,p, km/l. |
| 3  Result of an individual vehicle.  Final FC and FE result. | Output step 2 | , l/100 km; , l/100 km;  FECS,c, km/l. FECS,p, km/l. | Fuel consumption calculation according to paragraph 4.5.5.1.1. of this annex for individual vehicles in an interpolation family.  Fuel efficiency calculation according to paragraph 4.5.5.1.2. of this annex for individual vehicles in an interpolation family.  Final rounding of individual vehicle values shall be performed according to paragraph 6.1.8. of this Regulation.  FC and FE values shall be rounded to the first place of decimal.  Output is available for each individual vehicle. | , l/100 km; , l/100 km;  FECS,c,ind, km/l.  FECS,p,ind, km/l. |

4.2.1.2. Charge-sustaining fuel consumption and fuel efficiency for NOVC-FCHVs

4.2.1.2.1. Stepwise procedure for calculating the final test fuel consumption and fuel efficiency results of the charge-sustaining Type 1 test for NOVC-FCHVs

The results shall be calculated in the order described in Table A8/7. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

For the purpose of this table, the following nomenclature within the equations and results is used:

complete applicable test cycle;

every applicable cycle phase; for the purpose of EAERcity calculation (as applicable), p shall represent the city driving cycle;

CS charge-sustaining

Table A8/7

**Calculation of final charge-sustaining fuel consumption and fuel efficiency for NOVC-FCHVs (FE applicable for results after 3 phases only)**

Table A8/7 shall be performed separately for results after 4 phases and for results after 3 phases.

For results after 4-phases all the calculations in this table shall be for the complete cycle

For the 3-phase WLTP all the calculations in this table shall be for the 3-phase cycle and also for individual phases

| *Step No.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Appendix 7 to this annex. | Non-balanced charge-sustaining fuel consumption  FCCS,nb, kg/100km | Charge-sustaining fuel consumption FCCS,c,1 according to paragraph 2.2.6. of Appendix 7 to this annex.  The calculation of fuel consumption shall be performed separately for the applicable cycle and its phases.  For that purpose, the applicable phase or cycle FC values shall be used;  Phase-specific values according to paragraph 2.2.7. of Appendix 7 to this annex). | , kg/100 km; , kg/100 km. |
| 2 | Output step 1 | , kg/100 km; , kg/100 km. | REESS electric energy change correction.  Paragraphs 4.2.1.2.2. to 4.2.1.2.5. (where applicable) inclusive of this annex. | , kg/100 km;  For results after 3 phases  , kg/100 km; |
| 3  Result of a single test. | Output step 2 | , kg/100 km; , kg/100 km. | For results after 3 phases  Conversion of fuel consumption FC into fuel efficiency FE | , kg/100 km; , kg/100 km. , km/kg. , km/kg. |
| 4 | Output step 3 | For every test: , kg/100 km; , kg/100 km. , km/kg. , km/kg. | Averaging of tests and declared value according to paragraphs 1.2. to 1.2.3. inclusive of Annex B6. | , kg/100 km; , kg/100 km. , km/kg. , km/kg. |
| 5  If the interpolation method is not applied, step No. 6 is not required and the output of this step is the final result.  results of a Type 1 test for a test vehicle. | Output step 4 | , kg/100 km; , kg/100 km; , kg/100 km.  , km/kg. , km/kg; , km/ kg. | Alignment of phase values. Paragraph 1.2.4. of Annex B6,  and:  FC and FE values shall be rounded according to paragraph 6.1.8. of this Regulation.  FC shall be rounded to the third place of decimal.  FE shall be rounded to the nearest whole number.  In the case that the interpolation method is not applied, final rounding of FC shall be applied according to paragraph 6.1.8. of this Regulation to the second place of decimal. | , kg/100 km; , kg/100 km FECS,p,5, km/kg. FECS,c,5, km/kg. |
| 6  Result of an individual vehicle.  Final FC result. | Output step 5 | , kg/100 km; | Fuel consumption calculation according to paragraph 4.5.5.1.3. of this annex for individual vehicles in an interpolation family.  Final rounding of individual vehicle values shall be performed according to paragraph 6.1.8. of this Regulation.  FC values shall be rounded to the second place of decimal.  Output is available for each individual vehicle. | , kg/100 km; |

4.2.1.2.2. In the case that the correction according to paragraph 1.1.4. of Appendix 2 to this annex was not applied, the following charge-sustaining fuel consumption shall be used:

where:

is the charge-sustaining fuel consumption of the charge-sustaining Type 1 test according to Table A8/7, step No. 2, kg/100 km;

is the non-balanced charge-sustaining fuel consumption of the charge-sustaining Type 1 test, not corrected for the energy balance, according to Table A8/7, step No. 1, kg/100 km.

4.2.1.2.3. If the correction of the fuel consumption is required according to paragraph 1.1.3. of Appendix 2 to this annex or in the case that the correction according to paragraph 1.1.4. of Appendix 2 to this annex was applied, the fuel consumption correction coefficient shall be determined according to paragraph 2. of Appendix 2 to this annex. The corrected charge-sustaining fuel consumption shall be determined using the following equation:

where:

is the charge-sustaining fuel consumption of the charge-sustaining Type 1 test according to Table A8/7, step No. 2, kg/100 km;

is the non-balanced fuel consumption of the charge-sustaining Type 1 test, not corrected for the energy balance, according to Table A8/7, step No. 1, kg/100 km;

is the electric energy consumption of the charge-sustaining Type 1 test according to paragraph 4.3. of this annex, Wh/km;

is the fuel consumption correction coefficient according to paragraph 2.3.1. of Appendix 2 to this annex, (kg/100 km)/(Wh/km).

4.2.1.2.4. In the case that phase-specific fuel consumption correction coefficients have not been determined, the phase-specific fuel consumption shall be calculated using the following equation:

where:

is the charge-sustaining fuel consumption of phase p of the charge-sustaining Type 1 test according to Table A8/7, step No. 2, kg/100 km;

is the non-balanced fuel consumption of phase p of the charge-sustaining Type 1 test, not corrected for the energy balance, according to Table A8/7, step No. 1, kg/100 km;

is the electric energy consumption of phase p of the charge-sustaining Type 1 test, determined according to paragraph 4.3. of this annex, Wh/km;

is the fuel consumption correction coefficient according to paragraph 2.3.1. of Appendix 2 to this annex, (kg/100 km)/(Wh/km);

is the index of the individual phase within the applicable WLTP test cycle.

4.2.1.2.5. In the case that phase-specific fuel consumption correction coefficients have been determined, the phase-specific fuel consumption shall be calculated using the following equation:

where:

is the charge-sustaining fuel consumption of phase p of the charge-sustaining Type 1 test according to Table A8/7, step No. 2, kg/100 km;

is the non-balanced fuel consumption of phase p of the charge-sustaining Type 1 test, not corrected for the energy balance, according to Table A8/7, step No. 1, kg/100 km;

is the electric energy consumption of phase p of the charge-sustaining Type 1 test, determined according to paragraph 4.3. of this annex, Wh/km;

is the fuel consumption correction coefficient for the correction of the phase p according to paragraph 2.3.1.2. of Appendix 2 to this annex, (kg/100 km)/(Wh/km);

is the index of the individual phase within the applicable WLTP test cycle.

4.2.2. The charge-depleting fuel consumption and charge-depleting fuel efficiency for OVC-HEVs

For 4-phase WLTP test:

The utility factor-weighted charge-depleting fuel consumption shall be calculated using the following equation:

where:

is the utility factor weighted charge-depleting fuel consumption, l/100 km;

is the fuel consumption for phase j of the charge-depleting Type 1 test, determined according to paragraph 6. of Annex B7, l/100 km;

is the utility factor of phase j according to Appendix 5 to this annex;

is the index number for the considered phase;

is the number of phases driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied, k shall be the number of phases driven up to the end of the transition cycle of vehicle L

If the transition cycle number driven by vehicle H, , and, if applicable, by an individual vehicle within the vehicle interpolation family, , is lower than the transition cycle number driven by vehicle L the confirmation cycle of vehicle H and, if applicable, an individual vehicle shall be included in the calculation.

The fuel consumption of each phase of the confirmation cycle shall be calculated according to paragraph 6. of Annex B7 with the criteria emission over the complete confirmation cycle and the applicable CO2 phase value which shall be corrected to an electric energy consumption of zero, , by using the CO2 mass correction coefficient (KCO2) according to Appendix 2 to this annex.

For 3-phase WLTP test

The charge-depleting fuel efficiency shall be calculated using the following equation:

where:

is the charge-depleting fuel efficiency, km/l;

actual charge-depleting range defined in paragraph 4.4.5. of this annex, km;

is the fuel efficiency for cycle c of the charge-depleting Type 1 test, determined according to paragraph 6. of Annex B7, km/l;

;

is the index number for the considered cycle;

n is the number of applicable WLTP test cycles driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex

is the distance driven in the applicable WLTP test cycle c of the charge-depleting Type 1 test, km;

is the distance driven in the applicable WLTP test cycle n of the charge-depleting Type 1 test, km;

4.2.3. This paragraph is applicable only for 4-phase WLTP test

Utility factor-weighted fuel consumption for OVC-HEVs

The utility factor-weighted fuel consumption for OVC-HEVs from the charge-depleting and charge-sustaining Type 1 test shall be calculated using the following equation:

where:

is the utility factor-weighted fuel consumption, l/100 km;

is the utility factor of phase jaccording to Appendix 5 to this annex;

is the fuel consumption of phase j of the charge-depleting Type 1 test, determined according to paragraph 6. of Annex B7, l/100 km;

is the declared charge-depleting CO2 emission according to Table A8/8, step no. 14, g/km;

is the arithmetic average charge-depleting CO2 emission according to Table A8/8, step no. 13, g/km;

is the fuel consumption determined according to Table A8/6, step No. 1, l/100 km;

is the index number for the considered phase;

is the number of phases driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied, k shall be the number of phases driven up to the end of the transition cycle of vehicle L

If the transition cycle number driven by vehicle H, , and, if applicable, by an individual vehicle within the vehicle interpolation family is lower than the transition cycle number driven by vehicle L, , the confirmation cycle of vehicle H and, if applicable, an individual vehicle shall be included in the calculation.

The fuel consumption of each phase of the confirmation cycle shall be calculated according to paragraph 6. of Annex B7 with the criteria emission over the complete confirmation cycle and the applicable CO2 phase value which shall be corrected to an electric energy consumption of zero  by using the CO2 mass correction coefficient (KCO2) according to Appendix 2 to this annex.

4.3. Calculation of electric energy consumption

For the determination of the electric energy consumption based on the current and voltage determined according to Appendix 3 to this annex, the following equations shall be used:

where:

is the electric energy consumption over the considered period j based on the REESS depletion, Wh/km;

is the electric energy change of all REESSs during the considered period j, Wh;

is the distance driven in the considered period j, km;

and

where:

is the electric energy change of REESS i during the considered period j, Wh;

and

where:

is the voltage of REESS i during the considered period j determined according to Appendix 3 to this annex, V;

is the time at the beginning of the considered period j, s;

is the time at the end of the considered period j, s;

is the electric current of REESS i during the considered period j determined according to Appendix 3 to this annex, A;

is the index number of the considered REESS;

is the total number of REESS;

is the index for the considered period, where a period can be any combination of phases or cycles;

is the conversion factor from Ws to Wh.

4.3.1. This paragraph is applicable only for 4-phase WLTP test

Utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains for OVC-HEVs

The utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains shall be calculated using the following equation:

where:

is the utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains, Wh/km;

is the utility factor of phase j according to Appendix 5 to this annex;

is the electric energy consumption based on the recharged electric energy from the mains of phase j, Wh/km;

and

where:

is the electric energy consumption based on the REESS depletion of phase j of the charge-depleting Type 1 test according to paragraph 4.3. of this annex, Wh/km;

is the recharged electric energy from the mains determined according to paragraph 3.2.4.6. of this annex, Wh;

is the electric energy change of all REESSs of phase j according to paragraph 4.3. of this annex, Wh;

is the index number for the considered phase;

is the number of phases driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied, k is the number of phases driven up to the end of the transition cycle of L,nveh\_L.

4.3.2. This paragraph is applicable for 4-phase WLTP test only:

Utility factor-weighted electric energy consumption based on the recharged electric energy from the mains for OVC-HEVs

The utility factor-weighted electric energy consumption based on the recharged electric energy from the mains shall be calculated using the following equation:

where:

is the utility factor-weighted electric energy consumption based on the recharged electric energy from the mains, Wh/km;

is the utility factor of phase j according to Appendix 5 to this annex;

is the declared charge-depleting electric energy consumption based on the recharged electric energy from the mains for OVC-HEVs according to Table A8/8, step 14, Wh/km;

is the index number for the considered phase;

is the number of phases driven up to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

In the case that the interpolation method is applied, k is the number of phases driven up to the end of the transition cycle of vehicle L, nveh\_L.

4.3.3. Electric energy consumption for OVC-HEVs

4.3.3.1. Determination of cycle-specific electric energy consumption

The electric energy consumption based on the recharged electric energy from the mains and the equivalent all-electric range shall be calculated using the following equation:

where:

is the electric energy consumption of the applicable WLTP test cycle based on the recharged electric energy from the mains and the equivalent all-electric range, Wh/km;

is the recharged electric energy from the mains according to paragraph 3.2.4.6. of this annex, Wh;

is the equivalent all-electric range for OVC-HEVs according to paragraph 4.4.4.1. of this annex, km.

4.3.3.2. Determination of phase-specific electric energy consumption

The phase-specific electric energy consumption based on the recharged electric energy from the mains and the phase-specific equivalent all-electric range shall be calculated using the following equation:

where:

is the phase-specific electric energy consumption based on the recharged electric energy from the mains and the equivalent all-electric range, Wh/km;

is the recharged electric energy from the mains according to paragraph 3.2.4.6. of this annex, Wh;

is the phase-specific equivalent all-electric range according to paragraph 4.4.4.2. of this annex, km.

4.3.4. Electric energy consumption of PEVs

4.3.4.1. The electric energy consumption determined in this paragraph shall be calculated only if the vehicle was able to follow the applicable WLTP test cycle within the speed trace tolerances according to paragraph 2.6.8.3.1.2. of Annex B6 during the entire considered period.

4.3.4.2. Electric energy consumption determination of the applicable WLTP test cycle

The electric energy consumption of the applicable WLTP test cycle based on the recharged electric energy from the mains and the pure electric range shall be calculated using the following equation:

where:

is the electric energy consumption of the applicable WLTP test cycle based on the recharged electric energy from the mains and the pure electric range for the applicable WLTP test cycle, Wh/km;

is the recharged electric energy from the mains according to paragraph 3.4.4.3. of this annex, Wh;

is the pure electric range for the applicable WLTP test cycle as calculated according to paragraph 4.4.2.1.1. or paragraph 4.4.2.2.1. of this annex, depending on the PEV test procedure used, km.

4.3.4.3. Electric energy consumption determination of the applicable WLTP city test cycle (if applicable)

The electric energy consumption of the applicable WLTP city test cycle based on the recharged electric energy from the mains and the pure electric range for the applicable WLTP city test cycle shall be calculated using the following equation:

where:

is the electric energy consumption of the applicable WLTP city test cycle based on the recharged electric energy from the mains and the pure electric range for the applicable WLTP city test cycle, Wh/km;

is the recharged electric energy from the mains according to paragraph 3.4.4.3. of this annex, Wh;

is the pure electric range for the applicable WLTP city test cycle as calculated according to paragraph 4.4.2.1.2. or paragraph 4.4.2.2.2. of this annex, depending on the PEV test procedure used, km.

4.3.4.4. Electric energy consumption determination of the phase-specific values

The electric energy consumption of each individual phase based on the recharged electric energy from the mains and the phase-specific pure electric range shall be calculated using the following equation:

where:

is the electric energy consumption of each individual phase p based on the recharged electric energy from the mains and the phase-specific pure electric range, Wh/km

is the recharged electric energy from the mains according to paragraph 3.4.4.3. of this annex, Wh;

is the phase-specific pure electric range as calculated according to paragraph 4.4.2.1.3. or paragraph 4.4.2.2.3. of this annex, depending on the PEV test procedure used, km.

4.4. Calculation of electric ranges

4.4.1. All-electric ranges AER and for OVC-HEVs

4.4.1.1. All-electric range AER

The all-electric range AER for OVC-HEVs shall be determined from the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex as part of the Option 1 test sequence and referenced in paragraph 3.2.6.1. of this annex as part of the Option 3 test sequence by driving the applicable WLTP test cycle according to paragraph 1.4.2.1. of this annex. The AER is defined as the distance driven from the beginning of the charge-depleting Type 1 test to the point in time where the combustion engine starts consuming fuel.

4.4.1.2. All-electric range city (if applicable)

4.4.1.2.1. The all-electric range city for OVC-HEVs shall be determined from the charge-depleting Type 1 test described in paragraphs 3.2.4.1., 3.2.4.2. and 3.2.4.3. of this annex as part of the Option 1 test sequence by driving the applicable WLTP city test cycle according to paragraph 1.4.2.2. of this annex. The is defined as the distance driven from the beginning of the charge-depleting Type 1 test to the point in time where the combustion engine starts consuming fuel.

The point in time where the combustion engine starts consuming fuel shall be considered as the break-off criterion and shall replace the break-off criterion described in paragraph 3.2.4.4.

4.4.1.2.2. As an alternative to paragraph 4.4.1.2.1. of this annex, the all-electric range city may be determined from the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex by driving the applicable WLTP test cycles according to paragraph 1.4.2.1. of this annex. In that case, the charge-depleting Type 1 test by driving the applicable WLTP city test cycle shall be omitted and the all-electric range city shall be calculated using the following equation:

where:

AERcity is the all-electric range city, km;

is the usable REESS energy determined from the beginning of the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex by driving applicable WLTP test cycles until the point in time when the combustion engine starts consuming fuel, Wh;

is the weighted electric energy consumption of the pure electrically driven applicable WLTP city test cycles of the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex by driving applicable WLTP test cycle(s), Wh/km;

and

where:

is the electric energy change of all REESSs during phase j, Wh;

is the index number of the considered phase;

k+1 is the number of the phases driven from the beginning of the test until the point in time when the combustion engine starts consuming fuel;

and

where:

is the electric energy consumption for the jth pure electrically driven WLTP city test cycle of the charge-depleting Type 1 test according to paragraph 3.2.4.3. of this annex by driving applicable WLTP test cycles, Wh/km;

is the weighting factor for the jth pure electrically driven applicable WLTP city test cycle of the charge-depleting Type 1 test according to paragraph 3.2.4.3. of this annex by driving applicable WLTP test cycles;

is the index number of the pure electrically driven applicable WLTP city test cycle considered;

is the number of pure electrically driven applicable WLTP city test cycles;

and

where:

is the electric energy change of all REESSs during the first applicable WLTP city test cycle of the charge-depleting Type 1 test, Wh;

and

for .

4.4.2. Pure electric range for PEVs

The ranges determined in this paragraph shall only be calculated if the vehicle was able to follow the applicable WLTP test cycle within the speed trace tolerances according to paragraph 2.6.8.3.1.2. of Annex B6 during the entire considered period.

4.4.2.1. Determination of the pure electric ranges when the shortened Type 1 test procedure is applied

4.4.2.1.1. The pure electric range for the applicable WLTP test cycle PERWLTC for PEVs shall be calculated from the shortened Type 1 test as described in paragraph 3.4.4.2. of this annex using the following equations:

where:

PERWLTC is the pure electric range for the applicable WLTC test cycle for PEVs, km;

is the usable REESS energy determined from the beginning of the shortened Type 1 test procedure until the break-off criterion as defined in paragraph 3.4.4.2.3. of this annex is reached, Wh;

is the weighted electric energy consumption for the applicable WLTP test cycle of the shortened Type 1 test procedure, Wh/km;

and

where:

is the electric energy change of all REESSs during DS1 of the shortened Type 1 test procedure, Wh;

is the electric energy change of all REESSs during DS2 of the shortened Type 1 test procedure, Wh;

is the electric energy change of all REESSs during CSSM of the shortened Type 1 test procedure, Wh;

is the electric energy change of all REESSs during CSSE of the shortened Type 1 test procedure, Wh;

and

where:

is the electric energy consumption for the applicable WLTP test cycle of DSj of the shortened Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for the applicable WLTP test cycle of DSj of the shortened Type 1 test procedure;

and:

where:

is the weighting factor for the applicable WLTP test cycle of DSj of the shortened Type 1 test procedure;

is the electric energy change of all REESSs during the applicable WLTP test cycle of DS1 of the shortened Type 1 test procedure, Wh.

4.4.2.1.2. Pure Electric Range city (PERcity) (if applicable)

The pure electric range for the applicable WLTP city test cycle PERcity for PEVs shall be calculated from the shortened Type 1 test procedure as described in paragraph 3.4.4.2. of this annex using the following equations:

where:

PERcity is the pure electric range for the applicable WLTP city test cycle for PEVs, km;

is the usable REESS energy according to paragraph 4.4.2.1.1. of this annex, Wh;

is the weighted electric energy consumption for the applicable WLTP city test cycle of DS1 and DS2 of the shortened Type 1 test procedure, Wh/km;

and

where:

is the electric energy consumption for the applicable WLTP city test cycle where the first applicable WLTP city test cycle of DS1 is indicated asj = 1, the second applicable WLTP city test cycle of DS1 is indicated as j = 2, the first applicable WLTP city test cycle of DS2 is indicated as j = 3 and the second applicable WLTP city test cycle of DS2 is indicated as j = 4 of the shortened Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for the applicable WLTP city test cycle where the first applicable WLTP city test cycle of DS1 is indicated as j = 1, the second applicable WLTP city test cycle of DS1 is indicated as j = 2, the first applicable WLTP city test cycle of DS2 is indicated as j = 3 and the second applicable WLTP city test cycle of DS2 is indicated asj = 4,

and

where:

is the energy change of all REESSs during the first applicable WLTP city test cycle of DS1 of the shortened Type 1 test procedure, Wh.

4.4.2.1.3. The phase-specific pure electric range PERp for PEVs shall be calculated from the Type 1 test as described in paragraph 3.4.4.2. of this annex by using the following equations:

where:

PERp is the phase-specific pure electric range for PEVs, km;

is the usable REESS energy according to paragraph 4.4.2.1.1. of this annex, Wh;

is the weighted electric energy consumption for each individual phase of DS1 and DS2 of the shortened Type 1 test procedure, Wh/km;

In the case that phase p = low and phase p = medium, the following equations shall be used:

where:

is the electric energy consumption for phase p where the first phase p of DS1 is indicated as j = 1, the second phase p of DS1 is indicated as j = 2, the first phase p of DS2 is indicated as j = 3 and the second phase p of DS2 is indicated as j = 4 of the shortened Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for phase p where the first phase p of DS1 is indicated as j = 1, the second phase p of DS1 is indicated as j = 2, the first phase p of DS2 is indicated as j = 3, and the second phase p of DS2 is indicated as j = 4 of the shortened Type 1 test procedure;

and

where:

is the energy change of all REESSs during the first phase p of DS1 of the shortened Type 1 test procedure, Wh.

In the case that phase p = high and phase p = extra high, the following equations shall be used:

where:

is the electric energy consumption for phase p of DSj of the shortened Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for phase p of DSj of the shortened Type 1 test procedure

and

where:

is the electric energy change of all REESSs during the first phase p of DS1 of the shortened Type 1 test procedure, Wh.

4.4.2.2. Determination of the pure electric ranges when the consecutive cycle Type 1 test procedure is applied

4.4.2.2.1. The pure electric range for the applicable WLTP test cycle PERWLTP for PEVs shall be calculated from the Type 1 test as described in paragraph 3.4.4.1. of this annex using the following equations:

where:

is the usable REESS energy determined from the beginning of the consecutive cycle Type 1 test procedure until the break-off criterion according to paragraph 3.4.4.1.3. of this annex is reached, Wh;

is the electric energy consumption for the applicable WLTP test cycle determined from completely driven applicable WLTP test cycles of the consecutive cycle Type 1 test procedure, Wh/km;

and

where:

is the electric energy change of all REESSs during phase j of the consecutive cycle Type 1 test procedure, Wh;

is the index number of the phase;

is the number of phases driven from the beginning up to and including the phase where the break-off criterion is reached;

and:

where:

is the electric energy consumption for the applicable WLTP test cycle j of the consecutive cycle Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for the applicable WLTP test cycle j of the consecutive cycle Type 1 test procedure;

is the index number of the applicable WLTP test cycle;

is the whole number of complete applicable WLTP test cycles driven;

and

where:

is the electric energy change of all REESSs during the first applicable WLTP test cycle of the consecutive cycle Type 1 test procedure, Wh.

4.4.2.2.2. Pure Electric Range city (PERcity) (if applicable)

The pure electric range for the WLTP city test cycle PERcity for PEVs shall be calculated from the Type 1 test as described in paragraph 3.4.4.1. of this annex using the following equations:

where:

PERcity is the pure electric range for the WLTP city test cycle for PEVs, km;

is the usable REESS energy according to paragraph 4.4.2.2.1. of this annex, Wh;

is the electric energy consumption for the applicable WLTP city test cycle determined from completely driven applicable WLTP city test cycles of the consecutive cycle Type 1 test procedure, Wh/km;

and

where:

is the electric energy consumption for the applicable WLTP city test cycle j of the consecutive cycle Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the weighting factor for the applicable WLTP city test cycle j of the consecutive cycle Type 1 test procedure;

is the index number of the applicable WLTP city test cycle;

is the whole number of complete applicable WLTP city test cycles driven;

and

where:

is the electric energy change of all REESSs during the first applicable WLTP city test cycle of the consecutive cycle Type 1 test procedure, Wh.

4.4.2.2.3. The phase-specific pure electric range PERp for PEVs shall be calculated from the Type 1 test as described in paragraph 3.4.4.1. of this annex using the following equations:

where:

PERp is the phase-specific pure electric range for PEVs, km;

is the usable REESS energy according to paragraph 4.4.2.2.1. of this annex, Wh;

is the electric energy consumption for the considered phase p determined from completely driven phases p of the consecutive cycle Type 1 test procedure, Wh/km;

and

where:

is the jth electric energy consumption for the considered phase p of the consecutive cycle Type 1 test procedure according to paragraph 4.3. of this annex, Wh/km;

is the jth weighting factor for the considered phase p of the consecutive cycle Type 1 test procedure;

is the index number of the considered phase p;

is the whole number of complete WLTC phases p driven;

and

where:

is the electric energy change of all REESSs during the first driven phase p during the consecutive cycle Type 1 test procedure, Wh.

4.4.3. Charge-depleting cycle range for OVC-HEVs

The charge-depleting cycle range RCDC shall be determined from the charge-depleting Type 1 test described in paragraph 3.2.4.3. of this annex as part of the Option 1 test sequence and referenced in paragraph 3.2.6.1. of this annex as part of the Option 3 test sequence. The is the distance driven from the beginning of the charge-depleting Type 1 test to the end of the transition cycle according to paragraph 3.2.4.4. of this annex.

4.4.4. Equivalent all-electric range for OVC-HEVs

4.4.4.1. Determination of cycle-specific equivalent all-electric range

The cycle-specific equivalent all-electric range shall be calculated using the following equation:

For 4-phase WLTP test;

For 3-phase WLTP test;

where:

is the cycle-specific equivalent all-electric range, km;

is the arithmetic average of charge-sustaining CO2 emission according to Table A8/5, step No. 6 (MCO2,CS,c,6) for 4-phase WLTP test, g/km;

is the declared charge-sustaining CO2 emission according to Table A8/5, step No. 6 (MCO2,CS,c,declared) for 3-phase WLTP test, g/km;

is the arithmetic average of calculated for all individual charge-depleting tests according to the equation below, g/km;

is the charge-depleting cycle range according to paragraph 4.4.3. of this annex, km;

is the arithmetic average charge-depleting cycle range calculated for all individual charge-depleting tests, km;

and

where:

is the charge-depleting CO2 emission, g/km.;

is the CO2 emission determined according to paragraph 3.2.1. of Annex B7 of phase j of the charge-depleting Type 1 test, g/km;

is the distance driven in phase j of the charge-depleting Type 1 test, km;

is the index number of the considered phase;

is the number of phases driven up to the end of the transition cycle n according to paragraph 3.2.4.4. of this annex.

4.4.4.2. Determination of the phase-specific equivalent all-electric range

The phase-specific equivalent all-electric range shall be calculated using the following equation:

For 4-phase WLTP test:

For 3-phase WLTP test:

where:

is the phase-specific equivalent all-electric range for the considered phase p, km;

is the phase-specific CO2 emission from the charge-sustaining Type 1 test for the considered phase p according to Table A8/5, step No. 7 (MCO2,CS,p,7), g/km;

is the phase specific CO2 emission from the charge-sustaining Type 1 test for the considered phase p according to Table A8/5, step No. 6 (MCO2,CS,p,6), g/km;

is the arithmetic average of calculated for all individual charge-depleting tests according to the equation below, g/km;

are the electric energy changes of all REESSs during the considered phase j, Wh. ;

is the arithmetic average of electric energy changes of all REESSs during the considered phase j calculated for all individual charge-depleting tests, Wh.

is the arithmetic average of electric energy consumption over the considered phase p ( calculated according to the equation below for all individual charge-depleting tests, Wh/km;

is the index number of the considered phase;

k is the number of phases driven up to the end of the transition cycle n according to paragraph 3.2.4.4 of this annex;

and

where:

is the charge-depleting CO2 emission for the considered phase p, g/km. ;

is the CO2 emission determined according to paragraph 3.2.1. of Annex B7 of phase p in cycle c of the charge-depleting Type 1 test, g/km;

is the distance driven in the considered phase p of cycle c of the charge-depleting Type 1 test, km;

is the index number of the considered applicable WLTP test cycle;

is the index of the individual phase within the applicable WLTP test cycle;

is the number of applicable WLTP test cycles driven up to the end of the transition cycle n according to paragraph 3.2.4.4. of this annex;

and:

where:

is the electric energy consumption of the considered phase p based on the REESS depletion of the charge-depleting Type 1 test, Wh/km.;

is the electric energy consumption of the considered phase p of cycle c based on the REESS depletion of the charge-depleting Type 1 test according to paragraph 4.3. of this annex, Wh/km;

is the distance driven in the considered phase p of cycle c of the charge-depleting Type 1 test, km;

is the index number of the considered applicable WLTP test cycle;

is the index of the individual phase within the applicable WLTP test cycle;

is the number of applicable WLTP test cycles driven up to the end of the transition cycle n according to paragraph 3.2.4.4. of this annex.

For the 4-phase WLTP test;

The considered phase shall be the low phase, medium phase, high phase, extra high phase, and the city driving cycle.

For the 3-phase WLTP test;

The considered phase shall be the low phase, medium phase and high phase.

4.4.5. Actual charge-depleting range for OVC-HEVs

The actual charge-depleting range shall be calculated using the following equation:

where:

is the actual charge-depleting range, km;

is the charge-sustaining CO2 emission according to Table A8/5, step No. 7, g/km;

is the CO2 emission of the applicable WLTP test cycle n of the charge-depleting Type 1 test, g/km;

is the CO2 emission of the charge-depleting Type 1 test from the beginning of the charge-depleting Type 1 test up to and including the applicable WLTP test cycle (n-1), g/km;

is the distance driven in the applicable WLTP test cycle c of the charge-depleting Type 1 test, km;

is the distance driven in the applicable WLTP test cycle n of the charge-depleting Type 1 test, km;

is the index number of the considered applicable WLTP test cycle;

is the number of applicable WLTP test cycles driven including the transition cycle according to paragraph 3.2.4.4. of this annex;

and:

where:

is the CO2 emission of the charge-depleting Type 1 test from the beginning of the charge-depleting Type 1 test up to and including the applicable WLTP test cycle (n-1), g/km;

is the CO2 emission determined according to paragraph 3.2.1. of Annex B7 of the applicable WLTP test cycle c of the charge-depleting Type 1 test, g/km;

is the distance driven in the applicable WLTP test cycle c of the charge-depleting Type 1 test, km;

is the index number of the considered applicable WLTP test cycle;

is the number of applicable WLTP test cycles driven including the transition cycle according to paragraph 3.2.4.4. of this annex.

4.4.6. (Reserved)

4.5. Interpolation of individual vehicle values

4.5.1. Interpolation range

4.5.1.1. Interpolation range for NOVC- HEVs and OVC-HEVs

4.5.1.1.1. The interpolation method shall only be used if the difference in charge-sustaining CO2 over the applicable cycle resulting from the table below between test vehicles L and H is between a minimum of 5 g/km and a maximum defined in paragraph 4.5.1.1.2. of this annex.


|  |  |
| --- | --- |
| For 4-phase WLTP test | For 3-phase WLTP test |
| step 8 of Table A8/5 of Annex B8 | step 6 of Table A8/5 of Annex B8 |

4.5.1.1.2. The maximum difference in charge-sustaining CO2 emissions allowed over the applicable cycle resulting from the calculation of the charge-sustaining CO2 emission MCO2,CS from the table below between test vehicles L and H shall be 20 per cent of the charge-sustaining CO2 emissions from vehicle H plus 5 g/km, but shall be at least 15 g/km and not exceed 20 g/km. See Figure A8/3. This restriction does not apply for the application of a road load matrix family or when the calculation of the road load of vehicles L and H is based on the default road load.

|  |  |
| --- | --- |
| For 4-phase WLTP test | For 3-phase WLTP test |
| step 8 of Table A8/5 of Annex B8 | step 6 of Table A8/5 of Annex B8 |

Figure A8/3


**Interpolation range between vehicle H and vehicle L applied to EVs**



4.5.1.1.3. The allowed interpolation range defined in paragraph 4.5.1.1.2. of this annex may be increased by 10 g/km charge-sustaining CO2 if a vehicle M is tested within that family and the conditions according to paragraph 4.5.1.1.5. of this annex are fulfilled. This increase is allowed only once within an interpolation family. See Figure A8/4.

Figure A8/4

**Interpolation range for EVs with vehicle M**



4.5.1.1.4. At the request of the manufacturer and with approval of the responsible authority, the application of the interpolation method on individual vehicle values within a family may be extended if the maximum extrapolation of an individual vehicle (Step 9 in Table A8/5) is not more than 3 g/km above the charge-sustaining CO2 emission of vehicle H (Step 8 in Table A8/5) and/or is not more than 3 g/km below the charge-sustaining CO2 emission of vehicle L (Step 8 in Table A8/5). This extrapolation is valid only within the absolute boundaries of the interpolation range specified in this paragraph.

It is not necessary to check the above 3 g/km criteria for results after 3 phases.

For the application of a road load matrix family, or when the calculation of the road load of vehicles L and H is based on the default road load, extrapolation is not permitted.


4.5.1.1.5. Vehicle M

Vehicle M is a vehicle within the interpolation family between vehicles L and H with a cycle energy demand which is preferably closest to the average of vehicles L and H.

The limits of the selection of vehicle M (see Figure A8/5) are such that neither the difference in CO2 emission between vehicles H and M nor the difference in charge-sustaining CO2 emission between vehicles M and L is higher than the allowed charge-sustaining CO2 range according to paragraph 4.5.1.1.2. of this annex. The defined road load coefficients and the defined test mass shall be recorded.

Figure A8/5

**Limits for the selection of vehicle M**



For 4-phase WLTP

The linearity of the corrected measured and averaged charge-sustaining CO2 emission for vehicle M, MCO2,c,6,M according to step 6 of Table A8/5 of Annex B8, shall be verified against the linearly interpolated charge-sustaining CO2 emission between vehicles L and H over the applicable cycle by using the corrected measured and averaged charge-sustaining CO2 emission MCO2,c,6,H of vehicle H and MCO2,c,6,L of vehicle L, according to step 6 of Table A8/5 of Annex B8, for the linear CO2 emission interpolation.

For 3-phase WLTP


An additional averaging of tests using the charge-sustaining CO2-output of step 4a is necessary (not described in Table A8/5). The linearity of the corrected measured and averaged charge-sustaining CO2 emission for vehicle M, MCO2,c,4a,M according to step 4a of Table A8/5 of Annex B8, shall be verified against the linearly interpolated CO2 emission between vehicles L and H over the applicable cycle by using the corrected measured and averaged charge-sustaining CO2 emission MCO2,c,4a,H of vehicle H and MCO2,c,4a,L of vehicle L, according to step 4a of Table A8/5 of Annex B8, for the linear CO2 emission interpolation.

For 3-phase and 4-phase WLTP

The linearity criterion for vehicle M shall be considered fulfilled if the charge-sustaining CO2 emission of vehicle M over the applicable WLTC minus the charge-sustaining CO2 emission derived by interpolation is less than 2 g/km or 3 per cent of the interpolated value, whichever value is less, but at least 1 g/km. See Figure A8/6.

Figure A8/6

**Linearity criterion for vehicle M**



If the linearity criterion is fulfilled, the interpolation method shall be applicable for all individual vehicle values between vehicles L and H within the interpolation family.

If the linearity criterion is not fulfilled, the interpolation family shall be split into two sub-families for vehicles with a cycle energy demand between vehicles L and M, and vehicles with a cycle energy demand between vehicles M and H. In such a case, the final values of e.g. the charge-sustaining CO2 emissions of vehicle M shall be determined according to the same process as for vehicles L or H. See Table A8/5, Table A8/6, Table A8/8 and Table A8/9.

For vehicles with a cycle energy demand between that of vehicles L and M, each parameter of vehicle H necessary for the application of the interpolation method on individual OVC-HEV and NOVC-HEV values, shall be substituted by the corresponding parameter of vehicle M.

For vehicles with a cycle energy demand between that of vehicles M and H, each parameter of vehicle L that is necessary for the application of the interpolation method on individual OVC-HEV and NOVC-HEV values shall be substituted by the corresponding parameter of vehicle M.

4.5.2. Calculation of energy demand per period

The energy demand and distance driven per period p applicable for individual vehicles in the interpolation family shall be calculated according to the procedure in paragraph 5. of Annex B7 for the sets k of road load coefficients and masses according to paragraph 3.2.3.2.3. of Annex B7.

4.5.3. Calculation of the interpolation coefficient for individual vehicles

The interpolation coefficient per period shall be calculated for each considered period p using the following equation:

where:

is the interpolation coefficient for the considered individual vehicle for period p;

is the energy demand for the considered period for vehicle L according to paragraph 5. of Annex B7, Ws;

is the energy demand for the considered period for vehicle H according to paragraph 5. of Annex B7, Ws;

is the energy demand for the considered period for the individual vehicle according to paragraph 5. of Annex B7, Ws;

is the index of the individual period within the applicable test cycle.

In the case that the considered period p is the applicable WLTP test cycle, is named .

4.5.4. This paragraph is applicable only for 4-phase WLTP test

Interpolation of the CO2 emission for individual vehicles

4.5.4.1. Individual charge-sustaining CO2 emission for OVC-HEVs and NOVC-HEVs

The charge-sustaining CO2 emission for an individual vehicle shall be calculated using the following equation:

where:

is the charge-sustaining CO2 emission for an individual vehicle of the considered period p according to Table A8/5, step No. 9, g/km;

is the charge-sustaining CO2 emission for vehicle L of the considered period p according to Table A8/5, step No. 8, g/km;

is the charge-sustaining CO2 emission for vehicle H of the considered period p according to Table A8/5, step No. 8, g/km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable WLTP test cycle.

The considered periods shall be the low phase, medium phase, high phase, extra high phase and the applicable WLTP test cycle.

4.5.4.2. Individual utility factor-weighted charge-depleting CO2 emission for OVC-HEVs

The utility factor-weighted charge-depleting CO2 emission for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor-weighted charge-depleting CO2 emission for an individual vehicle, g/km;

is the utility factor-weighted charge-depleting CO2 emission for vehicle L, g/km;

is the utility factor-weighted charge-depleting CO2 emission for vehicle H, g/km;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.4.3. Individual utility factor-weighted CO2 emission for OVC-HEVs

The utility factor-weighted CO2 emission for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor-weighted CO2 emission for an individual vehicle, g/km;

is the utility factor-weighted CO2 emission for vehicle L, g/km;

is the utility factor-weighted CO2 emission for vehicle H, g/km**;**

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.5. Interpolation of the fuel consumption and fuel efficiency for individual vehicles

4.5.5.1. Individual charge-sustaining fuel consumption and fuel efficiency for OVC-HEVs and NOVC-HEVs

4.5.5.1.1. This paragraph is applicable only for 4-phase WLTP test

Individual charge-sustaining fuel consumption for OVC-HEVs and NOVC-HEVs

The charge-sustaining fuel consumption for an individual vehicle shall be calculated using the following equation:

where:

is the charge-sustaining fuel consumption for an individual vehicle of the considered period p according to Table A8/6, step No. 3, l/100 km;

is the charge-sustaining fuel consumption for vehicle L of the considered period p according to Table A8/6, step No. 2, l/100 km;

is the charge-sustaining fuel consumption for vehicle H of the considered period p according to Table A8/6, step No. 2, l/100 km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable WLTP test cycle.

The considered periods shall be the low phase, medium phase, high phase, extra high phase, and the applicable WLTP test cycle.

4.5.5.1.2. This paragraph is only applicable for the 3-phase WLTP:

Individual charge-sustaining fuel efficiency for OVC-HEVs and NOVC-HEVs

The charge-sustaining fuel efficiency for an individual vehicle shall be calculated using the following equation:

where:

is the charge-sustaining fuel consumption for an individual vehicle of the considered period p according to Table A8/6, step No. 3, km/l;

is the charge-sustaining fuel consumption for vehicle L of the considered period p according to Table A8/6, step No. 2, km/l;

is the charge-sustaining fuel consumption for vehicle H of the considered period p according to Table A8/6, step No. 2, km/l;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable WLTP test cycle.

The considered periods shall be the low phase, medium phase, high phase and the applicable WLTP test cycle.

4.5.5.2. Individual charge depleting fuel consumption for OVC-HEVs and individual charge-depleting fuel efficiency for OVC-HEVs

For 4-phase WLTP test

The utility factor-weighted charge-depleting fuel consumption for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor-weighted charge-depleting fuel consumption for an individual vehicle, l/100 km;

is the utility factor-weighted charge-depleting fuel consumption for vehicle L, l/100 km;

is the utility factor-weighted charge-depleting fuel consumption for vehicle H, l/100 km;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

For 3-phase WLTP test

The charge-depleting fuel efficiency for an individual vehicle shall be calculated using the following equation:

where:

is the charge-depleting fuel efficiency for an individual vehicle, km/l;

is the charge-depleting fuel efficiency for vehicle L, km/l;

is the charge-depleting fuel efficiency for vehicle H, km/l;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.5.3. This paragraph is applicable only for 4-phase WLTP test

Individual utility factor-weighted fuel consumption for OVC-HEVs

The utility factor-weighted fuel consumption for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor-weighted fuel consumption for an individual vehicle, l/100 km;

is the utility factor-weighted fuel consumption for vehicle L, l/100 km;

is the utility factor-weighted fuel consumption for vehicle H, l/100 km;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.6. Interpolation of electric energy consumption for individual vehicles

4.5.6.1. This paragraph is applicable only for 4-phase WLTP test

Individual utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains for OVC-HEVs

The utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains for an individual vehicle, Wh/km;

is the utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains for vehicle L, Wh/km;

is the utility factor-weighted charge-depleting electric energy consumption based on the recharged electric energy from the mains for vehicle H, Wh/km;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.6.2. This paragraph is applicable only for 4-phase WLTP test

Individual utility factor-weighted electric energy consumption based on the recharged electric energy from the mains for OVC-HEVs

The utility factor-weighted electric energy consumption based on the recharged electric energy from the mains for an individual vehicle shall be calculated using the following equation:

where:

is the utility factor weighted electric energy consumption based on the recharged electric energy from the mains for an individual vehicle, Wh/km;

is the utility factor weighted electric energy consumption based on the recharged electric energy from the mains for vehicle L, Wh/km;

is the utility factor weighted electric energy consumption based on the recharged electric energy from the mains for vehicle H, Wh/km;

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle.

4.5.6.3. Individual electric energy consumption for OVC-HEVs and PEVs

The electric energy consumption for an individual vehicle according to paragraph 4.3.3. of this annex in the case of OVC-HEVs and according to paragraph 4.3.4. of this annex in the case of PEVs shall be calculated using the following equation:

where:

is the electric energy consumption for an individual vehicle for the considered period p, Wh/km;

is the electric energy consumption for vehicle L for the considered period p, Wh/km;

is the electric energy consumption for vehicle H for the considered period p, Wh/km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable test cycle.

For the 4-phase WLTP;

The considered periods shall be the low phase, medium phase, high phase, extra high phase, the applicable WLTP city test cycle and the applicable WLTP test cycle.

For the 3-phase WLTP ;

The considered periods shall be the low phase, medium phase, high phase and the applicable WLTP test cycle.

4.5.7. Interpolation of electric ranges for individual vehicles

4.5.7.1. Individual all-electric range for OVC-HEVs

If the following criterion

where:

is the all-electric range of vehicle L for the applicable WLTP test cycle, km;

is the all-electric range of vehicle H for the applicable WLTP test cycle, km;

is the actual charge-depleting range of vehicle L, km;

is the actual charge-depleting range of vehicle H, km;

is fulfilled, the all-electric range for an individual vehicle shall be calculated using the following equation:

where:

is the all-electric range for an individual vehicle for the considered period p, km;

is the all-electric range for vehicle L for the considered period p, km;

is the all-electric range for vehicle H for the considered period p, km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable test cycle.

If the criterion defined in this paragraph is not fulfilled, the AER determined for vehicle H is applicable to all vehicles within the interpolation family.

For the 4-phase WLTP; The considered periods shall be the applicable WLTP city test cycle and the applicable WLTP test cycle.

For the 3-phase WLTP; The considered periods shall be the applicable WLTP test cycle.

4.5.7.2. Individual pure electric range for PEVs

The pure electric range for an individual vehicle shall be calculated using the following equation:

where:

is the pure electric range for an individual vehicle for the considered period p, km;

is the pure electric range for vehicle L for the considered period p, km;

is the pure electric range for vehicle H for the considered period p, km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable test cycle.

For the 4-phase WLTP only;

The considered periods shall be the low phase, medium phase, high phase, extra high phase, the applicable WLTP city test cycle and the applicable WLTP test cycle.

For the 3-phase WLTP only;

The considered periods shall be the applicable WLTP test cycle.

4.5.7.3. Individual equivalent all-electric range for OVC-HEVs

The equivalent all-electric range for an individual vehicle shall be calculated using the following equation:

where:

is the equivalent all-electric range for an individual vehicle for the considered period p, km;

is the equivalent all-electric range for vehicle L for the considered period p, km;

is the equivalent all-electric range for vehicle H for the considered period p, km;

is the interpolation coefficient for the considered individual vehicle for period p;

is the index of the individual period within the applicable test cycle.

For the 4-phase WLTP;

The considered periods shall be the low phase, medium phase, high phase, extra high phase, the applicable WLTP city test cycle and the applicable WLTP test cycle.

For the 3-phase WLTP only;

The considered periods shall be the applicable WLTP test cycle.

4.6. Stepwise procedure for calculating the final test results of OVC-HEVs

In addition to the stepwise procedure for calculating the final charge-sustaining test results for gaseous emission compounds according to paragraph 4.1.1.1. of this annex and for fuel consumption and fuel efficiency according to paragraph 4.2.1.1. of this annex, paragraphs 4.6.1. and 4.6.2. of this annex describe the stepwise calculation of the final charge-depleting as well as the final charge-sustaining and charge-depleting weighted test results.

4.6.1. Stepwise procedure for calculating the final test results of the charge-depleting Type 1 test for OVC-HEVs

The results shall be calculated in the order described in Table A8/8. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

For the purpose of this table, the following nomenclature within the equations and results is used:

c complete applicable test cycle;

p every applicable cycle phase; for the purpose of the city test cycle calculation (as applicable), p shall represent the city driving cycle;

i applicable criteria emission component;

CS charge-sustaining;

CO2 CO2 emission.

Table A8/8

**Calculation of final charge-depleting values (FE applicable for results after 3 phases only)**

Table A8/8 shall be performed separately for results after 4 phases and for results after 3 phases.

| *Step no.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Annex B8 | Charge-depleting test results | Results measured according to Appendix 3 to this annex, pre-calculated according to paragraph 4.3. of this annex.  Recharged electric energy according to paragraph 3.2.4.6. of this annex.  Cycle energy according to paragraph 5. of Annex B7.  CO2 emission according to paragraph 3.2.1. of Annex B7.  Mass of gaseous emission compound i according to paragraph 4.1.3.1.1. of Annex B8.  All-electric range determined according to paragraph 4.4.1.1. of this annex.  CO2 emission KCO2 correction coefficient might be necessary according to Appendix 2 to this annex.  Output is available for each test. | ΔEREESS,j, Wh;  dj, km;  EAC, Wh;  Ecycle, Ws;  MCO2,CD,j, g/km;  Mi,CD,j, g/km;  AER, km;  KCO2,  (g/km)/(Wh/km). |
| For results after 4 phases  Annex B8 |  | Usable battery energy according to paragraph 4.4.1.2.2. of this annex.  In the case that the applicable WLTC city test cycle was driven: all- electric range city according to paragraph 4.4.1.2.1. of this annex.  Particle number emissions (if applicable) according to paragraph 4. of Annex B7.  Particulate matter emissions according to paragraph 4. of Annex B7. | UBEcity, Wh;  AERcity, km.  PNCD,j, particles per kilometer;  PMCD,c, mg/km; |
| 2 | Output step 1 | ΔEREESS,j, Wh;  Ecycle, Ws. | Calculation of relative electric energy change for each cycle according to paragraph 3.2.4.5.2. of this annex.  Output is available for each test and each applicable WLTP test cycle. | REECi. |
| 3 | Output step 2 | REECi. | Determination of the transition and confirmation cycle according to paragraph 3.2.4.4. of this annex.  In the case that more than one charge-depleting test is available for one configuration, for the purpose of averaging, each test shall have the same transition cycle number nveh.  Determination of the charge-depleting cycle range according to paragraph 4.4.3. of this annex.  Output is available for each test. | nveh;  RCDC; km. |
| 4 | Output step 3 | nveh; | In the case that the interpolation method is used, the transition cycle shall be determined for vehicle H, L and, if applicable, M.  Check whether the interpolation criterion according to paragraph 6.3.2.2. (d) of this Regulation is fulfilled. | nveh,L;  nveh,H;  if applicable  nveh,M. |
| For results after 4 phases  5 | Output step 1 | Mi,CD,j, g/km;  PMCD,c, mg/km;  PNCD,j, particles per kilometer. | Calculation of combined values for emissions for nveh cycles; in the case that the interpolation method is applied, nveh,L cycles shall be used for nveh,H cycles and nveh,M cycles, if applicable.  Output is available for each test. | Mi,CD,c, g/km;  PMCD,c, mg/km;  PNCD,c, particles per kilometer. |
| For results after 4 phases  6 | Output step 5 | Mi,CD,c, g/km;  PMCD,c, mg/km;  PNCD,c, particles per kilometer. | Emission averaging of tests for each applicable WLTP test cycle within the charge-depleting Type 1 test and checking compliance with the limits according to Table A6/2 of Annex B6. | Mi,CD,c,ave, g/km;  PMCD,c,ave, mg/km;  PNCD,c,ave, particles per kilometer. |
| For results after 4 phases  7 | Output step 1 | ΔEREESS,j, Wh;  dj, km;  UBEcity, Wh. | In the case that AERcity is derived from the Type 1 test by driving the applicable WLTP test cycles, the value shall be calculated according to paragraph 4.4.1.2.2. of this annex.  In the case of more than one test,  ncity,pe shall be equal for each test.  Output is available for each test.  Averaging of AERcity. | AERcity, km;  AERcity,ave, km. |
| For results after 4 phases  8 | Output step 1 | dj, km; | Phase-specific and cycle-specific UF calculation.  Output is available for each test. | UFphase,j;  UFcycle,c. |
| Output step 3 | nveh; |
| Output step 4 | nveh,L; |
| For results after 4 phases  9 | Output step 1 | ΔEREESS,j, Wh;  dj, km;  EAC, Wh; | Calculation of the electric energy consumption based on the recharged energy according. to paragraphs 4.3.1. of this annex.  In the case of interpolation, nveh,L cycles shall be used. Therefore, due to the required correction of the CO2 emission, the electric energy consumption of the confirmation cycle and its phases shall be set to zero.  Output is available for each test. | ECAC,CD, Wh/km; |
| Output step 3 | nveh; |
| Output step 4 | nveh,L; |
| Output step 8 | UFphase,j; |
| 10 | Output step 1 | MCO2,CD,j, g/km;  KCO2, (g/km)/(Wh/km);  ΔEREESS,j, Wh;  dj, km;  nveh;  nveh,L;  UFphase,j. | Calculation of the charge-depleting CO2 emission according to paragraph 4.1.2. of this annex.  In the case that the interpolation method is applied, nveh,L cycles shall be used. With reference to paragraph 4.1.2. of this annex, the confirmation cycle shall be corrected according to Appendix 2 to this annex.  Output is available for each test. | MCO2,CD, g/km; |
| Output step 3 | dj, km; |
| Output step 4 | nveh; |
| Output step 8 | nveh,L;  UFphase,j. |
| 11 | Output step 1 | MCO2,CD,j, g/km;  Mi,CD,j, g/km;  KCO2, (g/km)/(Wh/km).  nveh;  nveh,L;  UFphase,j; | Calculation of the charge-depleting fuel consumption and fuel efficiency according to paragraph 4.2.2. of this annex.  In the case that the interpolation method is applied, nveh,L cycles shall be used. With reference to paragraph 4.1.2. of this annex, MCO2,CD,j of the confirmation cycle shall be corrected according to Appendix 2 to this annex.  For results after 4 phases,  the phase-specific fuel consumption FCCD,j shall be calculated using the corrected CO2 emission according to paragraph 6. of Annex B7.  Output is available for each test. | For results after 4 phases,  FCCD,j, l/100 km;  FCCD, l/100 km.  For results after 3 phases,  FECD, km/l. |
| Output step 3 | nveh; |
| Output step 4 | nveh,L; |
| Output step 8 | UFphase,j; |
| 12 | Output step 1 | ΔEREESS,j, Wh;  dj, km; | If applicable, calculation of the electric energy consumption from the first applicable WLTP test cycle .  Output is available for each test. | ECDC,CD,first, Wh/km |
| 13 | Output step 9 | ECAC,CD, Wh/km; | Averaging of tests for each vehicle.  In the case that the interpolation method is applied, the output is available for each vehicle H, L and, if applicable, M. | If applicable:  ECDC,CD,first,ave, Wh/km  For results after 4 phases,  ECAC,CD,ave, Wh/km;  MCO2,CD,ave, g/km;  FCCD,ave, l/100 km;  For results after 3 phases,  FECD,ave, km/l. |
| Output step 10 | MCO2,CD, g/km; |
| Output step 11 | FCCD, l/100 km; FECD, km/l. |
| Output step 12 | If applicable:  ECDC,CD,first, Wh/km. |
| 14 | Output step 13 | ECAC,CD,ave, Wh/km;  MCO2,CD,ave, g/km.  FECD,ave, km/l. | Declaration of charge-depleting electric energy consumption, fuel efficiency and CO2 emission for each vehicle.  Calculation of ECAC,weighted according to paragraph 4.3.2. of this annex.  In the case that the interpolation method is applied, the output is available for each vehicle H, L and, if applicable, M. | For results after 4 phases,  ECAC,CD,declared, Wh/km;  ECAC,weighted, Wh/km;  MCO2,CD,declared, g/km.  For results after 3 phases,  FECD,declared, km/l. |
| 15 | Output step 13 | ECAC,CD,ave, Wh/km;  If applicable:  ECDC,CD,first,ave, Wh/km; | If applicable:  Adjustment of electric energy consumption for the purpose of COP as described in paragraph 2.2. of Appendix 8 to this annex.  In the case that the interpolation method is applied, the output is available for each vehicle H, L and, if applicable, M. | ECDC,CD,COP, Wh/km; |
| Output step 14 | ECAC,CD,declared, Wh/km; |
| 16  If the interpolation method is not applied, step No. 17 is not required and the output of this step is the final result. | Output step 15 | If applicable: ECDC,CD,COP, Wh/km; | In the case that the interpolation method is applied, intermediate rounding shall be performed according to paragraph 6.1.8. of this Regulation:  MCO2,CD shall be rounded to the second place of decimal.  ECAC,CD,final and ECAC,weighted,final shall be rounded to the first place of decimal.  If applicable:  ECDC,CD,COP shall be rounded to the first place of decimal.  FCCD and FECD shall be rounded to the third place of decimal.  Output is available for vehicle H and for vehicle L and, if applicable, for vehicle M.  In case that the interpolation method is not applied, final rounding shall be applied according to paragraph 6.1.8. of this Regulation:  ECAC,CD , ECAC,weighted and MCO2,CD shall be rounded to the nearest whole number.    If applicable:  ECDC,CD,COP shall be rounded to the nearest whole number.    FCCD and FECD shall be rounded to the first place of decimal. | If applicable: ECDC,CD,COP,final, Wh/km;  For results after 4 phases,  ECAC,CD,final, Wh/km;  MCO2,CD,final, g/km;  ECAC,weighted,final, Wh/km;  FCCD,final, l/100 km;  For results after 3 phases,  FECD,final, km/l; |
| Output step 14 | ECAC,CD,declared, Wh/km;  ECAC,weighted, Wh/km;  FECD,declared, km/l;  MCO2,CD,declared, g/km. |
| Output step 13 | FCCD,ave, l/100 km; |
| 17  Result of an individual vehicle.  Final test result. | Output step 16 | If applicable: ECDC,CD,COP,final, Wh/km;  ECAC,CD,final, Wh/km;  MCO2,CD,final, g/km;  ECAC,weighted,final, Wh/km;  FCCD,final, l/100 km; FECD,final, km/l; | Interpolation of individual values based on input from vehicles H and L and, if applicable, vehicle M.  Final rounding of individual vehicle values shall be performed according to paragraph 6.1.8. of this Regulation.  ECAC,CD , ECAC,weighted and MCO2,CD shall be rounded to the nearest whole number.  If applicable:  ECDC,CD,COP shall be rounded to the nearest whole number.    FCCD shall be rounded to the first place of decimal.  Output is available for each individual vehicle. | If applicable: ECDC,CD,COP,ind, Wh/km;  For results after 4 phases,  ECAC,CD,ind, Wh/km;  MCO2,CD,ind, g/km;  ECAC,weighted,ind, Wh/km;  FCCD,ind, l/100 km;  For results after 3 phases,  FECD,ind, km/l; |

4.6.2. Stepwise procedure for calculating the final charge-sustaining and charge-depleting weighted test results of the Type 1 test for OVC-HEVs

The results shall be calculated in the order described in Table A8/9. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

For the purpose of this table, the following nomenclature within the equations and results is used:

considered period is the complete applicable test cycle;

every applicable cycle phase; for the purpose of EAERcity calculation (as applicable), p shall represent the city driving cycle;

applicable criteria emission component (except for CO2);

j index for the considered period;

CS charge-sustaining;

CD charge-depleting;

CO2 CO2 emission;

REESS Rechargeable Electric Energy Storage System.

Table A8/9

**Calculation of final charge-depleting and charge-sustaining weighted values (FE applicable for results after 3 phases only)**

Table A8/9 shall be performed separately for results after 4 phases and for results after 3 phases.

| *Step no.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Output step 1, Table A8/8 | Mi,CD,j, g/km;  PNCD,j, particles per kilometer;  PMCD,c, mg/km;  MCO2,CD,j, g/km;  ΔEREESS,j, Wh;  dj, km;  AER, km;  EAC, Wh; | Input from CD and CS post processing.  For results after 4 phases:  The arithmetic average of for all individual charge-depleting tests shall be calculated  Output in the case of CD is available for each CD test. Output in the case of CS is available once due to CS test averaged values.  In the case that the interpolation method is applied, the output (except of KCO2) is available for vehicle H, L and, if applicable, M.  CO2 emission correction coefficient KCO2 might be necessary according to Appendix 2 to this annex. | MCO2,CD,j, g/km;  AER, km;  EAC, Wh;  MCO2,CS,declared, g/km;  MCO2,CS,p,6, g/km;  MCO2,CS,c,6, g/km;  MCO2,CD,declared, g/km;  MCO2,CD,ave, g/km;  For results after 4 phases  Mi,CD,j, g/km;  PNCD,j, particles per kilometer;  PMCD,c, mg/km;  ΔEREESS,j, Wh;  dj, km;  AERcity,ave, km;  nveh;  RCDC, km;  nveh,L;  nveh,H;  UFphase,j;  UFcycle,c;  Mi,CS,c,6, g/km;  MCO2,CS,p, g/km ;  KCO2,  (g/km)/(Wh/km). |
| Output step 7, Table A8/8 | AERcity,ave, km; |
| Output step 3, Table A8/8 | nveh;  RCDC, km; |
| Output step 4, Table A8/8 | nveh,L;  nveh,H; |
| Output step 8, Table A8/8 | UFphase,j;  UFcycle,c; |
| Output step 6, Table A8/5 | Mi,CS,c,6, g/km;  For 4 phases WLTP test:  MCO2,CS,c,6, g/km; MCO2,CS,p,6, g/km: |
| Output step 7, Table A8/5 | MCO2,CS,7, g/km;  MCO2,CS,p,7, g/km; |
| Output step 14, Table A8/8 | MCO2,CD,declared, g/km; |
| Output step 13, Table A8/8 | MCO2,CD,ave, g/km; |
|  | KCO2,  (g/km)/(Wh/km). |
| For results after 4 phases  2 | Output step 1 | Mi,CD,j, g/km;  PNCD,j, particles per kilometer;  PMCD,c, mg/km;  nveh;  nveh,L;  UFphase,j;  UFcycle,c;  Mi,CS,c,6, g/km; | Calculation of weighted emission (except MCO2,weighted) compounds according to paragraphs 4.1.3.1.1. to 4.1.3.3. inclusive of this annex.  Remark:  Mi,CS,c,6 includes PNCS,c and PMCS,c.  Output is available for each CD test. | Mi,weighted, g/km;  PNweighted, particles per kilometer;  PMweighted, mg/km; |
| 3 | Output step 1 | MCO2,CD,j, g/km;  ΔEREESS,j, Wh;  dj, km;  nveh;  RCDC, km  MCO2,CS,declared, g/km;  MCO2,CS,p,6, g/km;  MCO2,CS,c,6, g/km;  MCO2,CS,p, g/km; | Calculation of equivalent all-electric range according to paragraphs 4.4.4.1. and 4.4.4.2. of this annex.  For results after 3 phases  Output is available for each CD test.  Calculation of actual charge-depleting range according to paragraph 4.4.5. of this annex.  Output is available for each CD test.  The arithmetic average of RCDA for all individual charge-depleting tests shall be calculated andshall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number. | EAER, km;  EAERp,3, km;  RCDA, km. |
| 4 | Output step 1 | AER, km; | Output is available for each CD test.  In the case that the interpolation method is applied, check the availability of AER interpolation between vehicle H, L and, if applicable, M according to paragraph 4.5.7.1. of this annex.  If the interpolation method is used, each test shall fulfil the requirement. | AER-interpolation availability. |
| Output step 3 | RCDA, km. |
| 5  If the interpolation method is not applied, step No. 9 is not required and the output of this step is the final result. | Output step 1  Output step 3 | AER, km;  EAER, km;  EAERp,3, km. | Averaging AER and AER declaration.  Averaging EAER (for results after 3 phases) and EAER declaration.  Alignment of phase specific EAERp:  The declared AER (for results after 4 phases) and EAER shall be rounded according to paragraph 6.1.8. of this Regulation to the number of decimal places specified in Table A6/1 of Annex B6.  In the case that the interpolation method is applied and the AER interpolation availability criterion is fulfilled, AERshall be rounded according to paragraph 6.1.8. of this Regulation to the first place of decimal.  In the case that the interpolation method is applied, EAERand EAERp shall be rounded according to paragraph 6.1.8. of this Regulation to the first place of decimal.  The output is available for each vehicles H and L and, if applicable, for vehicle M.  In the case that the interpolation method is applied but the criterion is not fulfilled, AER of vehicle H shall be applied for the whole interpolation family and shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number.  In the case that the interpolation method is not applied, AER, EAER and EAERp shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number. | AERave, km;  EAERdec, km;  EAERp,5, km;  For results after 4 phases  AERdec, km. |
| For results after 4 phases,  6 | Output step 1 | Mi,CD,j, g/km;  MCO2,CD,j, g/km;  nveh;  nveh,L;  UFphase,j;  Mi,CS,c,6, g/km;  MCO2,CS,declared, g/km.  MCO2,CD,declared, g/km;  MCO2,CD,ave, g/km; | Calculation of weighted CO2 emission and fuel consumption according to paragraphs 4.1.3.1.2. and 4.2.3. of this annex.  Output is available for each CD test.  In the case that the interpolation method is applied, nveh,L cycles shall be used. With reference to paragraph 4.1.2. of this annex, MCO2,CD,j of the confirmation cycle shall be corrected according to Appendix 2 to this annex. | MCO2,weighted, g/km;  FCweighted, l/100 km; |
| 7 | Output step 1 | EAC, Wh; | Calculation of the electric energy consumption based on EAER according to paragraphs 4.3.3.1. and 4.3.3.2. of this annex.  For results after 3 phases:  Output is available for each CD test. | EC, Wh/km;  ECp, Wh/km; |
| Output step 3 | EAER, km;  EAERp,3, km; |
| 8  If the interpolation method is not applied, step No. 9 is not required and the output of this step is the final result. | Output step 1 | AERcity, ave, km; | For results after 3 phases  Averaging EC and EC declaration.  Alignment of phase specific ECp  For results after 4 phases  Averaging of all values except EC and EAER and intermediate rounding of all values according to paragraph 6.1.8. of this Regulation.  In the case that the interpolation method is applied, intermediate rounding shall be performed according to paragraph 6.1.8. of this Regulation.  AERcity,ave, EAER and EAERp shall be rounded to the first place of decimal.  MCO2,weighted shall be rounded to the second place of decimal.  FCweighted shall be rounded to the third place of decimal.  EC and ECp shall be rounded to the first place of decimal.  The output is available for each vehicle H, vehicle L and, if applicable, vehicle M.  In case that the interpolation method is not applied, final rounding of the test results shall be applied according to paragraph 6.1.8. of this Regulation.  AERcity,final, EAER and EAERp shall be rounded to the nearest whole number.  MCO2,weighted shall be rounded to the nearest whole number.  FCweighted shall be rounded to the first place of decimal.  EC and ECp shall be rounded to the nearest whole number. | For results after 3 phases  ECdec, Wh/km;  ECp,final, Wh/km;  EAERfinal, km;  For results after 4 phases  AERcity,final, km;  MCO2,weighted,final, g/km;  FCweighted,final, l/100 km;  ECfinal, Wh/km;  ECp,final, Wh/km;  EAERfinal, km;  EAERp,final, km. |
| Output step 6 | MCO2,weighted, g/km;  FCweighted, l/100 km; |
| Output step 7 | EC, Wh/km;  ECp, Wh/km; |
| Output step 5 | EAER, km;  EAERp,5, km; |
| Output step 5 | AERdec, km;  AERave, km.. |
| 9  Result of an individual vehicle.  Final test result. | Output step 5 | AERdec, km; | Interpolation of individual values based on input from vehicle low, medium and high according to paragraph 4.5. of this annex, and final rounding according to paragraph 6.1.8. of this Regulation.  AERind,AERcity,ind, EAERind and EAERp,ind shall be rounded to the nearest whole number.  MCO2,weighted,ind shall be rounded to the nearest whole number.  FCweighted,ind shall be rounded to the first place of decimal.  ECind and ECp,ind shall be rounded to the nearest whole number.  Output is available for each individual vehicles.  RCDC,final shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number. | ECind, Wh/km;  ECp,ind, Wh/km;  EAERind, km;  For results after 4 phases,  AERind, km;  AERcity,ind, km;  MCO2,weighted,ind, g/km;  FCweighted,ind, l/100 km;  EAERp,ind, km.  RCDC,final, km; |
| Output step 8 | AERcity,final, km;  MCO2,weighted,final, g/km;  FCweighted,final, l/100 km;  ECfinal, Wh/km;  ECp,final, Wh/km;  EAERfinal, km;  EAERp,final, km; |
| Output step 4 | AER-interpolation availability |
| Output step 1 | RCDC, km; |

4.6.3. (Reserved)

4.7. Stepwise procedure for calculating the final test results of PEVs

The results shall be calculated in the order described in Table A8/10 of the consecutive cycle procedure and in the order described in Table A8/11 in the case of the shortened test procedure. All applicable results in the column "Output" shall be recorded. The column "Process" describes the paragraphs to be used for calculation or contains additional calculations.

4.7.1. Stepwise procedure for calculating the final test results of PEVs in case of the consecutive cycles procedure

For the purpose of this table, the following nomenclature within the questions and results is used:

j index for the considered period.

Table A8/10

**Calculation of final PEV values determined by application of the consecutive cycle Type 1 procedure**

Table A8/10 shall be performed separately for results after 4 phases and for results after 3 phases.

For results after 4 phases;

The considered periods shall be the low phase, medium phase, high phase, extra high phase, the applicable WLTP city test cycle and the applicable WLTP test cycle.

For results after 3 phases;

The considered periods shall be the low phase, medium phase, high phase and the applicable WLTP test cycle.

| *Step no.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Annex B8 | Test results | Results measured according to Appendix 3 to this annex and pre-calculated according to paragraph 4.3. of this annex.  Usable battery energy according to paragraph 4.4.2.2.1. of this annex.  Recharged electric energy according to paragraph 3.4.4.3. of this annex.  Output is available for each test.  EAC shall be rounded according to paragraph 6.1.8. of this Regulation to the first place of decimal. | ΔEREESS,j, Wh;  dj, km;  UBECCP, Wh;  EAC, Wh. |
| 2 | Output step 1 | ΔEREESS,j, Wh;  UBECCP, Wh. | Determination of the number of completely driven applicable WLTC phases and cycles according to paragraph 4.4.2.2. of this annex.  Output available for each test. | nWLTC;  ncity;  nlow;  nmed;  nhigh;  nexHigh. |
| 3 | Output step 1 | ΔEREESS,j, Wh;  UBECCP, Wh. | Calculation of weighting factors according to paragraph 4.4.2.2. of this annex.  *Note*: The number of weighting factors depends on the applicable cycle that was used (3- or 4-phase WLTC). In the case of 4-phase WLTCs, the output in brackets might be needed in addition.  Output is available for each test. | KWLTC,1  KWLTC,2  KWLTC,3  (KWLTC,4)  Kcity,1  Kcity,2  Kcity,3  (Kcity,4)  Klow,1  Klow,2  Klow,3  (Klow,4)  Kmed,1  Kmed,2  Kmed,3  (Kmed,4)  Khigh,1  Khigh,2  Khigh,3  (Khigh,4)  KexHigh,1  KexHigh,2  KexHigh,3  (KexHigh,4) |
| Output step 2 | nWLTC;  ncity;  nlow;  nmed;  nhigh;  nexHigh. |
| 4 | Output step 1 | ΔEREESS,j, Wh;  dj, km;  UBECCP, Wh. | Calculation of electric energy consumption at the REESSs according to paragraph 4.4.2.2. of this annex.  Calculation of the electric energy consumption from the first applicable WLTP test cycle ECDC,first.  Output is available for each test.  . | ECDC,WLTC, Wh/km;  ECDC,city, Wh/km;  ECDC,low, Wh/km;  ECDC,med, Wh/km;  ECDC,high, Wh/km;  ECDC,exHigh, Wh/km;  ECDC,first, Wh/km. |
| Output step 2 | nWLTC;  ncity;  nlow;  nmed;  nhigh;  nexHigh. |
| Output step 3 | All weighting  factors |
| 5 | Output step 1 | UBECCP, Wh; | Calculation of pure electric range according to paragraph 4.4.2.2. of this annex.  Output is available for each test. | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km. |
| Output step 4 | ECDC,WLTC, Wh/km;  ECDC,city, Wh/km;  ECDC,low, Wh/km;  ECDC,med, Wh/km;  ECDC,high, Wh/km;  ECDC,exHigh, Wh/km. |
| 6 | Output step 1 | EAC, Wh; | Calculation of electric energy consumption at the mains according to paragraph 4.3.4. of this annex.  Output is available for each test. | ECWLTC, Wh/km;  ECcity, Wh/km;  EClow, Wh/km;  ECmed, Wh/km;  EChigh, Wh/km;  ECexHigh, Wh/km. |
| Output step 5 | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km. |
| 7  If the interpolation method is not applied, step No. 10 is not required and the output of this step for PERWLTC,dec and ECWLTC,dec is the final result. | Output step 5 | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km; | Averaging of tests for all input values.  Declaration of PERWLTC,dec and ECWLTC,dec based on PERWLTC,ave and ECWLTC,ave.  Alignment of PER in case of city, low, med, high and exHigh based on the ratio between PERWLTC,dec and PERWLTC,ave:  Alignment of EC in case of city, low, med, high and exHigh based on the ratio between ECWLTC,dec and ECWLTC,ave:  In the case that the interpolation method is applied, the output is available for vehicle H and vehicle L. PERWLTC,dec as well as ECWLTC,dec shall be rounded according to paragraph 6.1.8. of this Regulation to the number of places of decimal as specified in Table A6/1 of Annex B6.  In the case that the interpolation method is not applied, PERWLTC,dec and ECWLTC,dec shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number.  . | PERWLTC,dec, km;  PERWLTC,ave, km;  PERcity,ave, km;  PERlow,ave, km;  PERmed,ave, km;  PERhigh,ave, km;  PERexHigh,ave, km;  ECWLTC,dec, Wh/km;  ECWLTC,ave, Wh/km;  ECcity,ave, Wh/km;  EClow,ave, Wh/km;  ECmed,ave, Wh/km;  EChigh,ave, Wh/km;  ECexHigh,ave, Wh/km;  ECDC,first,ave, Wh/km. |
| Output step 6 | ECWLTC, Wh/km;  ECcity, Wh/km;  EClow, Wh/km;  ECmed, Wh/km;  EChigh, Wh/km;  ECexHigh, Wh/km. |
| Output step 4 | ECDC,first, Wh/km. |
| 8 | Output step 7 | ECWLTC,dec, Wh/km;  ECWLTC,ave, Wh/km;  ECDC,first,ave, Wh/km. | Adjustment of the electric energy consumption for the purpose of COP as described in paragraph 1.2. of Appendix 8 to this annex.  In the case that the interpolation method is applied, the output is available for vehicle H and vehicle L. | ECDC,COP, Wh/km. |
| 9  If the interpolation method is not applied, step No. 10 is not required and the output of this step is the final result. | Output step 7 | PERcity,ave, km;  PERlow,ave, km;  PERmed,ave, km;  PERhigh,ave, km;  PERexHigh,ave, km;  ECcity,ave, Wh/km;  EClow,ave, Wh/km;  ECmed,ave, Wh/km;  EChigh,ave, Wh/km;  ECexHigh,ave, Wh/km; | Intermediate rounding according to paragraph 6.1.8. of this Regulation.  In the case that the interpolation method is applied, intermediate rounding shall be performed according to paragraph 6.1.8. of this Regulation:  PERcity and PERp shall be rounded to the first place of decimal.  ECcity and ECp shall be rounded to the first place of decimal.  ECDC,COP shall be rounded to the first place of decimal.  The output is available for vehicle H and vehicle L.  In case that the interpolation method is not applied, final rounding of the test results according to paragraph 6.1.8. of this Regulation:  PERcity and PERp shall be rounded to the nearest whole number.  ECcity and ECp shall be rounded to the nearest whole number.  ECDC,COP shall be rounded to the nearest whole number. | PERcity,final, km;  PERlow,final, km;  PERmed,final, km;  PERhigh,final, km;  PERexHigh,final, km;  ECcity,final, Wh/km;  EClow,final, Wh/km;  ECmed,final, Wh/km;  EChigh,final, Wh/km;  ECexHigh,final, Wh/km;  ECDC,COP,final, Wh/km. |
| Output step 8 | ECDC,COP, Wh/km. |
| 10  Result of an individual vehicle.  Final test result. | Output step 7 | PERWLTC,dec, km;  ECWLTC,dec, Wh/km | Interpolation of individual values based on input from vehicle H and vehicle L according to paragraph 4.5. of this annex, and final rounding according to paragraph 6.1.8. of this Regulation.  PERind, PERcity,ind, and PERp,ind shall be rounded to the nearest whole number.  ECind, ECcity and ECp,ind shall be rounded to the nearest whole number.  ECDC,COP,ind shall be rounded to the nearest whole number.  The output is available for each individual vehicle. | PERWLTC,ind, km;  PERcity,ind, km;  PERlow,ind, km;  PERmed,ind, km;  PERhigh,ind, km;  PERexHigh,ind, km;  ECWLTC,ind, Wh/km;  ECcity,ind, Wh/km;  EClow,ind, Wh/km;  ECmed,ind, Wh/km;  EChigh,ind, Wh/km;  ECexHigh,ind, Wh/km;  ECDC,COP,ind, Wh/km. |
| Output step 9 | PERcity,final, km;  PERlow,final, km;  PERmed,final, km;  PERhigh,final, km;  PERexHigh,final, km;  ECcity,final, Wh/km;  EClow,final, Wh/km;  ECmed,final, Wh/km;  EChigh,final, Wh/km;  ECexHigh,final, Wh/km;  ECDC,COP,final, Wh/km. |

4.7.2. Stepwise procedure for calculating the final test results of PEVs in case of the shortened test procedure

For the purpose of this table, the following nomenclature within the questions and results is used:

j index for the considered period.

Table A8/11

**Calculation of final PEV values determined by application the shortened Type 1 test procedure**

Table A8/11 shall be performed separately for results after 4 phases and for results after 3 phases.

For results after 4 phases;

The considered periods shall be the low phase, medium phase, high phase, extra high phase, the applicable WLTP city test cycle and the applicable WLTP test cycle.

For results after 3 phases;

The considered periods shall be the low phase, medium phase, high phase and the applicable WLTP test cycle.

| *Step no.* | *Source* | *Input* | *Process* | *Output* |
| --- | --- | --- | --- | --- |
| 1 | Annex B8 | Test results | Results measured according to Appendix 3 to this annex, and pre-calculated according to paragraph 4.3. of this annex.  Usable battery energy according to paragraph 4.4.2.1.1. of this annex.  Recharged electric energy according to paragraph 3.4.4.3. of this annex.  Output is available for each test.  EAC shall be rounded according to paragraph 6.1.8. of this Regulation to the first place of decimal. | ΔEREESS,j, Wh;  dj, km;  UBESTP, Wh;  EAC, Wh. |
| 2 | Output step 1 | ΔEREESS,j, Wh;  UBESTP, Wh. | Calculation of weighting factors according to paragraph 4.4.2.1. of this annex.  Output is available for each test. | KWLTC,1  KWLTC,2  Kcity,1  Kcity,2  Kcity,3  Kcity,4  Klow,1  Klow,2  Klow,3  Klow,4  Kmed,1  Kmed,2  Kmed,3  Kmed,4  Khigh,1  Khigh,2  KexHigh,1  KexHigh,2 |
| 3 | Output step 1  Output step 2 | ΔEREESS,j, Wh;  dj, km;  UBESTP, Wh.  All weighting factors | Calculation of electric energy consumption at the REESSs according to paragraph 4.4.2.1. of this annex.  Calculation of the electric energy consumption from the first applicable WLTP test cycle ECDC,first.  Output is available for each test. | ECDC,WLTC, Wh/km;  ECDC,city, Wh/km;  ECDC,low, Wh/km;  ECDC, med, Wh/km;  ECDC,high, Wh/km;  ECDC,exHigh, Wh/km;  ECDC,first, Wh/km. |
| 4 | Output step 1 | UBESTP, Wh; | Calculation of pure electric range according to paragraph 4.4.2.1. of this annex.  Output is available for each test. | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km. |
| Output step 3 | ECDC,WLTC, Wh/km;  ECDC,city, Wh/km;  ECDC,low, Wh/km;  ECDC, med, Wh/km;  ECDC,high, Wh/km;  ECDC,exHigh,  Wh/km. |
| 5 | Output step 1 | EAC, Wh; | Calculation of electric energy consumption at the mains according to paragraph 4.3.4. of this annex.  Output is available for each test. | ECWLTC, Wh/km;  ECcity, Wh/km;  EClow, Wh/km;  ECmed, Wh/km;  EChigh, Wh/km;  ECexHigh, Wh/km. |
| Output step 4 | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km. |
| 6  If the interpolation method is not applied, step No. 9 is not required and the output of this step for PERWLTC,dec and ECWLTC,dec is the final result. | Output step 4 | PERWLTC, km;  PERcity, km;  PERlow, km;  PERmed, km;  PERhigh, km;  PERexHigh, km; | Averaging of tests for all input values.  Declaration of PERWLTC,dec and ECWLTC,dec based on PERWLTC,ave and ECWLTC,ave.  Alignment of PER in case of city, low, med, high and exHigh based on the ratio between PERWLTC,dec and PERWLTC,ave:  Alignment of EC in case of city, low, med, high and exHigh based on the ratio between ECWLTC,dec and ECWLTC,ave:    In the case that the interpolation method is applied, the output is available for vehicle H and vehicle L. PERWLTC,dec as well as ECWLTC,dec shall be rounded according to paragraph 6.1.8. of this Regulation to the number of places of decimal specified in Table A6/1 of Annex B6.  In the case that the interpolation method is not applied, PERWLTC,dec and ECWLTC,dec shall be rounded according to paragraph 6.1.8. of this Regulation to the nearest whole number. | PERWLTC,dec, km;  PERWLTC,ave, km;  PERcity,ave, km;  PERlow,ave, km;  PERmed,ave, km;  PERhigh,ave, km;  PERexHigh,ave, km;  ECWLTC,dec, Wh/km;  ECWLTC,ave, Wh/km;  ECcity,ave, Wh/km;  EClow,ave, Wh/km;  ECmed,ave, Wh/km;  EChigh,ave, Wh/km;  ECexHigh,ave, Wh/km;  ECDC,first,ave, Wh/km. |
| Output step 5 | ECWLTC, Wh/km;  ECcity, Wh/km;  EClow, Wh/km;  ECmed, Wh/km;  EChigh, Wh/km;  ECexHigh, Wh/km. |
| Output step 3 | ECDC,first, Wh/km. |
| 7 | Output step 6 | ECWLTC,dec, Wh/km;  ECWLTC,ave, Wh/km;  ECDC,first,ave, Wh/km. | Adjustment of the electric energy consumption for the purpose of COP as described in paragraph 1.2. of Appendix 8 to this annex.  In the case that the interpolation method is applied, the output is available for vehicle H and vehicle L. | ECDC,COP, Wh/km. |
| 8  If the interpolation method is not applied, step No. 9 is not required and the output of this step is the final result. | Output step 6 | PERcity,ave, km;  PERlow,ave, km;  PERmed,ave, km;  PERhigh,ave, km;  PERexHigh,ave, km;  ECcity,ave, Wh/km;  EClow,ave, Wh/km;  ECmed,ave, Wh/km;  EChigh,ave, Wh/km;  ECexHigh,ave, Wh/km; | Intermediate rounding according to paragraph 6.1.8. of this Regulation.  In the case that the interpolation method is applied, intermediate rounding shall be performed according to paragraph 6.1.8. of this Regulation:  PERcity and PERp shall be rounded to the first place of decimal.  ECcity and ECp shall be rounded to the first place of decimal.  ECDC,COP shall be rounded to the first place of decimal.  The output is available for vehicle H and vehicle L.  In case that the interpolation method is not applied, final rounding of the test results according to paragraph 6.1.8. of this Regulation shall apply:  PERcity and PERp shall be rounded to the nearest whole number.  ECcity and ECp shall be rounded to the nearest whole number.  ECDC,COP shall be rounded to the nearest whole number. | PERcity,final, km;  PERlow,final, km;  PERmed,final, km;  PERhigh,final, km;  PERexHigh,final, km;  ECcity,final, Wh/km;  EClow,final, Wh/km;  ECmed,final, Wh/km;  EChigh,final, Wh/km;  ECexHigh,final, Wh/km;  ECDC,COP,final, Wh/km. |
| Output step 7 | ECDC,COP, Wh/km. |
| 9  Result of an individual vehicle.  Final test result. | Output step 6 | PERWLTC,dec, km;  ECWLTC,dec, Wh/km; | Interpolation of individual values based on input from vehicle H and vehicle L according to paragraph 4.5. of this annex, and final rounding according to paragraph 6.1.8. of this Regulation.  PERind, PERcity,ind, and PERp,ind shall be rounded to the nearest whole number.  ECind, ECcity and ECp,ind shall be rounded to the nearest whole number.  ECDC,COP,ind shall be rounded to the nearest whole number.  Output is available for each individual vehicle. | PERWLTC,ind, km;  PERcity,ind, km;  PERlow,ind, km;  PERmed,ind, km;  PERhigh,ind, km;  PERexHigh,ind, km;  ECWLTC,ind, Wh/km;  ECcity,ind, Wh/km;  EClow,ind, Wh/km;  ECmed,ind, Wh/km;  EChigh,ind, Wh/km;  ECexHigh,ind, Wh/km;  ECDC,COP,ind, Wh/km. |
| Output step 8 | PERcity,final, km;  PERlow,final, km;  PERmed,final, km;  PERhigh,final, km;  PERexHigh,final, km;  ECcity,final, Wh/km;  EClow,final, Wh/km;  ECmed,final, Wh/km;  EChigh,final, Wh/km;  ECexHigh,final, Wh/km;  ECDC,COP,final, Wh/km. |

Annex B8 - Appendix 1

**REESS state of charge profile**

1. Test sequences and REESS profiles: OVC-HEVs, charge-depleting and charge-sustaining test

1.1. Test sequence OVC-HEVs according to Option 1

Charge-depleting type 1 test with no subsequent charge-sustaining Type 1 test (Figure A8.App1/1)

# Figure A8.App1/1

# **OVC-HEVs, charge-depleting Type 1 test**




1.2. Test sequence OVC-HEVs according to Option 2

Charge-sustaining Type 1 test with no subsequent charge-depleting Type 1 test (Figure A8.App1/2).

# Figure A8.App1/2

# **OVC-HEVs, charge-sustaining Type 1 test**



1.3. Test sequence OVC-HEVs according to Option 3

Charge-depleting Type 1 test with subsequent charge-sustaining Type 1 test (Figure A8.App1/3).

# Figure A8.App1/3

# OVC-HEVs, charge-depleting type 1 test with subsequent charge-sustaining Type 1 test



1.4. Test sequence OVC-HEVs according to Option 4

Charge-sustaining Type 1 test with subsequent charge-depleting Type 1 test (Figure A8.App1/4)

Figure A8.App1/4

**OVC-HEVs, charge-sustaining Type 1 test with subsequent charge-depleting Type 1 test**



2. Test sequence NOVC-HEVs and NOVC-FCHVs

Charge-sustaining Type 1 test (Figure A8.App1/5)

# Figure A8.App1/5

# **NOVC-HEVs and NOVC-FCHVs, charge-sustaining Type 1 test**




3. Test sequences PEV

3.1. Consecutive cycles procedure (Figure A8.App1/6)

# Figure A8.App1/6


# **Consecutive cycles test sequence PEV**



3.2. Shortened test procedure (Figure A8.App1/7)

# Figure A8.App1/7

**Shortened test procedure test sequence for PEVs**



Annex B8 - Appendix 2

REESS energy change-based correction procedure

This appendix describes the procedure to correct the charge-sustaining Type 1 test CO2 emission for NOVC-HEVs and OVC-HEVs, and the charge-sustaining Type 1 test fuel consumption for NOVC-FCHVs as a function of the electric energy change of all REESSs.

1. General requirements

1.1. Applicability of this appendix

1.1.1. The correction shall be applied on the phase-specific fuel consumptions for NOVC-FCHVs and on the phase-specific CO2 emissions for NOVC-HEVs and OVC-HEVs of the charge-sustaining Type 1 test.

1.1.2. The application of the correction over the total cycle on the fuel consumption for NOVC-FCHVs, on the CO2 emission for NOVC-HEVs and OVC-HEVs is based on the REESS energy change of the charge-sustaining Type 1 test and the correction criterion c.

For the calculation of , paragraph 4.3. of this annex shall be used. The considered period j used in paragraph 4.3. of this annex is defined by the charge-sustaining Type 1 test. The correction criterion c shall be determined according to paragraph 1.2. of this Appendix.

1.1.3. The correction over the total cycle shall be applied on the fuel consumption for NOVC-FCHVs, the CO2 emission for NOVC-HEVs and OVC-HEVs if is negative which corresponds to REESS discharging and the correction criterion c calculated in paragraph 1.2. of this appendix is greater than the applicable threshold according to Table A8.App2/1.

1.1.4. The correction over the total cycle may be omitted on the fuel consumption for NOVC-FCHVs, the CO2 emission for NOVC-HEVs and OVC-HEVs and uncorrected values may be used if:

(a) is positive which corresponds to REESS charging and the correction criterion c calculated in paragraph 1.2. of this appendix is greater than the applicable threshold according to Table A8.App2/1;

(b) The correction criterion c calculated in paragraph 1.2. of this appendix is smaller than the applicable threshold according to Table A8.App2/1;

(c) The manufacturer can prove to the responsible authority by measurement that there is no relation between and charge-sustaining CO2 emission and and between charge-sustaining fuel consumption.

1.2. The correction criterion c is the ratio between the absolute value of the REESS electric energy change and the fuel energy and shall be calculated as follows:

where:

is the charge-sustaining REESS energy change according to paragraph 1.1.2. of this appendix, Wh;

is the charge-sustaining energy content of the consumed fuel according to paragraph 1.2.1. of this appendix in the case of NOVC-HEVs and OVC-HEVs, and according to paragraph 1.2.2. of this appendix in the case of NOVC-FCHVs, Wh.

1.2.1. Charge-sustaining fuel energy for NOVC-HEVs and OVC-HEVs

The charge-sustaining energy content of the consumed fuel for NOVC-HEVs and OVC-HEVs shall be calculated using the following equation:

where:

is the charge-sustaining energy content of the consumed fuel of the applicable WLTP test cycle of the charge-sustaining Type 1 test, Wh;

is the heating value according to Table A6.App2/1, kWh/l;

is the non-balanced charge-sustaining fuel consumption of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to paragraph 6. of Annex B7, using the gaseous emission compound values according to Table A8/5, step No. 2, l/100 km;

is the distance driven over the corresponding applicable WLTP test cycle, km;

conversion factor to Wh.

1.2.2. Charge-sustaining fuel energy for NOVC-FCHVs

The charge-sustaining energy content of the consumed fuel for NOVC-FCHVs shall be calculated using the following equation:

where:

is the charge-sustaining energy content of the consumed fuel of the applicable WLTP test cycle of the charge-sustaining Type 1 test, Wh;

is the lower heating value of hydrogen, MJ/kg;

is the non-balanced charge-sustaining fuel consumption of the charge-sustaining Type 1 test, not corrected for the energy balance, determined according to Table A8/7, step No. 1, kg/100 km;

is the distance driven over the corresponding applicable WLTP test cycle, km;

conversion factor to Wh.

Table A8.App2/1

**RCB correction criteria thresholds**

| *Applicable Type 1 test cycle* | *Low + Medium* | *Low + Medium +*  *High* | *Low + Medium +*  *High + Extra High* |
| --- | --- | --- | --- |
| Thresholds for correction criterion c | 0.015 | 0.01 | 0.005 |

2. Calculation of correction coefficients

2.1. The CO2 emission correction coefficient KCO2, the fuel consumption correction coefficients Kfuel,FCHV, as well as, if required by the manufacturer, the phase-specific correction coefficients KCO2,p and Kfuel,FCHV,p shall be developed based on the applicable charge-sustaining Type 1 test cycles.

In the case that vehicle H was tested for the development of the correction coefficient for CO2 emission for NOVC-HEVs and OVC-HEVs, the coefficient may be applied to vehicles that fulfil the same interpolation family criteria. For interpolation families which fulfil the criteria of the KCO2 correction factor family, defined in paragraph 6.3.11. of this Regulation, the same KCO2 value may be applied.

2.2. The correction coefficients shall be determined from a set of charge-sustaining Type 1 tests according to paragraph 3. of this appendix. The number of tests performed by the manufacturer shall be equal to or greater than five.

The state of charge of the REESS may be set prior to the test according to the manufacturer’s recommendation in agreement with the responsible authority and as described in paragraph 3. This practice shall only be used for the purpose of achieving a charge-sustaining Type 1 test with opposite sign of the .

The set of measurements shall fulfil the following criteria:

(a) The set shall contain at least one test with and at least one test with . is the sum of electric energy changes of all REESSs of test n calculated according to paragraph 4.3. of this annex.

(b) The difference in between the test with the highest negative electric energy change and the test with the highest positive electric energy change shall be greater than or equal to 5 g/km. This criterion shall not be applied for the determination of Kfuel,FCHV.

In the case of the determination of KCO2, the required number of tests may be reduced to three tests if all of the following criteria are fulfilled in addition to (a) and (b):

(c) The difference in between any two adjacent measurements, related to the electric energy change during the test, shall be less than or equal to 10 g/km.

(d) In addition to (b), the test with the highest negative electric energy change and the test with the highest positive electric energy change shall not be within the region that is defined by:

,

where:

is the energy content of the consumed fuel calculated according to paragraph 1.2. of this appendix, Wh.

(e) The difference in between the test with the highest negative electric energy change and the mid-point, and the difference in between the mid-point and the test with the highest positive electric energy change shall be similar and preferably be within the range defined by (d). If this requirement is not feasible, the responsible authority shall decide if a retest is necessary.

The correction coefficients determined by the manufacturer shall be reviewed and approved by the responsible authority prior to their application.

If the set of at least five tests does not fulfil criterion (a) or criterion (b) or both, the manufacturer shall provide evidence to the responsible authority as to why the vehicle is not capable of meeting either or both criteria. If the responsible authority is not satisfied with the evidence, it may require additional tests to be performed. If the criteria after additional tests are still not fulfilled, the responsible authority shall determine a conservative correction coefficient, based on the measurements.

2.3. Calculation of correction coefficients and

2.3.1. Determination of the fuel consumption correction coefficient

For NOVC-FCHVs, the fuel consumption correction coefficient , determined by driving a set of charge-sustaining Type 1 tests, is defined using the following equation:

where:

is the fuel consumption correction coefficient, (kg/100 km)/(Wh/km);

is the charge-sustaining electric energy consumption of test n based on the REESS depletion according to the equation below, Wh/km

is the mean charge-sustaining electric energy consumption of tests based on the REESS depletion according to the equation below, Wh/km;

is the charge-sustaining fuel consumption of test n, not corrected for the energy balance, according to Table A8/7, step No. 1, kg/100 km;

is the arithmetic average of the charge-sustaining fuel consumption of tests based on the fuel consumption, not corrected for the energy balance, according to the equation below, kg/100 km;

is the index number of the considered test;

is the total number of tests;

and:

and:

and:

where:

is the charge-sustaining REESS electric energy change of test n according to paragraph 1.1.2. of this appendix, Wh;

is the distance driven over the corresponding charge-sustaining Type 1 test n, km.

The fuel consumption correction coefficient shall be rounded according to paragraph 6.1.8. of this Regulation to four significant figures. The statistical significance of the fuel consumption correction coefficient shall be evaluated by the responsible authority.

2.3.1.1. It is permitted to apply the fuel consumption correction coefficient that was developed from tests over the whole applicable WLTP test cycle for the correction of each individual phase.

2.3.1.2. Additional to the requirements of paragraph 2.2. of this appendix, at the manufacturer’s request and upon approval of the responsible authority, separate fuel consumption correction coefficients for each individual phase may be developed. In this case, the same criteria as described in paragraph 2.2. of this appendix shall be fulfilled in each individual phase and the procedure described in paragraph 2.3.1. of this appendix shall be applied for each individual phase to determine each phase specific correction coefficient.

2.3.2. Determination of CO2 emission correction coefficient KCO2

For OVC-HEVs and NOVC-HEVs, the CO2 emission correction coefficient , determined by driving a set of charge-sustaining Type 1 tests, is defined by the following equation:

where:

is the CO2 emission correction coefficient, (g/km)/(Wh/km);

is the charge-sustaining electric energy consumption of test n based on the REESS depletion according to paragraph 2.3.1. of this appendix, Wh/km;

is the arithmetic average of the charge-sustaining electric energy consumption of tests based on the REESS depletion according to paragraph 2.3.1. of this appendix, Wh/km;

is the charge-sustaining CO2 emission of test n, not corrected for the energy balance, calculated according Table A8/5, step No. 2, g/km;

is the arithmetic average of the charge-sustaining CO2 emission of tests based on the CO2 emission, not corrected for the energy balance, according to the equation below, g/km;

is the index number of the considered test;

is the total number of tests;

and:

The CO2 emission correction coefficient shall be rounded according to paragraph 6.1.8. of this Regulation to four significant figures. The statistical significance of the CO2 emission correction coefficient shall be evaluated by the responsible authority.

2.3.2.1. It is permitted to apply the CO2 emission correction coefficient developed from tests over the whole applicable WLTP test cycle for the correction of each individual phase.

2.3.2.2. Additional to the requirements of paragraph 2.2. of this appendix, at the request of the manufacturer and upon approval of the responsible authority, separate CO2 emission correction coefficients for each individual phase may be developed. In this case, the same criteria as described in paragraph 2.2. of this appendix shall be fulfilled in each individual phase and the procedure described in paragraph 2.3.2. of this appendix shall be applied for each individual phase to determine phase-specific correction coefficients.

3. Test procedure for the determination of the correction coefficients

3.1. OVC-HEVs

For OVC-HEVs, one of the following test sequences according to Figure A8.App2/1 shall be used to measure all values that are necessary for the determination of the correction coefficients according to paragraph 2. of this appendix.

Figure A8.App2/1

**OVC-HEV test sequences**



3.1.1. Option 1 test sequence

3.1.1.1. Preconditioning and soaking

Preconditioning and soaking shall be conducted according to paragraph 2.1. of Appendix 4 to this annex.

3.1.1.2. REESS adjustment

Prior to the test procedure according to paragraph 3.1.1.3. of this appendix, the manufacturer may adjust the REESS. The manufacturer shall provide evidence that the requirements for the beginning of the test according to paragraph 3.1.1.3. of this appendix are fulfilled.

3.1.1.3. Test procedure

3.1.1.3.1. The driver-selectable mode for the applicable WLTP test cycle shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.1.1.3.2. For testing, the applicable WLTP test cycle according to paragraph 1.4.2. of this annex shall be driven.

3.1.1.3.3. Unless stated otherwise in this appendix, the vehicle shall be tested according to the Type 1 test procedure described in Annex B6.

3.1.2. Option 2 test sequence

3.1.2.1. Preconditioning

The test vehicle shall be preconditioned according to paragraph 2.1.1. or paragraph 2.1.2. of Appendix 4 to this annex.

3.1.2.2. REESS adjustment

After preconditioning, soaking according to paragraph 2.1.3. of Appendix 4 to this annex shall be omitted and a break, during which the REESS is permitted to be adjusted, shall be set to a maximum duration of 60 minutes. A similar break shall be applied in advance of each test. Immediately after the end of this break, the requirements of paragraph 3.1.2.3. of this appendix shall be applied.

Upon request of the manufacturer, an additional warm-up procedure may be conducted in advance of the REESS adjustment to ensure similar starting conditions for the correction coefficient determination. If the manufacturer requests this additional warm-up procedure, the identical warm-up procedure shall be applied repeatedly within the test sequence.

3.1.2.3. Test procedure

3.1.2.3.1. The driver-selectable mode for the applicable WLTP test cycle shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.1.2.3.2. For testing, the applicable WLTP test cycle according to paragraph 1.4.2. of this annex shall be driven.

3.1.2.3.3. Unless stated otherwise in this appendix, the vehicle shall be tested according to the Type 1 test procedure described in Annex B6.

3.1.2.3.4. When conducting a number of consecutive sequences, paragraph 2.2. of this appendix consisting of paragraphs 3.1.2.1. shall be omitted.

3.2. NOVC-HEVs and NOVC-FCHVs

For NOVC-HEVs and NOVC-FCHVs, one of the following test sequences according to Figure A8.App2/2 shall be used to measure all values that are necessary for the determination of the correction coefficients according to paragraph 2. of this appendix.

Figure A8.App2/2

**NOVC-HEV and NOVC-FCHV test sequences**

Option 1 test sequence

(paragraph 3.2.1. of this appendix)

Option 2 test sequence

(paragraph 3.2.2. of this appendix)

Preconditioning

Applicable WLTP test cycle

REESS adjustment within a similar break of max. 60min

Optional:

Additional warm up procedure

Preconditioning and soaking

Applicable WLTP test cycle

REESS adjustment

3.2.1. Option 1 test sequence

3.2.1.1. Preconditioning and soaking

The test vehicle shall be preconditioned and soaked according to paragraph 3.3.1. of this annex.

3.2.1.2. REESS adjustment

Prior to the test procedure, according to paragraph 3.2.1.3. of this appendix, the manufacturer may adjust the REESS. The manufacturer shall provide evidence that the requirements for the beginning of the test according to paragraph 3.2.1.3. of this appendix are fulfilled.

3.2.1.3. Test procedure

3.2.1.3.1. The driver-selectable mode for the applicable WLTP test cycle shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.2.1.3.2. For testing, the applicable WLTP test cycle according to paragraph 1.4.2. of this annex shall be driven.

3.2.1.3.3. Unless stated otherwise in this appendix, the vehicle shall be tested according to the charge-sustaining Type 1 test procedure described in Annex B6.

3.2.2. Option 2 test sequence

3.2.2.1. Preconditioning

The test vehicle shall be preconditioned according to paragraph 3.3.1.1. of this annex.

3.2.2.2. REESS adjustment

After preconditioning, the soaking according to paragraph 3.3.1.2. of this annex shall be omitted and a break, during which the REESS is permitted to be adjusted, shall be set to a maximum duration of 60 minutes. A similar break shall be applied in advance of each test. Immediately after the end of this break, the requirements of paragraph 3.2.2.3. of this appendix shall be applied.

Upon request of the manufacturer, an additional warm-up procedure may be conducted in advance of the REESS adjustment to ensure similar starting conditions for the correction coefficient determination. If the manufacturer requests this additional warm-up procedure, the identical warm-up procedure shall be applied repeatedly within the test sequence.

3.2.2.3. Test procedure

3.2.2.3.1. The driver-selectable mode for the applicable WLTP test cycle shall be selected according to paragraph 3. of Appendix 6 to this annex.

3.2.2.3.2. For testing, the applicable WLTP test cycle according to paragraph 1.4.2. of this annex shall be driven.

3.2.2.3.3. Unless stated otherwise in this appendix, the vehicle shall be tested according to the Type 1 test procedure described in Annex B6.

3.2.2.3.4. When conducting a number of consecutive sequences paragraph 3.2.2.1. shall be omitted.

4. As an option for the manufacturer, it is allowed to apply ΔMCO2,j defined in paragraph 4.5. of Appendix 2 to Annex B6 with the following modification:

is the efficiency of the alternator

0.67 in case is negative (corresponds to a discharge)

1.00 in case is positive (corresponds to a charge)

4.1. In this case, the corrected charge-sustaining CO2 emission defined in paragraphs 4.1.1.3., 4.1.1.4. and 4.1.1.5. of this annex shall be replaced by ΔMCO2,j instead of .

Annex B8 - Appendix 3

Determination of REESS current and REESS voltage for NOVC-HEVs, OVC-HEVs, PEVs and NOVC-FCHVs

1. Introduction

1.1. This appendix defines the method and required instrumentation to determine the REESS current and the REESS voltage of NOVC-HEVs, OVC-HEVs, PEVs and NOVC-FCHVs.

1.2. Measurement of REESS current and REESS voltage shall start at the same time as the test starts and shall end immediately after the vehicle has finished the test.

1.3. The REESS current and the REESS voltage of each phase shall be determined.

1.4. A list of the instrumentation used by the manufacturer to measure REESS voltage and current (including instrument manufacturer, model number, serial number, last calibration dates (where applicable)) during:

(a) The Type 1 test according to paragraph 3 of this annex;

(b) The procedure to determine the correction coefficients according to Appendix 2 of this annex (where applicable);

(c) For the 4-phase WLTP only;

The Ambient Temperature Correction Test (ATCT) as specified in Annex B6a

shall be provided to the responsible authority.

2. REESS current

REESS depletion is considered as a negative current.

2.1. External REESS current measurement

2.1.1. The REESS current(s) shall be measured during the tests using a clamp-on or closed type current transducer. The current measurement system shall fulfil the requirements specified in Table A8/1 of this annex. The current transducer(s) shall be capable of handling the peak currents at engine starts and temperature conditions at the point of measurement.

In order to have an accurate measurement, zero adjustment and degaussing shall be performed before the test according to the instrument manufacturer's instructions.

2.1.2. Current transducers shall be fitted to any of the REESS on one of the cables connected directly to the REESS and shall include the total REESS current.

In case of shielded wires, appropriate methods shall be applied in accordance with the responsible authority.

In order to easily measure the REESS current using external measuring equipment, the manufacturer should provide appropriate, safe and accessible connection points in the vehicle. If that is not feasible, the manufacturer is obliged to support the responsible authority in connecting a current transducer to one of the cables directly connected to the REESS in the manner described above in this paragraph.

2.1.3. The current transducer output shall be sampled with a minimum frequency of 20 Hz. The measured current shall be integrated over time, yielding the measured value of Q, expressed in ampere-hours Ah. The integration may be done in the current measurement system.

2.2. Vehicle on-board REESS current data

As an alternative to paragraph 2.1. of this appendix, the manufacturer may use on-board REESS current measurement data. The accuracy of these data shall be demonstrated to the responsible authority.

3. REESS voltage

During the tests described in paragraph 3. of this annex, the REESS voltage to be used for each category of test event shall be as specified in Table A8 App3/1 and as described in paragraphs 3.1. to 3.3. of this appendix.

3.1. External REESS voltage measurement

The REESS voltage shall be measured with the equipment and accuracy requirements specified in paragraph 1.1. of this annex. To measure the REESS voltage using external measuring equipment, the manufacturers shall support the responsible authority by providing REESS voltage measurement points and safety instructions.

3.2. Nominal REESS voltage

The nominal voltage of the REESS shall be determined according to IEC 60050-482.

3.3. Vehicle on-board REESS voltage data

As an alternative to the external REESS voltage measurement specified in paragraph 3.1. of this appendix, the manufacturer may use the vehicle on-board REESS voltage measurement data. The accuracy of these data shall be demonstrated to the responsible authority.

Table A8 App3/1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Test events* | *Paragraph. 3.1.* | *Paragraph 3.2.* | | *Paragraph 3.3.* |
| *60V or more* | *Less than 60V* |
| NOVC-HEV | shall not to be used | shall be used | | shall not to be used |
| OVC-HEV CS condition |
| NOVC-FCHV |
| OVC-FCHV CS condition |
| REESS energy change-based correction procedure (Appendix 2) |
| Break-Off Criterion calculation for CD-test (Annex B8, paragraph 3.2.5.4.3.) |
| OVC-HEV CD condition | may be used | shall not to be used | may be used | may be used |
| OVC-FCHV CD condition |
| PEV |

Annex B8 - Appendix 4

Preconditioning, soaking and REESS charging conditions of PEVs and OVC-HEVs

1. This appendix describes the test procedure for REESS and combustion engine preconditioning in preparation for:

(a) Electric range, charge-depleting and charge-sustaining measurements when testing OVC-HEVs; and

(b) Electric range measurements as well as electric energy consumption measurements when testing PEVs.

2. OVC-HEV preconditioning and soaking

2.1. Preconditioning and soaking when the test procedure starts with a charge-sustaining test

2.1.1. For preconditioning the combustion engine, the vehicle shall be driven over at least one applicable WLTP test cycle. During each driven preconditioning cycle, the charging balance of the REESS shall be determined. The preconditioning shall be stopped at the end of the applicable WLTP test cycle during which the break-off criterion is fulfilled according to paragraph 3.2.4.5. of this annex.

2.1.2. As an alternative to paragraph 2.1.1. of this appendix, at the request of the manufacturer and upon approval of the responsible authority, the state of charge of the REESS for the charge-sustaining Type 1 test may be set according to the manufacturer’s recommendation in order to achieve a test under charge-sustaining operating condition.

In such a case, a preconditioning procedure, such as that applicable to pure ICE vehicles as described in paragraph 2.6. of Annex B6, shall be applied.

2.1.3. Soaking of the vehicle shall be performed according to paragraph 2.7. of Annex B6.

2.2. Preconditioning and soaking when the test procedure starts with a charge-depleting test

2.2.1. OVC-HEVs shall be driven over at least one applicable WLTP test cycle. During each driven preconditioning cycle, the charging balance of the REESS shall be determined. The preconditioning shall be stopped at the end of the applicable WLTP test cycle during which the break-off criterion is fulfilled according to paragraph 3.2.4.5. of this annex.

2.2.2. Soaking of the vehicle shall be performed according to paragraph 2.7. of Annex B6. Forced cooling down shall not be applied to vehicles preconditioned for the Type 1 test. During soak, the REESS shall be charged using the normal charging procedure as defined in paragraph 2.2.3. of this appendix.

2.2.3. Application of a normal charge

Normal charging is the transfer of electricity to an electrified vehicle with a power of less than or equal to 22 kW.

Where there are several possible methods to perform a normal AC charge (e.g. cable, induction, etc.), the charging procedure via cable shall be used.

Where there are several AC charging power levels available, the highest normal charging power shall be used. An AC charging power lower than the highest normal AC charging power may be selected if recommended by the manufacturer and by approval of the responsible authority.

2.2.3.1. The REESS shall be charged at an ambient temperature as specified in paragraph 2.2.2.2. of Annex B6 with the on-board charger if fitted.

In the following cases, a charger recommended by the manufacturer and using the charging pattern prescribed for normal charging shall be used if:

(a) No on-board charger is fitted, or

(b) The charging time exceeds the soaking time defined in paragraph 2.7. of Annex B6.

The procedures in this paragraph exclude all types of special charges that could be automatically or manually initiated, e.g. equalization charges or servicing charges. The manufacturer shall declare that, during the test, a special charge procedure has not occurred.

2.2.3.2. End-of-charge criterion

The end-of-charge criterion is reached when the on-board or external instruments indicate that the REESS is fully charged. If the charging is performed during soaking and finished before the minimum required soaking time as defined in paragraph 2.7. of Annex B6, the vehicle shall stay connected to the grid at least until the minimum required soaking time is reached.

3. PEV preconditioning and soaking

3.1. Initial charging of the REESS

Initial charging of the REESS consists of discharging the REESS and applying a normal charge.

3.1.1. Discharging the REESS

The discharge procedure shall be performed according to the manufacturer’s recommendation. The manufacturer shall guarantee that the REESS is as fully depleted as is possible by the discharge procedure.

3.1.2. Soaking and application of a normal charge

Soaking of the vehicle shall be performed in accordance with paragraph 2.7. of Annex B6.

During soak, the REESS shall be charged using the normal charging procedure as defined in paragraph 2.2.3. of this appendix.

Annex B8 - Appendix 5

Utility factors (UF) for OVC-HEVs

1. Each Contracting Party may develop its own UFs.

2. The methodology recommended for the determination of a UF curve based on driving statistics is described in SAE J2841 (Sept. 2010, Issued 2009-03, Revised 2010-09).

3. For the calculation of a fractional utility factor UFj for the weighting of period j, the following equation shall be applied by using the coefficients from Table A8.App5/1.

where:

UFj utility factor for period j;

dj measured distance driven at the end of period j, km;

Ci ith coefficient (see Table A8.App5/1);

dn normalized distance (see Table A8.App5/1), km;

k number of terms and coefficients in the exponent;

j number of period considered;

i number of considered term/coefficient;

sum of calculated utility factors up to period (j-1).

Table A8.App5/1

**Parameters for the determination of fractional UFs (as applicable)**

|  |  |
| --- | --- |
| *Parameter* | *For the 4-phase WLTP only* |
| dn | 800 km |
| C1 | 26.25 |
| C2 | -38.94 |
| C3 | -631.05 |
| C4 | 5964.83 |
| C5 | -25095 |
| C6 | 60380.2 |
| C7 | -87517 |
| C8 | 75513.8 |
| C9 | -35749 |
| C10 | 7154.94 |

Annex B8 - Appendix 6

Selection of driver-selectable modes

1. General requirement

1.1. The manufacturer shall select the driver-selectable mode for the Type 1 test procedure according to paragraphs 2. to 4. inclusive of this appendix which enables the vehicle to follow the considered test cycle within the speed trace tolerances according to paragraph 2.6.8.3.1.2. of Annex B6. This shall apply to all vehicle systems with driver-selectable modes including those not solely specific to the transmission.

1.2. The manufacturer shall provide evidence to the responsible authority concerning:

(a) The availability of a predominant mode under the considered conditions;

(b) The maximum speed of the considered vehicle;

and if required:

(c) The best and worst case mode identified by the evidence on the fuel consumption and, if applicable, on the CO2 emission/fuel consumption in all modes. See paragraph 2.6.6.3. of Annex B6;

(d) The highest electric energy consuming mode;

(e) The cycle energy demand (according to paragraph 5 of Annex B7 where the target speed is replaced by the actual speed).

1.3. On the basis of technical evidence provided by the manufacturer and with the agreement of the responsible authority, the dedicated driver-selectable modes, such as "mountain mode" or "maintenance mode" which are not intended for normal daily operation but only for special limited purposes, shall not be considered. Irrespective of the driver-selectable mode selected for the Type 1 test according to paragraph 2. and 3. of this appendix, the vehicle shall comply with the criteria emissions limits in all remaining driver-selectable modes used for forward driving.

2. OVC-HEVs equipped with a driver-selectable mode under charge-depleting operating condition

For vehicles equipped with a driver-selectable mode, the mode for the charge-depleting Type 1 test shall be selected according to the following conditions.

# The flow chart in Figure A8.App6/1 illustrates the mode selection according to this paragraph.

2.1. If there is a predominant mode that enables the vehicle to follow the reference test cycle under charge-depleting operating condition, this mode shall be selected.

2.2. If there is no predominant mode or if there is a predominant mode but this mode does not enable the vehicle to follow the reference test cycle under charge-depleting operating condition, the mode for the test shall be selected according to the following conditions:

(a) If there is only one mode which allows the vehicle to follow the reference test cycle under charge-depleting operating conditions, this mode shall be selected;

(b) If several modes are capable of following the reference test cycleunder charge-depleting operating conditions and none of those modes is a configurable start mode, the worst case mode for electric energy consumption of those modes shall be selected;

(c) If several modes are capable of following the reference test cycleunder charge-depleting operating conditions and at least two of those modes are a configurable start mode, the worst case mode for electric energy consumption shall be selected from these configurable start modes.

2.3. If there is no mode according to paragraph 2.1. and paragraph 2.2. of this appendix that enables the vehicle to follow the reference test cycle, the reference test cycle shall be modified according to paragraph 9 of Annex B1:


(a) If there is a predominant mode which allows the vehicle to follow the modified reference test cycle under charge-depleting operating conditions, this mode shall be selected.


(b) If there is no predominant mode but other modes which allow the vehicle to follow the modified reference test cycle under charge-depleting operating condition, the worst case mode for electric energy consumption of those modes shall be selected. In the case that at least two or more configurable start modes, the worst case mode for electric energy consumption shall be selected from these configurable start modes;

(c) If there is no mode which allows the vehicle to follow the modified reference test cycle under charge-depleting operating condition, the mode or modes with the highest cycle energy demand shall be identified and the worst case mode for electric energy consumption shall be selected.

# Figure A8.App6/1a and Figure A8.App6/1b

# **Selection of driver-selectable mode for OVC-HEVs under charge-depleting operating condition**





3. OVC-HEVs, NOVC-HEVs and NOVC-FCHVs equipped with a driver- selectable mode under charge-sustaining operating condition

For vehicles equipped with a driver-selectable mode, the mode for the charge-sustaining Type 1 test shall be selected according to the following conditions.

# The flow chart in Figure A8.App6/2 illustrates the mode selection according to this paragraph.

3.1. If there is a predominant mode that enables the vehicle to follow the reference test cycle under charge-sustaining operating condition, this mode shall be selected.

3.2. If there is no predominant mode or if there is a predominant mode but this mode does not enable the vehicle to follow the reference test cycle under charge-sustaining operating condition, the mode for the test shall be selected according to the following conditions:

(a) If there is only one mode which allows the vehicle to follow the reference test cycle under charge-sustaining operating conditions, this mode shall be selected;

(b) If several modes are capable of following the reference test cycleunder charge-sustaining operating conditions and none of those modes is a configurable start mode, the vehicle shall be tested for criteria emissions and CO2 emissions in the best case mode and worst case mode. Best and worst case modes shall be identified by the evidence provided on the CO2 emissions in all modes. CO2 emissions shall be the arithmetic average of the test results in both modes. Test results for both modes shall be recorded.

At the request of the manufacturer, the vehicle may alternatively be tested with the driver-selectable mode in the worst case position for CO2 emissions;

(c) If several modes are capable of following the reference test cycleunder charge-sustaining operating conditions and at least two or more of those modes are a configurable start mode, the worst case mode for CO2 emissions and fuel consumption shall be selected from these configurable start modes.

3.3. If there is no mode according to paragraph 3.1. and paragraph 3.2. of this appendix that enables the vehicle to follow the reference test cycle, the reference test cycle shall be modified according to paragraph 9. of Annex B1:


(a) If there is a predominant mode which allows the vehicle to follow the modified reference test cycle under charge-sustaining operating condition, this mode shall be selected.


(b) If there is no predominant mode but other modes which allow the vehicle to follow the modified reference test cycle under charge-sustaining operating condition, the worst case mode for CO2 emissions and fuel consumption of these modes shall be selected.

(c) If there is no mode which allows the vehicle to follow the modified reference test cycle under charge-sustaining operating condition, the mode or modes with the highest cycle energy demand shall be identified and the worst case mode for CO2 emissions and fuel consumption of those modes shall be selected. In the case that at least two or more of these modes are a configurable start mode, the worst case mode for CO2 emissions and fuel consumption shall be selected from these modes.

# Figure A8.App6/2a and Figure A8.App6/2b

# **Selection of a driver-selectable mode for OVC-HEVs, NOVC-HEVs and NOVC- FCHVs under charge-sustaining operating condition**

****

****4. PEVs equipped with a driver-selectable mode

For vehicles equipped with a driver-selectable mode, the mode for the test shall be selected according to the following conditions.

# The flow chart in Figure A8.App6/3 illustrates the mode selection according to this paragraph.

4.1. If there is a predominant mode that enables the vehicle to follow the reference test cycle, this mode shall be selected.

4.2. If there is no predominant mode or if there is a predominant mode but this mode does not enable the vehicle to follow the reference test cycle,the mode for the test shall be selected according to the following conditions:

(a) If there is only one mode which allows the vehicle to follow the reference test cycle, this mode shall be selected;

(b) If several modes are capable of following the reference test cycle and none of those modes is a configurable start mode, the worst case mode for electric energy consumption of those modes shall be selected;

(c) If several modes are capable of following the reference test cycleand at least two of those modes are a configurable start mode, the worst case mode for electric energy consumptionshall be selected from these configurable start modes.

4.3. If there is no mode according to paragraph 4.1. and paragraph 4.2. of this appendix that enables the vehicle to follow the reference test cycle, the reference test cycle shall be modified according to paragraph 9. of Annex B1. The resulting test cycle shall be named as the applicable WLTP test cycle:


(a) If there is a predominant mode which allows the vehicle to follow the modified reference test cycle, this mode shall be selected;

(b) If there is no predominant mode but other modes which allow the vehicle to follow the modified reference test cycle, worst case mode for electric energy consumption of those modes shall be selected. In the case that at least two or more configurable start modes, the worst case mode for electric energy consumption shall be selected from these configurable start modes;

(c) If there is no mode which allows the vehicle to follow the modified reference test cycle, the mode or modes with the highest cycle energy demand shall be identified and the worst case mode for electric energy consumption shall be selected.

# Figure A8.App6/3a and Figure A8.App6/3b

# **Selection of the driver-selectable mode for PEVs**





Annex B8 - Appendix 7

Fuel consumption measurement of compressed hydrogen fuel cell hybrid vehicles

1. General requirements

Fuel consumption shall be measured using the gravimetric method in accordance with paragraph 2. of this appendix.

At the request of the manufacturer and with approval of the responsible authority, fuel consumption may be measured using either the pressure method or the flow method. In this case, the manufacturer shall provide technical evidence that the method yields equivalent results. The pressure and flow methods are described in ISO 23828.

2. Gravimetric method

Fuel consumption shall be calculated by measuring the mass of the fuel tank before and after the test.

2.1. Equipment and setting

2.1.1. An example of the instrumentation is shown in Figure A8.App7/1. One or more off-vehicle tanks shall be used to measure the fuel consumption. The off-vehicle tank(s) shall be connected to the vehicle fuel line between the original fuel tank and the fuel cell system.

2.1.2. For preconditioning, the originally installed tank or an external source of hydrogen may be used.

2.1.3. The refuelling pressure shall be adjusted to the manufacturer’s recommended value.

2.1.4. Difference of the gas supply pressures in lines shall be minimized when the lines are switched.

In the case that influence of pressure difference is expected, the manufacturer and the responsible authority shall agree whether correction is necessary or not.

2.1.5. Balance

2.1.5.1. The balance used for fuel consumption measurement shall meet the specification of Table A8.App7/1.

Table A8.App7/1

**Analytical balance verification criteria**

|  |  |  |
| --- | --- | --- |
| *Measurement system* | *Resolution* | *Precision* |
| Balance | 0.1 g maximum | ±0.02 maximum(a) |

(a) Fuel consumption (REESS charge balance = 0) during the test, in mass, standard deviation

2.1.5.2. The balance shall be calibrated in accordance with the specifications provided by the balance manufacturer or at least as often as specified in Table A8.App7/2.

Table A8.App7/2


**Instrument calibration intervals**

|  |  |
| --- | --- |
| *Instrument checks* | *Interval* |
| Precision | Yearly and at major maintenance |

2.1.5.3. Appropriate means for reducing the effects of vibration and convection, such as a damping table or a wind barrier, shall be provided.

Figure A8.App7/1

**Example of instrumentation**



where:

1 is the external fuel supply for preconditioning

2 is the pressure regulator

3 is the original tank

4 is the fuel cell system

5 is the balance

6 is/are off-vehicle tank(s) for fuel consumption measurement

2.2. Test procedure

2.2.1. The mass of the off-vehicle tank shall be measured before the test.

2.2.2. The off-vehicle tank shall be connected to the vehicle fuel line as shown in Figure A8.App7/1.

2.2.3. The test shall be conducted by fuelling from the off-vehicle tank.

2.2.4. The off-vehicle tank shall be removed from the line.

2.2.5. The mass of the tank and fuel consumed after the test shall be measured.

2.2.5.1. At the request of the manufacturer and with approval of the responsible authority, the change in weight of the hydrogen in the auxiliary line between points 2 and 4 in Figure A8.App7/1 due to changes in temperature and pressure may be taken into consideration.

2.2.6. The non-balanced charge-sustaining fuel consumption from the measured mass before and after the test shall be calculated using the following equation:

where:

is the non-balanced charge-sustaining fuel consumption measured during the test, kg/100 km;

g1 is the mass of the tank at the start of the test, kg;

g2 is the mass of the tank at the end of the test, kg;

d is the distance driven during the test, km.

2.2.7. Separate fuel consumption as defined in paragraphs 4.2.1.2.4. and 4.2.1.2.5. of this annex shall be calculated for each individual phase in accordance with paragraph 2.2. of this appendix. The test procedure shall be conducted with off-vehicle tanks and connections to the vehicle fuel line which are individually prepared for each phase.

Annex B8 - Appendix 8

Determination of additional electric energy consumption values required for checking the Conformity of Production of PEVs and OVC-HEVs

1. PEVs

1.1. The following value shall be determined and used as a reference value for verifying the conformity of production:

In the case that the interpolation method is applied,

In the case that the interpolation method is not applied,

where:

is the reference electric energy consumption of an individual vehicle for the conformity of production, Wh/km;

is the electric energy consumption of vehicle L determined according to paragraph 1.2. of this appendix, Wh/km;

is the electric energy consumption of vehicle H determined according to paragraph 1.2. of this appendix, Wh/km**;**

is the electric energy consumption of vehicle i determined according to paragraph 1.2. of this appendix, Wh/km**;**

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle, according to paragraph 4.5.3. of this annex.

1.2. Calculation of the , and

where:

i represents – in the case the interpolation method is applied – the index L for vehicle L and the index H for vehicle H. In the case the interpolation method is not applied, index i represents the vehicle tested.

is the aligned electric energy consumption of vehicle i based on the REESS depletion of the first applicable WLTP test cycle, Wh/km;

is the average of the measured electric energy consumption of vehicle i based on the REESS depletion of the first applicable WLTP test cycle according to paragraph 4.3. of this annex,  Wh/km;

is the alignment factor of vehicle i according to Table A8/10 Step no.7 for the consecutive cycle Type 1 procedure

or Table A8/11 Step no. 6 for the shortened Type 1 test procedure.

2. OVC-HEVs

This paragraph shall only be applied if there is no engine start in the first cycle of the charge-depleting Type 1 test during Type Approval. In the case there is an engine start, this paragraph shall be omitted.

2.1. The following value shall be determined and used as a reference value for verifying the conformity of production:

In the case that the interpolation method is applied,

In the case that the interpolation method is not applied,

where:

is the reference charge-depleting electric energy consumption of an individual vehicle for the conformity of production, Wh/km;

is the charge-depleting electric energy consumption of vehicle L determined according to paragraph 2.2. of this appendix, Wh/km;

is the charge-depleting electric energy consumption of vehicle H determined according to paragraph 2.2. of this appendix, Wh/km**;**

is the charge-depleting electric energy consumption of vehicle i determined according to paragraph 2.2. of this appendix, Wh/km**;**

is the interpolation coefficient for the considered individual vehicle for the applicable WLTP test cycle, according to paragraph 4.5.3. of this annex.

2.2. Calculation of the and

where:

i represents – in the case the interpolation method is applied – the index L for vehicle L and the index H for vehicle H. In the case the interpolation method is not applied, index i represents the vehicle tested.

is the aligned charge-depleting electric energy consumption based on the REESS depletion of the first applicable WLTC test cycle, Wh/km;

is average of the measured charge-depleting electric energy consumption of vehicle i based on the REESS depletion of the first applicable WLTC test cycle according to paragraph 4.3. of this annex, Wh/km;

is the alignment factor of vehicle i

where

For 4-phase WLTP test

where

is the declared charge-depleting electric energy consumption of vehicle i according to Table A8/8 Step no. 14, Wh/km;

is the average of the measured charge-depleting electric energy consumption of vehicle i according to Table A8/8 Step no. 13, Wh/km;

For 3-phase WLTP test

where

is the declared electric energy consumption of vehicle i of the charge-depleting Type 1 test according to Table A8/9 Step no. 8, Wh/km;

is the average of the measured electric energy consumption of vehicle i of the charge-depleting Type 1 test according to Table A8/9 Step no. 8, Wh/km.

Annex B9 – (Reserved)

Annexes Part C

Annex C1: (Reserved)

Annex C2: (Reserved)

Annex C3: Type 4 test

Determination of evaporative emissions from vehicles fuelled with petrol

Type 4 test procedures and test conditions

1. Introduction

This annex provides the method to determine the levels of evaporative emission from light-duty vehicles in a repeatable and reproducible manner designed to be representative of real world vehicle operation.

2. Technical requirements

2.1. The procedure includes the evaporative emissions test and two additional tests, one for the ageing of carbon canisters, as described in paragraph 5.1. of this annex, and one for the permeability of the fuel tank system, as described in paragraph 5.2. of this annex. The evaporative emissions test (Figure C3/4) determines hydrocarbon evaporative emissions as a consequence of diurnal temperature fluctuations and hot soaks during parking.

2.2. In the case that the fuel system contains more than one carbon canister, all references to the term "carbon canister" in this annex will apply to each carbon canister.

3. Vehicle

The vehicle shall be in good mechanical condition and have been run-in and driven at least 3,000 km before the test. For the purpose of the determination of evaporative emissions, the mileage and the age of the vehicle used for certification shall be recorded. The evaporative emission control system shall be connected and functioning correctly during the run-in period. The aged carbon canister shall not be installed during the run-in period.

A carbon canister aged according to the procedure described in paragraphs 5.1. to 5.1.3.1.3. inclusive of this annex shall not be installed until the start of the fuel drain and refill procedure specified in paragraph 6.5.1. of this annex.

4. Test equipment, calibration requirements and intervals

Unless stated otherwise in this paragraph, equipment used for testing shall be calibrated before its initial use and at appropriate service intervals thereafter. An appropriate service interval shall be either equipment manufacturer recommendation or according to good engineering practice.

4.1. Chassis dynamometer

The chassis dynamometer shall meet the requirements of paragraphs 2. to 2.4.2. inclusive of Annex B5.

4.2. Evaporative emission measurement enclosure

The evaporative emission measurement enclosure shall be a gas-tight rectangular measuring chamber able to contain the vehicle under test. The vehicle shall be accessible from all sides and the enclosure when sealed shall be gas-tight in accordance with paragraph 4.2.3.3. of this annex. The inner surface of the enclosure shall be impermeable and non-reactive to hydrocarbons. The temperature conditioning system shall be capable of controlling the internal enclosure air temperature to follow the prescribed temperature versus time profile throughout the test, and an average tolerance of 1 °C over the duration of the test.

The control system shall be tuned to provide a smooth temperature pattern that has a minimum of overshoot, hunting, and instability about the desired long-term ambient temperature profile. Interior surface temperatures shall not be less than 5 °C nor more than 55 °C at any time during the diurnal emission test.

Wall design shall be such as to promote good dissipation of heat. Interior surface temperatures shall not be below 20 °C, nor above 52 °C for the duration of the hot soak rest.

To accommodate the volume changes due to enclosure temperature changes, either a variable-volume or fixed-volume enclosure may be used.

4.2.1. Variable-volume enclosure

The variable-volume enclosure expands and contracts in response to the temperature change of the air mass in the enclosure. Two potential means of accommodating the internal volume changes are movable panel(s), or a bellows design, in which an impermeable bag or bags inside the enclosure expand(s) and contracts(s) in response to internal pressure changes by exchanging air from outside the enclosure. Any design for volume accommodation shall maintain the integrity of the enclosure as specified in paragraph 4.2.3. of this annex over the specified temperature range.

Any method of volume accommodation shall limit the differential between the enclosure internal pressure and the barometric pressure to a maximum value of ±0.5 kPa.

The enclosure shall be capable of latching to a fixed volume. A variable volume enclosure shall be capable of accommodating a +7 per cent change from its "nominal volume" (see paragraph 4.2.3.1.1. of this annex), taking into account temperature and barometric pressure variation during testing.

4.2.2. Fixed-volume enclosure

The fixed-volume enclosure shall be constructed with rigid panels that maintain a fixed enclosure volume, and meet the requirements below.

4.2.2.1. The enclosure shall be equipped with an outlet flow stream that withdraws air at a low, constant rate from the enclosure throughout the test. An inlet flow stream may provide make-up air to balance the outgoing flow with incoming ambient air. Inlet air shall be filtered with activated carbon to provide a relatively constant hydrocarbon level. Any method of volume accommodation shall maintain the differential between the enclosure internal pressure and the barometric pressure between 0 and -0.5 kPa.

4.2.2.2. The equipment shall be capable of measuring the mass of hydrocarbon in the inlet and outlet flow streams with a resolution of 0.01 gram. A bag sampling system may be used to collect a proportional sample of the air withdrawn from and admitted to the enclosure. Alternatively, the inlet and outlet flow streams may be continuously analysed using an on-line FID analyser and integrated with the flow measurements to provide a continuous record of the mass hydrocarbon removal.

4.2.3. Calibration of the enclosure

4.2.3.1. Initial determination of internal volume of the enclosure

4.2.3.1.1. Before its initial use, the internal volume of the chamber shall be determined as follows:

The internal dimensions of the chamber are carefully measured, allowing for any irregularities such as bracing struts. The internal volume of the chamber is determined from these measurements.

For variable-volume enclosures, the enclosure shall be latched to a fixed volume when the enclosure is held at an ambient temperature of 30 °C or at the choice of the manufacturer 29 °C. This nominal volume shall be repeatable within ±0.5 per cent of the reported value.

4.2.3.1.2. The net internal volume is determined by subtracting 1.42 m3 from the internal volume of the chamber. Alternatively the volume of the test vehicle with the luggage compartment and windows open may be used instead of the 1.42 m3.

4.2.3.1.3. The chamber shall be checked as in paragraph 4.2.3.3. of this annex. If the propane mass does not correspond to the injected mass to within ±2 per cent, then corrective action is required.

4.2.3.2. Determination of chamber background emissions

This operation determines that the chamber does not contain any materials that emit significant amounts of hydrocarbons. The check shall be carried out at the enclosure's introduction to service, after any operations in the enclosure which may affect background emissions and at a frequency of at least once per year.

4.2.3.2.1. Variable-volume enclosures may be operated in either latched or unlatched volume configuration, as described in paragraph 4.2.3.1.1. of this annex, ambient temperatures shall be maintained at 35 °C ± 2 °C, or at the choice of the manufacturer 36 °C ± 2 °C, throughout the 4-hour period mentioned below.

4.2.3.2.2. Fixed volume enclosures shall be operated with the inlet and outlet flow streams closed. Ambient temperatures shall be maintained at 35 °C ± 2 °C, or at the choice of the manufacturer 36 °C ± 2 °C, throughout the 4-hour period mentioned below.

4.2.3.2.3. The enclosure may be sealed and the mixing fan operated for a period of up to 12 hours before the 4-hour background sampling period begins.

4.2.3.2.4. The analyser (if required) shall be calibrated, then zeroed and spanned.

4.2.3.2.5. The enclosure shall be purged until a stable hydrocarbon reading is obtained, and the mixing fan turned on if not already on.

4.2.3.2.6. The chamber is then sealed and the background hydrocarbon concentration, temperature and barometric pressure are measured. These are the initial readings CHCi, Pi, Ti used in the enclosure background calculation.

4.2.3.2.7. The enclosure is allowed to stand undisturbed with the mixing fan on for a period of four hours.

4.2.3.2.8. At the end of this time the same analyser is used to measure the hydrocarbon concentration in the chamber. The temperature and the barometric pressure are also measured. These are the final readings CHCf, Pf, Tf.

4.2.3.2.9. The change in mass of hydrocarbons in the enclosure shall be calculated over the time of the test in accordance with paragraph 4.2.3.4. of this annex and shall not exceed 0.05 g.

4.2.3.3. Calibration and hydrocarbon retention test of the chamber

The calibration and hydrocarbon retention test in the chamber provides a check on the calculated volume in paragraph 4.2.3.1. of this annex and also measures any leak rate. The enclosure leak rate shall be determined at the enclosure's introduction to service, after any operations in the enclosure which may affect the integrity of the enclosure, and at least monthly thereafter. If six consecutive monthly retention checks are successfully completed without corrective action, the enclosure leak rate may be determined quarterly thereafter as long as no corrective action is required.

4.2.3.3.1. The enclosure shall be purged until a stable hydrocarbon concentration is reached. The mixing fan is turned on, if not already switched on. The hydrocarbon analyser is zeroed, calibrated if required, and spanned.

4.2.3.3.2. On variable-volume enclosures, the enclosure shall be latched to the nominal volume position. On fixed-volume enclosures the outlet and inlet flow streams shall be closed.

4.2.3.3.3. The ambient temperature control system is then turned on (if not already on) and adjusted for an initial temperature of 35 °C, or at the choice of the manufacturer 36 °C.

4.2.3.3.4. When the enclosure stabilises at 35 °C ± 2 °C, or at the choice of the manufacturer 36 °C ± 2 °C, the enclosure is sealed and the background concentration, temperature and barometric pressure measured. These are the initial readings CHCi, Pi, Ti used in the enclosure calibration.

4.2.3.3.5. A quantity of approximately 4 grams of propane is injected into the enclosure. The mass of propane shall be measured to an accuracy and precision of ±2 per cent of the measured value.

4.2.3.3.6. The contents of the chamber shall be allowed to mix for five minutes and then the hydrocarbon concentration, temperature and barometric pressure are measured. These are the readings CHCf, Pf, Tf for the calibration of the enclosure as well as the initial readings CHCi, Pi, Ti for the retention check.

4.2.3.3.7. Based on the readings taken according to paragraph 4.2.3.3.4. and 4.2.3.3.6. of this annex and the formula in paragraph 4.2.3.4. of this annex, the mass of propane in the enclosure is calculated. This shall be within ±2 per cent of the mass of propane measured in paragraph 4.2.3.3.5. of this annex.

4.2.3.3.8. For variable-volume enclosures the enclosure shall be unlatched from the nominal volume configuration. For fixed-volume enclosures, the outlet and inlet flow streams shall be opened.

4.2.3.3.9. The process is then begun of cycling the ambient temperature from 35 °C to 20 °C and back to 35 °C, or at the choice of the manufacturer 35.6 °C to 22.2 °C and back to 35.6 °C, over a 24-hour period according to the profile, or the alternative profile, specified in paragraph 6.5.9. of this annex within 15 minutes of sealing the enclosure. (Tolerances as specified in paragraph 6.5.9.1. of this annex.)

4.2.3.3.10. At the completion of the 24-hour cycling period, the final hydrocarbon concentration, temperature and barometric pressure are measured and recorded. These are the final readings CHCf, Pf, Tf for the hydrocarbon retention check.

4.2.3.3.11. Using the formula in paragraph 4.2.3.4. of this annex, the hydrocarbon mass is then calculated from the readings taken in paragraphs 4.2.3.3.6. and 4.2.3.3.10. of this annex. The mass may not differ by more than 3 per cent from the hydrocarbon mass given in paragraph 4.2.3.3.7. of this annex.

4.2.3.4. Calculations

The calculation of net hydrocarbon mass change within the enclosure is used to determine the chamber's hydrocarbon background and leak rate. Initial and final readings of hydrocarbon concentration, temperature and barometric pressure are used to calculate the mass change.

The calculation shall be undertaken in accordance with the equation in either paragraph 7.1. or alternatively paragraph 7.1.1. of this annex, using the following value for V.

V is the net enclosure volume, m3.

4.3. Analytical systems

The analytical systems shall meet the requirements of paragraphs 4.3.1. to. 4.3.3. of this annex.

Continuous measuring of hydrocarbons is not mandatory unless the fixed volume type enclosure is used.

4.3.1. Hydrocarbon analyser

4.3.1.1. The atmosphere within the chamber is monitored using a hydrocarbon detector of the FID type. Sample gas shall be drawn from the mid-point of one side wall or roof of the chamber and any bypass flow shall be returned to the enclosure, preferably to a point immediately downstream of the mixing fan.

4.3.1.2. The hydrocarbon analyser shall have a response time to 90 per cent of final reading of less than 1.5 seconds. Its stability shall be better than 2 per cent of full scale at zero and at 80 ± 20 per cent of full scale over a 15-minute period for all operational ranges.

4.3.1.3. The repeatability of the analyser expressed as one standard deviation shall be better than ±1 per cent of full scale deflection at zero and at 80 ± 20 per cent of full scale on all ranges used.

4.3.1.4. The operational ranges of the analyser shall be chosen to give best resolution over the measurement, calibration and leak checking procedures.

4.3.2. Hydrocarbon analyser data recording system

4.3.2.1. The hydrocarbon analyser shall be fitted with a device to record electrical signal output either by strip chart recorder or other data processing system at a frequency of at least once per minute. The recording system shall have operating characteristics at least equivalent to the signal being recorded and shall provide a permanent record of results. The record shall show a positive indication of the beginning and end of the hot soak or diurnal emission test (including beginning and end of sampling periods along with the time elapsed between start and completion of each test).

4.3.3. Checking of FID hydrocarbon analyser

4.3.3.1. Detector response optimisation

The FID shall be adjusted as specified by the instrument manufacturer. Propane in air should be used to optimise the response on the most common operating range.

4.3.3.2. Calibration of the hydrocarbon analyser

The analyser should be calibrated using propane in air and purified synthetic air. See paragraph 6.2. of Annex B5 of this Regulation.

Each of the normally used operating ranges are calibrated in accordance with paragraphs 4.3.3.2.1. to 4.3.3.2.4. of this annex.

4.3.3.2.1. Establish the calibration curve by at least five calibration points spaced as evenly as possible over the operating range. The nominal concentration of the calibration gas with the highest concentrations to be at least 80 per cent of the full scale.

4.3.3.2.2. Calculate the calibration curve by the method of least squares. If the resulting polynomial degree is greater than 3, then the number of calibration points shall be at least the number of the polynomial degree plus 2.

4.3.3.2.3. The calibration curve shall not differ by more than 2 per cent from the nominal value of each calibration gas.

4.3.3.2.4. Using the coefficients of the polynomial derived from paragraph 5 of Annex B5, a table of indicated reading against true concentration shall be drawn up in steps of no greater than 1 per cent of full scale. This is to be carried out for each analyser range calibrated. The table shall also contain other relevant data such as:

(a) Date of calibration, span and zero potentiometer readings (where applicable);

(b) Nominal scale;

(c) Reference data of each calibration gas used;

(d) The actual and indicated value of each calibration gas used together with the percentage differences;

(e) FID fuel and type;

(f) FID air pressure.

4.3.3.2.5. If it can be shown to the satisfaction of the responsible authority that alternative technology (e.g. computer, electronically controlled range switch) can give equivalent accuracy, then those alternatives may be used.

4.4. Temperature recording system

The temperature recording system shall meet the requirements of paragraphs 4.4.1. to 4.4.5. of this annex.

4.4.1. The temperature in the chamber is recorded at two points by temperature sensors which are connected so as to show a mean value. The measuring points are extended approximately 0.1 m into the enclosure from the vertical centre line of each side wall at a height of 0.9 ± 0.2 m.

4.4.2. The temperatures of the fuel tank(s) are recorded by means of the sensor positioned in the fuel tank as in paragraph 6.1.1. of this annex in the case of use of the gasoline canister load option (paragraph 6.5.5.3. of this annex).

4.4.3. Temperatures shall, throughout the evaporative emission measurements, be recorded or entered into a data processing system at a frequency of at least once per minute.

4.4.4. The accuracy of the temperature recording system shall be within ±1.0 K and the temperature shall be capable of being resolved to ±0.4 K.

4.4.5. The recording or data processing system shall be capable of resolving time to ±15 seconds.

4.5. Pressure recording system

The pressure recording system shall meet the requirements of paragraphs 4.5.1. to 4.5.3.

4.5.1. The difference Δp between barometric pressure within the test area and the enclosure internal pressure shall, throughout the evaporative emission measurements, be recorded or entered into a data processing system at a frequency of at least once per minute.

4.5.2. The accuracy of the pressure recording system shall be within ±0.3 kPa and the pressure shall be capable of being resolved to ±0.025 kPa.

4.5.3. The recording or data processing system shall be capable of resolving time to ±15 seconds.

4.6. Fans

The fans shall meet the requirements of paragraphs 4.6.1. and 4.6.2. of this annex.

4.6.1. By the use of one or more fans or blowers with the Sealed Housing Evaporative Determination (SHED) door(s) open, it shall be possible to reduce the hydrocarbons concentration in the chamber to the ambient hydrocarbon level.

4.6.2. The chamber shall have one or more fans or blowers of like capacity 0.1 to 0.5 m3/sec. with which to thoroughly mix the atmosphere in the enclosure. It shall be possible to attain an even temperature and hydrocarbon concentration in the chamber during measurements. The vehicle in the enclosure shall not be subjected to a direct stream of air from the fans or blowers.

4.7. Calibration gases

The gases shall meet the requirements of paragraphs 4.7.1. and 4.7.2. of this annex.

4.7.1. The following pure gases shall be available for calibration and operation:

Purified synthetic air: (purity < 1 ppm C1 equivalent,

≤1 ppm CO, ≤ 400 ppm CO2, ≤ 0.1 ppm NO;

oxygen content between 18 and 21 per cent by volume).

Hydrocarbon analyser fuel gas: defined in paragraph 6.1.2.4. of Annex B5 to this Regulation or (40 ± 2 per cent hydrogen, and balance helium with less than 1 ppm C1 equivalent hydrocarbon, less than 400 ppm CO2),

Propane (C3H8): 99.5 per cent minimum purity.

Butane (C4H10): 98 per cent minimum purity.

Nitrogen (N2): defined in paragraph 6.1.2.1. of Annex B5 to this Regulation or 98 per cent minimum purity.

4.7.2. Calibration and span gases shall be available containing mixtures of propane (C3H8) and purified synthetic air. The true concentrations of a calibration gas shall be within 2 per cent of the stated figures. The accuracy of the diluted gases obtained when using a gas divider shall be to within ±2 per cent of the true value. The concentrations specified in paragraphs 4.2.3. and 4.3.3. of this annex may also be obtained by the use of a gas divider using synthetic air as the dilutant gas.

4.8. Carbon canister weighing scale for depressurisation puff loss overflow measurement

The carbon canister weighing scale shall have an accuracy of ±0.02 g.

4.9. Fuel tank heating (only applicable for gasoline canister load option)

4.9.1. The fuel in the vehicle tank(s) shall be heated by a controllable source of heat; for example a heating pad of 2,000 W capacity is suitable. The heating system shall apply heat evenly to the tank walls beneath the level of the fuel so as not to cause local overheating of the fuel. Heat shall not be applied to the vapour in the tank above the fuel.

4.9.2. The tank heating device shall make it possible to heat the fuel in the tank evenly by 14 °C from 16 °C within 60 minutes, with the temperature sensor position as in paragraph 4.9.3. of this annex. The heating system shall be capable of controlling the fuel temperature to ±1.5 °C of the required temperature during the tank heating process.

4.9.3. The fuel tank of the vehicle shall, without introducing any leaks, be equipped with a temperature sensor to enable the temperature to be measured at the mid-point of the fuel in the fuel tank when filled to 40 per cent of its capacity.

5. Procedure for carbon canister bench ageing and PF determination

5.1. Carbon canister bench ageing

Before performing the hot soak and diurnal losses sequences, the carbon canister shall be aged according to the procedure described in Figure C3/1.

Figure C3/1

**Carbon canister bench ageing procedure**

Test start

Select new carbon canister sample.

5.1.1. Ageing through exposure to

temperature cycling

5.1.2. Ageing through exposure to vibration

5.1.3. Ageing through exposure to fuel vapour and determining BWC300

{

50 times

5.1.1. Ageing through exposure to temperature cycling


The carbon canister shall be cycled between temperatures from -15 °C to 60 °C in a dedicated temperature enclosure with 30 minutes of stabilisation at -15 °C and 60 °C. Each cycle shall last 210 minutes (see Figure C3/2).

The temperature gradient shall be as close as possible to 1 °C/min. No forced air flow should pass through the carbon canister.

The cycle shall be repeated 50 times consecutively. In total, this procedure lasts 175 hours.

Figure C3/2

**Temperature conditioning cycle**



5.1.2. Ageing through exposure to vibration

Following the temperature ageing procedure, the carbon canister shall be shaken vertically with the carbon canister mounted as per its orientation in the vehicle with an overall Grms (root mean square acceleration) > 1.5 m/sec2 with a frequency of 30 ±10 Hz. The test shall last 12 hours.

5.1.3. Ageing through exposure to fuel vapour and determining BWC300

5.1.3.1. Ageing shall consist of repeatedly loading with fuel vapour and purging with laboratory air.

5.1.3.1.1. After temperature and vibration ageing, the carbon canister shall be further aged with a mixture of market fuel as specified in paragraph 5.1.3.1.1.1. of this annex and nitrogen or air with a 50 ±15 per cent fuel vapour volume. The fuel vapour fill rate shall be 60 ±20 g/h.

The carbon canister shall be loaded to 2 gram breakthrough. Alternatively, loading shall be considered to be completed when the hydrocarbon concentration level at the vent outlet reaches 3,000 ppm.

5.1.3.1.1.1. The market fuel used for this test shall fulfil the same requirements as a reference fuel with respect to:

(a) Density at 15 °C;

(b) Vapour pressure;

(c) Distillation (70 °C, 100 °C, 150 °C);

(d) Hydrocarbon analysis (olefins, aromatics, benzene only);

(e) Oxygen content;

(f) Ethanol content.

5.1.3.1.2. The carbon canister shall be purged between 5 and 60 minutes after loading with 25 ±5 litres per minute of emission laboratory air until 300 bed volume exchanges are reached.

5.1.3.1.3. The procedures set out in paragraphs 5.1.3.1.1. and 5.1.3.1.2. of this annex shall be repeated 300 times after which the carbon canister shall be considered to be stabilised.

5.1.3.1.4. The procedure to measure the butane working capacity (BWC) with respect to the evaporative emission family in paragraph 6.6.3. of this Regulation shall consist of the following.

(a) The stabilised carbon canister shall be loaded to 2 gram breakthrough and subsequently purged a minimum of 5 times. Loading shall be performed with a mixture composed of 50 per cent butane and 50 per cent nitrogen by volume at a rate of 40 grams butane per hour.

(b) Purging shall be performed according to paragraph 5.1.3.1.2. of this annex.

(c) The BWC shall be recorded after each loading.

(d) BWC300 shall be calculated as the average of the last 5 BWCs.

5.1.3.2. If the aged carbon canister is provided by a supplier, the vehicle manufacturer shall inform the responsible authority in advance of the ageing process to enable the witnessing of any part of that process.

5.1.3.3. The manufacturer shall provide the responsible authority a test report including at least the following elements:

(a) Type of activated carbon;

(b) Loading rate;

(c) Fuel specifications.

5.2. Determination of the PF of the fuel tank system (see Figure C3/3)

Figure C3/3

**Determination of PF**

Test start

5.2.1. Fill the tank to 40 ±2 per cent of its nominal capacity with reference fuel

5.2.1. Soak for 3 weeks at 40 °C ±2 °C

5.2.2. Measurement of HC in the same conditions as for the 1st day of diurnal emission test:

HC3w

5.2.3. Soak for the remaining 17 weeks at 40 °C ±2 °C

5.2.4. Measurement of HC in the same conditions as for the 1st day of diurnal emission test:

HC20w

5.2.5. Permeability Factor = HC20w - HC3w

5.2.2. Drain and fill the tank to 40 per cent of its nominal capacity with reference fuel

5.2.4. Drain and fill the tank to 40 per cent of its nominal capacity with reference fuel

5.2.1. The fuel tank system representative of a family shall be selected and mounted on a rig in a similar orientation as in the vehicle. The tank shall be filled to 40 ±2 per cent of its nominal capacity with reference fuel at a temperature of 18 °C ±2 °C. The rig with the fuel tank system shall be placed in a room with a controlled temperature of 40 °C ±2 °C for 3 weeks.

5.2.2. At the end of the third week, the tank shall be drained and refilled with reference fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of its nominal capacity.

Within 6 to 36 hours, the rig with the fuel tank system shall be placed in an enclosure. The last 6 hours of this period shall be at an ambient temperature of 20 °C ±2 °C. In the enclosure, a diurnal procedure shall be performed over the first 24-hour period of the procedure described in paragraph 6.5.9. of this annex. The fuel vapour in the tank shall be vented to the outside of the enclosure to eliminate the possibility of the tank venting emissions being counted as permeation. The HC emissions shall be measured and the value shall be recorded as HC3W.

5.2.3. The rig with the fuel tank system shall be placed again in a room with a controlled temperature of 40 °C ±2 °C for the remaining 17 weeks.

5.2.4. At the end of the seventeenth week, the tank shall be drained and refilled with reference fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of its nominal tank capacity.

Within 6 to 36 hours, the rig with the fuel tank system shall be placed in an enclosure. The last 6 hours of this period shall be at an ambient temperature of 20 °C ±2 °C. In the enclosure, a diurnal procedure shall be performed over a first period of 24 hours of the procedure described according to paragraph 6.5.9. of this annex. The fuel tank system shall be vented to the outside of the enclosure to eliminate the possibility of the tank venting emissions being counted as permeation. The HC emissions shall be measured and the value shall be recorded in this case as HC20W.

5.2.5. The PF is the difference between HC20W and HC3W in g/24h calculated to 3 significant digits using the following equation:

5.2.6. If the PF is determined by a supplier, the vehicle manufacturer shall inform the responsible authority in advance of the determination to allow witness check in the supplier’s facility.

5.2.7. The manufacturer shall provide the responsible authority with a test report containing at least the following:

(a) A full description of the fuel tank system tested, including information on the type of tank tested, whether the tank is metal, monolayer non-metal or multilayer, and which types of materials are used for the tank and other parts of the fuel tank system;

(b) The weekly mean temperatures at which the ageing was performed;

(c) The HC measured at week 3 (HC3W);

(d) The HC measured at week 20 (HC20W);

(e) The resulting permeability factor (PF).

5.2.8. As an alternative to paragraphs 5.2.1. to 5.2.7. inclusive of this annex, a manufacturer using multilayer tanks or metal tanks may choose to use an Assigned Permeability Factor (APF) instead of performing the complete measurement procedure mentioned above:

APF multilayer/metal tank = 120 mg /24 h

Where the manufacturer chooses to use an APF, the manufacturer shall provide the responsible authority with a declaration in which the type of tank is clearly specified as well as a declaration of the type of materials used.

6. Test procedure for the measurement of hot soak and diurnal losses

6.1. Vehicle preparation

The vehicle shall be prepared in accordance with paragraphs 6.1.1. and 6.1.2. of this annex. At the request of the manufacturer and with approval of the responsible authority, non-fuel background emission sources (e.g. paint, adhesives, plastics, fuel/vapour lines, tyres, and other rubber or polymer components) may be reduced to typical vehicle background levels before testing (e.g. baking of tyres at temperatures of 50 °C or higher for appropriate periods, baking of the vehicle, draining washer fluid).

For a sealed fuel tank system, the vehicle carbon canisters shall be installed so that access to carbon canisters and connection/disconnection of carbon canisters can be done easily.

6.1.1. The vehicle shall be mechanically prepared before the test as follows:

(a) The exhaust system of the vehicle shall not exhibit any leaks. Openings in the exhaust system designed to remove condensate as described in paragraph 2.4.3. of Annex B6 shall be sealed prior to the test;

(b) The vehicle may be steam-cleaned before the test;

(c) In the case of use of the gasoline canister load option (paragraph 6.5.5.3. of this annex) the fuel tank of the vehicle shall be equipped with a temperature sensor to enable the temperature to be measured at the mid-point of the fuel in the fuel tank when filled to 40 per cent of its capacity;

(d) Additional fittings, adapters of devices may be fitted to the fuel system in order to allow a complete draining of the fuel tank. For this purpose it is not necessary to modify the shell of the tank;

(e) The manufacturer may propose a test method in order to take into account the loss of hydrocarbons by evaporation coming only from the fuel system of the vehicle.

6.1.2. The vehicle is taken into the test area where the ambient temperature is between 20 and 30 °C.

6.2. Mode selections and gear shift prescriptions

6.2.1. For vehicles with manual shift transmissions, the gear shift prescriptions specified in Annex B2 shall apply.

6.2.2. In the case of pure ICE vehicles, the mode shall be selected according to Annex B6.

6.2.3. In the case of NOVC-HEVs and OVC-HEVs, the mode shall be selected according to Appendix 6 to Annex B8.

6.2.4. Upon request of the responsible authority, the selected mode may be different from that described in paragraphs 6.2.2. and 6.2.3. of this annex.

6.3. Test conditions

The tests included in this annex shall be performed using the test conditions specific to interpolation family vehicle H with the highest cycle energy demand of all the interpolation families included in the evaporative emission family being considered.

Otherwise, at the request of the responsible authority, any cycle energy representative of a vehicle in the family may be used for the test.

6.4. Flow of the test procedure

The test procedure for non-sealed and sealed tank systems shall be followed according to the flow chart described in Figure C3/4.

The sealed fuel tank systems shall be tested with one of 2 options. One option is to test the vehicle with one continuous procedure. Another option, called the 'stand-alone test procedure', is to test the vehicle with two separate procedures which will allow repeating the dynamometer test and the diurnal tests without repeating the tank depressurisation puff loss overflow test and the depressurisation puff loss measurement.

Figure C3/4

**Test procedure flow charts**

**Start for: Non-sealed fuel tanks, sealed fuel tanks continuous and sealed fuel tanks stand-alone puff loss**

6.5.1. Fuel drain and refill to 40 %

6.5.2. Soak for 6 to 36 hours @ 23 °C

6.5.3. Preconditioning drive

**Start for: Sealed fuel tanks, stand-alone hot soak and diurnals**

6 to 36 hours

6.6.1.4. Fuel tank pressure relief

6.5.6. Dynamometer test

Start hot soak test within 7 minutes after dynamometer test and 2 minutes after engine being switched off

6.5.7. Hot soak test: MHS

6.5.8. Soak for 6 to 36 hours @ 20 °C

6.5.9. 1st day diurnal: MD1

6.5.9. 2nd day diurnal: MD2

7. Calculations

**End**

6.6.1.2. Fuel drain and refill to 15 %

6.5.5. Soak for 12 to 36 hours @ 23 °C

6.6.1.5. Load aged canister to 2 g breakthrough

6.6.1.5. Canister purge 85 % fuel consumption equivalent

6.6.1.6. Preparation of canister depressurisation puff loss loading   
(11-hour temperature cycle)

6.6.1.7.2. Puff loss loading

6.6.1.8. Measurement of puff loss overflow

**End of stand-alone puff loss test**

6.6.1.9. Soak for 6 to 36 hours @ 23 °C

6.6.1.9.1. Charge OVC-HEV REESS

6.6.1.10. Fuel drain and refill to 40 %

6.6.1.11. Soak for 6 to 36 hours @ 20 °C

6.6.1.12. Fuel tank depressurisation with canister disconnected

6.5.1. Fuel drain and refill to 40 %

6.5.2. Soak for 6 to 36 hours @ 23 °C

6.5.3. Preconditioning drive

6.6.1.9. Soak for 6 to 36 hours @ 23 °C

6.6.1.9.1. Charge OVC-HEV REESS

6.6.1.5. Load aged canister to 2 g breakthrough

6.6.1.5. Canister purge 85 % fuel consumption equivalent

6.7.2.1.3. Canister loading with puff loss simulated mass

6.5.4. Fuel drain and refill to 40 %

Start next fuel drain and refill within 1 hour

Start next soak within 5 minutes

Start next fuel drain and refill within 1 hour

Start next soak within 5 minutes

Start next soak within 5 minutes

Start puff loss loading within 15 minutes

Start next soak within 5 minutes

Yes

No

Sealed fuel tank system?

6.5.5.1. Charge OVC-HEV REESS

6.5.5.2. Load aged canister to 2 g breakthrough

6.6.1.3. Soak for 6 to 36 hours @ 20°C

6.5. Continuous test procedure for non-sealed fuel tank systems

6.5.1. Fuel drain and refill

The fuel tank of the vehicle shall be emptied. This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this. The fuel tank shall be refilled with reference fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of its nominal capacity.

6.5.2. Soak

Within 5 minutes after completing the fuel drain and refill, the vehicle shall be soaked for a minimum of 6 hours and a maximum of 36 hours at 23 °C ±3 °C.

6.5.3. Preconditioning drive

The vehicle shall be placed on a chassis dynamometer and driven over the following phases of the cycle described in Annex B1:

(a) For Class 1 vehicles:  
low, medium, low, low, medium, low

(b) For Class 2 and 3 vehicles: low, medium, high, medium.

For OVC-HEVs, the preconditioning drive shall be performed under the charge-sustaining operating condition as defined in paragraph 3.3.6. of this Regulation. Upon the request of responsible authority, any other mode may be used.

6.5.4. Fuel drain and refill

Within one hour after the preconditioning drive, the fuel tank of the vehicle shall be emptied. This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this. The fuel tank shall be refilled with test fuel at a temperature of 18 °C ±2 °C to 40 ±2 per cent of its nominal capacity.

6.5.5. Soak

Within five minutes of completing fuel drain and refill, the vehicle shall be parked for a minimum of 12 hours and a maximum of 36 hours at 23 °C ±3 °C.

During soaking, the procedures described in paragraphs 6.5.5.1. and 6.5.5.2. of this annex.may be performed either in the order of first paragraph 6.5.5.1. followed by paragraph 6.5.5.2. or in the order paragraph 6.5.5.2. followed by paragraph 6.5.5.1. The procedures described in paragraphs 6.5.5.1. and 6.5.5.2. may also be performed simultaneously.

6.5.5.1. REESS charge

For OVC-HEVs, the REESS shall be fully charged according to the charging requirements described in paragraph 2.2.3. of Appendix 4 to Annex B8.

6.5.5.2. Carbon canister loading

The carbon canister aged according to the sequence described in paragraph 5.1. to 5.1.3.1.3. inclusive of this annex shall be loaded to 2 gram breakthrough according to the procedure described in paragraph 6.5.5.2.1. of this annex.

One of the methods specified in paragraphs 6.5.5.3. and 6.5.5.4. of this annex shall be used to precondition the evaporative canister. For vehicles with multiple canisters, each canister shall be preconditioned separately.

6.5.5.2.1. Canister emissions are measured to determine breakthrough.

Breakthrough is here defined as the point at which the cumulative quantity of hydrocarbons emitted is equal to 2 grams.

6.5.5.2.2. Breakthrough may be verified using the evaporative emission enclosure as described in paragraphs 6.5.5.3. and 6.5.5.4. of this annex. Alternatively, breakthrough may be determined using an auxiliary evaporative canister connected downstream of the vehicle's canister. The auxiliary canister shall be well purged with dry air prior to loading.

6.5.5.2.3. The measuring chamber shall be purged for several minutes immediately before the test until a stable background is obtained. The chamber air mixing fan(s) shall be switched on at this time.

The hydrocarbon analyser shall be zeroed and spanned immediately before the test.

6.5.5.3. Canister loading with repeated heat builds to breakthrough

6.5.5.3.1. The fuel tank(s) of the vehicle(s) is (are) emptied using the fuel tank drain(s). This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this.

6.5.5.3.2. The fuel tank(s) is (are) refilled with test fuel at a temperature of between 10 to 14 °C to 40 ± 2 per cent of the tank's normal volumetric capacity. The fuel cap(s) of the vehicle shall be fitted at this point.

6.5.5.3.3. Within one hour of being refuelled the vehicle shall be placed, with the engine shut off, in the evaporative emission enclosure. The fuel tank temperature sensor is connected to the temperature recording system. A heat source shall be properly positioned with respect to the fuel tank(s) and connected to the temperature controller. The heat source is specified in paragraph 4.9. of this annex. In the case of vehicles fitted with more than one fuel tank, all the tanks shall be heated in the same way as described below. The temperatures of the tanks shall be identical to within ±1.5 °C.

6.5.5.3.4. The fuel may be artificially heated to the starting diurnal temperature of 20 °C ± 1 °C.

6.5.5.3.5. When the fuel temperature reaches at least 19 °C, the following steps shall be taken immediately: the purge blower shall be turned off; enclosure doors closed and sealed; and measurement initiated of the hydrocarbon level in the enclosure.

6.5.5.3.6. When the fuel temperature of the fuel tank reaches 20 °C a linear heat build of 15 °C begins. The fuel shall be heated in such a way that the temperature of the fuel during the heating conforms to the function below to within ±1.5 °C. The elapsed time of the heat build and temperature rise is recorded.

Tr = To + 0.2333 x t

|  |  |  |
| --- | --- | --- |
| Where: |  |  |
| Tr | = | required temperature (K), |
| To | = | initial temperature (K), |
| t | = | time from start of the tank heat build in minutes. |

6.5.5.3.7. As soon as break-through occurs or when the fuel temperature reaches 35 °C, whichever occurs first, the heat source is turned off, the enclosure doors unsealed and opened, and the vehicle fuel tank cap(s) removed. If break-through has not occurred by the time the fuel temperature 35 °C, the heat source is removed from the vehicle, the vehicle removed from the evaporative emission enclosure and the entire procedure outlined in paragraph 6.6.1.2. of this annex repeated until break-through occurs.

6.5.5.4. Butane loading to breakthrough

6.5.5.4.1. If the enclosure is used for the determination of the break-through (see paragraph 6.5.5.2.2. of this annex) the vehicle shall be placed, with the engine shut off, in the evaporative emission enclosure.

6.5.5.4.2. The evaporative emission canister shall be prepared for the canister loading operation. The canister shall not be removed from the vehicle, unless access to it in its normal location is so restricted that loading can only reasonably be accomplished by removing the canister from the vehicle. Special care shall be taken during this step to avoid damage to the components and the integrity of the fuel system.

6.5.5.4.3. The canister is loaded with a mixture composed of 50 per cent butane and 50 per cent nitrogen by volume at a rate of 40 grams butane per hour.

6.5.5.4.4. As soon as the canister reaches breakthrough, the vapour source shall be shut off.

6.5.5.4.5. The evaporative emission canister shall then be reconnected and the vehicle restored to its normal operating condition.

6.5.6. Dynamometer test

The test vehicle shall be pushed onto a dynamometer and shall be driven over the cycles described in paragraph 6.5.3.(a) or paragraph 6.5.3.(b) of this annex. OVC-HEVs shall be operated in charge-depleting operating condition. The engine shall be subsequently shut off. Exhaust emissions may be sampled during this operation and the results may be used for the purpose of exhaust emission and fuel consumption type approval if this operation meets the requirement described in Annex B6 or Annex B8.

6.5.7. Hot soak evaporative emissions test

Within 7 minutes after the dynamometer test and within 2 minutes of the engine being switched off, the hot soak evaporative emissions test shall be performed in accordance with paragraphs 6.5.7.1. to 6.5.7.8. of this annex. The hot soak losses shall be calculated according to paragraph 7.1. of this annex and recorded as MHS.

6.5.7.1. Before the completion of the test run the measuring chamber shall be purged for several minutes until a stable hydrocarbon background is obtained. The enclosure mixing fan(s) shall also be turned on at this time.

6.5.7.2. The hydrocarbon analyser shall be zeroed and spanned immediately prior to the test.

6.5.7.3. At the end of the driving cycle the engine bonnet shall be completely closed and all connections between the vehicle and the test stand disconnected. The vehicle is then driven to the measuring chamber with a minimum use of the accelerator pedal. The engine shall be turned off before any part of the vehicle enters the measuring chamber. The time at which the engine is switched off is recorded on the evaporative emission measurement data recording system and temperature recording begins. The vehicle's windows and luggage compartments shall be opened at this stage, if not already opened.

6.5.7.4. The vehicle shall be pushed or otherwise moved into the measuring chamber with the engine switched off.

6.5.7.5. The enclosure doors are closed and sealed gas-tight within two minutes of the engine being switched off and within seven minutes of the end of the conditioning drive.

6.5.7.6. The start of a 60 ± 0.5 minute hot soak period begins when the chamber is sealed. The hydrocarbon concentration, temperature and barometric pressure are measured to give the initial readings CHCi, Pi and Ti for the hot soak test. These figures are used in the evaporative emission calculation, paragraph 6. The ambient temperature T of the enclosure shall not be less than 23 °C and no more than 31 °C during the 60-minute hot soak period.

6.5.7.7. The hydrocarbon analyser shall be zeroed and spanned immediately before the end of the 60 ± 0.5 minute test period.

6.5.7.8. At the end of the 60 ± 0.5 minute test period, the hydrocarbon concentration in the chamber shall be measured. The temperature and the barometric pressure are also measured. These are the final readings CHCf, Pf and Tf for the hot soak test used for the calculation in paragraph 6. of this annex.

6.5.8. Soak

After the hot soak evaporative emissions test, the test vehicle shall be soaked for not less than 6 hours and not more than 36 hours between the end of the hot soak test and the start of the diurnal emission test. For at least the last 6 hours of this period the vehicle shall be soaked at 20 °C ±2 °C.

6.5.9. Diurnal testing

6.5.9.1. The test vehicle shall be exposed to two cycles of ambient temperature in accordance with the profile specified in Table C3/1 with a maximum deviation of ±2 °C at any time. The average temperature deviation from the profile, calculated using the absolute value of each measured deviation, shall not exceed ±1 °C. Ambient temperature shall be measured and recorded at least every minute. Temperature cycling shall begin at time Tstart = 0, as specified in paragraph 6.5.9.6. of this annex.

Table C3/1

**Diurnal ambient temperature profiles**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Diurnal ambient temperature profile for the calibration  of the enclosure and the diurnal emission test* | | | *Alternative diurnal ambient temperature profile for the calibration of the enclosure* | |
| *Time (hours)* | | *Temperature  (°Ci)* | *Time (hours)* | *Temperature  (°Ci)* |
| *Calibration* | *Test* |
| 13 | 0/24 | 20.0 | 0 | 35.6 |
| 14 | 1 | 20.2 | 1 | 35.3 |
| 15 | 2 | 20.5 | 2 | 34.5 |
| 16 | 3 | 21.2 | 3 | 33.2 |
| 17 | 4 | 23.1 | 4 | 31.4 |
| 18 | 5 | 25.1 | 5 | 29.7 |
| 19 | 6 | 27.2 | 6 | 28.2 |
| 20 | 7 | 29.8 | 7 | 27.2 |
| 21 | 8 | 31.8 | 8 | 26.1 |
| 22 | 9 | 33.3 | 9 | 25.1 |
| 23 | 10 | 34.4 | 10 | 24.3 |
| 24/0 | 11 | 35.0 | 11 | 23.7 |
| 1 | 12 | 34.7 | 12 | 23.3 |
| 2 | 13 | 33.8 | 13 | 22.9 |
| 3 | 14 | 32.0 | 14 | 22.6 |
| 4 | 15 | 30.0 | 15 | 22.2 |
| 5 | 16 | 28.4 | 16 | 22.5 |
| 6 | 17 | 26.9 | 17 | 24.2 |
| 7 | 18 | 25.2 | 18 | 26.8 |
| 8 | 19 | 24.0 | 19 | 29.6 |
| 9 | 20 | 23.0 | 20 | 31.9 |
| 10 | 21 | 22.0 | 21 | 33.9 |
| 11 | 22 | 20.8 | 22 | 35.1 |
| 12 | 23 | 20.2 | 23 | 3.4 |
|  |  |  | 24 | 35.6 |

6.5.9.2. The enclosure shall be purged for several minutes immediately before the test until a stable background is obtained. The chamber mixing fan(s) shall also be switched on at this time.

6.5.9.3. The test vehicle, with the powertrain shut off and the test vehicle windows and luggage compartment(s) opened, shall be moved into the measuring chamber. The mixing fan(s) shall be adjusted in such a way as to maintain a minimum air circulation speed of 8 km/h under the fuel tank of the test vehicle.

6.5.9.4. The hydrocarbon analyser shall be zeroed and spanned immediately before the test.

6.5.9.5. The enclosure doors shall be closed and sealed gas-tight.

6.5.9.6. Within 10 minutes of closing and sealing the doors, the hydrocarbon concentration, temperature and barometric pressure shall be measured to give initial readings of hydrocarbon concentration in the enclosure (CHCi), barometric pressure (Pi) and ambient chamber temperature (Ti) for the diurnal testing. Tstart= 0 starts at this time.

6.5.9.7. The hydrocarbon analyser shall be zeroed and spanned immediately before the end of each emission sampling period.

6.5.9.8. The end of the first and second emission sampling period shall occur at 24 hours ±6 minutes and 48 hours ±6 minutes, respectively, after the beginning of the initial sampling, as specified in paragraph 6.5.9.6. of this annex. The elapsed time shall be recorded.

At the end of each emission sampling period, the hydrocarbon concentration, temperature and barometric pressure shall be measured and used to calculate the diurnal test results using the equation in paragraph 7.1. of this annex. The result obtained from the first 24 hours shall be recorded as MD1. The result obtained from the second 24 hours shall be recorded as MD2.

6.6. Continuous test procedure for sealed fuel tank systems

6.6.1. In the case that the fuel tank relief pressure is greater than or equal to 30 kPa

6.6.1.1. The test shall be performed as described in paragraphs 6.5.1. to 6.5.3. inclusive of this annex.

6.6.1.2. Fuel drain and refill

Within one hour after the preconditioning drive, the fuel tank of the vehicle shall be emptied. This shall be done so as not to abnormally purge or abnormally load the evaporative control devices fitted to the vehicle. Removal of the fuel cap is normally sufficient to achieve this, otherwise the carbon canister shall be disconnected. The fuel tank shall be refilled with reference fuel at a temperature of 18 °C ±2 °C to 15 ±2 per cent of the tank's nominal capacity. The operations described in paragraphs 6.6.1.3., 6.6.1.4. and 6.6.1.5. of this annex shall be completed within a total of 36 hours and for the operations described in paragraphs 6.6.1.4. and 6.6.1.5. the vehicle shall not be exposed to temperatures above 25°C.

6.6.1.3. Soak

Within 5 minutes after completing fuel drain and refill, the vehicle shall be soaked for stabilisation for at least 6 hours at an ambient temperature of 20 °C ±2 °C.

6.6.1.4. Fuel tank depressurisation

The tank pressure shall be subsequently released so as not to abnormally raise the inside pressure of the fuel tank. This may be done by opening the fuel cap of the vehicle. Regardless of the method of depressurisation, the vehicle shall be returned to its original condition within 1 minute.

6.6.1.5. Carbon canister loading and purge

The carbon canister aged in accordance with the sequence described in paragraph 5.1. to 5.1.3.1.3. inclusive of this annex shall be loaded to 2 gram breakthrough according to the procedure described in paragraphs 6.5.5.4. to 6.5.5.4.5. inclusive to this annex, and shall be subsequently purged with 25 ±5 litres per minute with emission laboratory air. The volume of purge air shall not exceed the volume determined in accordance with the requirements of paragraph 6.6.1.5.1. This loading and purging can be done either (a) using an on-board carbon canister at a temperature of 20 °C or optionally 23 °C, or (b) by disconnecting the carbon canister. In both cases, no further relief of the tank pressure is allowed.

6.6.1.5.1. Determination of maximum purge volume

The maximum purge amount shall be determined by the following equation. In the case of OVC-HEVs, the vehicle shall be operated in charge-sustaining operating condition. This determination can also be done at a separate test or during the preconditioning drive.

where:

is the cumulative purge volume rounded to the nearest 0.1 litres measured using a suitable device (e.g. flowmeter connected to the vent of the carbon canister or equivalent) over the cold start preconditioning drive described in the paragraph 6.5.3. of this annex, l;

is the manufacturer’s nominal fuel tank capacity, l;

is the fuel consumption over the single purge cycle described in paragraph 6.5.3. of this annex which may be measured in either warm or cold start condition, l/100 km. For OVC-HEVs and NOVC-HEVs, fuel consumption shall be calculated according to paragraph 4.2.1. of Annex B8 of this Regulation;

is the theoretical distance to the nearest 0.1 km of a single purge cycle described in paragraph 6.5.3. of this annex, km.

6.6.1.6. Preparation of carbon canister depressurisation puff loss loading

After completing carbon canister loading and purging, the test vehicle shall be moved into an enclosure, either a SHED or an appropriate climatic chamber. It shall be demonstrated that the system is leak-free and the pressurisation is performed in a normal way during the test or by a separate test (e.g. by means of pressure sensor on the vehicle). The test vehicle shall be subsequently exposed to the first 11 hours of the ambient temperature profile specified for the diurnal emission test in Table C3/1 with a maximum deviation of ±2 °C at any time. The average temperature deviation from the profile, calculated using the absolute value of each measured deviation, shall not exceed ±1 °C. The ambient temperature shall be measured and recorded at least every 10 minutes.

6.6.1.7. Carbon canister puff loss loading

6.6.1.7.1. Fuel tank depressurisation before refuelling

The manufacturer shall ensure that the refuelling operation cannot be initiated before the sealed fuel tank system is fully depressurised to a pressure less than 2.5 kPa above ambient pressure in normal vehicle operation and use. At the request of the responsible authority, the manufacturer shall provide detailed information or demonstrate proof of operation (e.g. by means of pressure sensor on the vehicle). Any other technical solution may be allowed provided that a safe refuelling operation is ensured and that no excessive emissions are released to the atmosphere before the refuelling device is connected to the vehicle.

6.6.1.7.2. Within 15 minutes after the ambient temperature has reached 35 °C, the tank relief valve shall be opened to load the carbon canister. This loading procedure may be performed either inside or outside an enclosure. The carbon canister loaded according to this paragraph shall be disconnected and shall be kept in the soak area.

6.6.1.8. Measurement of depressurisation puff loss overflow

The depressurisation puff loss overflow shall be measured using the process in either paragraph 6.6.1.8.1. or 6.6.1.8.2. of this annex.

6.6.1.8.1. The depressurisation puff loss overflow from the vehicle carbon canister may be measured by using an additional carbon canister identical to the vehicle's carbon canister but not necessarily aged. The additional carbon canister shall be fully purged with dry air prior to loading and shall be connected directly at the outlet of the vehicle's canister with the shortest possible tube. The additional carbon canister shall be weighed before and after the procedure described in paragraph 6.6.1.7. of this annex.

6.6.1.8.2. The depressurisation puff loss overflow from the vehicle carbon canister during its depressurisation may be measured using a SHED.

Within 15 minutes after the ambient temperature has reached 35°C as described in paragraph 6.6.1.6. of this annex, the chamber shall be sealed and the measurement procedure shall be started.

The hydrocarbon analyser shall be zeroed and spanned, after which the hydrocarbon concentration (CHCi), temperature (Ti)and barometric pressure (Pi) shall be measured to give the initial readings CHCi, Pi and Ti for the sealed tank depressurisation puff loss overflow determination.

The ambient temperature T of the enclosure shall not be less than 25°C during the measurement procedure.

At the end of the procedure described in paragraph 6.6.1.7.2. of this annex, the hydrocarbon concentration (CHCf) in the chamber shall be measured after 300 ± 5 seconds. The temperature (Tf)and the barometric pressure (Pf) shall also be measured. These are the final readings CHCf, Pf and Tf for the sealed tank depressurisation puff loss overflow.

The sealed tank puff loss overflow result shall be calculated according to paragraph 7.1. of this annex and recorded.

6.6.1.8.3. There shall be no change in weight of the additional carbon canister when testing according to paragraph 6.6.1.8.1. or the result of the SHED measurement when testing according to paragraph 6.6.1.8.2., within the tolerance of ± 0.5 gram.

6.6.1.9. Soak

After completing puff loss loading the vehicle carbon canister shall be replaced with a dummy carbon canister (of the same specification as the original but not necessarily aged), the vehicle shall then be soaked at 23°±3 °C for 6 to 36 hours to stabilise the vehicle temperature.

6.6.1.9.1. REESS charge

For OVC-HEVs, the REESS shall be fully charged in accordance with the charging requirements described in paragraph 2.2.3. of Appendix 4 to Annex B8 during the soaking described in paragraph 6.6.1.9. of this annex.

6.6.1.10. Fuel drain and refill

The fuel tank of the vehicle shall be drained and filled up to 40 ±2 per cent of the tank's nominal capacity with reference fuel at a temperature of 18 °C ±2 °C.

6.6.1.11. Soak

The vehicle shall be subsequently parked for a minimum of 6 hours to a maximum of 36 hours in the soak area at 20 °C ±2 °C to stabilise the fuel temperature.

6.6.1.12. Fuel tank depressurisation

The tank pressure shall be subsequently released so as not to abnormally raise the inside pressure of the fuel tank. This may be done by opening the fuel cap of the vehicle. Regardless of the method of depressurisation, the vehicle shall be returned to its original condition within 1 minute. After this action, the vehicle carbon canister shall be connected again.

6.6.1.13. The procedures in paragraphs 6.5.6. to 6.5.9.8. inclusive of this annex shall be followed.

6.6.2. In the case that the fuel tank relief pressure is lower than 30 kPa

The test shall be performed as described in paragraphs 6.6.1.1. to 6.6.1.13. inclusive of this annex. However, in this case, the ambient temperature described in paragraph 6.5.9.1. of this annex shall be replaced by the profile specified in Table C3/2 of this annex for the diurnal emission test.

Table C3/2

**Ambient temperature profile of the alternative sequence for sealed fuel tank system**

| *Time (hours)* | *Temperature (°C)* |
| --- | --- |
| 0/24 | 20.0 |
| 1 | 20.4 |
| 2 | 20.8 |
| 3 | 21.7 |
| 4 | 23.9 |
| 5 | 26.1 |
| 6 | 28.5 |
| 7 | 31.4 |
| 8 | 33.8 |
| 9 | 35.6 |
| 10 | 37.1 |
| 11 | 38.0 |
| 12 | 37.7 |
| 13 | 36.4 |
| 14 | 34.2 |
| 15 | 31.9 |
| 16 | 29.9 |
| 17 | 28.2 |
| 18 | 26.2 |
| 19 | 24.7 |
| 20 | 23.5 |
| 21 | 22.3 |
| 22 | 21.0 |
| 23 | 20.2 |

6.7. Stand-alone test procedure for sealed fuel tank systems

6.7.1 Measurement of depressurisation puff loss loading mass

6.7.1.1. The procedures in paragraphs 6.6.1.1. to 6.6.1.7.2. inclusive of this annex shall be performed. The depressurisation puff loss loading mass is defined as the difference in weight of the vehicle carbon canister before paragraph 6.6.1.6. of this annex is applied and after paragraph 6.6.1.7.2. of this annex is applied.

6.7.1.2. The depressurisation puff loss overflow from the vehicle carbon canister shall be measured according to paragraphs 6.6.1.8.1. and 6.6.1.8.2. inclusive of this Annex and fulfil the requirements of paragraph 6.6.1.8.3. in this annex.

6.7.2. Hot soak and diurnal breathing evaporative emissions test

6.7.2.1. In the case that the fuel tank relief pressure is greater than or equal to 30 kPa

6.7.2.1.1. The test shall be performed as described in paragraphs 6.5.1. to 6.5.3. and 6.6.1.9. to 6.6.1.9.1. inclusive of this annex.

6.7.2.1.2. The carbon canister shall be aged according to the sequence described in paragraph 5.1. to 5.1.3.1.3. inclusive of this annex and shall be loaded and purged according to paragraph 6.6.1.5. of this annex.

6.7.2.1.3. The aged carbon canister shall subsequently be loaded according to the procedure described in paragraph 6.5.5.4. However, instead of loading to breakthrough as described in paragraph 6.5.5.4.4., the total loading mass shall be determined in accordance with paragraph 6.7.1.1. of this annex. At the request of the manufacturer, the reference fuel may alternatively be used instead of butane. The carbon canister shall be disconnected.

6.7.2.1.4. The procedures in paragraphs 6.6.1.10. to 6.6.1.13. inclusive of this annex shall be followed.

6.7.2.2. In the case that the fuel tank relief pressure is lower than 30 kPa

The test shall be performed as described in paragraphs 6.7.2.1.1. to 6.7.2.1.4. inclusive of this annex. However, in this case, the ambient temperature described in paragraph 6.5.9.1. of this annex shall be modified in accordance with the profile specified in Table A1/1 of this annex for the diurnal emission test.

7. Calculation of evaporative test results

7.1. The evaporative emission tests described in paragraphs 6. to 6.7.2.2. inclusive of this annex allow the hydrocarbon emissions from the puff loss overflow, diurnal and hot soak tests to be calculated. Evaporative losses from each of these tests shall be calculated using the initial and final hydrocarbon concentrations, temperatures and pressures in the enclosure, together with the net enclosure volume.

The following equation shall be used:

MHC

where:

MHC is the mass of hydrocarbons, grams;

MHC,out is the mass of hydrocarbons exiting the enclosure in the case of fixed volume enclosures for diurnal emission testing, grams;

MHC,in is the mass of hydrocarbon entering the enclosure in the case of fixed volume enclosures for diurnal emission testing, grams;

CHC is the measured hydrocarbon concentration in the enclosure, ppm volume in C1 equivalent;

V is the net enclosure volume corrected for the volume of the vehicle with the windows and the luggage compartment open, m3. If the volume of the vehicle is not known, a volume of 1.42 m3 shall be subtracted;

T is the ambient chamber temperature, K;

P is the barometric pressure, kPa;

H/C is the hydrogen to carbon ratio

where:

H/C is taken to be 2.33 for puff loss overflow measurement in SHED and diurnal test losses;

H/C is taken to be 2.20 for hot soak losses;

H/C is taken to be 2.67 for calibration;

k is 1.2 × 10-4 × (12 + H/C), (g × K/(m³ × kPa));

i is the initial reading;

f is the final reading;

7.1.1. As an alternative to the equation in paragraph 7.1. of this annex, for variable volume enclosures the following equation may be used at the choice of the manufacturer:

MHC

where:

MHC is the mass of hydrocarbons, grams;

CHC is the measured hydrocarbon concentration in the enclosure, ppm volume in C1 equivalent;

V is the net enclosure volume corrected for the volume of the vehicle with the windows and the luggage compartment open, m3. If the volume of the vehicle is not known, a volume of 1.42 m3 shall be subtracted;

Ti is the initial ambient chamber temperature, K;

Pi is the initial barometric pressure, kPa;

H/C is the hydrogen to carbon ratio;

H/C is taken to be 2.33 for puff loss overflow measurement in SHED and diurnal test losses;

H/C is taken to be 2.20 for hot soak losses;

H/C is taken to be 2.67 for calibration;

k is 1.2 × 10-4 × (12 + H/C), (g × K/(m³ × kPa))

i is the initial reading;

f is the final reading.

7.2. The result of (MHS + MD1 + MD2 + (2 × PF)) shall be below the limit defined in paragraph 6.6.2. of this Regulation.

8. Test report

The test report shall contain at least the following:

(a) Description of the soak periods, including time and mean temperatures;

(b) Description of aged carbon canister used and reference to exact ageing report;

(c) Mean temperature during the hot soak test;

(d) Measurement during hot soak test, HSL;

(e) Measurement of first diurnal, DL1st day;

(f) Measurement of second diurnal, DL2nd day;

(g) Final evaporative test result, calculated according to paragraph 7. of this annex;

(h) Declared fuel tank relief pressure of the system (for sealed tank systems);

(i) Puff loss loading value (in the case of using 'stand-alone test procedure' described in paragraph 6.7. of this annex).

**Annex C4**

**Type 5 test - Durability**

(Description of the endurance test for verifying the durability of pollution control devices)

1. Introduction

1.1. This annex describes the test for verifying the durability of anti-pollution devices equipping vehicles with positive ignition or compression-ignition engines.

The durability requirements shall be demonstrated using one of the two options set out in paragraphs 1.2. and 1.4. below.

1.2. The whole vehicle durability test shall preferably be performed on a vehicle with the cycle energy demand of the VH (as defined in paragraph 4.2.1.1.2. of Annex B4) with the highest cycle energy demand of all of the Interpolation Families to be included in the durability family and shall be driven on a test track, on the road, or on a chassis dynamometer. The cycle energy demand of the test vehicle may be further increased to cover future extensions.

1.3. (Reserved)

1.4. As an alternative to durability testing, where applicable a manufacturer may choose to apply the assigned deterioration factors from Table 3A and Table 3B (as applicable) in paragraph 6.7.2. of this Regulation.

1.5. (Reserved)

1.6. Deterioration factors are determined using either the procedures set out in paragraph 1.2. or using the assigned values in the table referred to in paragraph 1.4. of this annex. The deterioration factors are used to establish compliance with the requirements of the appropriate emissions limits set out in paragraph 6.3.10. of this Regulation during the target useful life of the vehicle.

2. Technical requirements

2.1. As the operating cycle for the whole vehicle durability test, the vehicle manufacturer shall use the Standard Road Cycle (SRC) described in Appendix 3 to this annex. This test cycle shall be conducted until the vehicle has covered its target useful life.

3. Test vehicle

3.1. The vehicle shall be VH. It shall be in good mechanical order; the engine and the anti-pollution devices shall be new. The vehicle may be the same as that presented for the Type 1 test; in this case the Type 1 test has to be done after the vehicle has run at least 3,000 km of the ageing cycle of Appendix 3. to this annex.

3.1.1. Special requirements for hybrid vehicles are provided in Appendix 4 to this annex.

4. Fuel

The durability test is conducted with a suitable commercially available fuel.

5. Vehicle maintenance and adjustments

Maintenance, adjustments as well as the use of the test vehicle's controls shall be those recommended by the manufacturer. If during the execution of the whole vehicle durability test the vehicle experiences a failure not related to emissions and/or fuel consumption and/or energy consumption, the manufacturer can fix the vehicle and continue with the durability test. Otherwise the manufacturer shall consult the approval authority to find a commonly agreed solution.

6. Vehicle operation on track, road or on chassis dynamometer

6.1. Operating cycle

During operation on track, road or on roller test bench, the distance shall be covered according to the driving schedule described in Appendix 3 of this annex.

6.2. The durability test, or if the manufacturer has chosen, the modified durability test shall be conducted until the vehicle has covered its target useful life.

6.3. Test equipment

6.3.1. Chassis dynamometer

6.3.1.1. When the durability test is performed on a chassis dynamometer, the dynamometer shall enable the cycle described in Appendix 3 of this annex to be carried out. In particular, it shall be equipped with systems simulating inertia and resistance to progress.

6.3.1.2. The road load coefficients to be used shall be those for vehicle high (VH).

6.3.1.3. The vehicle cooling system should enable the vehicle to operate at temperatures similar to those obtained on road (oil, water, exhaust system, etc.).

6.3.1.4. Certain other test bench adjustments and features are deemed to be identical, where necessary, to those described in Annex B5 to this Regulation (inertia, for example, which may be mechanical or electronic).

6.3.1.5. The vehicle may be moved, where necessary, to a different bench in order to conduct emission measurement tests.

6.3.2. Operation on track or road

When the durability test is completed on track or road, the test mass of the vehicle shall be the same as that retained for tests conducted on a chassis dynamometer.

7. Measuring emissions of pollutants

A first test is carried out when the vehicle has reached a mileage between 3,000 km and 5,000 km. Further tests are carried out at 20,000 km (±400 km) and then every 20,000 km (±400 km) or more frequently, at regular intervals until having covered the target useful life. Exhaust emissions are measured in accordance with the Type 1 Test as defined in paragraph 6.3. of this Regulation. At the choice of the manufacturer any of the above tests can be repeated. In such a case the average value of all the repeated tests shall be considered as a single value for the relevant mileage. After 80,000 km has been driven, it is no longer necessary to separately record the emissions results from the first 3 phases of WLTP.

The limit values to be complied with are those laid down in paragraph 6.3.10. of this Regulation.

In the case of vehicles equipped with periodically regenerating systems as defined in paragraph 3.8.1. of this Regulation, it shall be checked that the vehicle is not approaching a regeneration period. If this is the case, the vehicle shall be driven until the end of the regeneration. If a regeneration occurs during the emissions measurement, a new test (including preconditioning) shall be performed, and the first result not taken into account.

All exhaust emissions results shall be plotted as a function of the running distance on the system rounded to the nearest kilometre and the best fit straight line fitted by the method of least squares shall be drawn through all these data points.

For the criteria emissions from the 4 phases of a WLTP test. The data will be acceptable for use in the calculation of the deterioration factor only if the interpolated 5,000 km and target useful life points on this line are within the above mentioned limits.

The data are still acceptable when a best fit straight line crosses an applicable limit with a negative slope (the 5,000 km interpolated point is higher than the target useful life point) but the target useful life actual data point is below the limit.

For criteria emissions from the first 3 phases of a WLTP test

The data will be acceptable for use in the calculation of the deterioration factor only if the extrapolated 3,000 km and the target useful life points on this line are within the above mentioned limits.

7.1. A multiplicative exhaust emission deterioration factor shall be calculated for each pollutant as follows:

Where:

Mi1 =

For the criteria emissions from the 4 phases of a WLTP test - mass emission of the pollutant i in g/km interpolated to 5,000 km,

For criteria emissions from the first 3 phases of a WLTP test - mass emission of the pollutant i in g/km extrapolated to 3,000 km

Mi2 = mass emission of the pollutant i in g/km interpolated to the respective target useful life

These interpolated values shall be carried out to a minimum of four places to the right of the decimal point before dividing one by the other to determine the deterioration factor. The result shall be rounded to three places to the right of the decimal point.

If a deterioration factor is less than one, it is deemed to be equal to one.

At the request of a manufacturer, an additive exhaust emission deterioration factor shall be calculated for each pollutant as follows:

D . E . F . = Mi2 – Mi1

If the additive deterioration factor calculated with the above formula is negative, then it shall be put equal to zero.

These additive deterioration factors shall follow the same rules described for the multiplicative deterioration factors in relation to the criteria emissions from the 4 phases of a WLTP test and for criteria emissions from the first 3 phases of a WLTP test.

Annex C4 - Appendix 1 (Reserved)

Annex C4 - Appendix 2 (Reserved)

Annex C4 - Appendix 3

Standard Road Cycle (SRC)

1. Introduction

The Standard Road Cycle (SRC) is a kilometre accumulation cycle on VH. The vehicle may be run on a test track or on a kilometre accumulation dynamometer.

The cycle consists of 7 laps of a 6 km course. The length of the lap may be changed to accommodate the length of the mileage accumulation test track.

**Standard road cycle**

| *Lap* | *Description* | *Typical acceleration rate m/s²* |
| --- | --- | --- |
| 1 | (start engine) idle 10 seconds | 0 |
| 1 | Moderate acceleration to 48 km/h | 1.79 |
| 1 | Cruise at 48 km/h for ¼ lap | 0 |
| 1 | Moderate deceleration to 32 km/h | -2.23 |
| 1 | Moderate acceleration to 48 km/h | 1.79 |
| 1 | Cruise at 48 km/h for ¼ lap | 0 |
| 1 | Moderate deceleration to stop | -2.23 |
| 1 | Idle 5 seconds | 0 |
| 1 | Moderate acceleration to 56 km/h | 1.79 |
| 1 | Cruise at 56 km/h for ¼ lap | 0 |
| 1 | Moderate deceleration to 40 km/h | -2.23 |
| 1 | Moderate acceleration to 56 km/h | 1.79 |
| 1 | Cruise at 56 km/h for ¼ lap | 0 |
| 1 | Moderate deceleration to stop | -2.23 |
| 2 | Idle 10 seconds | 0 |
| 2 | Moderate acceleration to 64 km/h | 1.34 |
| 2 | Cruise at 64 km/h for ¼ lap | 0 |
| 2 | Moderate deceleration to 48 km/h | -2.23 |
| 2 | Moderate acceleration to 64 km/h | 1.34 |
| 2 | Cruise at 64 km/h for ¼ lap | 0 |
| 2 | Moderate deceleration to stop | -2.23 |
| 2 | Idle 5 seconds | 0 |
| 2 | Moderate acceleration to 72 km/h | 1.34 |
| 2 | Cruise at 72 km/h for ¼ lap | 0 |
| 2 | Moderate deceleration to 56 km/h | -2.23 |
| 2 | Moderate acceleration to 72 km/h | 1.34 |
| 2 | Cruise at 72 km/h for ¼ lap | 0 |
| 2 | Moderate deceleration to stop | -2.23 |
| 3 | Idle 10 seconds | 0 |
| 3 | Hard acceleration to 88 km/h | 1.79 |
| 3 | Cruise at 88 km/h for ¼ lap | 0 |
| 3 | Moderate deceleration to 72 km/h | -2.23 |
| 3 | Moderate acceleration to 88 km/h | 0.89 |
| 3 | Cruise at 88 km/h for ¼ lap | 0 |
| 3 | Moderate deceleration to 72 km/h | -2.23 |
| 3 | Moderate acceleration to 97 km/h | 0.89 |
| 3 | Cruise at 97 km/h for ¼ lap | 0 |
| 3 | Moderate deceleration to 80 km/h | -2.23 |
| 3 | Moderate acceleration to 97 km/h | 0.89 |
| 3 | Cruise at 97 km/h for ¼ lap | 0 |
| 3 | Moderate deceleration to stop | -1.79 |
| 4 | Idle 10 seconds | 0 |
| 4 | Hard acceleration to 129 km/h | 1.34 |
| 4 | Coast down to 113 km/h | -0.45 |
| 4 | Cruise at 113 km/h for ½ lap | 0 |
| 4 | Moderate deceleration to 80 km/h | -1.34 |
| 4 | Moderate acceleration to 105 km/h | 0.89 |
| 4 | Cruise at 105 km/h for ½ lap | 0 |
| 4 | Moderate deceleration to 80 km/h | -1.34 |
| 5 | Moderate acceleration to 121 km/h | 0.45 |
| 5 | Cruise at 121 km/h for ½ lap | 0 |
| 5 | Moderate deceleration to 80 km/h | -1.34 |
| 5 | Light acceleration to 113 km/h | 0.45 |
| 5 | Cruise at 113 km/h for ½ lap | 0 |
| 5 | Moderate deceleration to 80 km/h | -1.34 |
| 6 | Moderate acceleration to 113 km/h | 0.89 |
| 6 | Coast down to 97 km/h | -0.45 |
| 6 | Cruise at 97 km/h for ½ lap | 0 |
| 6 | Moderate deceleration to 80 km/h | -1.79 |
| 6 | Moderate acceleration to 104 km/h | 0.45 |
| 6 | Cruise at 104 km/h for ½ lap | 0 |
| 6 | Moderate deceleration to stop | -1.79 |
| 7 | Idle 45 seconds | 0 |
| 7 | Hard acceleration to 88 km/h | 1.79 |
| 7 | Cruise at 88 km/h for ¼ lap | 0 |
| 7 | Moderate deceleration to 64 km/h | -2.23 |
| 7 | Moderate acceleration to 88 km/h | 0.89 |
| 7 | Cruise at 88 km/h for ¼ lap | 0 |
| 7 | Moderate deceleration to 64 km/h | -2.23 |
| 7 | Moderate acceleration to 80 km/h | 0.89 |
| 7 | Cruise at 80 km/h for ¼ lap | 0 |
| 7 | Moderate deceleration to 64 km/h | -2.23 |
| 7 | Moderate acceleration to 80 km/h | 0.89 |
| 7 | Cruise at 80 km/h for ¼ lap | 0 |
| 7 | Moderate deceleration to stop | -2.23 |

The standard road cycle is represented graphically in the following figure:  


Annex C4 - Appendix 4

Special requirements for Hybrid Vehicles

1. Introduction

1.1. This appendix provides special requirements for the Type 5 test of OVC-HEVs and NOVC-HEVs, as set out in paragraphs 2. and 3. of this appendix.

2. For OVC-HEVs:

It is not allowed to charge the electrical energy/power storage device during mileage accumulation.

For OVC-HEVs with an operating mode switch, mileage accumulation should be driven in the mode which is automatically set after initiation of the vehicle start procedure (normal mode).

During the mileage accumulation a change into another hybrid mode is allowed if necessary in order to continue the mileage accumulation after agreement of the Technical Service.

The measurements of emissions of pollutants shall be carried out under the same conditions as specified in paragraph 3.2.5. of Annex B8.

3. For NOVC-HEVs:

Mileage accumulation shall be driven in the driver selectable mode which is always selected when the vehicle is switched on (predominant mode) or in the mode which is recommended by the manufacturer (if no predominant mode is available) after agreement of the Technical Service.

The measurements of emissions of pollutants shall be carried out in the same conditions as in the Type 1 test.

Annex C5

On-Board Diagnostics (OBD) for motor vehicles

1. Introduction

This annex applies to the functional aspects of On-Board Diagnostic (OBD) system for the emission control of motor vehicles.

2. (Reserved)

3. Requirements and tests

3.1. All vehicles shall be equipped with an OBD system so designed, constructed and installed in a vehicle as to enable it to identify types of deterioration or malfunction over the entire life of the vehicle. In achieving this objective, the Type Approval Authority shall accept that vehicles which have travelled distances in excess of the target useful life (according to paragraph 6.7. of this Regulation) referred to in paragraph 3.3.1. of this annex, may show some deterioration in OBD system performance such that the OBD thresholds set out in Table 4A and Table 4B (as applicable) in paragraph 6.8.2. of this Regulation may be exceeded before the OBD system signals a failure to the driver of the vehicle.

3.1.1. Access to the OBD system required for the inspection, diagnosis, servicing or repair of the vehicle shall be unrestricted and standardised. All emission-related fault codes shall be consistent with paragraph 6.5.3.5. of Appendix 1 to this annex.

3.2. The OBD system shall be so designed, constructed and installed in a vehicle as to enable it to comply with the requirements of this annex during conditions of normal use.

3.2.1. Temporary disablement of the OBD system

3.2.1.1. A manufacturer may disable the OBD system if its ability to monitor is affected by low fuel levels. Disablement shall not occur when the fuel tank level is above 20 per cent of the nominal capacity of the fuel tank.

3.2.1.2. A manufacturer may disable any specific OBD monitor for a given driving cycle for ambient or engine coolant temperatures below 266 K (-7 °C) or at elevations over 2,440 metres above sea level provided the manufacturer submits data and/or an engineering evaluation which adequately demonstrate that monitoring would be unreliable when such conditions exist. A manufacturer may also request disablement of any specific OBD monitor at other ambient or engine coolant temperatures or other elevations if they demonstrate to the authority with data and/or an engineering evaluation that misdiagnosis would occur under such conditions. It is not necessary to illuminate the Malfunction Indicator (MI) if OBD thresholds are exceeded during a regeneration provided no defect is present.

Engine coolant temperature is only deemed subject to approval, if it is used as a substitute to ambient temperature.

3.2.1.3. For vehicles designed to accommodate the installation of power take-off units, disablement of affected monitoring systems is permitted provided disablement occurs only when the power take-off unit is active.

In addition to the provisions of this paragraph the manufacturer may temporarily disable the OBD system in the following conditions:

(a) For flex fuel or mono/bi fuel gas vehicles during 1 minute after re-fuelling to allow for the recognition of fuel quality and composition by the ECU;

(b) For bi fuel vehicles during 5 seconds after fuel switching to allow for readjusting engine parameters;

(c) The manufacturer may deviate from these time limits if it can demonstrate that stabilisation of the fuelling system after re-fuelling or fuel switching takes longer for justified technical reasons. In any case, the OBD system shall be re-enabled as soon as either the fuel quality and composition is recognised, or the engine parameters are readjusted.

3.2.2. Engine misfire in vehicles equipped with positive ignition engines

3.2.2.1. Manufacturers may adopt higher misfire percentage malfunction criteria than those declared to the authority, under specific engine speed and load conditions where it can be demonstrated to the authority that the detection of lower levels of misfire would be unreliable.

3.2.2.2. When a manufacturer can demonstrate to the authority that the detection of higher levels of misfire percentages is still not feasible, or that misfire cannot be distinguished from other effects (e.g. rough roads, transmission shifts, after engine starting; etc.) the misfire monitoring system may be disabled when such conditions exist.

3.2.3. Identification of deterioration or malfunctions may also be done outside a driving cycle (e.g. after engine shutdown).

3.3. Description of tests

3.3.1. The tests are carried out on the vehicle used for the Type 5 durability test, given in Annex C4 to this Regulation, and using the test procedure in Appendix 1 to this annex. Tests are carried out at the conclusion of the Type 5 durability testing.

When no Type 5 durability testing is carried out, or at the request of the manufacturer, a suitably aged and representative vehicle may be used for these OBD demonstration tests.

3.3.2. The OBD system shall indicate the failure of an emission-related component or system when that failure results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

3.3.2.1. The OBD thresholds limits for vehicles that are type approved according to the emission limits set out in paragraph 6.3.10. of this Regulation are set out in Table 4A and Table 4B (as applicable) in paragraph 6.8.2. of this Regulation.

3.3.3. Monitoring requirements for vehicles equipped with positive ignition engines.

In satisfying the requirements of paragraph 3.3.2. of this annex the OBD system shall, at a minimum, monitor for:

3.3.3.1. The reduction in the efficiency of the catalytic converter with respect to emissions of NMHC and NOx. Manufacturers may monitor the front catalyst alone or in combination with the next catalyst(s) downstream. Each monitored catalyst or catalyst combination shall be considered malfunctioning when the emissions exceed the NMHC or NOx OBD thresholds set out in paragraph 6.8.2. of this Regulation.

3.3.3.2. The presence of engine misfire in the engine operating region bounded by the following lines:

(a) A maximum speed of 4,500 min-1 or 1,000 min-1 greater than the highest speed occurring during a Type 1 Test cycle, whichever is the lower;

(b) The positive torque line (i.e. engine load with the transmission in neutral);

(c) A line joining the following engine operating points: the positive torque line at 3,000 min-1 and a point on the maximum speed line defined in (a) above with the engine's manifold vacuum at 13.33 kPa lower than that at the positive torque line.

3.3.3.2.1. Specific monitoring rate for misfire:

(a) Catalytic converter protection. The engine misfire which causes the catalytic converter damage because of excessive heat, shall be monitored every 200 revolutions within the region specified in paragraph 3.3.3.2.

When the evaluated engine misfire rate is less than 5%, the limit can be fixed at 5%.

(b) Exceeding emission threshold. The engine misfire which causes to exceed an emission threshold shall be monitored every 1,000 revolutions within the region specified in paragraph 3.3.3.2.

When the evaluated engine misfire rate is less than 1%, the limit can be fixed at 1%.

3.3.3.3. Oxygen sensor deterioration

This paragraph shall mean that the deterioration of all oxygen sensors fitted and used for monitoring malfunctions of the catalytic converter according to the requirements of this annex shall be monitored.

3.3.3.4. Other emission control system components or systems, or emission related powertrain components or systems which are connected to a computer, if active on the selected fuel, the failure of which may result in tailpipe emissions exceeding any of the OBD thresholds set out in Table 4A and Table 4B (as applicable) in paragraph 6.8.2. of this Regulation.

The following is a non-exhaustive list providing examples of representative components and systems:

(a) Exhaust gas recirculation system

(b) Fuel system

(c) Secondary air system

(d) Valve timing system

(e) Atmosphere pressure sensor

(f) Intake air pressure sensor

(g) Intake air temperature sensor

(h) Air flow sensor

(i) Engine coolant temperature sensor

(j) Throttle sensor

(k) Cylinder identification sensor

(l) Crank angle sensor

3.3.3.5. Unless otherwise monitored, any other emission-related powertrain component connected to a computer, including any relevant sensors to enable monitoring functions to be carried out, shall be monitored for circuit continuity.

3.3.3.6. The electronic evaporative emission purge control shall, at a minimum, be monitored for circuit continuity.

3.3.3.7. For direct injection positive ignition engines any malfunction, which may lead to emissions exceeding the particulate OBD thresholds set out in paragraph 6.8.2. of this Regulation and which has to be monitored according to the requirements of this annex for compression ignition engines, shall be monitored.

3.3.4. Monitoring requirements for vehicles equipped with compression-ignition engines

In satisfying the requirements of paragraph 3.3.2. of this annex the OBD system shall monitor:

1. Where fitted, reduction in the efficiency of the catalytic converter.
2. Where fitted, the functionality and integrity of the particulate trap.
3. The fuel-injection system electronic fuel quantity and timing actuator(s) is/are monitored for circuit continuity and total functional failure.
4. Other emission control system components or systems, or emission-related power-train components or systems, which are connected to a computer, the failure of which may result in exhaust emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation. Examples of such systems or components are those for monitoring and control of air mass-flow, air volumetric flow (and temperature), boost pressure and inlet manifold pressure (and relevant sensors to enable these functions to be carried out).
5. Unless otherwise monitored, any other emission-related power-train component connected to a computer shall be monitored for circuit continuity.
6. Malfunctions and the reduction in efficiency of the EGR system shall be monitored.
7. Malfunctions and the reduction in efficiency of a NOx after-treatment system using a reagent and the reagent dosing sub-system shall be monitored.
8. Malfunctions and the reduction in efficiency of NOx after-treatment not using a reagent shall be monitored.

3.3.5. Manufacturers may demonstrate to the Type Approval Authority that certain components or systems need not be monitored if, in the event of their total failure or removal, emissions do not exceed the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

3.3.5.1. The following devices should however be monitored for total failure or removal (if removal would cause the applicable emission limits in paragraph 6.3.10. of this Regulation to be exceeded):

(a) A particulate trap fitted to compression ignition engines as a separate unit or integrated into a combined emission control device;

(b) A NOx after treatment system fitted to compression ignition engines as a separate unit or integrated into a combined emission control device;

(c) A Diesel Oxidation Catalyst (DOC) fitted to compression ignition engines as a separate unit or integrated into a combined emission control device.

3.3.5.2. The devices referred to in paragraph 3.3.5.1. of this annex shall also be monitored for any failure that would result in exceeding the applicable OBD thresholds set out in in paragraph 6.8.2. of this Regulation.

3.4. A sequence of diagnostic checks shall be initiated at each engine start and completed at least once provided that the correct test conditions are met. The test conditions shall be selected in such a way that they all occur under normal driving as represented by the Type 1 test.

3.5. Activation of malfunction indicator (MI)

3.5.1. The OBD system shall incorporate a malfunction indicator readily perceivable to the vehicle operator. The MI shall not be used for any other purpose except to indicate emergency start-up, emission default modes or limp-home routines to the driver. The MI shall be visible in all reasonable lighting conditions. When activated, it shall display a symbol in conformity with ISO 2575. A vehicle shall not be equipped with more than one general purpose MI for emission-related problems. Separate specific purpose tell tales (e. g. brake system, fasten seat belt, oil pressure, etc.) are permitted. The use of red colour for an MI is prohibited.

3.5.2. For strategies requiring more than two preconditioning cycles for MI activation, the manufacturer shall provide data and/or an engineering evaluation which adequately demonstrates that the monitoring system is equally effective and timely in detecting component deterioration. Strategies requiring on average more than ten driving cycles for MI activation are not accepted. The MI shall also activate whenever the engine control enters a permanent emission default mode of operation if any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation are exceeded or if the OBD system is unable to fulfil the basic monitoring requirements specified in paragraph 3.3.3. or 3.3.4. of this annex. The MI shall operate in a distinct warning mode, e.g. a flashing light, under any period during which engine misfire occurs at a level likely to cause catalyst damage, as specified by the manufacturer. The MI shall also activate when the vehicle's ignition is in the "key‑on" position before engine starting or cranking and de‑activate after engine starting if no malfunction has previously been detected.

3.6. Fault code storage

3.6.1. The OBD system shall record pending and confirmed fault code(s) indicating the status of the emission control system. Separate status codes (readiness codes) shall be used to identify correctly functioning emission control systems and those emission control systems which need further vehicle operation to be fully evaluated. If the MI is activated due to deterioration or malfunction or permanent emission default modes of operation, a fault code shall be stored that identifies the type of malfunction. A fault code shall also be stored in the cases referred to in paragraphs 3.3.3.5. and 3.3.4. (e) of this annex.

3.6.2. The distance travelled by the vehicle while the MI is activated shall be available at any instant through the serial port on the standard link connector.

3.6.3. In the case of vehicles equipped with positive ignition engines, misfiring cylinders need not be uniquely identified if a distinct single or multiple cylinder misfire fault code is stored.

3.7. Extinguishing the MI

3.7.1. If misfire at levels likely to cause catalyst damage (as specified by the manufacturer) is not present any more, or if the engine is operated after changes to speed and load conditions where the level of misfire will not cause catalyst damage, the MI may be switched back to the previous state of activation during the first driving cycle on which the misfire level was detected and may be switched to the normal activated mode on subsequent driving cycles. If the MI is switched back to the previous state of activation, the corresponding fault codes and stored freeze-frame conditions may be erased.

3.7.2. For all other malfunctions, the MI may be de-activated after three subsequent sequential driving cycles during which the monitoring system responsible for activating the MI ceases to detect the malfunction and if no other malfunction has been identified that would independently activate the MI.

3.8. Erasing a fault code

3.8.1. The OBD system may erase a fault code and the distance travelled and freeze-frame information if the same fault is not re-registered in at least 40 engine warm-up cycles or 40 driving cycles with vehicle operation in which the following criteria (a)-(c) are satisfied:

(a) Cumulative time since engine start is greater than or equal to 600 seconds;

(b) Cumulative vehicle operation at or above 40 km/h occurs for greater than or equal to 300 seconds;

(c) Continuous vehicle operation at idle (i.e. accelerator pedal released by driver and vehicle speed less than or equal to 1.6 km/h) for greater than or equal to 30 seconds.

3.9. Bi-fuelled gas vehicles

In general, for bi-fuelled gas vehicles for each of the fuel types (petrol and (NG/biomethane)/LPG)) all the OBD requirements as for a mono-fuelled vehicle are applicable. To this end one of the following two options in paragraphs 3.9.1. or 3.9.2. of this annex or any combination thereof, shall be used.

3.9.1. One OBD system for both fuel types.

3.9.1.1. The following procedures shall be executed for each diagnostic in a single OBD system for operation on petrol and on (NG/biomethane)/LPG, either independent of the fuel currently in use or fuel type specific:

(a) Activation of malfunction indicator (MI) (see paragraph 3.5. of this annex);

(b) Fault code storage (see paragraph 3.6. of this annex);

(c) Extinguishing the MI (see paragraph 3.7. of this annex);

(d) Erasing a fault code (see paragraph 3.8. of this annex).

For components or systems to be monitored, either separate diagnostics for each fuel type can be used or a common diagnostic.

3.9.1.2. The OBD system can reside in either one or more computers.

3.9.2. Two separate OBD systems, one for each fuel type.

3.9.2.1. The following procedures shall be executed independently of each other when the vehicle is operated on petrol or on (NG/biomethane)/LPG:

(a) Activation of malfunction indicator (MI) (see paragraph 3.5. of this annex);

(b) Fault code storage (see paragraph 3.6. of this annex);

(c) Extinguishing the MI (see paragraph 3.7. of this annex);

(d) Erasing a fault code (see paragraph 3.8. of this annex).

3.9.2.2. The separate OBD systems can reside in either one or more computers.

3.9.3. Specific requirements regarding the transmission of diagnostic signals from bi-fuelled gas vehicles.

3.9.3.1. On a request from a diagnostic scan tool, the diagnostic signals shall be transmitted on one or more source addresses. The use of source addresses is described in the standard listed in paragraph 6.5.3.2.(a) of Appendix 1 to this annex.

3.9.3.2. Identification of fuel specific information can be realized:

(a) By use of source addresses; and/or

(b) By use of a fuel select switch; and/or

(c) By use of fuel specific fault codes.

3.9.4. Regarding the status code (as described in paragraph 3.6. of this annex), one of the following two options has to be used, if one or more of the diagnostics reporting readiness is fuel type specific:

(a) The status code is fuel specific, i.e. use of two status codes, one for each fuel type;

(b) The status code shall indicate fully evaluated control systems for both fuel types (petrol and (NG/biomethane)/LPG)) when the control systems are fully evaluated for only one of the fuel types.

If none of the diagnostics reporting readiness is fuel type specific, then only one status code has to be supported.

3.10. Additional provisions for vehicles employing engine shut - off strategies.

3.10.1. Driving cycle

3.10.1.1. Autonomous engine restarts commanded by the engine control system following an engine stall may be considered a new driving cycle or a continuation of the existing driving cycle.

4. Requirements relating to the type approval of on-board diagnostic systems

4.1. A manufacturer may request to the Type Approval Authority that an OBD system be accepted for type approval even though the system contains one or more deficiencies such that the specific requirements of this annex are not fully met. The Type Approval Authority may approve up to two separate components or systems with one or more deficiencies.

When a manufacturer adopts specific conditions for misfire defined in paragraph 3.3.3.2.1. of this annex, these conditions shall not be considered as a deficiency.

4.2. In considering the request, the Type Approval Authority shall determine whether compliance with the requirements of this annex is infeasible or unreasonable.

The Type Approval Authority shall take into consideration data from the manufacturer that details such factors as, but not limited to, technical feasibility, lead time and production cycles including phase-in or phase-out of engines or vehicle designs and programmed upgrades of computers, the extent to which the resultant OBD system will be effective in complying with the requirements of this Regulation and that the manufacturer has demonstrated an acceptable level of effort towards compliance with the requirements of this Regulation.

4.2.1. The Type Approval Authority shall not accept any deficiency request that includes the complete lack of a required diagnostic monitor or the lack of mandated recording and reporting of data related to a monitor.

4.2.2. The Type Approval Authority will not accept any deficiency request that does not respect the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

4.3. In determining the identified order of deficiencies, deficiencies relating to paragraphs 3.3.3.1., 3.3.3.2. and 3.3.3.3. of this annex for positive ignition engines and paragraphs 3.3.4. (a), (b) and (c) of this annex for compression-ignition engines shall be identified first.

4.4. Prior to or at the time of type approval, no deficiency shall be granted in respect of the requirements of paragraph 6.5., except paragraph 6.5.3.5. of Appendix 1 to this annex.

4.5. Deficiency period

4.5.1. A deficiency may be carried-over for a period of two years after the date of type-approval unless it can be adequately demonstrated that substantial vehicle hardware modifications and additional lead-time beyond two years would be necessary to correct the deficiency. In such a case, the deficiency may be carried-over for a period not exceeding three years.

4.5.2. A manufacturer may request that the Type Approval Authority grant a deficiency retrospectively when such a deficiency is discovered after the original type-approval. In this case, the deficiency may be carried-over for a period of two years after the date of notification to the Type Approval Authority unless it can be adequately demonstrated that substantial vehicle hardware modifications and additional lead-time beyond two years would be necessary to correct the deficiency. In such a case, the deficiency may be carried-over for a period not exceeding three years.

4.6. At the request of the manufacturer, a vehicle with an OBD system may be accepted for type-approval with regard to emissions, even though the system contains one or more deficiencies such that the specific requirements of this annex are not fully met, provided that the specific administrative provisions set out in paragraphs 4.1. to 4.5.2. of this annex are complied with.

The Type Approval Authority shall notify its decision in granting a deficiency request to all other Contracting Parties to the 1958 Agreement applying this Regulation.

Annex C5 - Appendix 1

Functional aspects of On-Board Diagnostic (OBD) systems

1. This appendix describes the procedure of the test according to paragraph 3. of this annex. The procedure describes a method for checking the function of the On-Board Diagnostic (OBD) system installed on the vehicle by failure simulation of relevant systems in the engine management or emission control system. It also sets procedures for determining the durability of OBD systems.

The manufacturer shall make available the defective components and/or electrical devices which would be used to simulate failures. When measured over the Type 1 test cycle, such defective components or devices shall not cause the vehicle emissions to exceed any of the OBD thresholds set out in Table 4A and Table 4B (as applicable) in paragraph 6.8.2. of this Regulation by more than 20 per cent. For electrical failures (short/open circuit), the emissions may exceed these OBD thresholds by more than twenty per cent.

When the vehicle is tested with the defective component or device fitted, the OBD system is approved if the MI is activated. The OBD system is also approved if the MI is activated below the OBD thresholds.

2. Description of test

2.1. The testing of OBD systems consists of the following phases:

2.1.1. Simulation of malfunction of a component of the engine management or emission control system;

2.1.2. Preconditioning of the vehicle with a simulated malfunction over preconditioning specified in paragraph 6.2.1. or paragraph 6.2.2. of this appendix;

2.1.3. Driving the vehicle with a simulated malfunction over the Type 1 test cycle and measuring the emissions of the vehicle. When driving the vehicle with a simulated malfunction, the drive trace indices and tolerances set out in paragraph 2.6.8.3.2. of Annex B6 shall not apply;

2.1.4. Determining whether the OBD system reacts to the simulated malfunction and indicates malfunction in an appropriate manner to the vehicle driver.

2.2. Alternatively, at the request of the manufacturer, malfunction of one or more components may be electronically simulated according to the requirements of paragraph 6. of this appendix.

2.3. Manufacturers may request that monitoring take place outside the Type 1 test cycle if it can be demonstrated to the Type Approval Authority that monitoring during conditions encountered during the Type 1 test cycle would impose restrictive monitoring conditions when the vehicle is used in service.

2.4. For OVC-HEVs, testing shall be carried out under charge-sustaining conditions.

3. Test vehicle and fuel

3.1. Vehicle

The test vehicle shall meet the requirements of paragraph 2.3. of Annex B6 to this Regulation.

3.2. Fuel

The appropriate reference fuel as described in Annex B3 to this Regulation shall be used for testing. The fuel type for each failure mode to be tested (described in paragraph 6.3. of this appendix) may be selected by the Type Approval Authority from the reference fuels described in Annex B3 to this Regulation in the case of the testing of a mono-fuelled gas vehicle or of a bi-fuelled gas vehicle. The selected fuel type shall not be changed during any of the test phases (described in paragraphs 2.1. to 2.3. of this appendix). In the case of the use of LPG or NG/biomethane as a fuel it is permissible that the engine is started on petrol and switched to LPG or NG/biomethane after a pre-determined period of time which is controlled automatically and not under the control of the driver.

4. Test temperature and pressure

4.1. The test temperature and pressure shall meet the requirements of the Type 1 test as described in Annex B6 to this Regulation.

5. Test equipment

5.1. Chassis dynamometer

The chassis dynamometer shall meet the requirements of Annex B5 to this Regulation.

6. OBD test procedure

An overview of the OBD test procedure is provided in Figure C5.App1/1. This is for information purposes only.

Figure C5.App1/1

**Overview of demonstration test**

6.1. The operating cycle on the chassis dynamometer shall be the applicable WLTC driven in the Type 1 test, as specified in Annexes Part B.

6.1.1. The Type 1 test need not be performed for the demonstration of electrical failures (short/open circuit). The manufacturer may demonstrate these failure modes using driving conditions in which the component is used and the monitoring conditions are encountered. These conditions shall be reported in the type approval documentation.

6.1.2. At the beginning of each failure mode to be demonstrated, the fault code memory shall be cleared.

6.2. Vehicle preconditioning

6.2.1. Preconditioning for adaption

Preconditioning for adaption consists of two parts

(a) Preconditioning for adaption without fault

(b) Preconditioning for adaption with fault

upon the choice of the manufacturer.

The preconditioning for adaption consists of one or more consecutive WLTC 3-phase tests. At the request of the manufacturer and with the approval of the Type Approval Authority, alternative method for adaption may be used instead of 3-phase-tests.

If the fault code is stored after preconditioning for adaption, manufacturer shall delete the fault code.

6.2.2. Preconditioning for Monitoring

6.2.2.1. According to the engine type and after introduction of one of the failure modes given in paragraph 6.3. of this appendix, the vehicle shall be preconditioned by driving at least two consecutive 3-phase-WLTC tests.

6.2.3. At the request of the manufacturer with approval by Type Approval Authority, alternative preconditioning methods may be used.

The reason for the use of additional preconditioning cycles or alternative preconditioning methods as well as details of these cycles/methods shall be reported in the type approval documentation.

6.3. Failure modes to be tested

6.3.1. Positive ignition engined vehicles:

6.3.1.1. Replacement of the catalyst with a deteriorated or defective catalyst or electronic simulation of such a failure;

6.3.1.2. Engine misfire conditions according to the conditions for misfire monitoring given in paragraph 3.3.3.2. of this annex;

6.3.1.3. Replacement of the oxygen sensor with a deteriorated or defective oxygen sensor or electronic simulation of such a failure;

6.3.1.4. Electrical disconnection of any other emission-related component connected to a powertrain management computer (if active on the selected fuel type);

6.3.1.5.Electrical disconnection of the electronic evaporative purge control device (if equipped and if active on the selected fuel type).

6.3.2. Compression-ignition engined vehicles:

6.3.2.1. Where fitted, replacement of the catalyst with a deteriorated or defective catalyst or electronic simulation of such a failure.

6.3.2.2. Where fitted, total removal of the particulate trap or, where sensors are an integral part of the trap, a defective trap assembly.

6.3.2.3. Electrical disconnection of any fuelling system electronic fuel quantity and timing actuator.

6.3.2.4. Electrical disconnection of any other emission-related component connected to a powertrain management computer.

6.3.2.5. In meeting the requirements of paragraphs 6.3.2.3. and 6.3.2.4. of this appendix, and with the agreement of the Type Approval Authority, the manufacturer shall take appropriate steps to demonstrate that the OBD system will indicate a fault when disconnection occurs.

6.3.2.6. The manufacturer shall demonstrate that malfunctions of the EGR flow and cooler are detected by the OBD system during its approval test.

6.4. OBD system test

6.4.1. Vehicles fitted with positive ignition engines:

6.4.1.1. After vehicle preconditioning according to paragraph 6.2. of this appendix, the test vehicle is driven over a Type 1 test.

The MI shall be activated at the latest before the end of this test under any of the conditions given in paragraphs 6.4.1.2. to 6.4.1.6. of this appendix. The MI may also be activated during preconditioning. The Technical Service may substitute those failure modes with others in accordance with paragraph 3.3.3.4. of this annex**.** However, the total number of failures simulated shall not exceed four (4) for the purpose of type approval.

In the case of testing a bi-fuel gas vehicle, both fuel types shall be used within the maximum of four (4) simulated failures at the discretion of the Type Approval Authority.

6.4.1.2. Replacement of a catalyst with a deteriorated or defective catalyst or electronic simulation of a deteriorated or defective catalyst that results in emissions exceeding the NMHC OBD threshold or the NOx OBD threshold set out in paragraph 6.8.2. of this Regulation.

6.4.1.3. An induced misfire condition according to the conditions for misfire monitoring given in paragraph 3.3.3.2. of this annex that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.4.1.4. Replacement of an oxygen sensor with a deteriorated or defective oxygen sensor or electronic simulation of a deteriorated or defective oxygen sensor that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.4.1.5. Electrical disconnection of the electronic evaporative purge control device (if equipped and if active on the selected fuel type).

6.4.1.6. Electrical disconnection of any other emission-related powertrain component connected to a computer that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation (if active on the selected fuel type).

6.4.2. Vehicles fitted with compression-ignition engines:

6.4.2.1. After vehicle preconditioning according to paragraph 6.2. of this appendix, the test vehicle is driven over a Type 1 test.

The MI shall be activated at the latest before the end of this test under any of the conditions given in paragraphs 6.4.2.2. to 6.4.2.5 of this appendix. The MI may also be activated during preconditioning. The technical service may substitute those failure modes by others in accordance with paragraph 3.3.4. (d) of this annex. However, the total number of failures simulated shall not exceed four (4) for the purposes of type approval.

6.4.2.2. Where fitted, replacement of a catalyst with a deteriorated or defective catalyst or electronic simulation of a deteriorated or defective catalyst that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.4.2.3. Where fitted, total removal of the particulate trap or replacement of the particulate trap with a defective particulate trap meeting the conditions of paragraph 6.3.2.2. of this appendix that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.4.2.4. With reference to paragraph 6.3.2.5. of this appendix, disconnection of any fuelling system electronic fuel quantity and timing actuator that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.4.2.5. With reference to paragraph 6.3.2.5. of this appendix, disconnection of any other emission-related powertrain component connected to a computer that results in emissions exceeding any of the OBD thresholds set out in paragraph 6.8.2. of this Regulation.

6.5. Diagnostic signals

6.5.1. (Reserved)

6.5.1.1. Upon determination of the first malfunction of any component or system, "freeze-frame" engine conditions present at the time shall be stored in computer memory. Should a subsequent fuel system or misfire malfunction occur, any previously stored freeze-frame conditions shall be replaced by the fuel system or misfire conditions (whichever occurs first). Stored engine conditions shall include, but are not limited to calculated load value, engine speed (RPM), fuel trim value(s) (if available), fuel pressure (if available), vehicle speed (if available), engine coolant temperature, intake manifold pressure (if available), fuel system status (e.g. closed-loop, open-loop) (if available) and the fault code which caused the data to be stored. The manufacturer shall choose the most appropriate set of conditions facilitating effective repairs for freeze-frame storage. Only one frame of data is required. Manufacturers may choose to store additional frames provided that at least the required frame can be read by a generic scan tool meeting the specifications of paragraphs 6.5.3.2. and 6.5.3.3. of this appendix. If the fault code causing the conditions to be stored is erased in accordance with paragraph 3.8. of this annex, the stored engine conditions may also be erased.

6.5.1.2. If available, the following signals in addition to the required freeze-frame information shall be made available on demand through the serial port on the standardised data link connector, if the information is available to the on-board computer or can be determined using information available to the on-board computer: quantity of diagnostic trouble codes, engine coolant temperature, fuel system status (e.g. closed-loop, open-loop), fuel trim, ignition timing advance, intake air temperature, intake manifold air pressure, air flow rate, engine speed (RPM), throttle position sensor output value, secondary air status (upstream, downstream or atmosphere), calculated load value, vehicle speed, fuel pressure, oxygen sensor and lambda sensor.

The signals shall be provided in standard units based on the specifications given in paragraph 6.5.3. of this appendix. Actual signals shall be clearly identified separately from default value or limp-home signals.

6.5.1.3. For all emission control systems for which specific on-board evaluation tests are conducted according to this annex (catalyst, oxygen sensor, etc.), except misfire detection, fuel system monitoring and comprehensive component monitoring, the results of the most recent test performed by the vehicle and the limits to which the system is compared shall be made available through the serial data port on the standardised data link connector according to the specifications given in paragraph 6.5.3. of this appendix. For the monitored components and systems excepted above, a pass/fail indication for the most recent test results shall be available through the data link connector.

All data required to be stored in relation to OBD in-use performance according to the provisions of paragraph 7.6. of this appendix shall be available through the serial data port on the standardized data link connector according to the specifications given in paragraph 6.5.3. of this appendix.

6.5.1.4. The OBD requirements to which the vehicle is certified and the major emission control systems monitored by the OBD system consistent with paragraph 6.5.3.3. of this appendix shall be available through the serial data port on the standardised data link connector according to the specifications given in paragraph 6.5.3. of this appendix.

6.5.1.5. For all types of vehicles entering into service, the software calibration identification number shall be made available through the serial port on the standardised data link connector. The software calibration identification number shall be provided in a standardised format.

6.5.2. The emission control diagnostic system is not required to evaluate components during malfunction if such evaluation would result in a risk to safety or component failure.

6.5.3. The emission control diagnostic system shall provide for standardised and unrestricted access and conform to the following ISO standards and/or SAE specification. Later versions may be used at the manufacturers' discretion.

6.5.3.1. The following standard shall be used as the on-board to off-board communications link:

(a) ISO 15765-4:2011 "Road vehicles – Diagnostics on Controller Area Network (CAN) – Part 4: Requirements for emissions-related systems", dated 1 February 2011.

6.5.3.2. Standards used for the transmission of OBD relevant information:

(a) ISO 15031-5 "Road vehicles - communication between vehicles and external test equipment for emissions-related diagnostics – Part 5: Emissions-related diagnostic services", dated 1 April 2011 or SAE J1979 dated 23 February 2012;

(b) ISO 15031-4 "Road vehicles – Communication between vehicle and external test equipment for emissions related diagnostics – Part 4: External test equipment", dated 1 June 2005 or SAE J1978 dated 30 April 2002;

(c) ISO 15031-3 "Road vehicles – Communication between vehicle and external test equipment for emissions related diagnostics Part 3: Diagnostic connector and related electrical circuits: specification and use", dated 1 July 2004 or SAE J 1962 dated 26 July 2012;

(d) ISO 15031-6 "Road vehicles – Communication between vehicle and external test equipment for emissions related diagnostics – Part 6: Diagnostic trouble code definitions", dated 13 August 2010 or SAE J2012 dated 07 March 2013;

(e) ISO 27145 "Road vehicles – Implementation of World-Wide Harmonized On-Board Diagnostics (WWH-OBD)" dated 2012-08-15 with the restriction, that only the standard specified in paragraph 6.5.3.1.(a) may be used as a data link;

(f) SAE J 1979-2 “E/E Diagnostic Test Modes: OBDonUDS”, April 2021.

The standards (e) or (f) may be used as an option instead of (a).

6.5.3.3. Test equipment and diagnostic tools needed to communicate with OBD systems shall meet or exceed the functional specification given in the standard listed in paragraph 6.5.3.2.(b) of this appendix.

6.5.3.4. Basic diagnostic data, (as specified in paragraph 6.5.1.) and bi-directional control information shall be provided using the format and units described in the standard listed in paragraph 6.5.3.2.(a) of this appendix and must be available using a diagnostic tool meeting the requirements of the standard listed in paragraph 6.5.3.2.(b) of this appendix.

The vehicle manufacturer shall provide to the responsible standardisation body the details of any emission-related diagnostic data, e.g. PIDs, OBD monitor IDs, Test IDs not specified in the standard listed in paragraph 6.5.3.2.(a) of this appendix but related to this Regulation.

6.5.3.5. When a fault is registered, the manufacturer shall identify the fault using an appropriate ISO/SAE controlled fault code specified in one of the standards listed in paragraph 6.5.3.2.(d) of this appendix relating to "emission related system diagnostic trouble codes". If such identification is not possible, the manufacturer may use manufacturer controlled diagnostic trouble codes according to the same standard. The fault codes shall be fully accessible by standardised diagnostic equipment complying with the provisions of paragraph 6.5.3.3. of this appendix.

6.5.3.6. The connection interface between the vehicle and the diagnostic tester shall be standardised and shall meet all the requirements of the standard listed in paragraph 6.5.3.2.(c) of this appendix. The installation position shall be subject to agreement of the administrative department such that it is readily accessible by service personnel but protected from tampering by non-qualified personnel.

7. In-use performance

7.1. General requirements

7.1.1. Each monitor of the OBD system shall be executed at least once per driving cycle in which the monitoring conditions as specified in paragraph 7.2. of this appendix are met. Manufacturers may not use the calculated ratio (or any element thereof) or any other indication of monitor frequency as a monitoring condition for any monitor.

7.1.2. The In-Use Performance Ratio (IUPR) of a specific monitor M of the OBD systems and in-use performance of pollution control devices shall be:

IUPRM = NumeratorM / DenominatorM

7.1.3. Comparison of numerator and denominator gives an indication of how often a specific monitor is operating relative to vehicle operation. To ensure all manufacturers are tracking IUPRM in the same manner, detailed requirements are given for defining and incrementing these counters.

7.1.4. If, according to the requirements of this annex, the vehicle is equipped with a specific monitor M, IUPRM shall be greater or equal to the following minimum values:

(a) 0.260 for secondary air system monitors and other cold start related monitors;

(b) 0.520 for evaporative emission purge control monitors;

(c) 0.336 for all other monitors.

7.1.5. Vehicles shall comply with the requirements of paragraph 7.1.4. of this appendix for a mileage of at least the target useful life, as defined in paragraph 6.7. of this Regulation.

7.1.6. The requirements of this paragraph are deemed to be met for a particular monitor M, if for all vehicles of a particular OBD family manufactured in a particular calendar year the following statistical conditions hold:

(a) The average IUPRM is equal or above the minimum value applicable to the monitor;

(b) More than 50 per cent of all vehicles have an IUPRM equal or above the minimum value applicable to the monitor.

7.2. NumeratorM

7.2.1. The numerator of a specific monitor is a counter measuring the number of times a vehicle has been operated such that all monitoring conditions necessary for the specific monitor to detect a malfunction in order to warn the driver, as they have been implemented by the manufacturer, have been encountered. The numerator shall not be incremented more than once per driving cycle, unless there is reasoned technical justification.

7.3. DenominatorM

7.3.1. The purpose of the denominator is to provide a counter indicating the number of vehicle driving events, taking into account special conditions for a specific monitor. The denominator shall be incremented at least once per driving cycle, if during this driving cycle such conditions are met and the general denominator is incremented as specified in paragraph 7.5. of this appendix unless the denominator is disabled according to paragraph 7.7. of this appendix.

7.3.2. In addition to the requirements of paragraph 7.3.1. of this appendix:

(a) Secondary air system monitor denominator(s) shall be incremented if the commanded "on" operation of the secondary air system occurs for a time greater than or equal to 10 seconds. For purposes of determining this commanded "on" time, the OBD system may not include time during intrusive operation of the secondary air system solely for the purposes of monitoring.

(b) Denominators of monitors of systems only active during cold start shall be incremented if the component or strategy is commanded "on" for a time greater than or equal to 10 seconds.

(c) The denominator(s) for monitors of Variable Valve Timing (VVT) and/or control systems shall be incremented if the component is commanded to function (e.g., commanded "on", "open", "closed", "locked", etc.) on two or more occasions during the driving cycle or for a time greater than or equal to 10 seconds, whichever occurs first.

(d) For the following monitors, the denominator(s) shall be incremented by one if, in addition to meeting the requirements of this paragraph on at least one driving cycle, at least 800 cumulative kilometres of vehicle operation have been experienced since the last time the denominator was incremented:

(i) Diesel oxidation catalyst;

(ii) Diesel particulate filter.

(e) Without prejudice to requirements for the increment of denominators of other monitors the denominators of monitors of the following components shall be incremented if and only if the driving cycle started with a cold start:

(i) Liquid (oil, engine coolant, fuel, SCR reagent) temperature sensors;

(ii) Clean air (ambient air, intake air, charge air, inlet manifold) temperature sensors;

(iii) Exhaust (EGR recirculation/cooling, exhaust gas turbo-charging, catalyst) temperature sensors;

(f) The denominators of monitors of the boost pressure control system shall be incremented if all of the following conditions are met:

(i) The general denominator conditions arc fulfilled;

(ii) The boost pressure control system is active for a time greater than or equal to 15 seconds.

(g) Manufacturers may request to use special denominator conditions for certain components or systems and this request can be approved only if it can be demonstrated to the Type Approval Authority by submitting data and/or an engineering evaluation that those other conditions are necessary to allow for reliable detection of malfunctions.

7.3.3. For hybrid vehicles, vehicles that employ alternative engine start hardware or strategies (e.g. integrated starter and generators), or alternative fuel vehicles (e.g. dedicated, bi-fuel, or dual-fuel applications), the manufacturer may request the approval of the Type Approval Authority to use alternative criteria to those set out in this paragraph for incrementing the denominator. In general, the Type Approval Authority shall not approve alternative criteria for vehicles that only employ engine shut off at or near idle/vehicle stop conditions. Approval by the Type Approval Authority of the alternative criteria shall be based on the equivalence of the alternative criteria to determine the amount of vehicle operation relative to the measure of conventional vehicle operation in accordance with the criteria in this paragraph.

7.4. Ignition cycle counter

7.4.1. The ignition cycle counter indicates the number of ignition cycles a vehicle has experienced. The ignition cycle counter may not be incremented more than once per driving cycle.

7.5. General denominator

7.5.1. The general denominator is a counter measuring the number of times a vehicle has been operated. It shall be incremented within 10 seconds, if and only if, the following criteria are satisfied on a single driving cycle:

(a) Cumulative time since engine start is greater than or equal to 600 seconds while at an elevation of less than 2,440 m above sea level and at an ambient temperature of greater than or equal to -7 °C;

(b) Cumulative vehicle operation at or above 40 km/h occurs for greater than or equal to 300 seconds while at an elevation of less than 2,440 m above sea level and at an ambient temperature of greater than or equal to -7 °C;

(c) Continuous vehicle operation at idle (i.e. accelerator pedal released by driver and vehicle speed less than or equal to 1.6 km/h) for greater than or equal to 30 seconds while at an elevation of less than 2,440 m above sea level and at an ambient temperature of greater than or equal to -7 °C.

7.6. Reporting and increasing counters

7.6.1. The OBD system shall report, in accordance with the ISO 15031-5 specifications of the standard listed in paragraph 6.5.3.2.(a) of this appendix**,** the ignition cycle counter and general denominator as well as separate numerators and denominators for the following monitors, if their presence on the vehicle is required by this annex:

(a) Catalysts (each bank to be reported separately);

(b) Oxygen/exhaust gas sensors, including secondary oxygen sensors (each sensor to be reported separately);

(c) Evaporative system;

(d) EGR system;

(e) VVT system;

(f) Secondary air system;

(g) Particulate filter;

(h) NOx after-treatment system (e.g. NOx adsorber, NOx reagent/catalyst system);

(i) Boost pressure control system.

7.6.2. For specific components or systems that have multiple monitors, which are required to be reported by this point (e.g. oxygen sensor bank 1 may have multiple monitors for sensor response or other sensor characteristics), the OBD system shall separately track numerators and denominators for each of the specific monitors and report only the corresponding numerator and denominator for the specific monitor that has the lowest numerical ratio. If two or more specific monitors have identical ratios, the corresponding numerator and denominator for the specific monitor that has the highest denominator shall be reported for the specific component.

7.6.2.1. Numerators and denominators for specific monitors of components or systems, that are monitoring continuously for short circuit or open circuit failures are exempted from reporting.

"Continuously", if used in this context means monitoring is always enabled and sampling of the signal used for monitoring occurs at a rate no less than two samples per second and the presence or the absence of the failure relevant to that monitor has to be concluded within 15 seconds.

If for control purposes, a computer input component is sampled less frequently, the signal of the component may instead be evaluated each time sampling occurs.

It is not required to activate an output component/system for the sole purpose of monitoring that output component/system.

7.6.3. All counters, when incremented, shall be incremented by an integer of one.

7.6.4. The minimum value of each counter is 0, the maximum value shall not be less than 65,535, notwithstanding any other requirements on standardised storage and reporting of the OBD system.

7.6.5. If either the numerator or denominator for a specific monitor reaches its maximum value, both counters for that specific monitor shall be divided by two before being incremented again according to the provisions set in paragraphs 7.2. and 7.3. of this appendix. If the ignition cycle counter or the general denominator reaches its maximum value, the respective counter shall change to zero at its next increment according to the provisions set in paragraphs 7.4. and 7.5. of this appendix, respectively.

7.6.6. Each counter shall be reset to zero only when a non-volatile memory reset occurs (e.g. reprogramming event, etc.) or, if the numbers are stored in keep-alive memory (KAM), when KAM is lost due to an interruption in electrical power to the control module (e.g. battery disconnect, etc.).

7.6.7. The manufacturer shall take measures to ensure that the values of numerator and denominator cannot be reset or modified, except in cases provided for explicitly in this paragraph.

7.7. Disablement of numerators and denominators and of the general denominator

7.7.1. Within 10 seconds of a malfunction being detected, which disables a monitor required to meet the monitoring conditions of this annex (i.e. a pending or confirmed code is stored), the OBD system shall disable further incrementing of the corresponding numerator and denominator for each monitor that is disabled. When the malfunction is no longer detected (i.e., the pending code is erased through self-clearing or through a scan tool command), incrementing of all corresponding numerators and denominators shall resume within 10 seconds.

7.7.2. Within 10 seconds of the start of a Power Take-off Operation (PTO) that disables a monitor required to meet the monitoring conditions of this annex, the OBD system shall disable further incrementing of the corresponding numerator and denominator for each monitor that is disabled. When the PTO operation ends, incrementing of all corresponding numerators and denominators shall resume within 10 seconds.

7.7.3. The OBD system shall disable further incrementing of the numerator and denominator of a specific monitor within 10 seconds, if a malfunction of any component used to determine the criteria within the definition of the specific monitor's denominator (i.e. vehicle speed, ambient temperature, elevation, idle operation, engine cold start, or time of operation) has been detected and the corresponding pending fault code has been stored. Incrementing of the numerator and denominator shall resume within 10 seconds when the malfunction is no longer present (e.g. pending code erased through self-clearing or by a scan tool command).

7.7.4. The OBD system shall disable further incrementing of the general denominator within 10 seconds, if a malfunction has been detected of any component used to determine whether the criteria in paragraph 7.5. of this appendix are satisfied (i.e. vehicle speed, ambient temperature, elevation, idle operation, or time of operation) and the corresponding pending fault code has been stored. The general denominator may not be disabled from incrementing for any other condition. Incrementing of the general denominator shall resume within 10 seconds when the malfunction is no longer present (e.g. pending code erased through self-clearing or by a scan tool command).

**II. Justification**

1. The proposal incorporates corrections, clarifications and improvements to both series of amendments to UN Regulation No. 154 that have already been introduced in the 02 and 03 series of amendments to UN Regulation No. 154.
2. The proposal is based on ECE/TRANS/WP.29/GRPE/2024/3 and includes few additional proposals listed below:
   * GRPE-90-11-Rev.1: Proposal for Transitional Provisions regarding Supplement 2 for original and 01 series of amendments to UN Regulation No.154;
   * GRPE-91-11: only page 9 dealing with PEV run-in requirement.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2025 as outlined in proposed programme budget for 2025 (A/79/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. Page number will be updated prior to submission to WP.29 [↑](#footnote-ref-3)
3. The distinguishing numbers of the Contracting Parties to the 1958 Agreement are reproduced in Annex 3 to the Consolidated Resolution on the Construction of Vehicles (R.E.3), document ECE/TRANS/WP.29/78/Rev.6 – Annex 3 https://unece.org/transport/standards/transport/vehicle-regulations-wp29/resolutions. [↑](#footnote-ref-4)
4. Distinguishing number of the country which has granted/extended/refused/withdrawn approval (see approval provisions in the regulation). [↑](#footnote-ref-5)
5. Strike out what does not apply. [↑](#footnote-ref-6)
6. If the means of identification of type contains characters not relevant to describe the vehicle, component or separate technical unit types covered by this information document, such characters shall be represented in the documentation by the symbol '?' (e.g. ABC??123??). [↑](#footnote-ref-7)
7. As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.6, paragraph 2. - <https://unece.org/transport/vehicle-regulations/wp29/resolutions>. [↑](#footnote-ref-8)
8. Type of tyre according UN Regulation No. 117 [↑](#footnote-ref-9)
9. Where applicable. [↑](#footnote-ref-10)
10. Round to two decimal numbers. [↑](#footnote-ref-11)
11. For vehicles equipped with positive-ignition engines. [↑](#footnote-ref-12)
12. For compression-ignition engine vehicles. [↑](#footnote-ref-13)
13. Delete where not applicable (there are cases where nothing needs to be deleted when more than one entry is applicable) [↑](#footnote-ref-14)
14. Measured over the combined cycle [↑](#footnote-ref-15)
15. Measured over the combined cycle [↑](#footnote-ref-16)
16. Number of country according to footnote in paragraph 5.4.1. of this Regulation. [↑](#footnote-ref-17)
17. https://unece.org/transport/standards/transport/vehicleregulations-wp29/global-technical-regulations-gtrs?accordion=15 [↑](#footnote-ref-18)
18. Date to be replaced by the date of entry into force of this proposal when known [↑](#footnote-ref-19)