Proposal for a supplement to the original series of amendments to UN Regulation No. [175] (Acceleration Control for Pedal Error)

The text reproduced below is based on ECE/TRANS/WP.29/2024/154 and includes the amendments, marked in red below.

I. Proposal

*Paragraph 5.1.4.,* amend to read:

* + 1. The ACPE shall control acceleration when the vehicle is accelerated from standstill.

**5.1.4.1 If ACPE is not ready to perform an intervention 6 s after the initiation of the vehicle powertrain, information of this status shall be indicated to the driver. This information shall exist until the system has been successfully initialised.**

II. Justification

00 series text is not mentioned initialization, and this proposal aligns with the 01 series amendment.

\_\_\_\_\_\_\_\_\_\_\_