|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2024/129 |
| _unlogo | **Economic and Social Council** | Distr.: General27 August 2024Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**194th session**

Geneva, 12–15 November 2024

Item 4.8.12 of the provisional agenda

**1958 Agreement:**

**Consideration of draft amendments to existing**

**UN Regulations submitted by GRSP**

Proposal for Supplement 2 to the Original Version of UN Regulation No. 32 (Rear-end collision)

 Submitted by the Working Party on Passive Safety[[1]](#footnote-2)\*

 The text reproduced below was adopted by the Working Party on Passive Safety (GRSP) at its seventy-fifth session (ECE/TRANS/WP.29/GRSP/75, para. 30). It is based on ECE/TRANS/WP.29/GRSP/2024/7 as amended by annex VII to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2024 sessions.

*Paragraph 1., footnote 1,* amend to read:

"1 As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.**7**, para. 2 -
[**https://unece.org/transport/vehicle-regulations/wp29/resolutions**](https://unece.org/transport/vehicle-regulations/wp29/resolutions)"

*Paragraph 4.4.1.1., footnote 2,* amend to read:

"2 The distinguishing numbers of the Contracting Parties to the 1958 Agreement are reproduced in Annex 3 to the Consolidated Resolution on the Construction of Vehicles (R.E.3), document ECE/TRANS/WP.29/78/Rev.7, Annex 3 -
[**https://unece.org/transport/vehicle-regulations/wp29/resolutions**](https://unece.org/transport/vehicle-regulations/wp29/resolutions)"

*Annex 3,* shall be deleted

*Insert new Annex 3,*  to read:

"Annex 3

 Procedure for determining the "H" point and the actual torso angle for seating positions in motor vehicles1

 Appendix 1 - Description of the three dimensional "H" point machine1

 Appendix 2 - Three-dimensional reference system1

 Appendix 3 - Reference data concerning seating positions1

**1** The procedure is described in Addendum 6 of Mutual Resolution No. 1 (M.R.1)
(document ECE/TRANS/WP.29/1101/Amend.5);
see <https://unece.org/transport/vehicle-regulations/wp29/resolutions>"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2024 as outlined in proposed programme budget for 2024 (A/78/6 (Sect. 20), table 20.5), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)