|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2025/95 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  27 August 2025  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**197th session**

Geneva, 11–14 November 2025

Item 4.6.3 of the provisional agenda

**1958 Agreement:**

**Consideration of draft amendments to existing**

**UN Regulations submitted by GRPE**

Supplement 19 to the 05 series of amendments to UN Regulation No. 83

Submitted by the Working Party on Pollution and Energy[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Pollution and Energy (GRPE) at its ninety-second session (ECE/TRANS/WP.29/GRSP/92, para. 13). It is based on ECE/TRANS/WP.29/GRPE/2025/8 as amended by Annex IV of the session report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2025 sessions.

*Annex 8, Paragraph 5.2.6.*, amendto read:

"5.2.6. The time between dynamometer warming and the start of the emission test shall be no longer than 10 minutes if the dynamometer bearings are not independently heated. If the dynamometer bearings are independently heated, the emission test shall begin no longer than 20 minutes after dynamometer warming.

If frictional losses of the dynamometer can be stabilized without warming the dynamometer, the test can start following the dynamometer manufacturer’s recommendations. The manufacturer shall provide documentation on the validation of the systems upon request of the responsible authority."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2025 as outlined in proposed programme budget for 2025 (A/79/6 (Sect. 20), table 20.6), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)